(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 142)
    (no_connects 0)
    (area 101.924999 12.637439 171.635202 141.075001)
    (thickness 1.6)
    (drawings 4)
    (tracks 810)
    (zones 0)
    (modules 56)
    (nets 89)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.43)
    (user_trace_width 0.43)
    (user_trace_width 0.46)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (trace_clearance 0.01)
    (zone_clearance 0.096)
    (zone_45_only yes)
    (trace_min 0.25)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.5 0.8)
    (user_via 1.75 0.8)
    (user_via 2 0.8)
    (user_via 2.25 0.8)
    (user_via 2.5 0.8)
    (user_via 2.75 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 0.38)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /vcc1)
  (net 2 "Net-(1N4007-Pad2)")
  (net 3 /SDA)
  (net 4 /SCL)
  (net 5 "Net-(10k1-Pad1)")
  (net 6 /RelayTrig)
  (net 7 /RST)
  (net 8 GND)
  (net 9 "Net-(100k1-Pad1)")
  (net 10 /Vin)
  (net 11 "Net-(BZ1-Pad2)")
  (net 12 /gsmTX)
  (net 13 /gsmRX)
  (net 14 +12V)
  (net 15 /rel2)
  (net 16 /rel1)
  (net 17 /SensPin)
  (net 18 "Net-(K1-Pad3)")
  (net 19 "Net-(Q3-Pad2)")
  (net 20 /buzzer)
  (net 21 "Net-(U1-Pad19)")
  (net 22 "Net-(U1-Pad23)")
  (net 23 "Net-(U1-Pad24)")
  (net 24 "Net-(U1-Pad25)")
  (net 25 "Net-(U1-Pad26)")
  (net 26 "Net-(U1-Pad13)")
  (net 27 "Net-(C1-Pad2)")
  (net 28 "Net-(C2-Pad2)")
  (net 29 "Net-(C4-Pad2)")
  (net 30 "Net-(C5-Pad2)")
  (net 31 /SS)
  (net 32 /SCK)
  (net 33 /MOSI)
  (net 34 /MISO)
  (net 35 /RESET)
  (net 36 /RX_m)
  (net 37 /TX_m)
  (net 38 "Net-(J4-Pad3)")
  (net 39 "Net-(J5-Pad2)")
  (net 40 /RX_s)
  (net 41 /TX_s)
  (net 42 "Net-(U1-Pad2)")
  (net 43 "Net-(U1-Pad9)")
  (net 44 "Net-(U1-Pad20)")
  (net 45 "Net-(U1-Pad22)")
  (net 46 "Net-(U2-Pad9)")
  (net 47 "Net-(U2-Pad10)")
  (net 48 "Net-(U2-Pad11)")
  (net 49 "Net-(U2-Pad12)")
  (net 50 "Net-(U2-Pad13)")
  (net 51 "Net-(U2-Pad14)")
  (net 52 "Net-(U2-Pad15)")
  (net 53 "Net-(U2-Pad16)")
  (net 54 "Net-(U2-Pad17)")
  (net 55 "Net-(U2-Pad19)")
  (net 56 "Net-(U2-Pad20)")
  (net 57 "Net-(U2-Pad22)")
  (net 58 "Net-(U2-Pad23)")
  (net 59 "Net-(U2-Pad24)")
  (net 60 "Net-(U2-Pad25)")
  (net 61 "Net-(U2-Pad26)")
  (net 62 /+5V)
  (net 63 "Net-(J5-Pad3)")
  (net 64 "Net-(J5-Pad6)")
  (net 65 "Net-(J5-Pad8)")
  (net 66 "Net-(J5-Pad9)")
  (net 67 "Net-(J5-Pad10)")
  (net 68 "Net-(J5-Pad11)")
  (net 69 "Net-(J5-Pad12)")
  (net 70 "Net-(J5-Pad13)")
  (net 71 "Net-(J5-Pad14)")
  (net 72 /D+)
  (net 73 /D-)
  (net 74 "Net-(J5-Pad17)")
  (net 75 "Net-(J5-Pad19)")
  (net 76 "Net-(J5-Pad22)")
  (net 77 "Net-(J5-Pad23)")
  (net 78 "Net-(J5-Pad24)")
  (net 79 "Net-(J5-Pad27)")
  (net 80 "Net-(J5-Pad28)")
  (net 81 /vcc)
  (net 82 /EngOn)
  (net 83 "Net-(F1-Pad1)")
  (net 84 /Ignition)
  (net 85 /printTrig)
  (net 86 "Net-(R2-Pad2)")
  (net 87 /TrigPin)
  (net 88 "Net-(R4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.01)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /+5V)
    (add_net /D+)
    (add_net /D-)
    (add_net /EngOn)
    (add_net /Ignition)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RST)
    (add_net /RX_m)
    (add_net /RX_s)
    (add_net /RelayTrig)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SS)
    (add_net /SensPin)
    (add_net /TX_m)
    (add_net /TX_s)
    (add_net /TrigPin)
    (add_net /Vin)
    (add_net /buzzer)
    (add_net /gsmRX)
    (add_net /gsmTX)
    (add_net /printTrig)
    (add_net /rel1)
    (add_net /rel2)
    (add_net /vcc)
    (add_net /vcc1)
    (add_net GND)
    (add_net "Net-(100k1-Pad1)")
    (add_net "Net-(10k1-Pad1)")
    (add_net "Net-(1N4007-Pad2)")
    (add_net "Net-(BZ1-Pad2)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad11)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad13)")
    (add_net "Net-(J5-Pad14)")
    (add_net "Net-(J5-Pad17)")
    (add_net "Net-(J5-Pad19)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad22)")
    (add_net "Net-(J5-Pad23)")
    (add_net "Net-(J5-Pad24)")
    (add_net "Net-(J5-Pad27)")
    (add_net "Net-(J5-Pad28)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad9)")
  )
  (module Diodes_THT:D_5KP_P10.16mm_Horizontal (layer F.Cu) (tedit 5BF4F5CC)
    (at 142.113 125.857 270)
    (descr "D, 5KP series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.62*9.53mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
    (tags "D 5KP series Axial Horizontal pin pitch 10.16mm  length 7.62mm diameter 9.53mm")
    (fp_text reference 1N4007 (at 5.08 -5.825 270) (layer F.SilkS))
    (fp_text value D (at 5.08 5.825 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 /vcc1))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(1N4007-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_5KP_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BF4F5E7)
    (at 113 59 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 10k2 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /RST))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5BF4F489)
    (at 117.094 118.364 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 10uF2 (at 1.25 -3.81 270) (layer F.SilkS))
    (fp_text value CP (at 1.25 3.81 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /vcc1))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 5C02ADA3)
    (at 149.86 63.754 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 -6.05 90) (layer F.SilkS))
    (fp_text value SLAVE (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.46) (layers F.Cu F.Paste F.Mask)
      (net 87 /TrigPin))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 6 /RelayTrig))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.46) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.46) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C5-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U2-Pad15)"))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U2-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U2-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U2-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U2-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /RESET))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 /RX_m))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 /TX_m))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 20 /buzzer))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C0298E2)
    (at 121.412 47.117)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 4.7k1 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SDA))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029902)
    (at 121.412 51.181)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 4.7k2 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SCL))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029B76)
    (at 125.095 97.155)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 10k1 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(10k1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /RelayTrig))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029A8B)
    (at 107.061 71.628 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 10uF1 (at 1.25 -3.81 180) (layer F.SilkS))
    (fp_text value CP (at 1.25 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.9 1.9) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BF4F785)
    (at 135.5852 115.1128 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 100k1 (at 5.08 -2.31 180) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(100k1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029C20)
    (at 104.775 133.985)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 100uF1 (at 1.25 -3.81) (layer F.SilkS))
    (fp_text value CP (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /Vin))
    (pad 2 thru_hole circle (at 2.5 0) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029ABD)
    (at 107.061 85.09 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 100uF2 (at 1.25 -3.81 180) (layer F.SilkS))
    (fp_text value CP (at 1.25 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.9 1.9) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Vin))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_5KP_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029CCF)
    (at 152.146 108.585 270)
    (descr "D, 5KP series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.62*9.53mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
    (tags "D 5KP series Axial Horizontal pin pitch 10.16mm  length 7.62mm diameter 9.53mm")
    (fp_text reference D1 (at 5.08 -5.825 270) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 5.825 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.8 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Vin))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.8 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(100k1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_5KP_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-4pol (layer F.Cu) (tedit 5C02931F)
    (at 164.1856 87.122 90)
    (descr "4-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J1 (at 7.7724 3.4544 180) (layer F.SilkS))
    (fp_text value ToGSM (at 7.5 -6.6 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 15 0 90) (size 2.8 2.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 /gsmTX))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.8 2.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 /gsmRX))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.8 2.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 /vcc1))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.8 2.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-4pol.wrl
      (at (xyz 0.2953 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "governor:8 pin connector 2x4" (layer F.Cu) (tedit 5C029347)
    (at 132.5372 133.4516 90)
    (fp_text reference J4 (at 0 -21 90) (layer F.SilkS))
    (fp_text value "OUTPUT CONNECTOR" (at 0.12192 -10.55116 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -3 -17 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 +12V))
    (pad 4 thru_hole circle (at -3 -4 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 /rel2))
    (pad 5 thru_hole circle (at 3 -4 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 /rel1))
    (pad 8 thru_hole circle (at 3 -17 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole circle (at -3 -12.8 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 /Ignition))
    (pad 3 thru_hole circle (at -3 -8.2 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad3)"))
    (pad 7 thru_hole circle (at 3 -12.8 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 6 thru_hole circle (at 3 -8.2 90) (size 3.5 3.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 /SensPin))
  )
  (module Relays_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 5C029C7D)
    (at 149.606 130.81)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K1 (at 8.1 9.2) (layer F.SilkS))
    (fp_text value SANYOU_SRD_Form_C (at 9.81964 0.06096) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.6 2.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(1N4007-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(K1-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 /rel2))
    (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.8 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 /vcc1))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 /rel1))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5BF4F7A0)
    (at 117.602 105.791 270)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -3.56 450) (layer F.SilkS))
    (fp_text value Q_NPN_EBC (at 2.54 2.79 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 450) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(10k1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(1N4007-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5BF969DD)
    (at 144.78508 39.73068)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value buzzerTransistor (at 2.22 -3.084 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(BZ1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029EFD)
    (at 147.29968 45.8216 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(Q3-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 20 /buzzer))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Horizontal (layer F.Cu) (tedit 5BF4F468)
    (at 106.00436 118.24208)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (fp_text reference RelayPower1 (at 2.54 -20.58) (layer F.SilkS))
    (fp_text value L7812 (at 2.54 1.9) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58) (layer F.Fab))
    (pad 0 np_thru_hole oval (at 2.54 -16.66) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Vin))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /vcc1))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistors:RV_Disc_D9_W5.7_P5 (layer F.Cu) (tedit 5C029CB8)
    (at 141.097 119.761 90)
    (tags "varistor SIOV")
    (fp_text reference RV1 (at 2.5 5.35 90) (layer F.SilkS))
    (fp_text value MOV (at 2.5 -2.35 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5 3 90) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module TO_SOT_Packages_THT:TO-220_Horizontal (layer F.Cu) (tedit 5C029CA0)
    (at 160.528 119.253)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -20.58) (layer F.SilkS))
    (fp_text value Q_PMOS_GDS (at 2.54 1.9) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58) (layer F.Fab))
    (pad 0 np_thru_hole oval (at 2.54 -16.66) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(100k1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(F1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Vin))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buzzers_Beepers:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 5C029FA4)
    (at 161.163 46.736 90)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ1 (at 3.8 -7.2 90) (layer F.SilkS))
    (fp_text value Buzzer (at 3.8 7.4 90) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 90) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 90) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /vcc1))
    (pad 2 thru_hole circle (at 7.6 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(BZ1-Pad2)"))
    (model ${KISYS3DMOD}/Buzzers_Beepers.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C0299B3)
    (at 114.681 65.532 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -3.81 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.25 3.81 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.9 1.9) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.9 1.9) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029AE8)
    (at 113.665 89.535 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 -3.81 90) (layer F.SilkS))
    (fp_text value C_Small (at 1.25 3.81 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 159.9692 64.262 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 1.25 -3.81 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.25 3.81 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 159.9692 57.2516 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C5 (at 1.25 -3.81 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.25 3.81 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C029BCD)
    (at 125.603 101.727 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "SD PORT" (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 34 /MISO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 33 /MOSI))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 32 /SCK))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 31 /SS))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 5C02AD36)
    (at 129.9464 81.0768)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 -6.05) (layer F.SilkS))
    (fp_text value MASTER (at 0 6.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad e1 smd rect (at -4.25 -2.8) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.47) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.46) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.47) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C2-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 12 /gsmTX))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 13 /gsmRX))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 85 /printTrig))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 31 /SS))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask)
      (net 34 /MISO))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.47) (layers F.Cu F.Paste F.Mask)
      (net 32 /SCK))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad20)"))
    (pad e21 smd rect (at 4.25 -0.4) (size 1.6 0.49) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 40 /RX_s))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.38) (layers F.Cu F.Paste F.Mask)
      (net 41 /TX_s))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 82 /EngOn))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-4H_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 114.681 74.549 270)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 2.44 -3.525 270) (layer F.SilkS))
    (fp_text value Crystal (at 2.44 3.525 270) (layer F.Fab))
    (fp_text user %R (at 2.44 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 4.88 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-4H_Vertical (layer F.Cu) (tedit 5BF95DDB)
    (at 166.1668 64.5668 90)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y2 (at 2.44 -3.525 90) (layer F.SilkS))
    (fp_text value Crystal (at 2.44 3.525 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 130.048 57.912 270)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value FTDI (at 0 12.49 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /RESET))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /RX_m))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /TX_m))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029B16)
    (at 104.648 93.98)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C7 (at 1.25 -3.81) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.9 1.9) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Vin))
    (pad 2 thru_hole circle (at 2.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029C13)
    (at 104.902 124.587)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C8 (at 1.25 -3.81) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /Vin))
    (pad 2 thru_hole circle (at 2.5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029A7D)
    (at 107.061 78.486 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C9 (at 1.25 -3.81 180) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.9 1.9) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.9 1.9) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W5.0mm_P5.00mm (layer F.Cu) (tedit 5C029651)
    (at 149.733 31.242 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 5.0mm Capacitor")
    (fp_text reference C10 (at 2.5 -3.81 180) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 3.81 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 62 /+5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C02961B)
    (at 127.127 33.528 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C12 (at 1.25 -3.81 90) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.81 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 5C02A70D)
    (at 109.2454 37.37102 90)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference J5 (at -0.18034 -3.85572 180) (layer F.SilkS))
    (fp_text value FT232R (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at -0.12446 4.22148 180) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 /RX_s))
    (pad 2 smd rect (at -3.6 -3.575 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J5-Pad2)"))
    (pad 3 smd rect (at -3.6 -2.925 90) (size 1.75 0.38) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J5-Pad3)"))
    (pad 4 smd rect (at -3.6 -2.275 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 5 smd rect (at -3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 /TX_s))
    (pad 6 smd rect (at -3.6 -0.975 90) (size 1.75 0.38) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(J5-Pad6)"))
    (pad 7 smd rect (at -3.6 -0.325 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at -3.6 0.325 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J5-Pad8)"))
    (pad 9 smd rect (at -3.6 0.975 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J5-Pad9)"))
    (pad 10 smd rect (at -3.6 1.625 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J5-Pad10)"))
    (pad 11 smd rect (at -3.6 2.275 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J5-Pad11)"))
    (pad 12 smd rect (at -3.6 2.925 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J5-Pad12)"))
    (pad 13 smd rect (at -3.6 3.575 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J5-Pad13)"))
    (pad 14 smd rect (at -3.6 4.225 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J5-Pad14)"))
    (pad 0.41 smd rect (at 3.6 4.225 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 /D+))
    (pad 0.41 smd rect (at 3.6 3.575 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 73 /D-))
    (pad 17 smd rect (at 3.6 2.925 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J5-Pad17)"))
    (pad 18 smd rect (at 3.6 2.275 90) (size 1.75 0.38) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 3.6 1.625 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(J5-Pad19)"))
    (pad 20 smd rect (at 3.6 0.975 90) (size 1.75 0.38) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 21 smd rect (at 3.6 0.325 90) (size 1.75 0.38) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 22 smd rect (at 3.6 -0.325 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(J5-Pad22)"))
    (pad 23 smd rect (at 3.6 -0.975 90) (size 1.75 0.38) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(J5-Pad23)"))
    (pad 24 smd rect (at 3.6 -1.625 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(J5-Pad24)"))
    (pad 25 smd rect (at 3.6 -2.275 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 26 smd rect (at 3.6 -2.925 90) (size 1.75 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 27 smd rect (at 3.6 -3.575 90) (size 1.75 0.36) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(J5-Pad27)"))
    (pad 28 smd rect (at 3.6 -4.225 90) (size 1.75 0.38) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(J5-Pad28)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_A (layer F.Cu) (tedit 5C029860)
    (at 115.61572 25.87244 180)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J6 (at 0 -2.35 180) (layer F.SilkS))
    (fp_text value "USB A" (at 3.12928 4.13512 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.11 0 90) (size 2.2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole oval (at 4.57 0 90) (size 2.2 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 72 /D+))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 73 /D-))
    (pad 1 thru_hole oval (at 0 0 90) (size 2 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 62 /+5V))
    (pad 5 thru_hole circle (at 10.16 2.67 90) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -3.56 2.67 90) (size 3.3 3.3) (drill 2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:USB_B (layer F.Cu) (tedit 5C029F82)
    (at 161 28 90)
    (descr "USB B connector")
    (tags "USB_B USB_DEV")
    (fp_text reference J7 (at 11.05 1.27 180) (layer F.SilkS))
    (fp_text value "USB B" (at 4.7 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 2 1.42) (drill 0.81) (layers *.Cu *.Mask)
      (net 73 /D-))
    (pad 1 thru_hole oval (at 0 0) (size 2 1.6) (drill 0.81) (layers *.Cu *.Mask)
      (net 62 /+5V))
    (pad 4 thru_hole oval (at 2 0) (size 2 1.6) (drill 0.81) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole circle (at 2 2.54) (size 2 2) (drill 0.81) (layers *.Cu *.Mask)
      (net 72 /D+))
    (pad 5 thru_hole circle (at 4.7 7.27) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 4.7 -4.73) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_B.wrl
      (at (xyz 0.18 -0.05 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Inductors_THT:L_Axial_L9.5mm_D4.0mm_P12.70mm_Horizontal_Fastron_SMCC (layer F.Cu) (tedit 5C0298A7)
    (at 119.634 39.37)
    (descr "L, Axial series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.5*4mm^2, Fastron, SMCC, http://cdn-reichelt.de/documents/datenblatt/B400/DS_SMCC_NEU.pdf, http://cdn-reichelt.de/documents/datenblatt/B400/LEADEDINDUCTORS.pdf")
    (tags "L Axial series Axial Horizontal pin pitch 12.7mm  length 9.5mm diameter 4mm Fastron SMCC")
    (fp_text reference L1 (at 6.35 -3.06) (layer F.SilkS))
    (fp_text value L (at 6.35 3.06) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 62 /+5V))
    (pad 2 thru_hole oval (at 12.7 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (model Inductors_THT.3dshapes/L_Axial_L9.5mm_D4.0mm_P12.70mm_Horizontal_Fastron_SMCC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C029637)
    (at 138.303 32.131 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C11 (at 1.25 -3.81 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029912)
    (at 116.586 54.102 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 10k3 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 35 /RESET))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W5.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 124.1044 108.1532)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 5.0mm Capacitor")
    (fp_text reference C13 (at 2.5 -3.81) (layer F.SilkS))
    (fp_text value 0.1nF (at 2.5 3.81) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistors:RV_Disc_D9_W5.7_P5 (layer F.Cu) (tedit 5529CAF8)
    (at 135.636 122.428 180)
    (tags "varistor SIOV")
    (fp_text reference F1 (at 2.5 5.35 180) (layer F.SilkS))
    (fp_text value Polyfuse (at 2.5 -2.35 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 83 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5 3 180) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 +12V))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 5C029B44)
    (at 117.094 97.663)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J8 (at 1.27 -4.50088) (layer F.SilkS))
    (fp_text value Switch (at 1.27 4.50088) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 85 /printTrig))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029D50)
    (at 142.15872 89.408)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SensPin))
    (pad 2 thru_hole oval (at 10.16 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029CEC)
    (at 144.018 105.029 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 /TrigPin))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029FE3)
    (at 138.41476 89.01684 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 84 /Ignition))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029B31)
    (at 119.9896 82.1944 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 82 /EngOn))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C029FBF)
    (at 125.222 92.329)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 85 /printTrig))
    (pad 2 thru_hole oval (at 10.16 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 5C0292D8)
    (at 107 51 90)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW1 (at -0.09464 -0.2438 180) (layer F.SilkS))
    (fp_text value SW_DIP_x01 (at 0 4.15 90) (layer F.Fab))
    (fp_text user %R (at -0.07432 -0.15744 180) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
    (pad 1 smd rect (at -3.98 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 3.98 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 3.98 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 5C029D1C)
    (at 148.463 97.155)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value EL817C (at 3.81 4.93) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(R2-Pad2)"))
    (pad 3 thru_hole oval (at 7.62 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 /TrigPin))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 5C029FEA)
    (at 136.57072 72.14108)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value EL817C (at 3.81 4.93) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(R4-Pad2)"))
    (pad 3 thru_hole oval (at 7.62 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 82 /EngOn))
    (pad 2 thru_hole oval (at 0 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2 (layer F.Cu) (tedit 5C029280)
    (at 107 61 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U5 (at 0.59372 -1.88972 180) (layer F.SilkS))
    (fp_text value AMS1117 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 81 /vcc))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vin))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W5.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 162.179 94.361)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 5.0mm Capacitor")
    (fp_text reference C3 (at 2.5 -3.81) (layer F.SilkS))
    (fp_text value 0.1nF (at 2.5 3.81) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 81 /vcc))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W5.0mm_P5.00mm (layer F.Cu) (tedit 5C0299BE)
    (at 126.238 65.024 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 5.0mm Capacitor")
    (fp_text reference C6 (at 2.5 -3.81 180) (layer F.SilkS))
    (fp_text value 0.1nF (at 2.5 3.81 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 82 /EngOn))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 102 20) (end 102 141) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171 20) (end 102 20) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171 141) (end 171 20) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 141) (end 171 141) (angle 90) (layer Edge.Cuts) (width 0.15))
)
