| Nordic Thingy:52 v2.0.0

Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - a -

- active_time_ms : drv_ext_light_status_t
- adc_pin_no : batt_meas_param_t
- adc_pin_no_ain : batt_meas_param_t
- adv_param_handles : ble_tcs_s
- app_timer_prescaler : batt_meas_param_t

### - b -

- b : drv_ext_light_conf_t , drv_ext_light_rgb_intensity_t
- batt_chg_stat_pin_no : batt_meas_param_t
- batt_meas_param : batt_meas_init_t
- batt_mon_en_pin_no : batt_meas_param_t
- batt_mon_en_pin_used : batt_meas_param_t
- batt_voltage_limit_full : batt_meas_param_t
- batt_voltage_limit_low : batt_meas_param_t
- button_char_handles : ble_uis_s

### - c -

- clkx_div : drv_ext_light_init_t
- color : drv_ext_light_rgb_sequence_t
- color_handles : ble_tes_s
- colors : drv_ext_light_status_t
- config_handles : ble_tes_s , ble_tms_s , ble_tss_s
- conn_handle : ble_tcs_s , ble_tes_s , ble_tms_s , ble_tss_s , ble_uis_s
- conn_param_handles : ble_tcs_s
- cpu_wake_pin : drv_acc_cfg_t

### - d -

- data_handler : drv_gas_init_t
- delta_mv : state_of_charge_t
- dev_name_handles : ble_tcs_s

### - e -

- ec02_ppm : drv_ccs811_alg_result_t
- err_id : drv_ccs811_alg_result_t
- euler_handles : ble_tms_s
- evt_handler : batt_meas_init_t , ble_tcs_init_t , ble_tcs_s , ble_tes_init_t , ble_tes_s , ble_tms_init_t , ble_tms_s , ble_tss_init_t , ble_tss_s , drv_pressure_init_t

### - f -

- first_element_mv : state_of_charge_t

### - g -

- g : drv_ext_light_conf_t , drv_ext_light_rgb_intensity_t
- gas_handles : ble_tes_s
- gravity_handles : ble_tms_s

### - h -

- heading_handles : ble_tms_s
- humidity_handles : ble_tes_s

### - i -

- inactive_time_ms : drv_ext_light_status_t
- ioext_osc_status : drv_ext_light_status_t
- is_color_notif_enabled : ble_tes_s
- is_euler_notif_enabled : ble_tms_s
- is_gas_notif_enabled : ble_tes_s
- is_gravity_notif_enabled : ble_tms_s
- is_heading_notif_enabled : ble_tms_s
- is_humidity_notif_enabled : ble_tes_s
- is_mic_notif_enabled : ble_tss_s
- is_orientation_notif_enabled : ble_tms_s
- is_pedo_notif_enabled : ble_tms_s
- is_pressure_notif_enabled : ble_tes_s
- is_quat_notif_enabled : ble_tms_s
- is_raw_notif_enabled : ble_tms_s
- is_rot_mat_notif_enabled : ble_tms_s
- is_spkr_stat_notif_enabled : ble_tss_s
- is_tap_notif_enabled : ble_tms_s
- is_temperature_notif_enabled : ble_tes_s

### - l -

- led_char_handles : ble_uis_s
- led_write_handler : ble_uis_init_t , ble_uis_s
- level_percent : m_batt_meas_event_t

### - m -

- mic_handles : ble_tss_s
- mode : drv_pressure_init_t
- mono : drv_ext_light_conf_t

### - n -

- num_elements : state_of_charge_t
- num_lights : drv_ext_light_init_t

### - o -

- orientation_handles : ble_tms_s

### - p -

- p_data : drv_ext_light_conf_t
- p_light_conf : drv_ext_light_init_t
- p_status : drv_ext_light_data_t
- p_twi_cfg : drv_acc_cfg_t , drv_bh1745_cfg_t , drv_ccs811_cfg_t , drv_gas_init_t , drv_humidity_init_t , drv_lps22hb_twi_cfg_t , drv_pressure_init_t , drv_sx1509_cfg_t
- p_twi_conf : drv_ext_light_init_t
- p_twi_config : drv_hts221_twi_cfg_t
- p_twi_instance : drv_acc_cfg_t , drv_bh1745_cfg_t , drv_ccs811_cfg_t , drv_gas_init_t , drv_hts221_twi_cfg_t , drv_humidity_init_t , drv_lps22hb_twi_cfg_t , drv_pressure_init_t , drv_sx1509_cfg_t
- pedo_handles : ble_tms_s
- pin_char_handles : ble_uis_s
- pin_int : drv_hts221_twi_cfg_t , drv_lps22hb_twi_cfg_t , drv_pressure_init_t
- pin_write_handler : ble_uis_init_t , ble_uis_s
- pressure_handles : ble_tes_s

### - q -

- quat_handles : ble_tms_s

### - r -

- r : drv_ext_light_conf_t , drv_ext_light_rgb_intensity_t
- raw_data : drv_ccs811_alg_result_t
- raw_handles : ble_tms_s
- resync_pin : drv_ext_light_init_t
- rot_mat_handles : ble_tms_s

### - s -

- sequence_vals : drv_ext_light_rgb_sequence_t
- service_handle : ble_tcs_s , ble_tes_s , ble_tms_s , ble_tss_s , ble_uis_s
- spkr_handles : ble_tss_s
- spkr_stat_handles : ble_tss_s
- state_of_charge : batt_meas_param_t
- status : drv_ccs811_alg_result_t

### - t -

- tap_handles : ble_tms_s
- temperature_handles : ble_tes_s
- timer : drv_ext_light_data_t
- tvoc_ppb : drv_ccs811_alg_result_t
- twi_addr : drv_acc_cfg_t , drv_bh1745_cfg_t , drv_ccs811_cfg_t , drv_gas_init_t , drv_hts221_twi_cfg_t , drv_lps22hb_twi_cfg_t , drv_pressure_init_t
- type : drv_ext_light_conf_t , m_batt_meas_event_t

### - u -

- usb_detect_pin_no : batt_meas_param_t
- uuid_type : ble_tcs_s , ble_tes_s , ble_tms_s , ble_tss_s , ble_uis_s

### - v -

- valid_voltage : m_batt_meas_event_t
- voltage_divider : batt_meas_param_t
- voltage_mv : m_batt_meas_event_t
- voltage_to_soc : state_of_charge_t