| Nordic Thingy:52 v2.0.0

Data Fields
drv_ccs811_alg_result_t Struct Reference
Drivers » Gas sensor » CCS811 gas sensor

The algorithm result data of the CCS811 device. More...

## Data Fields

uint16_t | ec02_ppm
| The equivalent CO2 (eCO2) value in parts per million (ppm).
uint8_t | err_id
| The err_id according to the CCS811 err_id format (drv_ccs811_err_id_get).
uint16_t | raw_data
| The raw_data according to the CCS811 raw_data format (drv_ccs811_raw_data_get)
uint8_t | status
| The status according to the CCS811 status format (drv_ccs811_status_get).
uint16_t | tvoc_ppb
| The Total Volatile Organic Compound (TVOC) value in parts per billion (ppb).

## Detailed Description

The algorithm result data of the CCS811 device.

The documentation for this struct was generated from the following file:

- drv_ccs811.h