| Nordic Thingy:52 v2.0.0

Data Fields
ble_uis_init_t Struct Reference
BLE services » Thingy User Interface Service

LED Button Service init structure. This structure contains all options and data needed for initialization of the service. More...

## Data Fields

ble_uis_led_write_handler_t | led_write_handler
ble_uis_pin_write_handler_t | pin_write_handler

## Detailed Description

LED Button Service init structure. This structure contains all options and data needed for initialization of the service.

## Field Documentation

## ◆ led_write_handler

ble_uis_led_write_handler_t ble_uis_init_t::led_write_handler

Event handler to be called when the LED Characteristic is written.

## ◆ pin_write_handler

ble_uis_pin_write_handler_t ble_uis_init_t::pin_write_handler

Event handler to be called when the PIN Characteristic is written.

The documentation for this struct was generated from the following file:

- ble_uis.h