| Nordic Thingy:52 v2.0.0

Data Fields
drv_ext_light_status_t Struct Reference
Drivers » GPIO extender » GPIO extender LED driver

Struct used by the app_timer handler, mainly for power saving. More...

## Data Fields

uint32_t | active_time_ms
| Total time for a light to be on or dimmed.
drv_ext_light_color_mix_t | colors
| Color mix used for breathe, single-shot, or blink.
uint32_t | inactive_time_ms
| Total time for a light to be off.
drv_ext_light_ioext_osc_status_t | ioext_osc_status
| Status, holds information on the current use of the IO extender oscillator.

## Detailed Description

Struct used by the app_timer handler, mainly for power saving.

The documentation for this struct was generated from the following file:

- drv_ext_light.h