| Nordic Thingy:52 v2.0.0

Data Fields
drv_ext_light_conf_t Struct Reference
Drivers » GPIO extender » GPIO extender LED driver

Struct that defines the type of light (monochrome or RGB) and the corresponding connected pins. All lights are per definition sinked (The IO extender provides ground to the lights). More...

## Data Fields

drv_ext_light_data_t * | p_data
| Associated data for this light (app timer and timings).
drv_ext_light_reg_type_t | type
| Monochrome or RGB.
uint8_t | b
| RGB B pin.
uint8_t | g
| RGB G pin.
uint8_t | mono
| Monochrome pin.
uint8_t | r
| RGB R pin.

## Detailed Description

Struct that defines the type of light (monochrome or RGB) and the corresponding connected pins. All lights are per definition sinked (The IO extender provides ground to the lights).

The documentation for this struct was generated from the following file:

- drv_ext_light.h