| Nordic Thingy:52 v2.0.0

m_environment_flash.h
1 /*
2 Copyright (c) 2010 - 2017, Nordic Semiconductor ASA
3 All rights reserved.
4
5 Redistribution and use in source and binary forms, with or without modification,
6 are permitted provided that the following conditions are met:
7
8 1. Redistributions of source code must retain the above copyright notice, this
9 list of conditions and the following disclaimer.
10
11 2. Redistributions in binary form, except as embedded into a Nordic
12 Semiconductor ASA integrated circuit in a product or a software update for
13 such product, must reproduce the above copyright notice, this list of
14 conditions and the following disclaimer in the documentation and/or other
15 materials provided with the distribution.
16
17 3. Neither the name of Nordic Semiconductor ASA nor the names of its
18 contributors may be used to endorse or promote products derived from this
19 software without specific prior written permission.
20
21 4. This software, with or without modification, must only be used with a
22 Nordic Semiconductor ASA integrated circuit.
23
24 5. Any software provided in binary form under this license must not be reverse
25 engineered, decompiled, modified and/or disassembled.
26
27 THIS SOFTWARE IS PROVIDED BY NORDIC SEMICONDUCTOR ASA "AS IS" AND ANY EXPRESS
28 OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES
29 OF MERCHANTABILITY, NONINFRINGEMENT, AND FITNESS FOR A PARTICULAR PURPOSE ARE
30 DISCLAIMED. IN NO EVENT SHALL NORDIC SEMICONDUCTOR ASA OR CONTRIBUTORS BE
31 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
32 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE
33 GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
34 HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
35 LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT
36 OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
37 */
38
48 #ifndef __M_ENVIRONMENT_FLASH_H__
49 #define __M_ENVIRONMENT_FLASH_H__
50
51 #include "ble_tes.h"
52
55 typedef PACKED( struct
56 {
57 uint16_t mode_250ms;
58 uint16_t mode_1s;
59 uint16_t mode_10s;
60 uint16_t mode_60s;
61 }) m_gas_baseline_t;
62
71 uint32_t m_env_flash_config_store(const ble_tes_config_t * p_config);
72
80 uint32_t m_env_flash_config_load(ble_tes_config_t ** p_config);
81
90 uint32_t m_env_flash_baseline_store(const m_gas_baseline_t * p_baseline);
91
99 uint32_t m_env_flash_baseline_load(m_gas_baseline_t ** p_baseline);
100
112 uint32_t m_env_flash_init(const ble_tes_config_t * p_default_config,
113 ble_tes_config_t ** p_config,
114 const m_gas_baseline_t * p_default_baseline,
115 m_gas_baseline_t ** p_baseline);
116
117 #endif
118
m_env_flash_config_store
uint32_t m_env_flash_config_store(const ble_tes_config_t *p_config)
Function for storing the configuration.
m_env_flash_baseline_store
uint32_t m_env_flash_baseline_store(const m_gas_baseline_t *p_baseline)
Function for storing the gas sensor baseline.
m_env_flash_init
uint32_t m_env_flash_init(const ble_tes_config_t *p_default_config, ble_tes_config_t **p_config, const m_gas_baseline_t *p_default_baseline, m_gas_baseline_t **p_baseline)
Function for initializing weather station flash handling.
ble_tes.h
m_env_flash_baseline_load
uint32_t m_env_flash_baseline_load(m_gas_baseline_t **p_baseline)
Function for loading the gas sensor baseline.
m_env_flash_config_load
uint32_t m_env_flash_config_load(ble_tes_config_t **p_config)
Function for loading the configuration.