| Nordic Thingy:52 v2.0.0

Data Fields
drv_pressure_init_t Struct Reference
Drivers » Pressure sensor

Initialization struct for pressure driver. More...

## Data Fields

drv_pressure_evt_handler_t | evt_handler
| Event handler - called after a pin interrupt has been detected.
drv_pressure_mode_t | mode
| Current mode of operation.
nrf_drv_twi_config_t const * | p_twi_cfg
| The TWI configuration to use while the driver is enabled.
nrf_drv_twi_t const * | p_twi_instance
| The instance of TWI master to be used for transactions.
uint32_t | pin_int
| Interrupt pin.
uint8_t | twi_addr
| TWI address.

## Detailed Description

Initialization struct for pressure driver.

The documentation for this struct was generated from the following file:

- drv_pressure.h