| Nordic Thingy:52 v2.0.0

Data Fields
drv_acc_cfg_t Struct Reference
Drivers » Accelerometer

LIS3DH accelerometer configuration struct. More...

## Data Fields

uint8_t | cpu_wake_pin
| Pin on the nRF used to wake from sleep.
nrf_drv_twi_config_t const * | p_twi_cfg
| The TWI configuration to use while the driver is enabled.
nrf_drv_twi_t const * | p_twi_instance
| The instance of TWI master to be used for transactions.
uint8_t | twi_addr
| TWI (I2C) address of device.

## Detailed Description

LIS3DH accelerometer configuration struct.

The documentation for this struct was generated from the following file:

- drv_acc.h