| Nordic Thingy:52 v2.0.0

Modules
Here is a list of all modules:
[detail level 1 2 3]

▼BLE services | This section contains API documentation of the BLE services that are part of the Thingy firmware
Thingy Configuration Service | Thingy Configuration Service implementation
Thingy Environment Service | Thingy Environment Service implementation
Thingy Motion Service | Thingy Motion Service implementation
Thingy Sound Service | Thingy Sound Service implementation
Thingy User Interface Service | Thingy User Interface Service module
▼Drivers | This section contains API documentation of the drivers that are part of the Thingy firmware
▼Accelerometer | Low power accelerometer driver API
LIS3DH accelerometer | Definitions of LIS3DH constants
▼Color sensor | Digital color sensor API
BH1745 color sensor | BH1745 digital color sensor API
▼GPIO extender | GPIO extender API
GPIO extender LED driver | GPIO extender LED driver API
SX1509 GPIO extender driver | SX1509 GPIO extender API
▼Gas sensor | Digital gas sensor API
CCS811 gas sensor | CCS811 series ultra-low power digital gas sensor API
▼Humidity sensor | Humidity sensor API
HTS221 humidity sensor | HTS221 humidity sensor API
Microphone driver | Microphone driver API
▼Motion sensor | Motion sensor API
MPU-9250 motion sensor | MPU-9250 motion sensor
NFC driver | Near Field Communnication (NFC) driver API
▼Pressure sensor | Pressure sensor API
LPS22HB pressure sensor | LPS22HB pressure sensor API
Speaker driver | Speaker driver API
▼Thingy modules | This section contains API documentation of the modules that are part of the Thingy firmware
▼BLE | BLE handling module API
BLE flash configuration | BLE handling module flash configuration
Battery measurement | Battery measurement module API
▼Environment | Environment module API
Environment flash configuration | Environment module flash configuration
▼Motion | Motion module API
Motion flash configuration | Motion module flash configuration
Sound | Sound module API
▼User interface | User interface module API
User interface flash configuration | User interface module flash configuration
▼Utilities | This section contains API documentation of various utilities that are part of the Thingy firmware
Common macros | A set of useful macros
Eddystone beacon | Advertiser module. This module shows an example of using periodic timeslots on the radio when the SoftDevice is running
Settings for Sx150x LED driver registers | Settings for all LED driver registers on the Sx150x
Support functions | Support functions
Sx150x LED driver register calculation | Sx150x LED driver register calculation API