| Nordic Thingy:52 v2.0.0

Data Fields
ble_tes_s Struct Reference
BLE services » Thingy Environment Service

Thingy Environment Service structure. More...

## Data Fields

ble_gatts_char_handles_t | color_handles
ble_gatts_char_handles_t | config_handles
uint16_t | conn_handle
ble_tes_evt_handler_t | evt_handler
ble_gatts_char_handles_t | gas_handles
ble_gatts_char_handles_t | humidity_handles
bool | is_color_notif_enabled
bool | is_gas_notif_enabled
bool | is_humidity_notif_enabled
bool | is_pressure_notif_enabled
bool | is_temperature_notif_enabled
ble_gatts_char_handles_t | pressure_handles
uint16_t | service_handle
ble_gatts_char_handles_t | temperature_handles
uint8_t | uuid_type

## Detailed Description

Thingy Environment Service structure.

This structure contains status information related to the service.

## Field Documentation

## ◆ color_handles

ble_gatts_char_handles_t ble_tes_s::color_handles

Handles related to the gas characteristic (as provided by the S132 SoftDevice).

## ◆ config_handles

ble_gatts_char_handles_t ble_tes_s::config_handles

Handles related to the config characteristic (as provided by the S132 SoftDevice).

## ◆ conn_handle

uint16_t ble_tes_s::conn_handle

Handle of the current connection (as provided by the S110 SoftDevice). BLE_CONN_HANDLE_INVALID if not in a connection.

## ◆ evt_handler

ble_tes_evt_handler_t ble_tes_s::evt_handler

Event handler to be called for handling received data.

## ◆ gas_handles

ble_gatts_char_handles_t ble_tes_s::gas_handles

Handles related to the gas characteristic (as provided by the S132 SoftDevice).

## ◆ humidity_handles

ble_gatts_char_handles_t ble_tes_s::humidity_handles

Handles related to the humidity characteristic (as provided by the S132 SoftDevice).

## ◆ is_color_notif_enabled

bool ble_tes_s::is_color_notif_enabled

Variable to indicate if the peer has enabled notification of the characteristic.

## ◆ is_gas_notif_enabled

bool ble_tes_s::is_gas_notif_enabled

Variable to indicate if the peer has enabled notification of the characteristic.

## ◆ is_humidity_notif_enabled

bool ble_tes_s::is_humidity_notif_enabled

Variable to indicate if the peer has enabled notification of the characteristic.

## ◆ is_pressure_notif_enabled

bool ble_tes_s::is_pressure_notif_enabled

Variable to indicate if the peer has enabled notification of the characteristic.

## ◆ is_temperature_notif_enabled

bool ble_tes_s::is_temperature_notif_enabled

Variable to indicate if the peer has enabled notification of the characteristic.

## ◆ pressure_handles

ble_gatts_char_handles_t ble_tes_s::pressure_handles

Handles related to the pressure characteristic (as provided by the S132 SoftDevice).

## ◆ service_handle

uint16_t ble_tes_s::service_handle

Handle of Thingy Environment Service (as provided by the S110 SoftDevice).

## ◆ temperature_handles

ble_gatts_char_handles_t ble_tes_s::temperature_handles

Handles related to the temperature characteristic (as provided by the S132 SoftDevice).

## ◆ uuid_type

uint8_t ble_tes_s::uuid_type

UUID type for Thingy Environment Service Base UUID.

The documentation for this struct was generated from the following file:

- ble_tes.h