| Nordic Thingy:52 v2.0.0

Data Fields
m_batt_meas_event_t Struct Reference
Thingy modules » Battery measurement

The struct passed to the handler with relevant battery information. More...

## Data Fields

uint8_t | level_percent
| Remaining battery capacity percent.
m_batt_meas_event_type_t | type
| Given event type.
bool | valid_voltage
| True if an event is generated by a ADC conversion.
uint16_t | voltage_mv
| Battery voltage given in millivolts.

## Detailed Description

The struct passed to the handler with relevant battery information.

The documentation for this struct was generated from the following file:

- m_batt_meas.h