| Nordic Thingy:52 v2.0.0

Data Fields
ble_uis_s Struct Reference
BLE services » Thingy User Interface Service

LED Button Service structure. This structure contains various status information for the service. More...

## Data Fields

ble_gatts_char_handles_t | button_char_handles
uint16_t | conn_handle
ble_gatts_char_handles_t | led_char_handles
ble_uis_led_write_handler_t | led_write_handler
ble_gatts_char_handles_t | pin_char_handles
ble_uis_pin_write_handler_t | pin_write_handler
uint16_t | service_handle
uint8_t | uuid_type

## Detailed Description

LED Button Service structure. This structure contains various status information for the service.

## Field Documentation

## ◆ button_char_handles

ble_gatts_char_handles_t ble_uis_s::button_char_handles

Handles related to the Button Characteristic.

## ◆ conn_handle

uint16_t ble_uis_s::conn_handle

Handle of the current connection (as provided by the BLE stack). BLE_CONN_HANDLE_INVALID if not in a connection.

## ◆ led_char_handles

ble_gatts_char_handles_t ble_uis_s::led_char_handles

Handles related to the LED Characteristic.

## ◆ led_write_handler

ble_uis_led_write_handler_t ble_uis_s::led_write_handler

Event handler to be called when the LED Characteristic is written.

## ◆ pin_char_handles

ble_gatts_char_handles_t ble_uis_s::pin_char_handles

Handles related to the PIN Characteristic.

## ◆ pin_write_handler

ble_uis_pin_write_handler_t ble_uis_s::pin_write_handler

Event handler to be called when the PIN Characteristic is written.

## ◆ service_handle

uint16_t ble_uis_s::service_handle

Handle of LED Button Service (as provided by the BLE stack).

## ◆ uuid_type

uint8_t ble_uis_s::uuid_type

UUID type for the LED Button Service.

The documentation for this struct was generated from the following file:

- ble_uis.h