| Nordic Thingy:52 v2.0.0

Data Fields
drv_ext_light_init_t Struct Reference
Drivers » GPIO extender » GPIO extender LED driver

Struct for initializing the light driver. More...

## Data Fields

drv_ext_light_clkx_div_t | clkx_div
| IO extender clock divider.
uint8_t | num_lights
| Number of connected lights.
drv_ext_light_conf_t const * | p_light_conf
| Array of lights, each with their specific configuraion.
drv_sx1509_cfg_t const * | p_twi_conf
| pointer to TWI (I2C) configuration for communication between master and IO extender.
uint8_t | resync_pin
| Pin used to resync IO extender counters. Use DRV_EXT_LIGHT_INVALID_RESYNC_PIN if unused.

## Detailed Description

Struct for initializing the light driver.

The documentation for this struct was generated from the following file:

- drv_ext_light.h