| Nordic Thingy:52 v2.0.0

Data Fields
batt_meas_param_t Struct Reference
Thingy modules » Battery measurement

Input parameters for m_batt_meas. More...

## Data Fields

uint8_t | adc_pin_no
| Analog in pin connected to battery (with possible voltage divider).
nrf_saadc_input_t | adc_pin_no_ain
| Same as above, but given as nrf_saadc_input_t. These two values must correspond.
uint16_t | app_timer_prescaler
| App timer prescaler. See APP_TIMER_PRESCALER.
uint8_t | batt_chg_stat_pin_no
| Pin connected to "Charging status output pin" (CSO) of the battery charger.
uint8_t | batt_mon_en_pin_no
| Pin for enabling battery monitoring.
bool | batt_mon_en_pin_used
| Indicates if a pin is used to enable battery monitoring. (E.g. activates a voltage divider).
uint16_t | batt_voltage_limit_full
| Full voltage limit [milliVolts].
uint16_t | batt_voltage_limit_low
| Low voltage limit [milliVolts].
state_of_charge_t | state_of_charge
| Information on mapping from voltage to state of charge.
uint8_t | usb_detect_pin_no
| Pin = high when USB is connected.
voltage_divider_t | voltage_divider
| Voltage divider type containing resistor information.

## Detailed Description

Input parameters for m_batt_meas.

The documentation for this struct was generated from the following file:

- m_batt_meas.h