| Nordic Thingy:52 v2.0.0

Data Fields
state_of_charge_t Struct Reference
Thingy modules » Battery measurement

Struct for providing m_batt_meas with information on converting voltage to state of charge (Remaining battery capacity). More...

## Data Fields

uint8_t | delta_mv
| Distance in voltage between elements in the SoC vector [mV].
uint16_t | first_element_mv
| Voltage of the first element in the vector [mV];.
uint16_t | num_elements
| Number of elements in the voltage to state of charge vector.
uint8_t const * | voltage_to_soc
| Pointer to vector mapping from voltage to state of charge.

## Detailed Description

Struct for providing m_batt_meas with information on converting voltage to state of charge (Remaining battery capacity).

The documentation for this struct was generated from the following file:

- m_batt_meas.h