| Nordic Thingy:52 v2.0.0

Data Fields
ble_tss_init_t Struct Reference
BLE services » Thingy Sound Service

Thingy Sound Service initialization structure. More...

## Data Fields

ble_tss_evt_handler_t | evt_handler

## Detailed Description

Thingy Sound Service initialization structure.

This structure contains the initialization information for the service. The application must fill this structure and pass it to the service using the ble_tss_init function.

## Field Documentation

## ◆ evt_handler

ble_tss_evt_handler_t ble_tss_init_t::evt_handler

Event handler to be called for handling received data.

The documentation for this struct was generated from the following file:

- ble_tss.h