| Nordic Thingy:52 v2.0.0

Data Fields
ble_tcs_s Struct Reference
BLE services » Thingy Configuration Service

Thingy Configuration Service structure. More...

## Data Fields

ble_gatts_char_handles_t | adv_param_handles
uint16_t | conn_handle
ble_gatts_char_handles_t | conn_param_handles
ble_gatts_char_handles_t | dev_name_handles
ble_tcs_evt_handler_t | evt_handler
uint16_t | service_handle
uint8_t | uuid_type

## Detailed Description

Thingy Configuration Service structure.

This structure contains status information related to the service.

## Field Documentation

## ◆ adv_param_handles

ble_gatts_char_handles_t ble_tcs_s::adv_param_handles

Handles related to the pressure characteristic (as provided by the S132 SoftDevice).

## ◆ conn_handle

uint16_t ble_tcs_s::conn_handle

Handle of the current connection (as provided by the S110 SoftDevice). BLE_CONN_HANDLE_INVALID if not in a connection.

## ◆ conn_param_handles

ble_gatts_char_handles_t ble_tcs_s::conn_param_handles

Handles related to the config characteristic (as provided by the S132 SoftDevice).

## ◆ dev_name_handles

ble_gatts_char_handles_t ble_tcs_s::dev_name_handles

Handles related to the temperature characteristic (as provided by the S132 SoftDevice).

## ◆ evt_handler

ble_tcs_evt_handler_t ble_tcs_s::evt_handler

Event handler to be called for handling received data.

## ◆ service_handle

uint16_t ble_tcs_s::service_handle

Handle of Thingy Configuration Service (as provided by the S110 SoftDevice).

## ◆ uuid_type

uint8_t ble_tcs_s::uuid_type

UUID type for Thingy Configuration Service Base UUID.

The documentation for this struct was generated from the following file:

- ble_tcs.h