| Nordic Thingy:52 v2.0.0

Data Fields
ble_tss_s Struct Reference
BLE services » Thingy Sound Service

Thingy Sound Service structure. More...

## Data Fields

ble_gatts_char_handles_t | config_handles
uint16_t | conn_handle
ble_tss_evt_handler_t | evt_handler
bool | is_mic_notif_enabled
bool | is_spkr_stat_notif_enabled
ble_gatts_char_handles_t | mic_handles
uint16_t | service_handle
ble_gatts_char_handles_t | spkr_handles
ble_gatts_char_handles_t | spkr_stat_handles
uint8_t | uuid_type

## Detailed Description

Thingy Sound Service structure.

This structure contains status information related to the service.

## Field Documentation

## ◆ config_handles

ble_gatts_char_handles_t ble_tss_s::config_handles

Handles related to the config characteristic (as provided by the S132 SoftDevice).

## ◆ conn_handle

uint16_t ble_tss_s::conn_handle

Handle of the current connection (as provided by the S110 SoftDevice). BLE_CONN_HANDLE_INVALID if not in a connection.

## ◆ evt_handler

ble_tss_evt_handler_t ble_tss_s::evt_handler

Event handler to be called for handling received data.

## ◆ is_mic_notif_enabled

bool ble_tss_s::is_mic_notif_enabled

Variable to indicate if the peer has enabled notification of the characteristic.

## ◆ is_spkr_stat_notif_enabled

bool ble_tss_s::is_spkr_stat_notif_enabled

Variable to indicate if the peer has enabled notification of the characteristic.

## ◆ mic_handles

ble_gatts_char_handles_t ble_tss_s::mic_handles

Handles related to the microphone characteristic (as provided by the S132 SoftDevice).

## ◆ service_handle

uint16_t ble_tss_s::service_handle

Handle of Thingy Sound Service (as provided by the S110 SoftDevice).

## ◆ spkr_handles

ble_gatts_char_handles_t ble_tss_s::spkr_handles

Handles related to the speaker characteristic (as provided by the S132 SoftDevice).

## ◆ spkr_stat_handles

ble_gatts_char_handles_t ble_tss_s::spkr_stat_handles

Handles related to the speaker status characteristic (as provided by the S132 SoftDevice).

## ◆ uuid_type

uint8_t ble_tss_s::uuid_type

UUID type for Thingy Sound Service Base UUID.

The documentation for this struct was generated from the following file:

- ble_tss.h