| Nordic Thingy:52 v2.0.0

Data Fields
drv_humidity_init_t Struct Reference
Drivers » Humidity sensor

Initialization struct for the humidity driver. More...

## Data Fields

nrf_drv_twi_config_t const * | p_twi_cfg
| The TWI configuration to use while the driver is enabled.
nrf_drv_twi_t const * | p_twi_instance
| The instance of TWI master to be used for transactions.

## Detailed Description

Initialization struct for the humidity driver.

The documentation for this struct was generated from the following file:

- drv_humidity.h