(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 7)
    (zones 0)
    (modules 3)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "supoh137/"))
  )
  (net 0 "")
  (net_class Default "Ceci est la Netclass par défaut."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 60A3CE00)
    (at 45.72 43.18)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference REF** (at 5.08 2.37) (layer B.SilkS) hide)
    (fp_text value R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (at 5.08 -2.37) (layer B.Fab) hide)
    (fp_text user 10k (at 5.08 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SIP:SIP3_11.6x8.5mm (layer F.Cu) (tedit 60A3CD87)
    (at 48.26 39.37)
    (descr RECOM,R78EXX,https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf)
    (tags "SIP3 Regulator Module")
    (fp_text reference REF** (at 2.54 3.3 180) (layer F.SilkS) hide)
    (fp_text value SIP3_11.6x8.5mm (at 2.54 -8 180) (layer F.Fab) hide)
    (fp_text user OH137 (at 2.54 -2.7 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_SIP.3dshapes/SIP3_11.6x8.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_bornier-3_P5.08mm (layer B.Cu) (tedit 60A3CE79)
    (at 45.72 66.04)
    (descr "simple 3-pin terminal block, pitch 5.08mm, revamped version of bornier3")
    (tags "terminal block bornier3")
    (fp_text reference "DATA   -     +" (at 5.05 4.65) (layer B.SilkS))
    (fp_text value TerminalBlock_bornier-3_P5.08mm (at 5.08 -5.08) (layer B.Fab) hide)
    (fp_text user %R (at 5.08 0) (layer B.Fab))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-3_P5.08mm.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Defi tireur JBG" (at 50.8 73.66) (layer F.Cu))
  (gr_circle (center 36.83 53.34) (end 38.1 54.61) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 64.77 53.34) (end 66.04 54.61) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 64.77 31.75) (end 66.04 33.02) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 64.77 73.66) (end 66.77 73.66) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 36.83 73.66) (end 38.83 73.66) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 36.83 31.75) (end 38.1 33.02) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.31 29.21) (end 34.29 29.21) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.31 76.2) (end 67.31 29.21) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 34.29 76.2) (end 67.31 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 34.29 29.21) (end 34.29 76.2) (layer Edge.Cuts) (width 0.15))
)
