(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (date "lun. 30 mars 2015")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 110.998 126.365)
    (grid_origin 110.998 126.365)
    (pcbplotparams
      (layerselection 0x0000030_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/IOREF")
  (net 2 "/Reset")
  (net 3 "+5V")
  (net 4 "GND")
  (net 5 "/Vin")
  (net 6 "/A2")
  (net 7 "/A3")
  (net 8 "/AREF")
  (net 9 "/A4(SDA)")
  (net 10 "/9(**)")
  (net 11 "/5(**)")
  (net 12 "Relay D10")
  (net 13 "unconnected-(P1-Pad1)")
  (net 14 "Ultrasonic_Trig 6")
  (net 15 "Ultrasonic_Echo d7")
  (net 16 "unconnected-(P5-Pad1)")
  (net 17 "unconnected-(P1-Pad4)")
  (net 18 "unconnected-(P6-Pad1)")
  (net 19 "unconnected-(P7-Pad1)")
  (net 20 "/8")
  (net 21 "led 1 D11")
  (net 22 "unconnected-(P8-Pad1)")
  (net 23 "Net-(D1-Pad2)")
  (net 24 "Net-(D2-Pad2)")
  (net 25 "Net-(D3-Pad2)")
  (net 26 "Soil sensor A5")
  (net 27 "led 2 d12")
  (net 28 "Light sensor A1")
  (net 29 "led 3 d13")
  (net 30 "Light Sensor A0")
  (net 31 "dht 11 out")
  (net 32 "unconnected-(P3-Pad1)")
  (net 33 "/0(Rx)")
  (net 34 "/1(Tx)")
  (net 35 "/2")
  (net 36 "/3(**)")
  (footprint "Socket_Arduino_Uno:Socket_Strip_Arduino_1x08" locked (layer "F.Cu")
    (tedit 552168D2)
    (at 138.938 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 8.89 -2.54) (layer "F.SilkS"))
    (fp_text value "Power" (at 8.89 -4.064) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 13 "unconnected-(P1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "/IOREF") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "/Reset") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 17 "unconnected-(P1-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 3 "+5V") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 5 "/Vin") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl"
      (offset (xyz 8.889999866 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Socket_Arduino_Uno:Socket_Strip_Arduino_1x06" locked (layer "F.Cu")
    (tedit 552168D6)
    (at 161.798 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P2" (at 6.604 -2.54) (layer "F.SilkS"))
    (fp_text value "Analog" (at 6.604 -4.064) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 30 "Light Sensor A0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 28 "Light sensor A1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 6 "/A2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 7 "/A3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 9 "/A4(SDA)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 26 "Soil sensor A5") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x06.wrl"
      (offset (xyz 6.349999905 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Socket_Arduino_Uno:Socket_Strip_Arduino_1x10" locked (layer "F.Cu")
    (tedit 552168BF)
    (at 129.794 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P3" (at 11.43 2.794) (layer "F.SilkS"))
    (fp_text value "Digital" (at -16.51 5.818) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 32 "unconnected-(P3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 9 "/A4(SDA)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 8 "/AREF") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 29 "led 3 d13") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 27 "led 2 d12") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 21 "led 1 D11") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 12 "Relay D10") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 20.32 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 10 "/9(**)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 22.86 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 20 "/8") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x10.wrl"
      (offset (xyz 11.42999983 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Socket_Arduino_Uno:Socket_Strip_Arduino_1x08" locked (layer "F.Cu")
    (tedit 552168C7)
    (at 156.718 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P4" (at 8.89 2.794) (layer "F.SilkS"))
    (fp_text value "Digital" (at 8.89 4.318) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 14 "Ultrasonic_Trig 6") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 15 "Ultrasonic_Echo d7") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 11 "/5(**)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 31 "dht 11 out") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 36 "/3(**)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 35 "/2") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 34 "/1(Tx)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 33 "/0(Rx)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl"
      (offset (xyz 8.889999866 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Socket_Arduino_Uno:Arduino_1pin" locked (layer "F.Cu")
    (tedit 5524FC39)
    (at 124.968 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P5" (at 0 -3.048) (layer "F.SilkS") hide)
    (fp_text value "CONN_01X01" (at 0 2.794) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask "F.SilkS")
      (net 16 "unconnected-(P5-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "Socket_Arduino_Uno:Arduino_1pin" locked (layer "F.Cu")
    (tedit 5524FC4A)
    (at 177.038 118.745)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P6" (at 0 -3.048) (layer "F.SilkS") hide)
    (fp_text value "CONN_01X01" (at 0 2.794) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask "F.SilkS")
      (net 18 "unconnected-(P6-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "Socket_Arduino_Uno:Arduino_1pin" locked (layer "F.Cu")
    (tedit 5524FC2F)
    (at 126.238 75.565)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P7" (at 0 -3.048) (layer "F.SilkS") hide)
    (fp_text value "CONN_01X01" (at 0 2.794) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask "F.SilkS")
      (net 19 "unconnected-(P7-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "Socket_Arduino_Uno:Arduino_1pin" locked (layer "F.Cu")
    (tedit 5524FC41)
    (at 177.038 90.805)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P8" (at 0 -3.048) (layer "F.SilkS") hide)
    (fp_text value "CONN_01X01" (at 0 2.794) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask "F.SilkS")
      (net 22 "unconnected-(P8-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 152.918 118.745 90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 4.385 -2.27 90) (layer "F.SilkS"))
    (fp_text value "Light Sensor" (at 4.385 9.89 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Light sensor A1") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 121.158 107.315 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 6.35 -2.72 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 6.35 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "led 3 d13") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 165.623 118.04 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 4.385 -2.27 90) (layer "F.SilkS"))
    (fp_text value "Humidity Sensor" (at 4.385 7.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Soil sensor A5") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 154.178 83.185 -90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 4.385 -2.27 90) (layer "F.SilkS"))
    (fp_text value "Ultrasonic Sensor" (at 4.385 9.89 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Ultrasonic_Echo d7") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Ultrasonic_Trig 6") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 161.798 98.425 -90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -3.96 -270) (layer "F.SilkS"))
    (fp_text value "LED_Small" (at 1.27 3.96 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 141.478 83.185 -90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 4.385 -2.27 90) (layer "F.SilkS"))
    (fp_text value "Relay 1 channel" (at 4.385 7.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Relay D10") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 131.318 107.315 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 6.35 -2.72 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 6.35 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "led 1 D11") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 138.938 98.425 -90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 1.27 -3.96 -270) (layer "F.SilkS"))
    (fp_text value "LED_Small" (at 1.27 3.96 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 138.938 118.745 90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 4.385 -2.27 90) (layer "F.SilkS"))
    (fp_text value "Light Sensor" (at 4.385 9.89 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Light Sensor A0") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 149.098 98.425 -90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 1.27 -3.96 -270) (layer "F.SilkS"))
    (fp_text value "LED_Small" (at 1.27 3.96 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 164.338 83.185 -90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 4.385 -2.27 90) (layer "F.SilkS"))
    (fp_text value "Temperature Sensor" (at 4.385 7.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "dht 11 out") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 126.238 107.315 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "potee.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 6.35 -2.72 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 6.35 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(D2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "led 2 d12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 179.578 88.519) (end 177.038 85.979) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 177.038 128.905) (end 179.578 123.825) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 177.038 74.549) (end 175.514 70.485) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 179.578 123.825) (end 179.578 121.285) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 110.998 70.485) (end 110.998 128.905) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 179.578 121.285) (end 179.578 88.519) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 110.998 128.905) (end 177.038 128.905) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 175.514 70.485) (end 110.998 70.485) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 177.038 85.979) (end 177.038 74.549) (layer "Edge.Cuts") (width 0.15))
  (gr_text "1" (at 138.938 121.285 90) (layer "F.SilkS"))
)
