(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:Buzzer" (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BZ" (id 0) (at 3.81 1.27 0))
      (property "Value" "Buzzer" (id 1) (at 3.81 -1.27 0))
      (property "Footprint" "" (id 2) (at -0.635 2.54 90))
      (property "Datasheet" "~" (id 3) (at -0.635 2.54 90))
      (property "ki_keywords" "quartz resonator ceramic" (id 4) (at 0 0 0))
      (property "ki_description" "Buzzer, polarized" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "*Buzzer*" (id 6) (at 0 0 0))
      (symbol "Buzzer_0_1"
        (arc (start 0 -3.175) (mid 3.175 0) (end 0 3.175)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.651 1.905)
            (xy -1.143 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.397 2.159)
            (xy -1.397 1.651)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 3.175)
            (xy 0 -3.175)
          )
          (fill (type none))
        )
      )
      (symbol "Buzzer_1_1"
        (pin passive line (at -2.54 2.54 0) (length 2.54)
          (name "-")
          (number "1")
        )
        (pin passive line (at -2.54 -2.54 0) (length 2.54)
          (name "+")
          (number "2")
        )
      )
    )
    (symbol "Device:R_US" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.54 0 90))
      (property "Value" "R_US" (id 1) (at -2.54 0 90))
      (property "Footprint" "" (id 2) (at 1.016 -0.254 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_US_0_1"
        (polyline
          (pts
            (xy 0 -2.286)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 1.016 -1.143)
            (xy 0 -1.524)
            (xy -1.016 -1.905)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 1.016 0.381)
            (xy 0 0)
            (xy -1.016 -0.381)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 1.016 1.905)
            (xy 0 1.524)
            (xy -1.016 1.143)
            (xy 0 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "R_US_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Lib_Arduino:Arduino_Mega2560_Shield" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "XA" (id 0) (at 2.54 0 90))
      (property "Value" "Arduino_Mega2560_Shield" (id 1) (at -2.54 0 90))
      (property "Footprint" "" (id 2) (at 17.78 69.85 0))
      (property "Datasheet" "https://store.arduino.cc/arduino-mega-2560-rev3" (id 3) (at 17.78 69.85 0))
      (property "ki_keywords" "Arduino MPU Shield" (id 4) (at 0 0 0))
      (property "ki_description" "Shield for Arduino Mega 2560" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Arduino_Mega2560_Shield" (id 6) (at 0 0 0))
      (symbol "Arduino_Mega2560_Shield_0_0"
        (rectangle (start -25.4 -58.42) (end 25.4 58.42)
          (fill (type background))
        )
        (rectangle (start -20.32 -54.61) (end -12.7 -54.61)
          (fill (type none))
        )
        (rectangle (start -19.05 -31.75) (end -12.7 -31.75)
          (fill (type none))
        )
        (rectangle (start -19.05 -19.05) (end -12.7 -19.05)
          (fill (type none))
        )
        (rectangle (start -19.05 26.67) (end -12.7 26.67)
          (fill (type none))
        )
        (rectangle (start -17.78 -26.67) (end -16.51 -26.67)
          (fill (type none))
        )
        (rectangle (start -17.78 -24.13) (end -16.51 -24.13)
          (fill (type none))
        )
        (rectangle (start -16.51 -25.4) (end -13.97 -25.4)
          (fill (type none))
        )
        (rectangle (start -16.51 -24.13) (end -16.51 -26.67)
          (fill (type none))
        )
        (rectangle (start -16.51 54.61) (end -12.7 54.61)
          (fill (type none))
        )
        (rectangle (start -15.24 34.29) (end -12.7 34.29)
          (fill (type none))
        )
        (rectangle (start -15.24 36.83) (end -12.7 36.83)
          (fill (type none))
        )
        (rectangle (start -12.7 -54.61) (end -12.7 -48.26)
          (fill (type none))
        )
        (rectangle (start -12.7 -31.75) (end -12.7 -38.1)
          (fill (type none))
        )
        (rectangle (start -12.7 26.67) (end -12.7 27.94)
          (fill (type none))
        )
        (rectangle (start -12.7 34.29) (end -12.7 33.02)
          (fill (type none))
        )
        (rectangle (start -12.7 41.91) (end -12.7 36.83)
          (fill (type none))
        )
        (rectangle (start -12.7 49.53) (end -12.7 54.61)
          (fill (type none))
        )
        (rectangle (start -6.35 48.26) (end -6.35 45.72)
          (fill (type none))
        )
        (rectangle (start -2.54 45.72) (end -6.35 45.72)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -21.59 21.59)
            (xy -12.7 21.59)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -12.7 -19.05)
            (xy -12.7 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -12.7 10.16)
            (xy -12.7 21.59)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 12.7 -54.61)
            (xy 16.51 -54.61)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 12.7 54.61)
            (xy 16.51 54.61)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 17.78 -34.29)
            (xy 16.51 -34.29)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 15.24 36.83)
            (xy 15.24 27.94)
            (xy 20.32 26.67)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 15.24 44.45)
            (xy 15.24 53.34)
            (xy 16.51 54.61)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 20.32 -31.75)
            (xy 17.78 -33.02)
            (xy 17.78 -35.56)
            (xy 20.32 -36.83)
          )
          (fill (type none))
        )
        (rectangle (start 6.35 45.72) (end 2.54 45.72)
          (fill (type none))
        )
        (rectangle (start 6.35 46.99) (end 6.35 45.72)
          (fill (type none))
        )
        (text "Analogue I/O" (at -12.7 1.27 900))
        (text "I²C" (at -12.7 30.48 900))
        (text "Misc." (at -12.7 -25.4 900))
        (text "Power" (at -12.7 -43.18 900))
        (text "PWM" (at 15.24 -34.29 900))
        (text "PWM" (at 15.24 40.64 900))
        (text "Serial" (at -12.7 45.72 900))
        (text "SPI" (at 0 45.72 0))
      )
      (symbol "Arduino_Mega2560_Shield_1_0"
        (rectangle (start 12.7 -54.61) (end 12.7 -3.81)
          (fill (type none))
        )
        (rectangle (start 12.7 54.61) (end 12.7 3.81)
          (fill (type none))
        )
        (text "GPIO" (at 12.7 0 900))
      )
      (symbol "Arduino_Mega2560_Shield_1_1"
        (pin power_in line (at -33.02 -44.45 0) (length 7.62)
          (name "3.3V")
          (number "3V3")
        )
        (pin power_in line (at -33.02 -46.99 0) (length 7.62)
          (name "5V")
          (number "5V1")
        )
        (pin power_in line (at 1.27 66.04 270) (length 7.62)
          (name "SPI_5V")
          (number "5V2")
        )
        (pin power_in line (at -33.02 -49.53 0) (length 7.62)
          (name "5V")
          (number "5V3")
        )
        (pin power_in line (at -33.02 -52.07 0) (length 7.62)
          (name "5V")
          (number "5V4")
        )
        (pin bidirectional line (at -33.02 21.59 0) (length 7.62)
          (name "A0")
          (number "A0")
        )
        (pin bidirectional line (at -33.02 19.05 0) (length 7.62)
          (name "A1")
          (number "A1")
        )
        (pin bidirectional line (at -33.02 -3.81 0) (length 7.62)
          (name "A10")
          (number "A10")
        )
        (pin bidirectional line (at -33.02 -6.35 0) (length 7.62)
          (name "A11")
          (number "A11")
        )
        (pin bidirectional line (at -33.02 -8.89 0) (length 7.62)
          (name "A12")
          (number "A12")
        )
        (pin bidirectional line (at -33.02 -11.43 0) (length 7.62)
          (name "A13")
          (number "A13")
        )
        (pin bidirectional line (at -33.02 -13.97 0) (length 7.62)
          (name "A14")
          (number "A14")
        )
        (pin bidirectional line (at -33.02 -16.51 0) (length 7.62)
          (name "A15")
          (number "A15")
        )
        (pin bidirectional line (at -33.02 16.51 0) (length 7.62)
          (name "A2")
          (number "A2")
        )
        (pin bidirectional line (at -33.02 13.97 0) (length 7.62)
          (name "A3")
          (number "A3")
        )
        (pin bidirectional line (at -33.02 11.43 0) (length 7.62)
          (name "A4")
          (number "A4")
        )
        (pin bidirectional line (at -33.02 8.89 0) (length 7.62)
          (name "A5")
          (number "A5")
        )
        (pin bidirectional line (at -33.02 6.35 0) (length 7.62)
          (name "A6")
          (number "A6")
        )
        (pin bidirectional line (at -33.02 3.81 0) (length 7.62)
          (name "A7")
          (number "A7")
        )
        (pin bidirectional line (at -33.02 1.27 0) (length 7.62)
          (name "A8")
          (number "A8")
        )
        (pin bidirectional line (at -33.02 -1.27 0) (length 7.62)
          (name "A9")
          (number "A9")
        )
        (pin input line (at -33.02 -19.05 0) (length 7.62)
          (name "AREF")
          (number "AREF")
        )
        (pin bidirectional line (at -33.02 54.61 0) (length 7.62)
          (name "D0_RX0")
          (number "D0")
        )
        (pin bidirectional line (at -33.02 52.07 0) (length 7.62)
          (name "D1_TX0")
          (number "D1")
        )
        (pin bidirectional line (at 33.02 34.29 180) (length 7.62)
          (name "D10")
          (number "D10")
        )
        (pin bidirectional line (at 33.02 31.75 180) (length 7.62)
          (name "D11")
          (number "D11")
        )
        (pin bidirectional line (at 33.02 29.21 180) (length 7.62)
          (name "D12")
          (number "D12")
        )
        (pin bidirectional line (at 33.02 26.67 180) (length 7.62)
          (name "D13")
          (number "D13")
        )
        (pin bidirectional line (at -33.02 36.83 0) (length 7.62)
          (name "D14_TX3")
          (number "D14")
        )
        (pin bidirectional line (at -33.02 39.37 0) (length 7.62)
          (name "D15_RX3")
          (number "D15")
        )
        (pin bidirectional line (at -33.02 41.91 0) (length 7.62)
          (name "D16_TX2")
          (number "D16")
        )
        (pin bidirectional line (at -33.02 44.45 0) (length 7.62)
          (name "D17_RX2")
          (number "D17")
        )
        (pin bidirectional line (at -33.02 46.99 0) (length 7.62)
          (name "D18_TX1")
          (number "D18")
        )
        (pin bidirectional line (at -33.02 49.53 0) (length 7.62)
          (name "D19_RX1")
          (number "D19")
        )
        (pin bidirectional line (at 33.02 54.61 180) (length 7.62)
          (name "D2_INT0")
          (number "D2")
        )
        (pin bidirectional line (at -33.02 34.29 0) (length 7.62)
          (name "D20_SDA")
          (number "D20")
        )
        (pin bidirectional clock (at -33.02 31.75 0) (length 7.62)
          (name "D21_SCL")
          (number "D21")
        )
        (pin bidirectional line (at 33.02 24.13 180) (length 7.62)
          (name "D22")
          (number "D22")
        )
        (pin bidirectional line (at 33.02 21.59 180) (length 7.62)
          (name "D23")
          (number "D23")
        )
        (pin bidirectional line (at 33.02 19.05 180) (length 7.62)
          (name "D24")
          (number "D24")
        )
        (pin bidirectional line (at 33.02 16.51 180) (length 7.62)
          (name "D25")
          (number "D25")
        )
        (pin bidirectional line (at 33.02 13.97 180) (length 7.62)
          (name "D26")
          (number "D26")
        )
        (pin bidirectional line (at 33.02 11.43 180) (length 7.62)
          (name "D27")
          (number "D27")
        )
        (pin bidirectional line (at 33.02 8.89 180) (length 7.62)
          (name "D28")
          (number "D28")
        )
        (pin bidirectional line (at 33.02 6.35 180) (length 7.62)
          (name "D29")
          (number "D29")
        )
        (pin bidirectional line (at 33.02 52.07 180) (length 7.62)
          (name "D3_INT1")
          (number "D3")
        )
        (pin bidirectional line (at 33.02 3.81 180) (length 7.62)
          (name "D30")
          (number "D30")
        )
        (pin bidirectional line (at 33.02 1.27 180) (length 7.62)
          (name "D31")
          (number "D31")
        )
        (pin bidirectional line (at 33.02 -1.27 180) (length 7.62)
          (name "D32")
          (number "D32")
        )
        (pin bidirectional line (at 33.02 -3.81 180) (length 7.62)
          (name "D33")
          (number "D33")
        )
        (pin bidirectional line (at 33.02 -6.35 180) (length 7.62)
          (name "D34")
          (number "D34")
        )
        (pin bidirectional line (at 33.02 -8.89 180) (length 7.62)
          (name "D35")
          (number "D35")
        )
        (pin bidirectional line (at 33.02 -11.43 180) (length 7.62)
          (name "D36")
          (number "D36")
        )
        (pin bidirectional line (at 33.02 -13.97 180) (length 7.62)
          (name "D37")
          (number "D37")
        )
        (pin bidirectional line (at 33.02 -16.51 180) (length 7.62)
          (name "D38")
          (number "D38")
        )
        (pin bidirectional line (at 33.02 -19.05 180) (length 7.62)
          (name "D39")
          (number "D39")
        )
        (pin bidirectional line (at 33.02 49.53 180) (length 7.62)
          (name "D4")
          (number "D4")
        )
        (pin bidirectional line (at 33.02 -21.59 180) (length 7.62)
          (name "D40")
          (number "D40")
        )
        (pin bidirectional line (at 33.02 -24.13 180) (length 7.62)
          (name "D41")
          (number "D41")
        )
        (pin bidirectional line (at 33.02 -26.67 180) (length 7.62)
          (name "D42")
          (number "D42")
        )
        (pin bidirectional line (at 33.02 -29.21 180) (length 7.62)
          (name "D43")
          (number "D43")
        )
        (pin bidirectional line (at 33.02 -31.75 180) (length 7.62)
          (name "D44")
          (number "D44")
        )
        (pin bidirectional line (at 33.02 -34.29 180) (length 7.62)
          (name "D45")
          (number "D45")
        )
        (pin bidirectional line (at 33.02 -36.83 180) (length 7.62)
          (name "D46")
          (number "D46")
        )
        (pin bidirectional line (at 33.02 -39.37 180) (length 7.62)
          (name "D47")
          (number "D47")
        )
        (pin bidirectional line (at 33.02 -41.91 180) (length 7.62)
          (name "D48")
          (number "D48")
        )
        (pin bidirectional line (at 33.02 -44.45 180) (length 7.62)
          (name "D49")
          (number "D49")
        )
        (pin bidirectional line (at 33.02 46.99 180) (length 7.62)
          (name "D5")
          (number "D5")
        )
        (pin bidirectional line (at 33.02 -46.99 180) (length 7.62)
          (name "D50")
          (number "D50")
        )
        (pin bidirectional line (at 33.02 -49.53 180) (length 7.62)
          (name "D51")
          (number "D51")
        )
        (pin bidirectional line (at 33.02 -52.07 180) (length 7.62)
          (name "D52")
          (number "D52")
        )
        (pin bidirectional line (at 33.02 -54.61 180) (length 7.62)
          (name "D53_SS")
          (number "D53")
        )
        (pin bidirectional line (at 33.02 44.45 180) (length 7.62)
          (name "D6")
          (number "D6")
        )
        (pin bidirectional line (at 33.02 41.91 180) (length 7.62)
          (name "D7")
          (number "D7")
        )
        (pin bidirectional line (at 33.02 39.37 180) (length 7.62)
          (name "D8")
          (number "D8")
        )
        (pin bidirectional line (at 33.02 36.83 180) (length 7.62)
          (name "D9")
          (number "D9")
        )
        (pin power_in line (at -33.02 -31.75 0) (length 7.62)
          (name "GND")
          (number "GND1")
        )
        (pin power_in line (at -33.02 -34.29 0) (length 7.62)
          (name "GND")
          (number "GND2")
        )
        (pin power_in line (at -33.02 -36.83 0) (length 7.62)
          (name "GND")
          (number "GND3")
        )
        (pin power_in line (at 3.81 66.04 270) (length 7.62)
          (name "SPI_GND")
          (number "GND4")
        )
        (pin power_in line (at -33.02 -39.37 0) (length 7.62)
          (name "GND")
          (number "GND5")
        )
        (pin power_in line (at -33.02 -41.91 0) (length 7.62)
          (name "GND")
          (number "GND6")
        )
        (pin output line (at -33.02 -26.67 0) (length 7.62)
          (name "IOREF")
          (number "IORF")
        )
        (pin input line (at -6.35 66.04 270) (length 7.62)
          (name "SPI_MISO")
          (number "MISO")
        )
        (pin output line (at -3.81 66.04 270) (length 7.62)
          (name "SPI_MOSI")
          (number "MOSI")
        )
        (pin open_collector input_low (at -33.02 -24.13 0) (length 7.62)
          (name "RESET")
          (number "RST1")
        )
        (pin open_collector input_low (at 6.35 66.04 270) (length 7.62)
          (name "SPI_RESET")
          (number "RST2")
        )
        (pin output clock (at -1.27 66.04 270) (length 7.62)
          (name "SPI_SCK")
          (number "SCK")
        )
        (pin bidirectional clock (at -33.02 26.67 0) (length 7.62)
          (name "SCL")
          (number "SCL")
        )
        (pin bidirectional line (at -33.02 29.21 0) (length 7.62)
          (name "SDA")
          (number "SDA")
        )
        (pin power_in line (at -33.02 -54.61 0) (length 7.62)
          (name "VIN")
          (number "VIN")
        )
      )
    )
  )
  (junction (at 175.26 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 69.85) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 20.32) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 36.83) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 119.38) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 53.34) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 135.89) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 187.96 86.36) (xy 187.96 83.82)))
  (wire (pts (xy 175.26 111.76) (xy 175.26 113.03)))
  (wire (pts (xy 175.26 69.85) (xy 186.69 69.85)))
  (wire (pts (xy 96.52 102.87) (xy 149.86 86.36)))
  (wire (pts (xy 175.26 53.34) (xy 185.42 53.34)))
  (wire (pts (xy 175.26 86.36) (xy 187.96 86.36)))
  (wire (pts (xy 116.84 162.56) (xy 175.26 162.56)))
  (wire (pts (xy 96.52 92.71) (xy 149.86 53.34)))
  (wire (pts (xy 149.86 53.34) (xy 175.26 53.34)))
  (wire (pts (xy 16.51 90.17) (xy 16.51 177.8)))
  (wire (pts (xy 175.26 86.36) (xy 175.26 87.63)))
  (wire (pts (xy 30.48 107.95) (xy 17.78 107.95)))
  (wire (pts (xy 120.65 129.54) (xy 175.26 129.54)))
  (wire (pts (xy 19.05 138.43) (xy 19.05 175.26)))
  (wire (pts (xy 30.48 95.25) (xy 13.97 95.25)))
  (wire (pts (xy 185.42 53.34) (xy 185.42 100.33)))
  (wire (pts (xy 149.86 30.48) (xy 175.26 30.48)))
  (wire (pts (xy 96.52 87.63) (xy 149.86 36.83)))
  (wire (pts (xy 184.15 36.83) (xy 184.15 105.41)))
  (wire (pts (xy 186.69 69.85) (xy 186.69 92.71)))
  (wire (pts (xy 175.26 36.83) (xy 184.15 36.83)))
  (wire (pts (xy 190.5 68.58) (xy 218.44 68.58)))
  (wire (pts (xy 30.48 97.79) (xy 12.7 97.79)))
  (wire (pts (xy 175.26 135.89) (xy 241.3 135.89)))
  (wire (pts (xy 149.86 135.89) (xy 175.26 135.89)))
  (wire (pts (xy 15.24 179.07) (xy 120.65 179.07)))
  (wire (pts (xy 15.24 92.71) (xy 15.24 179.07)))
  (wire (pts (xy 149.86 119.38) (xy 175.26 119.38)))
  (wire (pts (xy 12.7 181.61) (xy 123.19 181.61)))
  (wire (pts (xy 149.86 46.99) (xy 175.26 46.99)))
  (wire (pts (xy 175.26 45.72) (xy 175.26 46.99)))
  (wire (pts (xy 120.65 129.54) (xy 120.65 179.07)))
  (wire (pts (xy 175.26 102.87) (xy 189.23 102.87)))
  (wire (pts (xy 19.05 175.26) (xy 116.84 175.26)))
  (wire (pts (xy 175.26 20.32) (xy 182.88 20.32)))
  (wire (pts (xy 17.78 107.95) (xy 17.78 176.53)))
  (wire (pts (xy 175.26 119.38) (xy 190.5 119.38)))
  (wire (pts (xy 189.23 76.2) (xy 218.44 76.2)))
  (wire (pts (xy 175.26 95.25) (xy 175.26 96.52)))
  (wire (pts (xy 175.26 62.23) (xy 175.26 63.5)))
  (wire (pts (xy 186.69 92.71) (xy 218.44 92.71)))
  (wire (pts (xy 13.97 95.25) (xy 13.97 180.34)))
  (wire (pts (xy 149.86 36.83) (xy 175.26 36.83)))
  (wire (pts (xy 175.26 36.83) (xy 175.26 38.1)))
  (wire (pts (xy 121.92 180.34) (xy 121.92 113.03)))
  (wire (pts (xy 121.92 113.03) (xy 175.26 113.03)))
  (wire (pts (xy 187.96 83.82) (xy 218.44 83.82)))
  (wire (pts (xy 149.86 20.32) (xy 175.26 20.32)))
  (wire (pts (xy 149.86 63.5) (xy 175.26 63.5)))
  (wire (pts (xy 175.26 69.85) (xy 175.26 71.12)))
  (wire (pts (xy 96.52 118.11) (xy 149.86 135.89)))
  (wire (pts (xy 241.3 66.04) (xy 260.35 66.04)))
  (wire (pts (xy 175.26 78.74) (xy 175.26 80.01)))
  (wire (pts (xy 96.52 90.17) (xy 149.86 46.99)))
  (wire (pts (xy 175.26 53.34) (xy 175.26 54.61)))
  (wire (pts (xy 190.5 119.38) (xy 190.5 68.58)))
  (wire (pts (xy 17.78 176.53) (xy 118.11 176.53)))
  (wire (pts (xy 96.52 82.55) (xy 149.86 20.32)))
  (wire (pts (xy 175.26 152.4) (xy 175.26 154.94)))
  (wire (pts (xy 175.26 128.27) (xy 175.26 129.54)))
  (wire (pts (xy 189.23 102.87) (xy 189.23 76.2)))
  (wire (pts (xy 116.84 175.26) (xy 116.84 162.56)))
  (wire (pts (xy 96.52 95.25) (xy 149.86 63.5)))
  (wire (pts (xy 241.3 135.89) (xy 241.3 66.04)))
  (wire (pts (xy 123.19 181.61) (xy 124.46 96.52)))
  (wire (pts (xy 96.52 85.09) (xy 149.86 30.48)))
  (wire (pts (xy 13.97 180.34) (xy 121.92 180.34)))
  (wire (pts (xy 124.46 96.52) (xy 175.26 96.52)))
  (wire (pts (xy 16.51 177.8) (xy 119.38 177.8)))
  (wire (pts (xy 175.26 135.89) (xy 175.26 137.16)))
  (wire (pts (xy 118.11 152.4) (xy 175.26 152.4)))
  (wire (pts (xy 96.52 97.79) (xy 149.86 69.85)))
  (wire (pts (xy 118.11 176.53) (xy 118.11 152.4)))
  (wire (pts (xy 184.15 105.41) (xy 218.44 105.41)))
  (wire (pts (xy 30.48 138.43) (xy 19.05 138.43)))
  (wire (pts (xy 30.48 90.17) (xy 16.51 90.17)))
  (wire (pts (xy 30.48 92.71) (xy 15.24 92.71)))
  (wire (pts (xy 175.26 144.78) (xy 175.26 146.05)))
  (wire (pts (xy 175.26 21.59) (xy 175.26 20.32)))
  (wire (pts (xy 185.42 100.33) (xy 218.44 100.33)))
  (wire (pts (xy 149.86 102.87) (xy 175.26 102.87)))
  (wire (pts (xy 175.26 162.56) (xy 175.26 160.02)))
  (wire (pts (xy 175.26 102.87) (xy 175.26 104.14)))
  (wire (pts (xy 96.52 113.03) (xy 149.86 119.38)))
  (wire (pts (xy 149.86 69.85) (xy 175.26 69.85)))
  (wire (pts (xy 175.26 29.21) (xy 175.26 30.48)))
  (wire (pts (xy 119.38 146.05) (xy 175.26 146.05)))
  (wire (pts (xy 149.86 86.36) (xy 175.26 86.36)))
  (wire (pts (xy 12.7 97.79) (xy 12.7 181.61)))
  (wire (pts (xy 182.88 114.3) (xy 217.17 114.3)))
  (wire (pts (xy 119.38 146.05) (xy 119.38 177.8)))
  (wire (pts (xy 96.52 107.95) (xy 149.86 102.87)))
  (wire (pts (xy 182.88 20.32) (xy 182.88 114.3)))
  (wire (pts (xy 96.52 100.33) (xy 149.86 80.01)))
  (wire (pts (xy 175.26 119.38) (xy 175.26 120.65)))
  (wire (pts (xy 149.86 80.01) (xy 175.26 80.01)))
  (image (at 241.3 74.93) (scale 2.5931))
  (symbol (lib_id "Device:R_US") (at 175.26 107.95 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 106.6799 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 107.9499 0))
    (property "Footprint" "" (id 2) (at 176.276 108.204 90))
    (property "Datasheet" "~" (id 3) (at 175.26 107.95 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 175.26 124.46 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 123.1899 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 124.4599 0))
    (property "Footprint" "" (id 2) (at 176.276 124.714 90))
    (property "Datasheet" "~" (id 3) (at 175.26 124.46 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 175.26 25.4 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 24.1299 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 25.3999 0))
    (property "Footprint" "" (id 2) (at 176.276 25.654 90))
    (property "Datasheet" "~" (id 3) (at 175.26 25.4 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Buzzer") (at 177.8 157.48 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Buzzer" (id 0) (at 181.61 156.2099 0))
    (property "Value" "1PC" (id 1) (at 181.61 158.7499 0))
    (property "Footprint" "" (id 2) (at 177.165 154.94 90))
    (property "Datasheet" "~" (id 3) (at 177.165 154.94 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Lib_Arduino:Arduino_Mega2560_Shield") (at 63.5 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "XA?" (id 0) (at 63.5 167.64 0))
    (property "Value" "Arduino_Mega2560" (id 1) (at 63.5 167.64 0))
    (property "Footprint" "" (id 2) (at 81.28 36.83 0))
    (property "Datasheet" "https://store.arduino.cc/arduino-mega-2560-rev3" (id 3) (at 81.28 36.83 0))
    (pin "3V3")
    (pin "5V1")
    (pin "5V2")
    (pin "5V3")
    (pin "5V4")
    (pin "A0")
    (pin "A1")
    (pin "A10")
    (pin "A11")
    (pin "A12")
    (pin "A13")
    (pin "A14")
    (pin "A15")
    (pin "A2")
    (pin "A3")
    (pin "A4")
    (pin "A5")
    (pin "A6")
    (pin "A7")
    (pin "A8")
    (pin "A9")
    (pin "AREF")
    (pin "D0")
    (pin "D1")
    (pin "D10")
    (pin "D11")
    (pin "D12")
    (pin "D13")
    (pin "D14")
    (pin "D15")
    (pin "D16")
    (pin "D17")
    (pin "D18")
    (pin "D19")
    (pin "D2")
    (pin "D20")
    (pin "D21")
    (pin "D22")
    (pin "D23")
    (pin "D24")
    (pin "D25")
    (pin "D26")
    (pin "D27")
    (pin "D28")
    (pin "D29")
    (pin "D3")
    (pin "D30")
    (pin "D31")
    (pin "D32")
    (pin "D33")
    (pin "D34")
    (pin "D35")
    (pin "D36")
    (pin "D37")
    (pin "D38")
    (pin "D39")
    (pin "D4")
    (pin "D40")
    (pin "D41")
    (pin "D42")
    (pin "D43")
    (pin "D44")
    (pin "D45")
    (pin "D46")
    (pin "D47")
    (pin "D48")
    (pin "D49")
    (pin "D5")
    (pin "D50")
    (pin "D51")
    (pin "D52")
    (pin "D53")
    (pin "D6")
    (pin "D7")
    (pin "D8")
    (pin "D9")
    (pin "GND1")
    (pin "GND2")
    (pin "GND3")
    (pin "GND4")
    (pin "GND5")
    (pin "GND6")
    (pin "IORF")
    (pin "MISO")
    (pin "MOSI")
    (pin "RST1")
    (pin "RST2")
    (pin "SCK")
    (pin "SCL")
    (pin "SDA")
    (pin "VIN")
  )
  (symbol (lib_id "Device:R_US") (at 175.26 58.42 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 57.1499 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 58.4199 0))
    (property "Footprint" "" (id 2) (at 176.276 58.674 90))
    (property "Datasheet" "~" (id 3) (at 175.26 58.42 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 175.26 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 90.1699 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 91.4399 0))
    (property "Footprint" "" (id 2) (at 176.276 91.694 90))
    (property "Datasheet" "~" (id 3) (at 175.26 91.44 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 175.26 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 139.6999 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 140.9699 0))
    (property "Footprint" "" (id 2) (at 176.276 141.224 90))
    (property "Datasheet" "~" (id 3) (at 175.26 140.97 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 175.26 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 73.6599 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 74.9299 0))
    (property "Footprint" "" (id 2) (at 176.276 75.184 90))
    (property "Datasheet" "~" (id 3) (at 175.26 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 175.26 41.91 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 177.8 40.6399 0))
    (property "Value" "1MΩ" (id 1) (at 177.8 41.9099 0))
    (property "Footprint" "" (id 2) (at 176.276 42.164 90))
    (property "Datasheet" "~" (id 3) (at 175.26 41.91 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "Buzzer") (unit 1) (value "1PC") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1MΩ") (footprint "")
    )
    (path
      (reference "XA?") (unit 1) (value "Arduino_Mega2560") (footprint "")
    )
  )
)
