(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ESP32_NODEMCU" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U?" (id 0) (at 0 35.56 0))
    (property "Value" "ESP32_NODEMCU" (id 1) (at 0 33.02 0))
    (property "Footprint" "MODULE_ESP32_NODEMCU" (id 2) (at 2.54 33.02 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "STANDARD" "Manufacturer Recommendations" (id 4) (at 5.08 -38.1 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "6.6 mm" (id 5) (at 0 0 0))
    (property "MANUFACTURER" "Espressif" (id 6) (at -2.54 -12.7 0))
    (property "ki_locked" "" (id 7) (at 0 0 0))
    (symbol "ESP32_NODEMCU_0_0"
      (pin power_in line (at -15.24 27.94 0) (length 5.08)
        (name "3V3")
        (number "1")
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 5.08)
        (name "D19")
        (number "10")
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 5.08)
        (name "D21")
        (number "11")
      )
      (pin input line (at -15.24 -10.16 0) (length 5.08)
        (name "RX0")
        (number "12")
      )
      (pin output line (at -15.24 -12.7 0) (length 5.08)
        (name "TX0")
        (number "13")
      )
      (pin bidirectional line (at -15.24 -17.78 0) (length 5.08)
        (name "D22")
        (number "14")
      )
      (pin bidirectional line (at -15.24 -20.32 0) (length 5.08)
        (name "D23")
        (number "15")
      )
      (pin bidirectional line (at 13.97 -12.7 180) (length 5.08)
        (name "EN")
        (number "16")
      )
      (pin input line (at 13.97 -10.16 180) (length 5.08)
        (name "VP_D36")
        (number "17")
      )
      (pin input line (at 13.97 -7.62 180) (length 5.08)
        (name "VN_D39")
        (number "18")
      )
      (pin input line (at 13.97 -2.54 180) (length 5.08)
        (name "D34")
        (number "19")
      )
      (pin power_in line (at -15.24 25.4 0) (length 5.08)
        (name "GND")
        (number "2")
      )
      (pin input line (at 13.97 0 180) (length 5.08)
        (name "D35")
        (number "20")
      )
      (pin bidirectional line (at 13.97 2.54 180) (length 5.08)
        (name "D32")
        (number "21")
      )
      (pin bidirectional line (at 13.97 5.08 180) (length 5.08)
        (name "D33")
        (number "22")
      )
      (pin bidirectional line (at 13.97 7.62 180) (length 5.08)
        (name "D25")
        (number "23")
      )
      (pin bidirectional line (at 13.97 10.16 180) (length 5.08)
        (name "D26")
        (number "24")
      )
      (pin bidirectional line (at 13.97 12.7 180) (length 5.08)
        (name "D27")
        (number "25")
      )
      (pin bidirectional line (at 13.97 15.24 180) (length 5.08)
        (name "D14")
        (number "26")
      )
      (pin bidirectional line (at 13.97 17.78 180) (length 5.08)
        (name "D12")
        (number "27")
      )
      (pin bidirectional line (at 13.97 20.32 180) (length 5.08)
        (name "D13")
        (number "28")
      )
      (pin power_in line (at 13.97 25.4 180) (length 5.08)
        (name "GND")
        (number "29")
      )
      (pin bidirectional line (at -15.24 20.32 0) (length 5.08)
        (name "D15")
        (number "3")
      )
      (pin power_in line (at 13.97 27.94 180) (length 5.08)
        (name "5V")
        (number "30")
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 5.08)
        (name "D2")
        (number "4")
      )
      (pin bidirectional line (at -15.24 15.24 0) (length 5.08)
        (name "D4")
        (number "5")
      )
      (pin input line (at -15.24 10.16 0) (length 5.08)
        (name "RX2")
        (number "6")
      )
      (pin output line (at -15.24 7.62 0) (length 5.08)
        (name "TX2")
        (number "7")
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 5.08)
        (name "D5")
        (number "8")
      )
      (pin bidirectional line (at -15.24 0 0) (length 5.08)
        (name "D18")
        (number "9")
      )
    )
  )
)
