(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "3.3")
  (net 3 "DHT22_Val2")
  (net 4 "unconnected-(J1-Pad4)")
  (net 5 "DHT22_Val1")
  (net 6 "unconnected-(J2-Pad4)")
  (net 7 "SCL")
  (net 8 "SDA")
  (net 9 "unconnected-(J4-Pad2)")
  (net 10 "unconnected-(J4-Pad3)")
  (net 11 " V.Battery")
  (net 12 "Temp_Val")
  (net 13 "unconnected-(J5-Pad4)")
  (net 14 "unconnected-(J6-Pad4)")
  (net 15 "DOUT")
  (net 16 "SCK")
  (net 17 "Value B")
  (net 18 "unconnected-(U1-Pad1)")
  (net 19 "unconnected-(U1-Pad4)")
  (net 20 "unconnected-(U1-Pad9)")
  (net 21 "unconnected-(U1-Pad10)")
  (net 22 "unconnected-(U1-Pad11)")
  (net 23 "unconnected-(U1-Pad12)")
  (net 24 "unconnected-(U1-Pad13)")
  (net 25 "unconnected-(U1-Pad14)")
  (net 26 "unconnected-(U1-Pad15)")
  (net 27 "unconnected-(U1-Pad16)")
  (net 28 "unconnected-(U1-Pad17)")
  (net 29 "unconnected-(U1-Pad18)")
  (net 30 "unconnected-(U1-Pad19)")
  (net 31 "unconnected-(U1-Pad22)")
  (net 32 "unconnected-(U1-Pad23)")
  (net 33 "unconnected-(U1-Pad24)")
  (net 34 "unconnected-(U1-Pad27)")
  (net 35 "unconnected-(U1-Pad28)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 161.925 42.005 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 10.16 -2.45 90) (layer "F.SilkS"))
    (fp_text value "100 Ohm" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 " V.Battery") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Value B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 164.02 83.185 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -4.445 -2.985 90) (layer "F.SilkS"))
    (fp_text value "Gravity WattMeter" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "3.3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "SDA") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 170.18 56.165 180)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.06) (layer "F.SilkS"))
    (fp_text value "Battery Reader" (at 0 8.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "unconnected-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J4-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 " V.Battery") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 115.38 89.535 90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "HX711" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "3.3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "DOUT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "SCK") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 161.925 59.42 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "100 Ohm" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Value B") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 115.285 67.945 90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.89) (layer "F.SilkS"))
    (fp_text value "DHT22" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "3.3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "DHT22_Val1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "unconnected-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 115.285 59.69 90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Temp2" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "3.3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Temp_Val") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J6-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 115.19 52.705 90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.795 90) (layer "F.SilkS"))
    (fp_text value "Temp1" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "3.3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Temp_Val") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MKR WAN:MKR WAN" (layer "F.Cu")
    (tedit 6391A316)
    (at 127.635 46.355 -90)
    (property "MANUFACTURER" "Arduino")
    (property "MAXIMUM_PACKAGE_HEIGHT" "")
    (property "PARTREV" "5")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 4.075 -26.535 90) (layer "F.SilkS"))
    (fp_text value "MKR WAN" (at 11.06 1.165 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 59.25 -22.75 270) (size 2.25 2.25) (drill 2.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 59.25 -2.25 270) (size 2.25 2.25) (drill 2.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.25 -22.75 270) (size 2.25 2.25) (drill 2.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.25 -2.25 270) (size 2.25 2.25) (drill 2.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 22.1348 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(U1-Pad1)") (pinfunction "PA03_VREFA/AREF") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at 24.6748 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Value B") (pinfunction "PA02_AIN0/DAC0/A0") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 27.2148 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Temp_Val") (pinfunction "PB02_AIN10/A1") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 29.7548 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(U1-Pad4)") (pinfunction "PB03_AIN11/A2") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at 32.2948 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 5 "DHT22_Val1") (pinfunction "PA04_AIN4/A3") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at 34.8348 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 3 "DHT22_Val2") (pinfunction "PA05_AIN5/A4") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at 37.3748 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 15 "DOUT") (pinfunction "PA06_AIN6/A5") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 39.9148 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 16 "SCK") (pinfunction "PA07_AIN7/A6") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 42.4548 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U1-Pad9)") (pinfunction "PA22_TC4-W0/0") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 44.9948 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(U1-Pad10)") (pinfunction "PA23_TC4-W1/1") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at 47.5348 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U1-Pad11)") (pinfunction "PA10_TCC0-W2/~2") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at 50.0748 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-Pad12)") (pinfunction "PA11_TCC0-W3/~3") (pintype "bidirectional"))
    (pad "13" thru_hole circle (at 52.6148 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U1-Pad13)") (pinfunction "PB10_TCC0-W4/~4") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 55.1548 -2.34 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U1-Pad14)") (pinfunction "PB11_TCC0-W5/~5") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 55.1548 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U1-Pad15)") (pinfunction "PA20_TCC0-W6") (pintype "bidirectional"))
    (pad "16" thru_hole circle (at 52.6148 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(U1-Pad16)") (pinfunction "PA21_TCC0-W7") (pintype "bidirectional"))
    (pad "17" thru_hole circle (at 50.0748 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(U1-Pad17)") (pinfunction "PA16_S1_MOSI") (pintype "bidirectional"))
    (pad "18" thru_hole circle (at 47.5348 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(U1-Pad18)") (pinfunction "PA17_S1_SCK") (pintype "bidirectional"))
    (pad "19" thru_hole circle (at 44.9948 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 30 "unconnected-(U1-Pad19)") (pinfunction "PA19_S1_MISO") (pintype "bidirectional"))
    (pad "20" thru_hole circle (at 42.4548 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 8 "SDA") (pinfunction "PA08_S0_I2C_SDA") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 39.9148 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 7 "SCL") (pinfunction "PA09_S0_I2C_SCL") (pintype "bidirectional"))
    (pad "22" thru_hole circle (at 37.3748 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 31 "unconnected-(U1-Pad22)") (pinfunction "PB23_S5_RX") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at 34.8348 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 32 "unconnected-(U1-Pad23)") (pinfunction "PB22_S5_TX") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at 32.2948 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 33 "unconnected-(U1-Pad24)") (pinfunction "RESET") (pintype "input"))
    (pad "25" thru_hole circle (at 29.7548 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "26" thru_hole circle (at 27.2148 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3") (pinfunction "+3V3") (pintype "power_in"))
    (pad "27" thru_hole circle (at 24.6748 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 34 "unconnected-(U1-Pad27)") (pinfunction "VIN") (pintype "power_in"))
    (pad "28" thru_hole circle (at 22.1348 -22.66 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 35 "unconnected-(U1-Pad28)") (pinfunction "+5V") (pintype "power_in"))
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 115.285 78.74 90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.54 90) (layer "F.SilkS"))
    (fp_text value "DHT22" (at 0 10.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "3.3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "DHT22_Val2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 110.49 39.37) (end 177.165 39.37) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 177.165 110.49) (end 111.125 110.49) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.49 110.49) (end 112.395 110.49) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 177.165 39.37) (end 177.165 110.49) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.49 39.37) (end 110.49 110.49) (layer "Edge.Cuts") (width 0.1))
  (gr_text "EI-2I4 PROJET" (at 171.45 78.105 -90) (layer "Edge.Cuts"))
  (gr_text "BRIRMI-COURIVAULT-LAVINAY" (at 173.99 77.47 -90) (layer "User.1"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.165 110.49)
        (xy 110.49 110.49)
        (xy 110.503616 39.37)
        (xy 177.165 39.37)
      )
    )
  )
)
