(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001000_fffffffe)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "TX")
  (net 2 "RX")
  (net 3 "unconnected-(A0-Pad3)")
  (net 4 "GND")
  (net 5 "Dout")
  (net 6 "Psck")
  (net 7 "TH1")
  (net 8 "Temp")
  (net 9 "TH2")
  (net 10 "unconnected-(A0-Pad5)")
  (net 11 "unconnected-(A0-Pad13)")
  (net 12 "unconnected-(A0-Pad7)")
  (net 13 "unconnected-(A0-Pad15)")
  (net 14 "unconnected-(A0-Pad9)")
  (net 15 "Alim")
  (net 16 "unconnected-(A0-Pad18)")
  (net 17 "Micro")
  (net 18 "unconnected-(A0-Pad20)")
  (net 19 "unconnected-(A0-Pad21)")
  (net 20 "unconnected-(A0-Pad22)")
  (net 21 "SDA")
  (net 22 "SCL")
  (net 23 "unconnected-(A0-Pad25)")
  (net 24 "VBat")
  (net 25 "unconnected-(A0-Pad27)")
  (net 26 "unconnected-(A0-Pad28)")
  (net 27 "unconnected-(A0-Pad30)")
  (net 28 "AlimCapt")
  (net 29 "unconnected-(JMicro1-Pad4)")
  (net 30 "unconnected-(JTH1-Pad4)")
  (net 31 "unconnected-(JTH2-Pad4)")
  (net 32 "SHDN")
  (net 33 "unconnected-(A0-Pad11)")
  (net 34 "Net-(JConv1-Pad3)")
  (net 35 "unconnected-(JBat1-Pad3)")
  (net 36 "unconnected-(JBat1-Pad4)")
  (net 37 "unconnected-(JT1-Pad3)")
  (net 38 "unconnected-(JT2-Pad3)")
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 67.31 75.74)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Jlum1" (at 0 -2.06) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "AlimCapt") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "SDA") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.25 80.01 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.254724 -3.81 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "VBat") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(JConv1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 67.31 98.33)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Jlora1" (at 0 -2.06) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Alim") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "RX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "TX") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 124.45 74.93 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JConv2" (at -1.905 -2.965 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "AlimCapt") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(JConv1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "SHDN") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 74.12 110.49 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Alim") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Dout") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Psck") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 124.92 110.49 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JTH2" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "AlimCapt") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "TH2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "unconnected-(JTH2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 67.31 87.17)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JMicro1" (at 0 -2.06) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "AlimCapt") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Micro") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "unconnected-(JMicro1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 99.79 110.49 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JT2" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "AlimCapt") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "unconnected-(JT2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Temp") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 86.82 110.49 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JTH1" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "AlimCapt") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "TH1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "unconnected-(JTH1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Module:Arduino_Nano" (layer "F.Cu")
    (tedit 58ACAF70)
    (at 85.09 100.32 90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A0" (at 7.62 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Arduino_Nano_v3.x" (at 8.89 19.05) (layer "F.Fab"))
    (fp_text user "USB" (at 7.62 35.56 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.35 19.05) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "TX") (pinfunction "D1/TX") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "RX") (pinfunction "D0/RX") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(A0-Pad3)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(A0-Pad5)") (pinfunction "D2") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Dout") (pinfunction "D3") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(A0-Pad7)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Psck") (pinfunction "D5") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(A0-Pad9)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "TH1") (pinfunction "D7") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 33 "unconnected-(A0-Pad11)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Temp") (pinfunction "D9") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(A0-Pad13)") (pinfunction "D10") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "TH2") (pinfunction "D11") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(A0-Pad15)") (pinfunction "D12") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "SHDN") (pinfunction "D13") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Alim") (pinfunction "3V3") (pintype "power_out"))
    (pad "18" thru_hole oval (at 15.24 30.48 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(A0-Pad18)") (pinfunction "AREF") (pintype "input"))
    (pad "19" thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Micro") (pinfunction "A0") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at 15.24 25.4 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(A0-Pad20)") (pinfunction "A1") (pintype "bidirectional"))
    (pad "21" thru_hole oval (at 15.24 22.86 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(A0-Pad21)") (pinfunction "A2") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 15.24 20.32 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(A0-Pad22)") (pinfunction "A3") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "SDA") (pinfunction "A4") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "SCL") (pinfunction "A5") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 15.24 12.7 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(A0-Pad25)") (pinfunction "A6") (pintype "bidirectional"))
    (pad "26" thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "VBat") (pinfunction "A7") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 15.24 7.62 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(A0-Pad27)") (pinfunction "+5V") (pintype "power_out"))
    (pad "28" thru_hole oval (at 15.24 5.08 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(A0-Pad28)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "29" thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval (at 15.24 0 90) (size 1 1) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(A0-Pad30)") (pinfunction "VIN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 107.94 74.93 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JConv1" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Alim") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(JConv1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(JConv1-Pad3)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.71 80.01 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0.254724 -3.81 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "VBat") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 112.49 110.49 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JT1" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "AlimCapt") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "unconnected-(JT1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Temp") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 86.82 74.93 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "Fichier: PCB_montage.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JBat1" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JConv1-Pad3)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "unconnected-(JBat1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "unconnected-(JBat1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 59.055 67.31) (end 128.905 67.31) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 128.905 118.11) (end 59.055 118.11) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 128.905 67.31) (end 128.905 118.11) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 59.055 118.11) (end 59.055 83.185) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 59.055 83.185) (end 59.055 67.31) (layer "Edge.Cuts") (width 0.2))
  (zone (net 4) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.905 118.11)
        (xy 59.055 118.11)
        (xy 59.055 67.31)
        (xy 128.905 67.31)
      )
    )
  )
)
