(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J4-Pad1)")
  (net 2 "unconnected-(J4-Pad2)")
  (net 3 "unconnected-(J4-Pad3)")
  (net 4 "unconnected-(J4-Pad4)")
  (net 5 "unconnected-(J4-Pad5)")
  (net 6 "unconnected-(J4-Pad6)")
  (net 7 "Net-(CAP5-Pad1)")
  (net 8 "Net-(CAP6-Pad1)")
  (net 9 "Net-(CAP7-Pad1)")
  (net 10 "unconnected-(J2-Pad4)")
  (net 11 "unconnected-(J2-Pad5)")
  (net 12 "unconnected-(J2-Pad6)")
  (net 13 "unconnected-(J2-Pad7)")
  (net 14 "unconnected-(J2-Pad8)")
  (net 15 "unconnected-(J3-Pad1)")
  (net 16 "unconnected-(J3-Pad2)")
  (net 17 "unconnected-(J3-Pad3)")
  (net 18 "unconnected-(J3-Pad4)")
  (net 19 "unconnected-(J3-Pad5)")
  (net 20 "unconnected-(J3-Pad8)")
  (net 21 "unconnected-(J4-Pad7)")
  (net 22 "unconnected-(J4-Pad8)")
  (net 23 "unconnected-(J4-Pad9)")
  (net 24 "unconnected-(J4-Pad10)")
  (net 25 "unconnected-(J4-Pad11)")
  (net 26 "unconnected-(J4-Pad12)")
  (net 27 "unconnected-(J4-Pad13)")
  (net 28 "unconnected-(J4-Pad14)")
  (net 29 "unconnected-(J4-Pad15)")
  (net 30 "unconnected-(J4-Pad16)")
  (net 31 "Net-(J1-Pad10)")
  (net 32 "Net-(J1-Pad9)")
  (net 33 "Net-(CAP10-Pad1)")
  (net 34 "Net-(CAP11-Pad1)")
  (net 35 "Net-(CAP12-Pad1)")
  (net 36 "Net-(J1-Pad5)")
  (net 37 "Net-(J1-Pad3)")
  (net 38 "Net-(J1-Pad2)")
  (net 39 "Net-(J1-Pad1)")
  (net 40 "Net-(CAP1-Pad1)")
  (net 41 "Net-(CAP2-Pad1)")
  (net 42 "Net-(CAP3-Pad1)")
  (net 43 "Net-(CAP4-Pad1)")
  (net 44 "Net-(J1-Pad8)")
  (net 45 "Net-(J1-Pad7)")
  (net 46 "Net-(J1-Pad6)")
  (net 47 "Net-(CAP8-Pad1)")
  (net 48 "Net-(CAP9-Pad1)")
  (net 49 "GND")
  (net 50 "Net-(J2-Pad1)")
  (net 51 "Net-(J2-Pad2)")
  (net 52 "Net-(J2-Pad3)")
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D32A)
    (at 95.5 53.721)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP3" (at 0 -4.765 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 42 "Net-(CAP3-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D32A)
    (at 83.058 73.097)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP5" (at 0 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 7 "Net-(CAP5-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63DD2BF1)
    (at 83.058 53.721)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP2" (at -0.315 -4.63 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 41 "Net-(CAP2-Pad1)") (pinfunction "1") (pintype "passive") (zone_connect 0))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63DD2C2C)
    (at 69.64 53.721)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP1" (at 0 -4.388 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 40 "Net-(CAP1-Pad1)") (pinfunction "1") (pintype "passive") (zone_connect 0))
  )
  (footprint "Headers_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 107 56.075)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x10_Male" (at -3.175 22.142) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D32A)
    (at 83.058 95.957)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP8" (at 0 -4.705 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 47 "Net-(CAP8-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D32A)
    (at 69.64 73.097)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP4" (at 0 -4.81 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 43 "Net-(CAP4-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D32A)
    (at 95.5 95.957)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP9" (at 0 -4.445 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 48 "Net-(CAP9-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D38E)
    (at 95.5 116.717)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP12" (at 0 -4.445 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at -0.127 -5.588 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 35 "Net-(CAP12-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D38E)
    (at 83.058 116.717)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP11" (at 0.254 -4.445 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at -0.127 -5.588 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 34 "Net-(CAP11-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Headers_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 59 66.4)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J3-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J3-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D38E)
    (at 69.64 116.717)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP10" (at 0 -4.445 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at -0.127 -5.588 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 33 "Net-(CAP10-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Headers_2.54mm:PinHeader_2x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 59 89.25)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 1.27 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J4-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J4-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "unconnected-(J4-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J4-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J4-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J4-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J4-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J4-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J4-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(J4-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J4-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J4-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "unconnected-(J4-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D32A)
    (at 69.64 95.957)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP7" (at -0.195 -4.795 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 9 "Net-(CAP7-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "InakiNagore_Library_Footprint:CapacitiveSensor" (layer "F.Cu")
    (tedit 63A8D32A)
    (at 95.5 73.097)
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (clearance 1)
    (fp_text reference "CAP6" (at 0.18 -4.93 unlocked) (layer "F.SilkS"))
    (fp_text value "CapacitiveButton" (at 0 -8.255 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 -0.127) (size 7 7) (layers "F.Cu")
      (net 8 "Net-(CAP6-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Headers_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 107 83)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -0.1 -2) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J2-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J2-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J2-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 102.875 94 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(CAP12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J2-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 103 58)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(CAP2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 103 75.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(CAP7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J1-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 103 55.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -2.55 0.1) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(CAP3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 103 72.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(CAP6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J1-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 103 82)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(CAP9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(J1-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 102.91 86.11 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(CAP10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(J2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 102.925 69.65)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(CAP5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 102.925 61.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(CAP1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 102.725 89.55 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(CAP11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 102.85 66.15)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -2.325 0.9) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(CAP4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 103 79)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "CapacitiveKeypad.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(CAP8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J1-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 105.664 38.4) (end 60.4 38.349254) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 105.664 38.4) (mid 109.04397 39.80003) (end 110.444 43.18) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 110.5 124.734466) (mid 109.035534 128.27) (end 105.5 129.734466) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 55.499254 43.25) (end 55.5 124.734466) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 55.499254 43.25) (mid 56.93465 39.78465) (end 60.4 38.349254) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 60.5 129.734466) (mid 56.964466 128.27) (end 55.5 124.734466) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 60.5 129.734466) (end 105.5 129.734466) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 110.5 124.734466) (end 110.444 43.18) (layer "Edge.Cuts") (width 0.2))
  (zone (net 49) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.508) (thermal_bridge_width 0.508)
      (hatch_thickness 0.254) (hatch_gap 1.143) (hatch_orientation 45)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 117.266007 133.251246)
        (xy 50.210007 132.743246)
        (xy 49.784 26.416)
        (xy 118.364 26.416)
      )
    )
  )
  (zone (net 49) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.508) (thermal_bridge_width 0.508)
      (hatch_thickness 0.254) (hatch_gap 1.778) (hatch_orientation 45)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 116.84 132.969)
        (xy 49.276 132.969)
        (xy 50.292 26.924)
        (xy 117.856 26.416)
      )
    )
  )
)
