(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "OM5-Gerber/")
    )
  )
  (net 0 "")
  (net 1 "Net-(E1-Pad133)")
  (net 2 "Net-(A1-Pad2)")
  (net 3 "Net-(A1-Pad1)")
  (net 4 "unconnected-(Ch1-Pad1)")
  (net 5 "Net-(A4-Pad1)")
  (net 6 "Net-(A2-Pad2)")
  (net 7 "Net-(A3-Pad2)")
  (net 8 "Net-(A4-Pad2)")
  (net 9 "Net-(A5-Pad2)")
  (net 10 "Net-(A6-Pad2)")
  (net 11 "Net-(Ch1-Pad3)")
  (net 12 "Net-(Ch1-Pad4)")
  (net 13 "unconnected-(Ch1-Pad2)")
  (net 14 "unconnected-(E1-Pad0)")
  (net 15 "Net-(E1-Pad1)")
  (net 16 "Net-(E1-Pad2)")
  (net 17 "Net-(E1-Pad3)")
  (net 18 "Net-(E1-Pad4)")
  (net 19 "Net-(E1-Pad5)")
  (net 20 "Net-(E1-Pad6)")
  (net 21 "Net-(E1-Pad7)")
  (net 22 "Net-(E1-Pad14)")
  (net 23 "Net-(E1-Pad15)")
  (net 24 "Net-(E1-Pad16)")
  (net 25 "Net-(E1-Pad17)")
  (net 26 "Net-(E1-Pad18)")
  (net 27 "unconnected-(E1-Pad21)")
  (net 28 "Net-(E1-Pad33)")
  (net 29 "Net-(E1-Pad34)")
  (net 30 "unconnected-(E1-Pad37)")
  (net 31 "unconnected-(E1-Pad38)")
  (net 32 "unconnected-(E1-Pad39)")
  (net 33 "unconnected-(E1-Pad40)")
  (net 34 "Net-(J1-Pad10)")
  (net 35 "Net-(Ch1-Pad6)")
  (net 36 "Net-(E1-Pad150)")
  (net 37 "Net-(E1-Pad35)")
  (net 38 "Net-(E1-Pad36)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 181.61 78.105)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Male" (at 0 4.87) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Ch1-Pad3)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(Ch1-Pad4)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F)
    (at 165.01 82.55)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NC1" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 20 "Net-(E1-Pad6)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(A1-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 158.75 110.49 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Ch1" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "3.7_Charge_MH_CD42" (at 0 15.03 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(Ch1-Pad1)") (pinfunction "VIN") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(Ch1-Pad2)") (pinfunction "IN-GND") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Ch1-Pad3)") (pinfunction "BAT-GND") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(Ch1-Pad4)") (pinfunction "BAT+") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "OUT-GND") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(Ch1-Pad6)") (pinfunction "OUT-5V") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 184.15 102.87)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Five2" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Male" (at 0 4.87) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(E1-Pad150)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(Ch1-Pad6)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 153.67 82.55)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Head1x10-OMv5" (at 0 25.19) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(E1-Pad6)") (pinfunction "ACD0") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(E1-Pad5)") (pinfunction "ADC1") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(E1-Pad4)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(E1-Pad3)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(E1-Pad2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(E1-Pad1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(E1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(E1-Pad14)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(E1-Pad133)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F)
    (at 165.01 88.9)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NC3" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 18 "Net-(E1-Pad4)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(A3-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "00TTXfootprint:ESP32-S2-mini" (layer "F.Cu")
    (tedit 0)
    (at 170.18 73.66)
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "E1" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "ESP32-S2-Mini" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -11.43 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "unconnected-(E1-Pad0)") (pinfunction "EN") (pintype "input"))
    (pad "1" thru_hole circle (at -8.89 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(E1-Pad1)") (pinfunction "ADC1_0") (pintype "input"))
    (pad "2" thru_hole circle (at -8.89 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(E1-Pad2)") (pinfunction "ADC1_1") (pintype "input"))
    (pad "3" thru_hole circle (at -11.43 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(E1-Pad3)") (pinfunction "ADC1_2") (pintype "input"))
    (pad "4" thru_hole circle (at -8.89 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(E1-Pad4)") (pinfunction "ADC1_3") (pintype "input"))
    (pad "5" thru_hole circle (at -11.43 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(E1-Pad5)") (pinfunction "ADC1_4") (pintype "input"))
    (pad "6" thru_hole circle (at -8.89 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(E1-Pad6)") (pinfunction "ADC1_5") (pintype "input"))
    (pad "7" thru_hole circle (at -11.43 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(E1-Pad7)") (pinfunction "ADC1_6") (pintype "input"))
    (pad "8" thru_hole circle (at -8.89 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(A6-Pad2)") (pinfunction "ADC1_7") (pintype "input"))
    (pad "9" thru_hole circle (at -11.43 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(A5-Pad2)") (pinfunction "ADC1_8") (pintype "input"))
    (pad "10" thru_hole circle (at -8.89 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(A4-Pad2)") (pinfunction "ADC1_9") (pintype "input"))
    (pad "11" thru_hole circle (at -11.43 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(A3-Pad2)") (pinfunction "ADC2_0") (pintype "input"))
    (pad "12" thru_hole circle (at -11.43 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(A2-Pad2)") (pinfunction "ADC2_1") (pintype "input"))
    (pad "13" thru_hole circle (at -8.89 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad2)") (pinfunction "ADC2_2") (pintype "input"))
    (pad "14" thru_hole circle (at -8.89 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(E1-Pad14)") (pinfunction "ADC2_3") (pintype "input"))
    (pad "15" thru_hole circle (at 8.89 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(E1-Pad15)") (pinfunction "ADC2_4") (pintype "input"))
    (pad "16" thru_hole circle (at 11.43 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(E1-Pad16)") (pinfunction "ADC2_5") (pintype "input"))
    (pad "17" thru_hole circle (at 8.89 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(E1-Pad17)") (pinfunction "ADC2_6") (pintype "input"))
    (pad "18" thru_hole circle (at 11.43 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(E1-Pad18)") (pinfunction "ADC2_7") (pintype "input"))
    (pad "21" thru_hole circle (at 8.89 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "unconnected-(E1-Pad21)") (pinfunction "21") (pintype "input"))
    (pad "33" thru_hole circle (at 11.43 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(E1-Pad33)") (pinfunction "FSPI_HD_io4") (pintype "input"))
    (pad "34" thru_hole circle (at 8.89 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(E1-Pad34)") (pinfunction "FSPI_SCO_dqs") (pintype "input"))
    (pad "35" thru_hole circle (at 11.43 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(E1-Pad35)") (pinfunction "FSPI_D_io6") (pintype "input"))
    (pad "36" thru_hole circle (at 8.89 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(E1-Pad36)") (pinfunction "FSPI_CLK_io7") (pintype "input"))
    (pad "37" thru_hole circle (at 11.43 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "unconnected-(E1-Pad37)") (pinfunction "FSPI_Q") (pintype "input"))
    (pad "38" thru_hole circle (at 8.89 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "unconnected-(E1-Pad38)") (pinfunction "FSPI_WP") (pintype "input"))
    (pad "39" thru_hole circle (at 11.43 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "unconnected-(E1-Pad39)") (pinfunction "CLK3") (pintype "input"))
    (pad "40" thru_hole circle (at 8.89 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "unconnected-(E1-Pad40)") (pinfunction "CLK2") (pintype "input"))
    (pad "129" thru_hole circle (at 8.89 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "GND") (pintype "input"))
    (pad "130" thru_hole circle (at 11.43 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "GND") (pintype "input"))
    (pad "133" thru_hole circle (at -11.43 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(E1-Pad133)") (pinfunction "3.3V") (pintype "input"))
    (pad "150" thru_hole circle (at 11.43 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(E1-Pad150)") (pinfunction "VBUS") (pintype "input"))
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 170.03 91.385)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(E1-Pad35)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(E1-Pad35)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 156.21 102.87)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Five1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Male" (at 0 4.87) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(E1-Pad150)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(Ch1-Pad6)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 154.94 109.22)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 3.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 158.75 77.47 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "S1" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "SSD1306" (at 0 9.95 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "GND") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(E1-Pad150)") (pinfunction "VCC") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(E1-Pad33)") (pinfunction "SCL") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(E1-Pad34)") (pinfunction "SDA") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F)
    (at 165.01 98.425)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NC6" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at -43.75 7.365) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(E1-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(A6-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 185.42 109.22)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 3.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F)
    (at 165.01 95.25)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NC5" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 16 "Net-(E1-Pad2)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(A5-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 185.42 78.74)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at -16.727 19.71) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F)
    (at 165.01 85.725)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NC2" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 19 "Net-(E1-Pad5)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(A2-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 154.94 78.74)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 186.69 82.55)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Head1x10-OMv5" (at 0 25.19) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad2)") (pinfunction "ACD0") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(A2-Pad2)") (pinfunction "ADC1") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(A3-Pad2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(A4-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(A5-Pad2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(A6-Pad2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(E1-Pad16)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(E1-Pad15)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(E1-Pad133)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 180.34 110.49 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "SW_SPST" (at 0 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(E1-Pad150)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(Ch1-Pad6)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 170.03 77.415)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.25 -2) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(E1-Pad36)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(E1-Pad36)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F)
    (at 165.19 92.075)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NC4" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 17 "Net-(E1-Pad3)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(A4-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "B.Cu")
    (tedit 5A1DD157)
    (at 175.895 100.33 -90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 1.27 3.56 90) (layer "B.SilkS"))
    (fp_text value "DRV5033AJxLPG" (at 1.27 -2.79 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(E1-Pad133)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(A4-Pad1)") (pinfunction "OUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 101.6 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 26 "Net-(E1-Pad18)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(A1-Pad1)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 104.775 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 25 "Net-(E1-Pad17)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 5 "Net-(A4-Pad1)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 95.25 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "A5" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 5 "Net-(A4-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 9 "Net-(A5-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 92.075 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "A4" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 5 "Net-(A4-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 8 "Net-(A4-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "B.Cu")
    (tedit 5A1DD157)
    (at 175.895 85.09 -90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 1.27 3.56 90) (layer "B.SilkS"))
    (fp_text value "DRV5033AJxLPG" (at 1.27 -2.79 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(E1-Pad133)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad10)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad1)") (pinfunction "OUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 85.725 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "A2" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(A1-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 6 "Net-(A2-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 88.9 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "A3" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(A1-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 7 "Net-(A3-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 98.425 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "A6" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 5 "Net-(A4-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 10 "Net-(A6-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 165.01 82.55 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "OpenMuscle5.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "A1" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab") hide)
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(A1-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 2 "Net-(A1-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (gr_rect (start 152.4 76.2) (end 187.96 111.76) (layer "Edge.Cuts") (width 0.1) (fill none))
)
