(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "Stat Tracker")
    (date "2023-06-10")
    (rev "2.1")
    (comment 1 "Added a jack for triggering external hardware")
  )
  (lib_symbols
    (symbol "35RAPC4BV4:35RAPC4BV4" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -5.08 7.62 0))
      (property "Value" "35RAPC4BV4" (id 1) (at -5.08 -7.62 0))
      (property "Footprint" "SWITCHCRAFT_35RAPC4BV4" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "PARTREV" "G" (id 4) (at 0 0 0))
      (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 0 0 0))
      (property "MAXIMUM_PACKAGE_HIEGHT" "12.573mm" (id 6) (at 0 0 0))
      (property "MANUFACTURER" "Switchcraft Inc." (id 7) (at 0 0 0))
      (symbol "35RAPC4BV4_0_0"
        (rectangle (start -6.1079 -3.6883) (end 4.6871 6.4717)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -5.715 2.413)
            (xy -5.08 2.413)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.413)
            (xy -4.445 2.413)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy -5.08 2.413)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 -2.286)
            (xy -5.715 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 2.413)
            (xy -4.445 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 1.143)
            (xy -2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.54)
            (xy -1.905 1.143)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.381 -3.683)
            (xy -1.016 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 -5.08)
            (xy -0.381 -3.683)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.778 -2.54)
            (xy 1.778 -4.318)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.778 -2.54)
            (xy 5.08 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.778 0)
            (xy 1.778 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.778 0)
            (xy 5.08 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 2.54)
            (xy -1.27 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.778 -4.826)
            (xy 1.524 -3.556)
            (xy 2.032 -3.556)
            (xy 1.778 -4.826)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 1.778 2.286)
            (xy 1.524 1.016)
            (xy 2.032 1.016)
            (xy 1.778 2.286)
          )
          (fill (type outline))
        )
        (pin passive line (at 7.62 5.08 180) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 7.62 -5.08 180) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at 7.62 2.54 180) (length 2.54)
          (name "~")
          (number "4")
        )
        (pin passive line (at 7.62 -2.54 180) (length 2.54)
          (name "~")
          (number "5")
        )
      )
    )
    (symbol "Connector:Barrel_Jack_MountingPin" (in_bom yes) (on_board yes)
      (property "Reference" "J1" (id 0) (at -5.08 1.2701 90))
      (property "Value" "Barrel Jack" (id 1) (at -5.08 -1.2699 90))
      (property "Footprint" "Connector_BarrelJack:BarrelJack_Horizontal" (id 2) (at 1.016 1.27 0))
      (property "Datasheet" "~" (id 3) (at 1.016 1.27 0))
      (property "ki_keywords" "DC power barrel jack connector" (id 4) (at 0 0 0))
      (property "ki_description" "DC Barrel Jack with a mounting pin" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "BarrelJack*" (id 6) (at 0 0 0))
      (symbol "Barrel_Jack_MountingPin_0_1"
        (rectangle (start -5.08 3.81) (end 5.08 -3.81)
          (fill (type background))
        )
        (arc (start -3.302 3.175) (mid -3.937 2.54) (end -3.302 1.905)
          (fill (type none))
        )
        (arc (start -3.302 3.175) (mid -3.937 2.54) (end -3.302 1.905)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 5.08 2.54)
            (xy 3.81 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -2.54)
            (xy -2.54 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -2.54)
            (xy 2.54 -2.54)
            (xy 5.08 -2.54)
          )
          (fill (type none))
        )
        (rectangle (start 3.683 3.175) (end -3.302 1.905)
          (fill (type outline))
        )
      )
      (symbol "Barrel_Jack_MountingPin_1_1"
        (polyline
          (pts
            (xy -1.016 -4.572)
            (xy 1.016 -4.572)
          )
          (fill (type none))
        )
        (text "Mounting" (at 0 -4.191 0))
        (pin passive line (at 7.62 2.54 180) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 7.62 -2.54 180) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 0 -7.62 90) (length 3.048)
          (name "MountPin")
          (number "3")
        )
      )
    )
    (symbol "Custom_Displays:Impulse_Counter" (in_bom yes) (on_board yes)
      (property "Reference" "L1" (id 0) (at 0 10.16 0))
      (property "Value" "Impulse_Counter" (id 1) (at 0 7.62 0))
      (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Resistance" "" (id 4) (at 0 0 0))
      (property "Inductance" "" (id 5) (at 0 0 0))
      (symbol "Impulse_Counter_0_0"
        (text "1 2 3" (at 0 -2.54 0))
      )
      (symbol "Impulse_Counter_0_1"
        (rectangle (start -10.16 5.08) (end 10.16 -5.08)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 8.89 0)
            (xy 10.16 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -10.16 0)
            (xy -8.89 0)
            (xy -7.62 1.27)
            (xy -5.08 -1.27)
            (xy -2.54 1.27)
            (xy -1.27 0)
            (xy 0 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (arc (start 1.27 0) (mid 3.438 -0.898) (end 2.54 1.27)
          (fill (type none))
        )
        (arc (start 2.54 1.27) (mid 1.642 -0.898) (end 3.81 0)
          (fill (type none))
        )
        (arc (start 3.81 0) (mid 5.978 -0.898) (end 5.08 1.27)
          (fill (type none))
        )
        (arc (start 5.08 1.27) (mid 4.182 -0.898) (end 6.35 0)
          (fill (type none))
        )
        (arc (start 6.35 0) (mid 8.518 -0.898) (end 7.62 1.27)
          (fill (type none))
        )
        (arc (start 7.62 1.27) (mid 6.722 -0.898) (end 8.89 0)
          (fill (type none))
        )
      )
      (symbol "Impulse_Counter_1_1"
        (pin power_in line (at -12.7 2.54 0) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin power_out line (at 12.7 2.54 180) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Device:D" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "Diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "D_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Impulse_Counter_1" (in_bom yes) (on_board yes)
      (property "Reference" "L2" (id 0) (at 0 10.16 0))
      (property "Value" "Impulse_Counter" (id 1) (at 0 7.62 0))
      (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Resistance" "" (id 4) (at 0 0 0))
      (property "Inductance" "" (id 5) (at 0 0 0))
      (symbol "Impulse_Counter_1_0_0"
        (text "1 2 3" (at 0 -2.54 0))
      )
      (symbol "Impulse_Counter_1_0_1"
        (rectangle (start -10.16 5.08) (end 10.16 -5.08)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 8.89 0)
            (xy 10.16 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -10.16 0)
            (xy -8.89 0)
            (xy -7.62 1.27)
            (xy -5.08 -1.27)
            (xy -2.54 1.27)
            (xy -1.27 0)
            (xy 0 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (arc (start 1.27 0) (mid 3.438 -0.898) (end 2.54 1.27)
          (fill (type none))
        )
        (arc (start 2.54 1.27) (mid 1.642 -0.898) (end 3.81 0)
          (fill (type none))
        )
        (arc (start 3.81 0) (mid 5.978 -0.898) (end 5.08 1.27)
          (fill (type none))
        )
        (arc (start 5.08 1.27) (mid 4.182 -0.898) (end 6.35 0)
          (fill (type none))
        )
        (arc (start 6.35 0) (mid 8.518 -0.898) (end 7.62 1.27)
          (fill (type none))
        )
        (arc (start 7.62 1.27) (mid 6.722 -0.898) (end 8.89 0)
          (fill (type none))
        )
      )
      (symbol "Impulse_Counter_1_1_1"
        (pin power_in line (at -12.7 2.54 0) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin power_out line (at 12.7 2.54 180) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "NodeMCU_Devkit:113990105" (pin_names (offset 0.762)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 74.93 7.62 0))
      (property "Value" "113990105" (id 1) (at 74.93 5.08 0))
      (property "Footprint" "113990105" (id 2) (at 74.93 2.54 0))
      (property "Datasheet" "https://www.seeedstudio.com/NodeMCU-v2-Lua-based-ESP8266-development-kit.html" (id 3) (at 74.93 0 0))
      (property "Description" "NodeMCU DEVKIT V1.0" (id 4) (at 74.93 -2.54 0))
      (property "Height" "7.35" (id 5) (at 74.93 -5.08 0))
      (property "Manufacturer_Name" "Seeed Studio" (id 6) (at 74.93 -7.62 0))
      (property "Manufacturer_Part_Number" "113990105" (id 7) (at 74.93 -10.16 0))
      (property "Mouser Part Number" "713-113990105" (id 8) (at 74.93 -12.7 0))
      (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Seeed-Studio/113990105?qs=SElPoaY2y5KMx8k1roAIKw%3D%3D" (id 9) (at 74.93 -15.24 0))
      (property "Arrow Part Number" "113990105" (id 10) (at 74.93 -17.78 0))
      (property "Arrow Price/Stock" "https://www.arrow.com/en/products/113990105/seeed-technology-limited?region=nac" (id 11) (at 74.93 -20.32 0))
      (property "ki_description" "NodeMCU DEVKIT V1.0" (id 12) (at 0 0 0))
      (symbol "113990105_0_0"
        (pin bidirectional line (at 0 0 0) (length 5.08)
          (name "A0_-_ADC_EX")
          (number "1")
        )
        (pin power_in line (at 0 -22.86 0) (length 5.08)
          (name "GND_1")
          (number "10")
        )
        (pin power_in line (at 0 -25.4 0) (length 5.08)
          (name "VDD3V3_1")
          (number "11")
        )
        (pin input line (at 0 -27.94 0) (length 5.08)
          (name "EN")
          (number "12")
        )
        (pin input line (at 0 -30.48 0) (length 5.08)
          (name "NRST")
          (number "13")
        )
        (pin power_in line (at 0 -33.02 0) (length 5.08)
          (name "GND_2")
          (number "14")
        )
        (pin power_in line (at 0 -35.56 0) (length 5.08)
          (name "VDD5V")
          (number "15")
        )
        (pin power_in line (at 78.74 -35.56 180) (length 5.08)
          (name "VDD3V3_2")
          (number "16")
        )
        (pin power_in line (at 78.74 -33.02 180) (length 5.08)
          (name "GND_3")
          (number "17")
        )
        (pin bidirectional line (at 78.74 -30.48 180) (length 5.08)
          (name "D10_-_TXD0_/_GPIO1")
          (number "18")
        )
        (pin bidirectional line (at 78.74 -27.94 180) (length 5.08)
          (name "D9_-__RXD0_/_GPIO3")
          (number "19")
        )
        (pin bidirectional line (at 0 -2.54 0) (length 5.08)
          (name "ADC")
          (number "2")
        )
        (pin bidirectional line (at 78.74 -25.4 180) (length 5.08)
          (name "D8_-_GPIO15_/_TXD2_/_HSPICS")
          (number "20")
        )
        (pin bidirectional line (at 78.74 -22.86 180) (length 5.08)
          (name "D7_-_GPIO13_/_RXD2_/_HSPID")
          (number "21")
        )
        (pin bidirectional line (at 78.74 -20.32 180) (length 5.08)
          (name "D6_-_GPIO12_/_HSPIQ")
          (number "22")
        )
        (pin bidirectional line (at 78.74 -17.78 180) (length 5.08)
          (name "D5_-_GPIO14_/_HSPICLK")
          (number "23")
        )
        (pin power_in line (at 78.74 -15.24 180) (length 5.08)
          (name "GND_4")
          (number "24")
        )
        (pin power_in line (at 78.74 -12.7 180) (length 5.08)
          (name "VDD3V3_3")
          (number "25")
        )
        (pin bidirectional line (at 78.74 -10.16 180) (length 5.08)
          (name "D4_-_GPIO2_/_TXD1")
          (number "26")
        )
        (pin bidirectional line (at 78.74 -7.62 180) (length 5.08)
          (name "D3_-_GPIO0")
          (number "27")
        )
        (pin bidirectional line (at 78.74 -5.08 180) (length 5.08)
          (name "D2_-_GPIO4")
          (number "28")
        )
        (pin bidirectional line (at 78.74 -2.54 180) (length 5.08)
          (name "D1_-_GPIO5")
          (number "29")
        )
        (pin passive line (at 0 -5.08 0) (length 5.08)
          (name "RESV")
          (number "3")
        )
        (pin bidirectional line (at 78.74 0 180) (length 5.08)
          (name "D0_-_GPIO16")
          (number "30")
        )
        (pin bidirectional line (at 0 -7.62 0) (length 5.08)
          (name "D12_-_GPIO10_/_SD_D3")
          (number "4")
        )
        (pin bidirectional line (at 0 -10.16 0) (length 5.08)
          (name "D11_-_GPIO9_/_SD_D2")
          (number "5")
        )
        (pin bidirectional line (at 0 -12.7 0) (length 5.08)
          (name "SPI_INT_/_SD_D1")
          (number "6")
        )
        (pin bidirectional line (at 0 -15.24 0) (length 5.08)
          (name "SPI_MOSI_/_SD_CMD")
          (number "7")
        )
        (pin bidirectional line (at 0 -17.78 0) (length 5.08)
          (name "SPI_MISO_/_SD_D0")
          (number "8")
        )
        (pin bidirectional line (at 0 -20.32 0) (length 5.08)
          (name "SPI_CLK_/_SD_CLK")
          (number "9")
        )
      )
      (symbol "113990105_0_1"
        (polyline
          (pts
            (xy 5.08 2.54)
            (xy 73.66 2.54)
            (xy 73.66 -38.1)
            (xy 5.08 -38.1)
            (xy 5.08 2.54)
          )
          (fill (type none))
        )
      )
    )
    (symbol "Switch:SW_Push" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 1.27 2.54 0))
      (property "Value" "SW_Push" (id 1) (at 0 -1.524 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "~" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "switch normally-open pushbutton push-button" (id 4) (at 0 0 0))
      (property "ki_description" "Push button switch, generic, two pins" (id 5) (at 0 0 0))
      (symbol "SW_Push_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Transistor_BJT:2N3906" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.905 0))
      (property "Value" "2N3906" (id 1) (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 5.08 -1.905 0))
      (property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3906-D.PDF" (id 3) (at 0 0 0))
      (property "ki_keywords" "PNP Transistor" (id 4) (at 0 0 0))
      (property "ki_description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?92*" (id 6) (at 0 0 0))
      (symbol "2N3906_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 -1.778)
            (xy 1.778 -2.286)
            (xy 1.27 -1.27)
            (xy 2.286 -1.778)
            (xy 2.286 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "2N3906_1_1"
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "1")
        )
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
  )
  (junction (at 176.53 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 53.34 151.13) (diameter 0) (color 0 0 0 0))
  (junction (at 160.02 97.79) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 44.45 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 54.61 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 52.07 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 190.5 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 160.02 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 219.71 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 176.53 97.79) (diameter 0) (color 0 0 0 0))
  (junction (at 44.45 124.46) (diameter 0) (color 0 0 0 0))
  (junction (at 151.13 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 146.05 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 54.61 142.24) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 138.43 144.78) (xy 146.05 144.78)))
  (wire (pts (xy 208.28 106.68) (xy 219.71 106.68)))
  (wire (pts (xy 182.88 114.3) (xy 182.88 88.9)))
  (wire (pts (xy 144.78 88.9) (xy 86.36 88.9)))
  (wire (pts (xy 57.15 129.54) (xy 57.15 119.38)))
  (wire (pts (xy 176.53 100.33) (xy 223.52 100.33)))
  (wire (pts (xy 160.02 95.25) (xy 148.59 95.25)))
  (wire (pts (xy 57.15 119.38) (xy 59.69 119.38)))
  (wire (pts (xy 48.26 144.78) (xy 59.69 144.78)))
  (wire (pts (xy 176.53 97.79) (xy 176.53 100.33)))
  (wire (pts (xy 68.58 95.25) (xy 52.07 95.25)))
  (wire (pts (xy 148.59 82.55) (xy 149.86 82.55)))
  (wire (pts (xy 58.42 162.56) (xy 62.23 162.56)))
  (wire (pts (xy 151.13 144.78) (xy 160.02 144.78)))
  (wire (pts (xy 54.61 116.84) (xy 59.69 116.84)))
  (wire (pts (xy 54.61 124.46) (xy 54.61 116.84)))
  (wire (pts (xy 139.7 114.3) (xy 139.7 63.5)))
  (wire (pts (xy 223.52 100.33) (xy 223.52 88.9)))
  (wire (pts (xy 148.59 121.92) (xy 148.59 119.38)))
  (wire (pts (xy 146.05 82.55) (xy 128.27 82.55)))
  (wire (pts (xy 54.61 132.08) (xy 59.69 132.08)))
  (wire (pts (xy 38.1 132.08) (xy 44.45 132.08)))
  (wire (pts (xy 68.58 63.5) (xy 68.58 76.2)))
  (wire (pts (xy 151.13 148.59) (xy 151.13 144.78)))
  (wire (pts (xy 218.44 88.9) (xy 219.71 88.9)))
  (wire (pts (xy 52.07 95.25) (xy 52.07 121.92)))
  (wire (pts (xy 182.88 88.9) (xy 190.5 88.9)))
  (wire (pts (xy 38.1 127) (xy 44.45 127)))
  (wire (pts (xy 171.45 97.79) (xy 176.53 97.79)))
  (wire (pts (xy 190.5 106.68) (xy 200.66 106.68)))
  (wire (pts (xy 160.02 97.79) (xy 160.02 95.25)))
  (wire (pts (xy 68.58 88.9) (xy 76.2 88.9)))
  (wire (pts (xy 138.43 114.3) (xy 139.7 114.3)))
  (wire (pts (xy 182.88 144.78) (xy 182.88 124.46)))
  (wire (pts (xy 190.5 88.9) (xy 190.5 106.68)))
  (wire (pts (xy 138.43 121.92) (xy 146.05 121.92)))
  (wire (pts (xy 223.52 88.9) (xy 219.71 88.9)))
  (wire (pts (xy 160.02 144.78) (xy 182.88 144.78)))
  (wire (pts (xy 52.07 121.92) (xy 52.07 132.08)))
  (wire (pts (xy 76.2 63.5) (xy 68.58 63.5)))
  (wire (pts (xy 138.43 142.24) (xy 142.24 142.24)))
  (wire (pts (xy 128.27 82.55) (xy 128.27 76.2)))
  (wire (pts (xy 219.71 88.9) (xy 219.71 106.68)))
  (wire (pts (xy 38.1 129.54) (xy 44.45 129.54)))
  (wire (pts (xy 44.45 129.54) (xy 57.15 129.54)))
  (wire (pts (xy 142.24 100.33) (xy 176.53 100.33)))
  (wire (pts (xy 53.34 142.24) (xy 54.61 142.24)))
  (wire (pts (xy 148.59 119.38) (xy 152.4 119.38)))
  (wire (pts (xy 53.34 151.13) (xy 53.34 142.24)))
  (wire (pts (xy 172.72 129.54) (xy 172.72 132.08)))
  (wire (pts (xy 138.43 132.08) (xy 172.72 132.08)))
  (wire (pts (xy 142.24 142.24) (xy 142.24 100.33)))
  (wire (pts (xy 138.43 129.54) (xy 148.59 129.54)))
  (wire (pts (xy 146.05 121.92) (xy 146.05 144.78)))
  (wire (pts (xy 62.23 162.56) (xy 62.23 151.13)))
  (wire (pts (xy 58.42 148.59) (xy 151.13 148.59)))
  (wire (pts (xy 52.07 132.08) (xy 54.61 132.08)))
  (wire (pts (xy 138.43 111.76) (xy 144.78 111.76)))
  (wire (pts (xy 59.69 134.62) (xy 58.42 134.62)))
  (wire (pts (xy 172.72 121.92) (xy 172.72 119.38)))
  (wire (pts (xy 68.58 76.2) (xy 76.2 76.2)))
  (wire (pts (xy 190.5 88.9) (xy 193.04 88.9)))
  (wire (pts (xy 144.78 111.76) (xy 144.78 88.9)))
  (wire (pts (xy 172.72 119.38) (xy 175.26 119.38)))
  (wire (pts (xy 139.7 63.5) (xy 86.36 63.5)))
  (wire (pts (xy 160.02 114.3) (xy 160.02 97.79)))
  (wire (pts (xy 53.34 154.94) (xy 53.34 151.13)))
  (wire (pts (xy 38.1 121.92) (xy 52.07 121.92)))
  (wire (pts (xy 44.45 129.54) (xy 44.45 132.08)))
  (wire (pts (xy 160.02 97.79) (xy 163.83 97.79)))
  (wire (pts (xy 160.02 144.78) (xy 160.02 124.46)))
  (wire (pts (xy 128.27 76.2) (xy 86.36 76.2)))
  (wire (pts (xy 54.61 142.24) (xy 59.69 142.24)))
  (wire (pts (xy 146.05 116.84) (xy 146.05 82.55)))
  (wire (pts (xy 68.58 76.2) (xy 68.58 88.9)))
  (wire (pts (xy 146.05 144.78) (xy 151.13 144.78)))
  (wire (pts (xy 62.23 151.13) (xy 53.34 151.13)))
  (wire (pts (xy 176.53 82.55) (xy 176.53 97.79)))
  (wire (pts (xy 48.26 154.94) (xy 48.26 144.78)))
  (wire (pts (xy 54.61 142.24) (xy 54.61 132.08)))
  (wire (pts (xy 175.26 82.55) (xy 176.53 82.55)))
  (wire (pts (xy 44.45 124.46) (xy 44.45 127)))
  (wire (pts (xy 148.59 82.55) (xy 148.59 95.25)))
  (wire (pts (xy 44.45 124.46) (xy 54.61 124.46)))
  (wire (pts (xy 38.1 124.46) (xy 44.45 124.46)))
  (wire (pts (xy 58.42 134.62) (xy 58.42 148.59)))
  (wire (pts (xy 68.58 88.9) (xy 68.58 95.25)))
  (wire (pts (xy 138.43 116.84) (xy 146.05 116.84)))
  (text "Kill Tracker Solenoid" (at 189.23 80.01 0))
  (text "Death Tracker Solenoid" (at 147.32 72.39 0))
  (symbol (lib_id "Switch:SW_Push") (at 81.28 88.9 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW2" (id 0) (at 81.28 81.28 0))
    (property "Value" "Delay" (id 1) (at 81.28 83.82 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 81.28 83.82 0))
    (property "Datasheet" "~" (id 3) (at 81.28 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:2N3906") (at 180.34 119.38 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q2" (id 0) (at 185.42 118.1099 0))
    (property "Value" "2N3906" (id 1) (at 185.42 120.6499 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 185.42 121.285 0))
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3906-D.PDF" (id 3) (at 180.34 119.38 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Switch:SW_Push") (at 81.28 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW1" (id 0) (at 81.28 68.58 0))
    (property "Value" "Advance" (id 1) (at 81.28 71.12 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 81.28 71.12 0))
    (property "Datasheet" "~" (id 3) (at 81.28 71.12 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "35RAPC4BV4:35RAPC4BV4") (at 30.48 127 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J2" (id 0) (at 29.966 115.57 0))
    (property "Value" "35RAPC4BV4" (id 1) (at 29.966 118.11 0))
    (property "Footprint" "35RAPC4BV4:SWITCHCRAFT_35RAPC4BV4" (id 2) (at 30.48 127 0))
    (property "Datasheet" "" (id 3) (at 30.48 127 0))
    (property "PARTREV" "G" (id 4) (at 30.48 127 0))
    (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 30.48 127 0))
    (property "MAXIMUM_PACKAGE_HIEGHT" "12.573mm" (id 6) (at 30.48 127 0))
    (property "MANUFACTURER" "Switchcraft Inc." (id 7) (at 30.48 127 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 172.72 125.73 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R4" (id 0) (at 175.26 124.4599 0))
    (property "Value" "5k" (id 1) (at 175.26 126.9999 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (id 2) (at 170.942 125.73 90))
    (property "Datasheet" "~" (id 3) (at 172.72 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Custom_Displays:Impulse_Counter") (at 162.56 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L1" (id 0) (at 162.56 74.93 0))
    (property "Value" "Impulse_Counter" (id 1) (at 162.56 77.47 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 162.56 85.09 0))
    (property "Datasheet" "" (id 3) (at 162.56 85.09 0))
    (property "Resistance" "" (id 4) (at 162.56 85.09 0))
    (property "Inductance" "" (id 5) (at 162.56 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:Barrel_Jack_MountingPin") (at 50.8 162.56 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 49.5299 167.64 90))
    (property "Value" "Barrel Jack" (id 1) (at 54.61 170.18 90))
    (property "Footprint" "Connector_BarrelJack:BarrelJack_Horizontal" (id 2) (at 49.53 161.544 0))
    (property "Datasheet" "~" (id 3) (at 49.53 161.544 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Transistor_BJT:2N3906") (at 157.48 119.38 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q1" (id 0) (at 162.56 118.1099 0))
    (property "Value" "2N3906" (id 1) (at 162.56 120.6499 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 162.56 121.285 0))
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3906-D.PDF" (id 3) (at 157.48 119.38 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "NodeMCU_Devkit:113990105") (at 59.69 109.22 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 99.06 101.6 0))
    (property "Value" "Node MCU" (id 1) (at 99.06 104.14 0))
    (property "Footprint" "NodeMCU_Devkit:113990105" (id 2) (at 134.62 106.68 0))
    (property "Datasheet" "https://www.seeedstudio.com/NodeMCU-v2-Lua-based-ESP8266-development-kit.html" (id 3) (at 134.62 109.22 0))
    (property "Description" "NodeMCU DEVKIT V1.0" (id 4) (at 134.62 111.76 0))
    (property "Height" "7.35" (id 5) (at 134.62 114.3 0))
    (property "Manufacturer_Name" "Seeed Studio" (id 6) (at 134.62 116.84 0))
    (property "Manufacturer_Part_Number" "113990105" (id 7) (at 134.62 119.38 0))
    (property "Mouser Part Number" "713-113990105" (id 8) (at 134.62 121.92 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Seeed-Studio/113990105?qs=SElPoaY2y5KMx8k1roAIKw%3D%3D" (id 9) (at 134.62 124.46 0))
    (property "Arrow Part Number" "113990105" (id 10) (at 134.62 127 0))
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/113990105/seeed-technology-limited?region=nac" (id 11) (at 134.62 129.54 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:D") (at 204.47 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D2" (id 0) (at 204.47 100.33 0))
    (property "Value" "D" (id 1) (at 204.47 102.87 0))
    (property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (id 2) (at 204.47 106.68 0))
    (property "Datasheet" "~" (id 3) (at 204.47 106.68 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 81.28 63.5 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW3" (id 0) (at 81.28 55.88 0))
    (property "Value" "Mode" (id 1) (at 81.28 58.42 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 81.28 58.42 0))
    (property "Datasheet" "~" (id 3) (at 81.28 58.42 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 148.59 125.73 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R3" (id 0) (at 151.13 124.4599 0))
    (property "Value" "5k" (id 1) (at 151.13 126.9999 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (id 2) (at 146.812 125.73 90))
    (property "Datasheet" "~" (id 3) (at 148.59 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "Impulse_Counter_1") (lib_id "Custom_Displays:Impulse_Counter") (at 205.74 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L2" (id 0) (at 205.74 81.28 0))
    (property "Value" "Impulse_Counter" (id 1) (at 205.74 83.82 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 205.74 91.44 0))
    (property "Datasheet" "" (id 3) (at 205.74 91.44 0))
    (property "Resistance" "" (id 4) (at 205.74 91.44 0))
    (property "Inductance" "" (id 5) (at 205.74 91.44 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D") (at 167.64 97.79 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D1" (id 0) (at 167.64 91.44 0))
    (property "Value" "D" (id 1) (at 167.64 93.98 0))
    (property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (id 2) (at 167.64 97.79 0))
    (property "Datasheet" "~" (id 3) (at 167.64 97.79 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "D1") (unit 1) (value "D") (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal")
    )
    (path
      (reference "D2") (unit 1) (value "D") (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal")
    )
    (path
      (reference "J1") (unit 1) (value "Barrel Jack") (footprint "Connector_BarrelJack:BarrelJack_Horizontal")
    )
    (path
      (reference "J2") (unit 1) (value "35RAPC4BV4") (footprint "35RAPC4BV4:SWITCHCRAFT_35RAPC4BV4")
    )
    (path
      (reference "L1") (unit 1) (value "Impulse_Counter") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical")
    )
    (path
      (reference "L2") (unit 1) (value "Impulse_Counter") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical")
    )
    (path
      (reference "Q1") (unit 1) (value "2N3906") (footprint "Package_TO_SOT_THT:TO-92_Inline")
    )
    (path
      (reference "Q2") (unit 1) (value "2N3906") (footprint "Package_TO_SOT_THT:TO-92_Inline")
    )
    (path
      (reference "R3") (unit 1) (value "5k") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R4") (unit 1) (value "5k") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal")
    )
    (path
      (reference "SW1") (unit 1) (value "Advance") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical")
    )
    (path
      (reference "SW2") (unit 1) (value "Delay") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical")
    )
    (path
      (reference "SW3") (unit 1) (value "Mode") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical")
    )
    (path
      (reference "U1") (unit 1) (value "Node MCU") (footprint "NodeMCU_Devkit:113990105")
    )
  )
)
