(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 99.06 127)
    (grid_origin 180.28 30.02)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../PCB/")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(Q1-Pad1)")
  (net 9 "Net-(Q1-Pad2)")
  (net 10 "Net-(Q2-Pad2)")
  (net 11 "Net-(R3-Pad2)")
  (net 12 "Net-(R4-Pad2)")
  (net 13 "Net-(SW1-Pad2)")
  (net 14 "Net-(SW2-Pad2)")
  (net 15 "Net-(SW3-Pad2)")
  (net 16 "unconnected-(U1-Pad30)")
  (net 17 "unconnected-(U1-Pad26)")
  (net 18 "unconnected-(U1-Pad24)")
  (net 19 "unconnected-(U1-Pad23)")
  (net 20 "unconnected-(U1-Pad20)")
  (net 21 "unconnected-(U1-Pad19)")
  (net 22 "unconnected-(U1-Pad18)")
  (net 23 "unconnected-(U1-Pad13)")
  (net 24 "unconnected-(U1-Pad12)")
  (net 25 "unconnected-(U1-Pad9)")
  (net 26 "unconnected-(U1-Pad8)")
  (net 27 "unconnected-(U1-Pad7)")
  (net 28 "unconnected-(U1-Pad6)")
  (net 29 "unconnected-(U1-Pad3)")
  (net 30 "unconnected-(U1-Pad2)")
  (net 31 "unconnected-(U1-Pad1)")
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 161.23 55.42)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "5k" (at 3.81 1.92) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.05 -2.7) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(Q2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 123.13 75.74 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "D" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.596645 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 137.1 63.77 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56 90) (layer "F.SilkS"))
    (fp_text value "2N3906" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NodeMCU_Devkit:113990105" (layer "F.Cu")
    (tedit 6259E2D6)
    (at 149.8 71.93 90)
    (descr "NodeMCU V1.0")
    (tags "Undefined or Miscellaneous")
    (property "Arrow Part Number" "113990105")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/113990105/seeed-technology-limited?region=nac")
    (property "Description" "NodeMCU DEVKIT V1.0")
    (property "Height" "7.35")
    (property "Manufacturer_Name" "Seeed Studio")
    (property "Manufacturer_Part_Number" "113990105")
    (property "Mouser Part Number" "713-113990105")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Seeed-Studio/113990105?qs=SElPoaY2y5KMx8k1roAIKw%3D%3D")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "U1" (at 11.43 17.78 90) (layer "F.SilkS"))
    (fp_text value "Node MCU" (at 11.43 17.78 90) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 31 "unconnected-(U1-Pad1)") (pinfunction "A0_-_ADC_EX") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at 0 2.54 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 30 "unconnected-(U1-Pad2)") (pinfunction "ADC") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 0 5.08 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 29 "unconnected-(U1-Pad3)") (pinfunction "RESV") (pintype "passive"))
    (pad "4" thru_hole circle (at 0 7.62 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 7 "Net-(J2-Pad3)") (pinfunction "D12_-_GPIO10_/_SD_D3") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at 0 10.16 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 6 "Net-(J2-Pad2)") (pinfunction "D11_-_GPIO9_/_SD_D2") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at 0 12.7 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 28 "unconnected-(U1-Pad6)") (pinfunction "SPI_INT_/_SD_D1") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at 0 15.24 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 27 "unconnected-(U1-Pad7)") (pinfunction "SPI_MOSI_/_SD_CMD") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 0 17.78 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 26 "unconnected-(U1-Pad8)") (pinfunction "SPI_MISO_/_SD_D0") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 0 20.32 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 25 "unconnected-(U1-Pad9)") (pinfunction "SPI_CLK_/_SD_CLK") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 0 22.86 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 5 "Net-(J1-Pad2)") (pinfunction "GND_1") (pintype "power_in"))
    (pad "11" thru_hole circle (at 0 25.4 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 8 "Net-(Q1-Pad1)") (pinfunction "VDD3V3_1") (pintype "power_in"))
    (pad "12" thru_hole circle (at 0 27.94 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 24 "unconnected-(U1-Pad12)") (pinfunction "EN") (pintype "input"))
    (pad "13" thru_hole circle (at 0 30.48 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 23 "unconnected-(U1-Pad13)") (pinfunction "NRST") (pintype "input"))
    (pad "14" thru_hole circle (at 0 33.02 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 5 "Net-(J1-Pad2)") (pinfunction "GND_2") (pintype "power_in"))
    (pad "15" thru_hole circle (at 0 35.56 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "Net-(J1-Pad1)") (pinfunction "VDD5V") (pintype "power_in"))
    (pad "16" thru_hole circle (at 22.86 35.56 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 8 "Net-(Q1-Pad1)") (pinfunction "VDD3V3_2") (pintype "power_in"))
    (pad "17" thru_hole circle (at 22.86 33.02 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "Net-(D1-Pad2)") (pinfunction "GND_3") (pintype "power_in"))
    (pad "18" thru_hole circle (at 22.86 30.48 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 22 "unconnected-(U1-Pad18)") (pinfunction "D10_-_TXD0_/_GPIO1") (pintype "bidirectional"))
    (pad "19" thru_hole circle (at 22.86 27.94 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 21 "unconnected-(U1-Pad19)") (pinfunction "D9_-__RXD0_/_GPIO3") (pintype "bidirectional"))
    (pad "20" thru_hole circle (at 22.86 25.4 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 20 "unconnected-(U1-Pad20)") (pinfunction "D8_-_GPIO15_/_TXD2_/_HSPICS") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 22.86 22.86 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 12 "Net-(R4-Pad2)") (pinfunction "D7_-_GPIO13_/_RXD2_/_HSPID") (pintype "bidirectional"))
    (pad "22" thru_hole circle (at 22.86 20.32 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 11 "Net-(R3-Pad2)") (pinfunction "D6_-_GPIO12_/_HSPIQ") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at 22.86 17.78 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 19 "unconnected-(U1-Pad23)") (pinfunction "D5_-_GPIO14_/_HSPICLK") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at 22.86 15.24 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 18 "unconnected-(U1-Pad24)") (pinfunction "GND_4") (pintype "power_in"))
    (pad "25" thru_hole circle (at 22.86 12.7 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 8 "Net-(Q1-Pad1)") (pinfunction "VDD3V3_3") (pintype "power_in"))
    (pad "26" thru_hole circle (at 22.86 10.16 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 17 "unconnected-(U1-Pad26)") (pinfunction "D4_-_GPIO2_/_TXD1") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at 22.86 7.62 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 13 "Net-(SW1-Pad2)") (pinfunction "D3_-_GPIO0") (pintype "bidirectional"))
    (pad "28" thru_hole circle (at 22.86 5.08 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 15 "Net-(SW3-Pad2)") (pinfunction "D2_-_GPIO4") (pintype "bidirectional"))
    (pad "29" thru_hole circle (at 22.86 2.54 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 14 "Net-(SW2-Pad2)") (pinfunction "D1_-_GPIO5") (pintype "bidirectional"))
    (pad "30" thru_hole circle (at 22.86 0 180) (size 1.75 1.75) (drill 0.889) (layers *.Cu *.Mask "F.SilkS")
      (net 16 "unconnected-(U1-Pad30)") (pinfunction "D0_-_GPIO16") (pintype "bidirectional"))
    (pad "31" thru_hole circle (at 1.02 -4.06 180) (size 1.46 1.46) (drill 2.92) (layers *.Cu *.Mask "F.SilkS"))
    (pad "32" thru_hole circle (at 21.8 -4.06 180) (size 1.46 1.46) (drill 2.92) (layers *.Cu *.Mask "F.SilkS"))
    (pad "33" thru_hole circle (at 1.06 39.62 180) (size 1.46 1.46) (drill 2.92) (layers *.Cu *.Mask "F.SilkS"))
    (pad "34" thru_hole circle (at 21.8 39.62 180) (size 1.46 1.46) (drill 2.92) (layers *.Cu *.Mask "F.SilkS"))
    (model "C:/Users/Seth/Downloads/NodeMCU v2--3DModel-STEP-269445.STEP"
      (offset (xyz 11.5 -17.5 5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LOGO" (layer "F.Cu")
    (tedit 0)
    (at 122.48 58.72)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "35RAPC4BV4:SWITCHCRAFT_35RAPC4BV4" (layer "F.Cu")
    (tedit 648C9866)
    (at 168.12 35.1 -90)
    (property "MANUFACTURER" "Switchcraft Inc.")
    (property "MAXIMUM_PACKAGE_HIEGHT" "12.573mm")
    (property "PARTREV" "G")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -2.54 5.08 90) (layer "F.SilkS"))
    (fp_text value "35RAPC4BV4" (at 0 -5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -3.8 0 270) (size 2.7 2.7) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -1.35 -2 270) (size 2.7 2.7) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.35 0 270) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 4.25 -2 270) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 8 0 270) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)") (pintype "passive"))
    (model "C:/Users/Seth/Downloads/35RAPC4BV4--3DModel-STEP-1/35RAPC4BV4--3DModel-STEP-1.STEP"
      (offset (xyz -5 1 7))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 104.08 60.5 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at -0.92 5.9 180) (layer "F.SilkS"))
    (fp_text value "Mode" (at 0.48 6.3 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(SW3-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 123.13 70.66 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "D" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 106.62 85.9 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Inductance" "")
    (property "Resistance" "")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L1" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "Impulse_Counter" (at -1.96 -7.52 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "+") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "-") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 147.26 85.9 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Inductance" "")
    (property "Resistance" "")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L2" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "Impulse_Counter" (at -2.42 -7.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.1 0.98 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)") (pinfunction "+") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "-") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 137.1 56.69 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -3.56 90) (layer "F.SilkS"))
    (fp_text value "2N3906" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(Q2-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 104.08 50.34 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at -1.18 6.1 180) (layer "F.SilkS"))
    (fp_text value "Advance" (at 0.72 7.6 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(SW1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 5A1DBF6A)
    (at 186.3175 41.1 -90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -6 5.75 90) (layer "F.SilkS"))
    (fp_text value "Barrel Jack" (at -3.46 -5.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "3" thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad2)") (pinfunction "MountPin") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Seth/Downloads/54_00167/54-00167.step"
      (offset (xyz -7 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 -180 -90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 104.08 55.42 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at -1.1 6 180) (layer "F.SilkS"))
    (fp_text value "Delay" (at 0.5 6.4 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(SW2-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 161.23 63.04)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "StatTracker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "5k" (at 3.81 1.92) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 101.014214 123.985786) (end 191.885786 123.985786) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 191.9 29.1) (end 101.014214 29.114214) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.014214 31.114214) (mid 99.6 29.7) (end 101.014214 29.114214) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 191.9 29.1) (mid 193.314214 29.685786) (end 193.9 31.1) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 101.014214 123.985786) (mid 99.6 123.4) (end 99.014214 121.985786) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 193.885786 121.985786) (mid 193.3 123.4) (end 191.885786 123.985786) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.014214 31.114214) (end 99.014214 121.985786) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 193.885786 121.985786) (end 193.9 31.1) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Planetside2 Stat Tracker Rev 2.1\nDesigned by Robert Proaps" (at 190.44 108.76 90) (layer "F.SilkS"))
  (gr_text "Nanite Systems: Battlefield Technologies" (at 117.166781 67.170989) (layer "F.SilkS"))
  (gr_text "10mm" (at 146.48 119.92) (layer "Cmts.User"))
  (zone (net 5) (net_name "Net-(J1-Pad2)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.9 124)
        (xy 99 124)
        (xy 99 29.1)
        (xy 193.9 29.1)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad2)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.9 124)
        (xy 99 124)
        (xy 99 29.1)
        (xy 193.9 29.1)
      )
    )
  )
)
