(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J1-Pad1)")
  (net 2 "+5V")
  (net 3 "unconnected-(J1-Pad3)")
  (net 4 "unconnected-(J1-Pad4)")
  (net 5 "unconnected-(J1-Pad5)")
  (net 6 "GND")
  (net 7 "unconnected-(J1-Pad7)")
  (net 8 "unconnected-(J1-Pad8)")
  (net 9 "BUSY")
  (net 10 "unconnected-(J1-Pad10)")
  (net 11 "RESET")
  (net 12 "unconnected-(J1-Pad12)")
  (net 13 "D{slash}C")
  (net 14 "MOSI")
  (net 15 "MISO")
  (net 16 "unconnected-(J1-Pad16)")
  (net 17 "unconnected-(J1-Pad17)")
  (net 18 "unconnected-(J1-Pad18)")
  (net 19 "SCLK")
  (net 20 "EKCS")
  (net 21 "unconnected-(J1-Pad22)")
  (net 22 "unconnected-(J1-Pad24)")
  (net 23 "unconnected-(J1-Pad27)")
  (net 24 "unconnected-(J1-Pad28)")
  (net 25 "unconnected-(J1-Pad29)")
  (net 26 "unconnected-(J1-Pad31)")
  (net 27 "unconnected-(J1-Pad32)")
  (net 28 "unconnected-(J1-Pad33)")
  (net 29 "unconnected-(J1-Pad35)")
  (net 30 "unconnected-(J1-Pad36)")
  (net 31 "unconnected-(J1-Pad37)")
  (net 32 "unconnected-(J1-Pad38)")
  (net 33 "unconnected-(J1-Pad40)")
  (net 34 "unconnected-(P2-Pad9)")
  (net 35 "unconnected-(P2-Pad12)")
  (net 36 "unconnected-(P2-Pad2)")
  (net 37 "unconnected-(J1-Pad14)")
  (net 38 "unconnected-(J1-Pad20)")
  (net 39 "unconnected-(J1-Pad25)")
  (net 40 "unconnected-(J1-Pad30)")
  (net 41 "unconnected-(J1-Pad34)")
  (net 42 "unconnected-(J1-Pad39)")
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 139.78 43.1)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 139.78 173.1)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 29.78 43.1)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 111.775 106.14)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H11" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 111.856 84.201)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H22" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 111.775 135.14 180)
    (descr "surface-mounted straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x20 2.54mm double row")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 5.095 -24.88) (layer "F.SilkS"))
    (fp_text value "Raspberry_Pi_2_3" (at 0 26.46) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.525 -24.13 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "unconnected-(J1-Pad1)") (pinfunction "3V3") (pintype "power_in"))
    (pad "2" smd rect (at 2.525 -24.13 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "5V") (pintype "power_in"))
    (pad "3" smd rect (at -2.525 -21.59 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "unconnected-(J1-Pad3)") (pinfunction "SDA/GPIO2") (pintype "bidirectional"))
    (pad "4" smd rect (at 2.525 -21.59 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "unconnected-(J1-Pad4)") (pinfunction "5V") (pintype "power_in"))
    (pad "5" smd rect (at -2.525 -19.05 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(J1-Pad5)") (pinfunction "SCL/GPIO3") (pintype "bidirectional"))
    (pad "6" smd rect (at 2.525 -19.05 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd rect (at -2.525 -16.51 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(J1-Pad7)") (pinfunction "GCLK0/GPIO4") (pintype "bidirectional"))
    (pad "8" smd rect (at 2.525 -16.51 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(J1-Pad8)") (pinfunction "GPIO14/TXD") (pintype "bidirectional"))
    (pad "9" smd rect (at -2.525 -13.97 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "10" smd rect (at 2.525 -13.97 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(J1-Pad10)") (pinfunction "GPIO15/RXD") (pintype "bidirectional"))
    (pad "11" smd rect (at -2.525 -11.43 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "BUSY") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "12" smd rect (at 2.525 -11.43 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "unconnected-(J1-Pad12)") (pinfunction "GPIO18/PWM0") (pintype "bidirectional"))
    (pad "13" smd rect (at -2.525 -8.89 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "RESET") (pinfunction "GPIO27") (pintype "bidirectional"))
    (pad "14" smd rect (at 2.525 -8.89 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(J1-Pad14)") (pinfunction "GND") (pintype "power_in"))
    (pad "15" smd rect (at -2.525 -6.35 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "D{slash}C") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "16" smd rect (at 2.525 -6.35 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(J1-Pad16)") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "17" smd rect (at -2.525 -3.81 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(J1-Pad17)") (pinfunction "3V3") (pintype "power_in"))
    (pad "18" smd rect (at 2.525 -3.81 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(J1-Pad18)") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "19" smd rect (at -2.525 -1.27 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "MOSI") (pinfunction "MOSI0/GPIO10") (pintype "bidirectional"))
    (pad "20" smd rect (at 2.525 -1.27 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "unconnected-(J1-Pad20)") (pinfunction "GND") (pintype "power_in"))
    (pad "21" smd rect (at -2.525 1.27 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "MISO") (pinfunction "MISO0/GPIO9") (pintype "bidirectional"))
    (pad "22" smd rect (at 2.525 1.27 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(J1-Pad22)") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "23" smd rect (at -2.525 3.81 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "SCLK") (pinfunction "SCLK0/GPIO11") (pintype "bidirectional"))
    (pad "24" smd rect (at 2.525 3.81 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(J1-Pad24)") (pinfunction "~{CE0}/GPIO8") (pintype "bidirectional"))
    (pad "25" smd rect (at -2.525 6.35 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(J1-Pad25)") (pinfunction "GND") (pintype "power_in"))
    (pad "26" smd rect (at 2.525 6.35 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "EKCS") (pinfunction "~{CE1}/GPIO7") (pintype "bidirectional"))
    (pad "27" smd rect (at -2.525 8.89 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "unconnected-(J1-Pad27)") (pinfunction "ID_SD/GPIO0") (pintype "bidirectional"))
    (pad "28" smd rect (at 2.525 8.89 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "unconnected-(J1-Pad28)") (pinfunction "ID_SC/GPIO1") (pintype "bidirectional"))
    (pad "29" smd rect (at -2.525 11.43 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(J1-Pad29)") (pinfunction "GCLK1/GPIO5") (pintype "bidirectional"))
    (pad "30" smd rect (at 2.525 11.43 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(J1-Pad30)") (pinfunction "GND") (pintype "power_in"))
    (pad "31" smd rect (at -2.525 13.97 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(J1-Pad31)") (pinfunction "GCLK2/GPIO6") (pintype "bidirectional"))
    (pad "32" smd rect (at 2.525 13.97 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(J1-Pad32)") (pinfunction "PWM0/GPIO12") (pintype "bidirectional"))
    (pad "33" smd rect (at -2.525 16.51 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "unconnected-(J1-Pad33)") (pinfunction "PWM1/GPIO13") (pintype "bidirectional"))
    (pad "34" smd rect (at 2.525 16.51 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(J1-Pad34)") (pinfunction "GND") (pintype "power_in"))
    (pad "35" smd rect (at -2.525 19.05 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(J1-Pad35)") (pinfunction "GPIO19/MISO1") (pintype "bidirectional"))
    (pad "36" smd rect (at 2.525 19.05 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "unconnected-(J1-Pad36)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "37" smd rect (at -2.525 21.59 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(J1-Pad37)") (pinfunction "GPIO26") (pintype "bidirectional"))
    (pad "38" smd rect (at 2.525 21.59 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(J1-Pad38)") (pinfunction "GPIO20/MOSI1") (pintype "bidirectional"))
    (pad "39" smd rect (at -2.525 24.13 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(J1-Pad39)") (pinfunction "GND") (pintype "power_in"))
    (pad "40" smd rect (at 2.525 24.13 180) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(J1-Pad40)") (pinfunction "GPIO21/SCLK1") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 111.775 164.14)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H13" (at 5.065 -1.58) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 134.775 164.14)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H14" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 111.856 55.499)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H21" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Left" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 95.6 69.85)
    (descr "surface-mounted straight pin header, 1x12, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x12 2.54mm single row style1 pin1 left")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "P2" (at 0 -16.3) (layer "F.SilkS"))
    (fp_text value "Conn_01x12_Male" (at 0 16.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.655 -13.97) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 1.655 -11.43) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "unconnected-(P2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.655 -8.89) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 1.655 -6.35) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "SCLK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.655 -3.81) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "MISO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.655 -1.27) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "MOSI") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at -1.655 1.27) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "EKCS") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 1.655 3.81) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "D{slash}C") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at -1.655 6.35) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(P2-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 1.655 8.89) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "RESET") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at -1.655 11.43) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "BUSY") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 1.655 13.97) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(P2-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Left.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 134.775 106.14)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H12" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 29.78 173.1)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "hp_newspaper_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_rect (start 114.65 61.85) (end 115.65 77.85) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_rect (start 24.78 38.1) (end 144.78 178.1) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "The latest algorithm announced by Edge Impulse further's the company's quest to \nmake on-device machine learning accessible to all skill levels. The new heart \nrate measurement algorithm is boasted to squeeze results from the noisiest of \nsensor data using just one-sixteenth the memory of their competition. \n\nEdge Impulse also does well to demystify the complexities of using their \nalgorithms with detailed documentation and user examples. Along with tools to \nhardware optimize your ML model on edge devices such as the Raspberry Pi. " (at 90.805 160.02) (layer "B.SilkS"))
  (gr_text "Open Source Hardware Association Selects \nOctober to be Open Hardware Month." (at 92.71 113.03) (layer "B.SilkS"))
  (gr_text "Sports pg. 5 - Hackster Picks pg. 7 - Events pg. 10 - Projects pg. 11" (at 85.09 174.625) (layer "B.SilkS"))
  (gr_text "After much anticipation, the next generation of Pi's \nhit the market in 4GB and 8GB variants. Early reports \nfrom testers indicate that the Raspberry Pi 5 is \nhands down the most powerful Pi to date. It offers \n{dblquote}beastly{dblquote} performance with new PCIe connectivity and \na new Pi custom ASIC, the Raspberry Pi RP1 chip. The \nproduct brief states the following in regards to the \nnew RP1 chip:\n{dblquote}For the first time, this is a full-size Raspberry Pi \ncomputer using silicon built in-house at Raspberry Pi. \nThe RP1 {dblquote}southbridge{dblquote} provides the bulk of the I/O \ncapabilities for Raspberry Pi 5, and delivers a step \nchange in peripheral performance and functionality. \nAggregate USB bandwidth is more than doubled, yielding \nfaster transfer speeds to external UAS drives and other \nhigh-speed peripherals; the dedicated two-lane 1Gbps MIPI \ncamera and display interfaces present on earlier models \nhave been replaced by a pair of four-lane 1.5Gbps MIPI \ntransceivers, tripling total bandwidth, and supporting any \ncombination of up to two cameras or displays; peak SD card \nperformance is doubled, through support for the SDR104 \nhigh-speed mode; and for the first time the platform \nexposes a single-lane PCI Express 2.0 interface, providing \nsupport for high-bandwidth peripherals.{dblquote}" (at 141.605 139.7) (layer "B.SilkS"))
  (gr_text "The Wizarding World of Edge Impulse \nOpen to All" (at 90.805 148.59) (layer "B.SilkS"))
  (gr_text "The FPGAs \nThat Lived." (at 143.51 76.835) (layer "B.SilkS"))
  (gr_text "Is AI He Who Must Not Be Named in Disguise?!" (at 67.945 93.345) (layer "B.SilkS"))
  (gr_text "Issue 001 - October 31, 2023" (at 118.745 47.625) (layer "B.SilkS"))
  (gr_text "by Knitronics" (at 50.8 48.26) (layer "B.SilkS"))
  (gr_text "Ministry of Microcontrollers\nAnnouces Raspberry 5!" (at 121.285 114.935) (layer "B.SilkS"))
  (gr_text "With the rise in great AI beings such as ChatGPT, many have been concerned about where \nthe future will lead as they continue to evolve... From writing homework essays, to \nresumes, to even full symphonies the abilities of this humble ML algorithm are \nimpressive. But is this great skill secretly coming from a dark place?? Would that \nperhaps explain it's swift rise to power? Only time will tell." (at 104.14 99.695) (layer "B.SilkS"))
  (gr_text "Exclusive!!" (at 129.54 53.34) (layer "B.SilkS"))
  (gr_text "The 7 Series FPGAs proved their \nability to survive with the \nannouncement from AMD they their \nlifecycle has been extended for \nat least the next 13 years through \nthe year 2035.  \n\nWill we continue to see great \nthings from the FPGAs? Many rely on \nthem in their current projects so \nthe hope will be to see them thrive!" (at 143.51 90.17) (layer "B.SilkS"))
  (gr_text "The Hackster Headlines" (at 86.36 43.18) (layer "B.SilkS"))
  (gr_text "The Open Source Hardware Association (OSHWA) is planning a lot for this month in \nthe name of open source hardware. The idea is to encourage the maker/engineering \ncommunity to host talks and small events (where safe) throughout the month to \nfoster technological knowledge and encourage research that is accessible, \ncollaborative, and respects user freedom.\n\nUsers are encouraged to document their projects all through the month of October \nin preparation for Open Hardware Summit 2024 to be held in Montreal (Hello, \nCanada!). OSHWA is currently accepting submissions on their sites for pitches for \ntalks, workshops and exhibition tables.\n\nCheck out the latest Hackster Cafe Chats to learn about the process of certifying \nyour own projects as open source, becoming a member of OSHWA, and all of the \nways to get involved!" (at 92.71 128.905) (layer "B.SilkS"))
  (gr_text "The spooky season has brought on \na plethora of spooky projects. \nWill makers on the site dare to \ntry their hand at any??? \n\nThis October is shaping up to be \nquite eventful for makers with \nthe release of a new Pi as well." (at 143.51 62.23) (layer "B.SilkS"))
)
