(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:Heater" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "Heater" (at -2.032 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "heater R resistor" (at 0 0 0))
      (property "ki_description" "Resistive heater" (at 0 0 0))
      (symbol "Heater_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.524)
            (xy 1.016 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -1.524)
            (xy -1.016 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -0.508)
            (xy -1.016 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0.508)
            (xy -1.016 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "Heater_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "LED" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "LED diode" (at 0 0 0))
      (property "ki_description" "Light emitting diode" (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Potentiometer_US" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RV" (at -4.445 0 90))
      (property "Value" "R_Potentiometer_US" (at -2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "resistor variable" (at 0 0 0))
      (property "ki_description" "Potentiometer, US symbol" (at 0 0 0))
      (property "ki_fp_filters" "Potentiometer*" (at 0 0 0))
      (symbol "R_Potentiometer_US_0_1"
        (polyline
          (pts
            (xy 0 -2.286)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.524 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.143 0)
            (xy 2.286 0.508)
            (xy 2.286 -0.508)
            (xy 1.143 0)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 1.016 -1.143)
            (xy 0 -1.524)
            (xy -1.016 -1.905)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 1.016 0.381)
            (xy 0 0)
            (xy -1.016 -0.381)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 1.016 1.905)
            (xy 0 1.524)
            (xy -1.016 1.143)
            (xy 0 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "R_Potentiometer_US_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "3")
          (number "3")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 0.762 0.508 0))
      (property "Value" "R_Small" (at 0.762 -1.016 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R resistor" (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:1N4001" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "1N4001" (at 0 -2.54 0))
      (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (at 0 0 0))
      (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (at 0 0 0))
      (property "Sim.Device" "D" (at 0 0 0))
      (property "Sim.Pins" "1=K 2=A" (at 0 0 0))
      (property "ki_keywords" "diode" (at 0 0 0))
      (property "ki_description" "50V 1A General Purpose Rectifier Diode, DO-41" (at 0 0 0))
      (property "ki_fp_filters" "D*DO?41*" (at 0 0 0))
      (symbol "1N4001_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "1N4001_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "MCU_Module:Arduino_Nano_v3.x" (in_bom yes) (on_board yes)
      (property "Reference" "A" (at -10.16 23.495 0))
      (property "Value" "Arduino_Nano_v3.x" (at 5.08 -24.13 0))
      (property "Footprint" "Module:Arduino_Nano" (at 0 0 0))
      (property "Datasheet" "http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf" (at 0 0 0))
      (property "ki_keywords" "Arduino nano microcontroller module USB" (at 0 0 0))
      (property "ki_description" "Arduino Nano v3.x" (at 0 0 0))
      (property "ki_fp_filters" "Arduino*Nano*" (at 0 0 0))
      (symbol "Arduino_Nano_v3.x_0_1"
        (rectangle (start -10.16 22.86) (end 10.16 -22.86)
          (fill (type background))
        )
      )
      (symbol "Arduino_Nano_v3.x_1_1"
        (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
          (name "D1/TX")
          (number "1")
        )
        (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
          (name "D7")
          (number "10")
        )
        (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
          (name "D8")
          (number "11")
        )
        (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
          (name "D9")
          (number "12")
        )
        (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
          (name "D10")
          (number "13")
        )
        (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
          (name "D11")
          (number "14")
        )
        (pin bidirectional line (at -12.7 -15.24 0) (length 2.54)
          (name "D12")
          (number "15")
        )
        (pin bidirectional line (at -12.7 -17.78 0) (length 2.54)
          (name "D13")
          (number "16")
        )
        (pin power_out line (at 2.54 25.4 270) (length 2.54)
          (name "3V3")
          (number "17")
        )
        (pin input line (at 12.7 5.08 180) (length 2.54)
          (name "AREF")
          (number "18")
        )
        (pin bidirectional line (at 12.7 0 180) (length 2.54)
          (name "A0")
          (number "19")
        )
        (pin bidirectional line (at -12.7 15.24 0) (length 2.54)
          (name "D0/RX")
          (number "2")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "A1")
          (number "20")
        )
        (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
          (name "A2")
          (number "21")
        )
        (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
          (name "A3")
          (number "22")
        )
        (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
          (name "A4")
          (number "23")
        )
        (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
          (name "A5")
          (number "24")
        )
        (pin bidirectional line (at 12.7 -15.24 180) (length 2.54)
          (name "A6")
          (number "25")
        )
        (pin bidirectional line (at 12.7 -17.78 180) (length 2.54)
          (name "A7")
          (number "26")
        )
        (pin power_out line (at 5.08 25.4 270) (length 2.54)
          (name "+5V")
          (number "27")
        )
        (pin input line (at 12.7 15.24 180) (length 2.54)
          (name "~{RESET}")
          (number "28")
        )
        (pin power_in line (at 2.54 -25.4 90) (length 2.54)
          (name "GND")
          (number "29")
        )
        (pin input line (at 12.7 12.7 180) (length 2.54)
          (name "~{RESET}")
          (number "3")
        )
        (pin power_in line (at -2.54 25.4 270) (length 2.54)
          (name "VIN")
          (number "30")
        )
        (pin power_in line (at 0 -25.4 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
          (name "D2")
          (number "5")
        )
        (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
          (name "D3")
          (number "6")
        )
        (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
          (name "D4")
          (number "7")
        )
        (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
          (name "D5")
          (number "8")
        )
        (pin bidirectional line (at -12.7 0 0) (length 2.54)
          (name "D6")
          (number "9")
        )
      )
    )
    (symbol "Motor:Fan_ALT" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "M" (at 3.81 5.08 0))
      (property "Value" "Fan_ALT" (at 3.81 2.54 0))
      (property "Footprint" "" (at 0 -1.27 0))
      (property "Datasheet" "~" (at 0 -1.27 0))
      (property "ki_keywords" "Fan Motor" (at 0 0 0))
      (property "ki_description" "Fan without PWM or tach, alternative symbol" (at 0 0 0))
      (property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*" (at 0 0 0))
      (symbol "Fan_ALT_0_1"
        (arc (start -4.572 0) (mid -2.286 -0.5988) (end 0 0)
          (fill (type none))
        )
        (arc (start -4.318 1.524) (mid -2.4153 0.0291) (end 0 0)
          (fill (type none))
        )
        (arc (start -1.524 -4.318) (mid -0.0291 -2.4153) (end 0 0)
          (fill (type none))
        )
        (arc (start 0 -4.572) (mid 0.5988 -2.286) (end 0 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -5.08)
            (xy 0 -4.572)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 4.572)
            (xy 0 5.08)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 4.572)
          (fill (type none))
        )
        (arc (start 0 4.572) (mid -0.5988 2.286) (end 0 0)
          (fill (type none))
        )
        (arc (start 1.524 4.318) (mid 0.0291 2.4153) (end 0 0)
          (fill (type none))
        )
        (arc (start 4.318 -1.524) (mid 2.4153 -0.0291) (end 0 0)
          (fill (type none))
        )
        (arc (start 4.572 0) (mid 2.286 0.5988) (end 0 0)
          (fill (type none))
        )
      )
      (symbol "Fan_ALT_1_1"
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -7.62 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Sensor_Temperature:LM35-D" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -6.35 6.35 0))
      (property "Value" "LM35-D" (at 1.27 6.35 0))
      (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (at 0 -10.16 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm35.pdf" (at 0 0 0))
      (property "ki_keywords" "temperature sensor thermistor" (at 0 0 0))
      (property "ki_description" "Precision centigrade temperature sensor, SOIC-8" (at 0 0 0))
      (property "ki_fp_filters" "SOIC*" (at 0 0 0))
      (symbol "LM35-D_0_1"
        (rectangle (start -7.62 5.08) (end 7.62 -5.08)
          (fill (type background))
        )
        (circle (center -4.445 -2.54) (radius 1.27)
          (fill (type outline))
        )
        (rectangle (start -3.81 -1.905) (end -5.08 0)
          (fill (type outline))
        )
        (arc (start -3.81 3.175) (mid -4.445 3.8073) (end -5.08 3.175)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 0.635)
            (xy -4.445 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.27)
            (xy -4.445 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.905)
            (xy -4.445 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.54)
            (xy -4.445 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 3.175)
            (xy -5.08 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 3.175)
            (xy -4.445 3.175)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 3.175)
            (xy -3.81 0)
          )
          (fill (type none))
        )
      )
      (symbol "LM35-D_1_1"
        (pin output line (at 10.16 0 180) (length 2.54)
          (name "V_{OUT}")
          (number "1")
        )
        (pin no_connect line (at -2.54 -5.08 90) (length 2.54) hide
          (name "NC")
          (number "2")
        )
        (pin no_connect line (at -2.54 5.08 270) (length 2.54) hide
          (name "NC")
          (number "3")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin no_connect line (at 2.54 -5.08 90) (length 2.54) hide
          (name "NC")
          (number "5")
        )
        (pin no_connect line (at 5.08 -5.08 90) (length 2.54) hide
          (name "NC")
          (number "6")
        )
        (pin no_connect line (at 7.62 2.54 180) (length 2.54) hide
          (name "NC")
          (number "7")
        )
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "+V_{S}")
          (number "8")
        )
      )
    )
    (symbol "Transistor_FET:IRF540N" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at 6.35 1.905 0))
      (property "Value" "IRF540N" (at 6.35 0 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (at 6.35 -1.905 0))
      (property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf540n.pdf" (at 0 0 0))
      (property "ki_keywords" "HEXFET N-Channel MOSFET" (at 0 0 0))
      (property "ki_description" "33A Id, 100V Vds, HEXFET N-Channel MOSFET, TO-220" (at 0 0 0))
      (property "ki_fp_filters" "TO?220*" (at 0 0 0))
      (symbol "IRF540N_0_1"
        (polyline
          (pts
            (xy 0.254 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.905)
            (xy 0.254 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.27)
            (xy 0.762 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0.508)
            (xy 0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 2.286)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 0)
            (xy 0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.778)
            (xy 3.302 -1.778)
            (xy 3.302 1.778)
            (xy 0.762 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0)
            (xy 2.032 0.381)
            (xy 2.032 -0.381)
            (xy 1.016 0)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 2.794 0.508)
            (xy 2.921 0.381)
            (xy 3.683 0.381)
            (xy 3.81 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.302 0.381)
            (xy 2.921 -0.254)
            (xy 3.683 -0.254)
            (xy 3.302 0.381)
          )
          (fill (type none))
        )
        (circle (center 1.651 0) (radius 2.794)
          (fill (type none))
        )
        (circle (center 2.54 -1.778) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 2.54 1.778) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "IRF540N_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "G")
          (number "1")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "D")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "S")
          (number "3")
        )
      )
    )
    (symbol "power:+12V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+12V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+12V\"" (at 0 0 0))
      (symbol "+12V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+12V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+12V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 204.47 133.35) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 77.47 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 179.07 41.91) (diameter 0) (color 0 0 0 0))
  (junction (at 77.47 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 80.01 35.56) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 77.47 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 151.13) (diameter 0) (color 0 0 0 0))
  (junction (at 77.47 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 90.17 35.56) (diameter 0) (color 0 0 0 0))
  (junction (at 53.34 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 171.45 41.91) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 35.56) (diameter 0) (color 0 0 0 0))
  (junction (at 179.07 110.49) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 41.91) (diameter 0) (color 0 0 0 0))
  (junction (at 207.01 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 80.01 55.88) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 195.58 59.69) (xy 220.98 59.69)))
  (wire (pts (xy 85.09 100.33) (xy 124.46 100.33)))
  (wire (pts (xy 189.23 90.17) (xy 189.23 105.41)))
  (wire (pts (xy 62.23 35.56) (xy 71.12 35.56)))
  (wire (pts (xy 223.52 57.15) (xy 223.52 106.68)))
  (wire (pts (xy 186.69 133.35) (xy 204.47 133.35)))
  (wire (pts (xy 120.65 127) (xy 120.65 30.48)))
  (wire (pts (xy 207.01 63.5) (xy 171.45 63.5)))
  (wire (pts (xy 44.45 127) (xy 120.65 127)))
  (wire (pts (xy 71.12 55.88) (xy 71.12 35.56)))
  (wire (pts (xy 196.85 99.06) (xy 220.98 99.06)))
  (wire (pts (xy 179.07 110.49) (xy 179.07 143.51)))
  (wire (pts (xy 196.85 77.47) (xy 220.98 77.47)))
  (polyline (pts (xy 86.36 160.02) (xy 86.36 166.37)))
  (wire (pts (xy 77.47 92.71) (xy 77.47 95.25)))
  (wire (pts (xy 53.34 121.92) (xy 77.47 121.92)))
  (wire (pts (xy 207.01 121.92) (xy 137.16 121.92)))
  (wire (pts (xy 77.47 73.66) (xy 77.47 74.93)))
  (wire (pts (xy 106.68 97.79) (xy 106.68 63.5)))
  (wire (pts (xy 63.5 92.71) (xy 77.47 92.71)))
  (wire (pts (xy 149.86 92.71) (xy 163.83 92.71)))
  (wire (pts (xy 106.68 97.79) (xy 124.46 97.79)))
  (wire (pts (xy 90.17 76.2) (xy 90.17 81.28)))
  (wire (pts (xy 189.23 113.03) (xy 189.23 110.49)))
  (wire (pts (xy 63.5 55.88) (xy 71.12 55.88)))
  (wire (pts (xy 123.19 30.48) (xy 123.19 156.21)))
  (wire (pts (xy 220.98 39.37) (xy 195.58 39.37)))
  (wire (pts (xy 137.16 113.03) (xy 137.16 121.92)))
  (wire (pts (xy 189.23 90.17) (xy 196.85 90.17)))
  (wire (pts (xy 179.07 41.91) (xy 207.01 41.91)))
  (wire (pts (xy 63.5 58.42) (xy 63.5 55.88)))
  (wire (pts (xy 76.2 30.48) (xy 76.2 54.61)))
  (wire (pts (xy 80.01 55.88) (xy 90.17 55.88)))
  (wire (pts (xy 134.62 41.91) (xy 134.62 62.23)))
  (wire (pts (xy 193.04 30.48) (xy 123.19 30.48)))
  (wire (pts (xy 207.01 106.68) (xy 207.01 121.92)))
  (wire (pts (xy 142.24 41.91) (xy 158.75 41.91)))
  (wire (pts (xy 189.23 105.41) (xy 149.86 105.41)))
  (wire (pts (xy 207.01 82.55) (xy 207.01 63.5)))
  (wire (pts (xy 71.12 73.66) (xy 71.12 55.88)))
  (wire (pts (xy 80.01 35.56) (xy 80.01 44.45)))
  (wire (pts (xy 53.34 72.39) (xy 53.34 121.92)))
  (wire (pts (xy 92.71 163.83) (xy 168.91 163.83)))
  (polyline (pts (xy 88.9 153.67) (xy 86.36 153.67)))
  (wire (pts (xy 90.17 90.17) (xy 90.17 88.9)))
  (wire (pts (xy 142.24 62.23) (xy 142.24 41.91)))
  (wire (pts (xy 90.17 35.56) (xy 90.17 38.1)))
  (wire (pts (xy 77.47 74.93) (xy 77.47 76.2)))
  (wire (pts (xy 137.16 151.13) (xy 137.16 137.16)))
  (wire (pts (xy 80.01 68.58) (xy 80.01 72.39)))
  (wire (pts (xy 186.69 90.17) (xy 149.86 90.17)))
  (wire (pts (xy 92.71 166.37) (xy 163.83 166.37)))
  (wire (pts (xy 193.04 124.46) (xy 193.04 30.48)))
  (wire (pts (xy 90.17 35.56) (xy 134.62 35.56)))
  (wire (pts (xy 195.58 39.37) (xy 195.58 59.69)))
  (wire (pts (xy 137.16 121.92) (xy 137.16 137.16)))
  (wire (pts (xy 77.47 90.17) (xy 90.17 90.17)))
  (wire (pts (xy 80.01 55.88) (xy 80.01 58.42)))
  (wire (pts (xy 196.85 77.47) (xy 196.85 99.06)))
  (wire (pts (xy 163.83 166.37) (xy 163.83 100.33)))
  (wire (pts (xy 80.01 52.07) (xy 80.01 55.88)))
  (wire (pts (xy 189.23 129.54) (xy 208.28 129.54)))
  (wire (pts (xy 171.45 41.91) (xy 179.07 41.91)))
  (wire (pts (xy 77.47 73.66) (xy 71.12 73.66)))
  (wire (pts (xy 168.91 163.83) (xy 168.91 97.79)))
  (wire (pts (xy 63.5 81.28) (xy 63.5 92.71)))
  (wire (pts (xy 207.01 57.15) (xy 223.52 57.15)))
  (wire (pts (xy 220.98 99.06) (xy 220.98 77.47)))
  (wire (pts (xy 163.83 49.53) (xy 163.83 92.71)))
  (wire (pts (xy 158.75 41.91) (xy 158.75 154.94)))
  (wire (pts (xy 48.26 43.18) (xy 62.23 43.18)))
  (wire (pts (xy 48.26 43.18) (xy 48.26 121.92)))
  (wire (pts (xy 189.23 110.49) (xy 179.07 110.49)))
  (wire (pts (xy 137.16 151.13) (xy 179.07 151.13)))
  (wire (pts (xy 71.12 35.56) (xy 80.01 35.56)))
  (wire (pts (xy 243.84 156.21) (xy 243.84 124.46)))
  (wire (pts (xy 77.47 88.9) (xy 77.47 90.17)))
  (wire (pts (xy 80.01 72.39) (xy 53.34 72.39)))
  (wire (pts (xy 63.5 66.04) (xy 63.5 73.66)))
  (wire (pts (xy 179.07 41.91) (xy 179.07 110.49)))
  (wire (pts (xy 90.17 45.72) (xy 90.17 48.26)))
  (wire (pts (xy 186.69 90.17) (xy 186.69 133.35)))
  (wire (pts (xy 77.47 121.92) (xy 137.16 121.92)))
  (wire (pts (xy 77.47 76.2) (xy 90.17 76.2)))
  (wire (pts (xy 76.2 54.61) (xy 44.45 54.61)))
  (polyline (pts (xy 86.36 153.67) (xy 86.36 160.02)))
  (wire (pts (xy 92.71 154.94) (xy 158.75 154.94)))
  (wire (pts (xy 158.75 41.91) (xy 171.45 41.91)))
  (wire (pts (xy 243.84 124.46) (xy 193.04 124.46)))
  (wire (pts (xy 208.28 137.16) (xy 137.16 137.16)))
  (wire (pts (xy 204.47 133.35) (xy 205.74 133.35)))
  (polyline (pts (xy 86.36 166.37) (xy 88.9 166.37)))
  (wire (pts (xy 168.91 97.79) (xy 149.86 97.79)))
  (wire (pts (xy 134.62 40.64) (xy 134.62 35.56)))
  (wire (pts (xy 77.47 105.41) (xy 77.47 121.92)))
  (wire (pts (xy 48.26 121.92) (xy 53.34 121.92)))
  (wire (pts (xy 175.26 147.32) (xy 175.26 95.25)))
  (wire (pts (xy 137.16 158.75) (xy 137.16 151.13)))
  (wire (pts (xy 223.52 106.68) (xy 207.01 106.68)))
  (wire (pts (xy 171.45 63.5) (xy 171.45 41.91)))
  (wire (pts (xy 175.26 95.25) (xy 149.86 95.25)))
  (wire (pts (xy 92.71 158.75) (xy 137.16 158.75)))
  (wire (pts (xy 163.83 100.33) (xy 149.86 100.33)))
  (wire (pts (xy 80.01 35.56) (xy 90.17 35.56)))
  (wire (pts (xy 77.47 90.17) (xy 77.47 92.71)))
  (wire (pts (xy 76.2 30.48) (xy 120.65 30.48)))
  (wire (pts (xy 44.45 54.61) (xy 44.45 127)))
  (wire (pts (xy 189.23 118.11) (xy 189.23 129.54)))
  (wire (pts (xy 196.85 49.53) (xy 163.83 49.53)))
  (wire (pts (xy 207.01 97.79) (xy 207.01 106.68)))
  (wire (pts (xy 220.98 59.69) (xy 220.98 39.37)))
  (wire (pts (xy 106.68 63.5) (xy 87.63 63.5)))
  (wire (pts (xy 123.19 156.21) (xy 243.84 156.21)))
  (circle (center 134.62 41.91) (radius 2.54)
    (fill (type none))
  )
  (rectangle (start 57.15 27.94) (end 67.31 50.8)
    (fill (type none))
  )
  (rectangle (start 72.39 146.05) (end 100.33 181.61)
    (fill (type none))
  )
  (rectangle (start 77.47 148.59) (end 92.71 175.26)
    (fill (type none))
  )
  (rectangle (start 50.8 19.05) (end 69.85 52.07)
    (fill (type none))
  )
  (image (at 31.75 69.85) (scale 1.61035))
  (image (at 236.22 53.34) (scale 1.40625))
  (image (at 236.22 90.17) (scale 1.40625))
  (text "Fan\nMotor" (at 69.85 88.9 0))
  (text "A2" (at 252.73 58.42 0))
  (text "Temperature  Control System" (at 200.66 190.5 0))
  (text "LM35D" (at 233.68 100.33 0))
  (text "Gate" (at 87.63 63.5 0))
  (text "GND" (at 88.9 158.75 0))
  (text "Red" (at 207.01 44.45 0))
  (text "Board 2" (at 93.98 30.48 0))
  (text "LM35D" (at 233.68 64.77 0))
  (text "Heaters" (at 80.01 43.18 0))
  (text "* LM35D is attached \nto the 36 Ohm cement \ntype Resistor Heater"
    (at 96.52 50.8 0)
  )
  (text "Drain" (at 81.28 59.69 0))
  (text "A1" (at 219.71 140.97 0))
  (text "Orange" (at 208.28 83.82 0))
  (text "Gate" (at 85.09 100.33 0))
  (text "SDA" (at 88.9 163.83 0))
  (text "36\nOhm" (at 76.2 52.07 0))
  (text "Temperature Set Point" (at 215.9 133.35 0))
  (text "(0 to 1.66V)\n(Set Point 0 to 160 Deg C)\n" (at 210.82 138.43 0))
  (text "External 12VDC\n1 Amp Power Supply" (at 54.61 25.4 0))
  (text "Fan Setting 0 to 100%\n(0 to 5V)" (at 181.61 151.13 0))
  (text "Green" (at 208.28 97.79 0))
  (text "IRF540N" (at 83.82 66.04 0))
  (text "IRF540N" (at 27.94 87.63 0))
  (text "i2CLCD2004" (at 78.74 151.13 0))
  (text "Brown" (at 191.77 49.53 0))
  (text "Board 1" (at 149.86 30.48 0))
  (text "Source" (at 81.28 68.58 0))
  (text "Drain" (at 77.47 97.79 0))
  (text "A4" (at 96.52 163.83 0))
  (text "*" (at 77.47 55.88 0))
  (text "Jumper" (at 123.19 41.91 0))
  (text "30\nOhm" (at 85.09 52.07 0))
  (text "Fan Speed and Temperature Controller" (at 194.31 175.26 0))
  (text "SLC" (at 88.9 166.37 0))
  (text "IRF540N" (at 80.01 105.41 0))
  (text "Air Temperature\nChamber Middle" (at 245.11 92.71 0))
  (text "Heater Temperature\nControlled Variable" (at 245.11 55.88 0))
  (text "Yellow" (at 190.5 92.71 0))
  (text "5V" (at 90.17 154.94 0))
  (text "PWMD11" (at 110.49 101.6 0))
  (text "A0" (at 250.19 95.25 0))
  (text "20x4 Character\nDisplay" (at 77.47 173.99 0))
  (text "PWMD10" (at 109.22 97.79 0))
  (text "A5" (at 96.52 166.37 0))
  (text "I2C Bus" (at 78.74 160.02 0))
  (text "A3" (at 185.42 153.67 0))
  (text "Black" (at 208.28 57.15 0))
  (text "Dec 18, 2023" (at 219.71 194.31 0))
  (symbol (lib_id "power:GND") (at 62.23 43.18 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 62.23 49.53 0))
    (property "Value" "GND" (at 62.23 48.26 0))
    (property "Footprint" "" (at 62.23 43.18 0))
    (property "Datasheet" "" (at 62.23 43.18 0))
    (pin "1")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Sensor_Temperature:LM35-D") (at 207.01 90.17 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U2" (at 215.9 89.535 0))
    (property "Value" "LM35-D" (at 215.9 92.075 0))
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (at 207.01 100.33 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm35.pdf" (at 207.01 90.17 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Diode:1N4001") (at 90.17 85.09 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D1" (at 92.71 84.455 90))
    (property "Value" "1N4001" (at 92.71 86.995 90))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (at 90.17 85.09 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (at 90.17 85.09 0))
    (property "Sim.Device" "D" (at 90.17 85.09 0))
    (property "Sim.Pins" "1=K 2=A" (at 90.17 85.09 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "D1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 63.5 77.47 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D3" (at 67.31 78.4225 90))
    (property "Value" "LED" (at 67.31 80.9625 90))
    (property "Footprint" "" (at 63.5 77.47 0))
    (property "Datasheet" "~" (at 63.5 77.47 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "D3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 189.23 115.57 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R5-10K" (at 190.5 115.57 0))
    (property "Value" "R_Small" (at 191.77 117.475 0))
    (property "Footprint" "" (at 189.23 115.57 0))
    (property "Datasheet" "~" (at 189.23 115.57 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "R5-10K") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Motor:Fan_ALT") (at 77.47 82.55 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "M2" (at 83.82 81.915 0))
    (property "Value" "Fan_ALT" (at 83.82 84.455 0))
    (property "Footprint" "" (at 77.47 83.82 0))
    (property "Datasheet" "~" (at 77.47 83.82 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "M2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 90.17 41.91 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R2" (at 92.71 41.275 0))
    (property "Value" "220" (at 92.71 43.815 0))
    (property "Footprint" "" (at 88.392 41.91 90))
    (property "Datasheet" "~" (at 90.17 41.91 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "MCU_Module:Arduino_Nano_v3.x") (at 137.16 87.63 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "A1" (at 141.6559 113.03 0))
    (property "Value" "Arduino_Nano_v3.x" (at 141.6559 115.57 0))
    (property "Footprint" "Module:Arduino_Nano" (at 137.16 87.63 0))
    (property "Datasheet" "http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf" (at 137.16 87.63 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "A1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Sensor_Temperature:LM35-D") (at 207.01 49.53 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U1" (at 215.9 48.895 0))
    (property "Value" "LM35-D" (at 215.9 51.435 0))
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (at 207.01 59.69 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm35.pdf" (at 207.01 49.53 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_FET:IRF540N") (at 82.55 63.5 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q1" (at 76.2 64.135 0))
    (property "Value" "IRF540N" (at 76.2 61.595 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (at 76.2 65.405 0))
    (property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf540n.pdf" (at 82.55 63.5 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "Q1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+12V") (at 62.23 35.56 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 62.23 39.37 0))
    (property "Value" "+12V" (at 62.23 31.75 0))
    (property "Footprint" "" (at 62.23 35.56 0))
    (property "Datasheet" "" (at 62.23 35.56 0))
    (pin "1")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:Heater") (at 83.82 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R4" (at 86.36 47.625 0))
    (property "Value" "Heater" (at 86.36 50.165 0))
    (property "Footprint" "" (at 82.042 48.26 90))
    (property "Datasheet" "~" (at 83.82 48.26 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "R4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 90.17 52.07 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D2" (at 93.98 53.0225 90))
    (property "Value" "LED" (at 93.98 55.5625 90))
    (property "Footprint" "" (at 90.17 52.07 0))
    (property "Datasheet" "~" (at 90.17 52.07 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Potentiometer_US") (at 208.28 133.35 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "RV1" (at 210.82 132.715 0))
    (property "Value" "R_Potentiometer_US" (at 210.82 135.255 0))
    (property "Footprint" "" (at 208.28 133.35 0))
    (property "Datasheet" "~" (at 208.28 133.35 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "RV1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Potentiometer_US") (at 179.07 147.32 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "RV2" (at 181.61 146.685 0))
    (property "Value" "R_Potentiometer_US" (at 181.61 149.225 0))
    (property "Footprint" "" (at 179.07 147.32 0))
    (property "Datasheet" "~" (at 179.07 147.32 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "RV2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_FET:IRF540N") (at 80.01 100.33 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q2" (at 73.66 99.695 0))
    (property "Value" "IRF540N" (at 73.66 102.235 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (at 73.66 102.235 0))
    (property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf540n.pdf" (at 80.01 100.33 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "Q2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 63.5 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R3" (at 66.04 61.595 0))
    (property "Value" "220" (at 66.04 64.135 0))
    (property "Footprint" "" (at 61.722 62.23 90))
    (property "Datasheet" "~" (at 63.5 62.23 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "R3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:Heater") (at 80.01 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 82.55 47.625 0))
    (property "Value" "Heater" (at 82.55 50.165 0))
    (property "Footprint" "" (at 78.232 48.26 90))
    (property "Datasheet" "~" (at 80.01 48.26 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Temperature Controller_2"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
