(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Conn_01x02_Pin_1"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x02_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x02, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x02_Pin_1_1_1"
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
			)
		)
		(symbol "Conn_01x02_Pin_2"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x02_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x02, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x02_Pin_2_1_1"
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
			)
		)
		(symbol "Connector:Conn_01x02_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x02_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x02, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x02_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Driver_Display:CR2013-MI2120"
			(pin_names
				(offset 0.762)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -17.526 13.97 0)
			)
			(property "Value" "CR2013-MI2120"
				(at 1.905 13.97 0)
			)
			(property "Footprint" "Display:CR2013-MI2120"
				(at 0 -17.78 0)
			)
			(property "Datasheet" "http://pan.baidu.com/s/11Y990"
				(at -16.51 12.7 0)
			)
			(property "Description" "ILI9341 controller, SPI TFT LCD Display, 9-pin breakout PCB, 4-pin SD card interface, 5V/3.3V"
				(at 0 0 0)
			)
			(property "ki_keywords" "driver display"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*CR2013*MI2120*"
				(at 0 0 0)
			)
			(symbol "CR2013-MI2120_0_0"
				(text "320x240 LCD"
					(at 0.889 2.032 0)
				)
				(text "ILI9341"
					(at -5.461 4.572 0)
				)
				(text "SD Card Slot"
					(at -5.461 -3.048 0)
				)
				(text "SPI Interface"
					(at -5.461 -0.508 0)
				)
			)
			(symbol "CR2013-MI2120_0_1"
				(rectangle
					(start -17.78 12.7)
					(end 17.78 -12.7)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -6.35 6.35)
					(end 8.255 -5.08)
					(fill
						(type none)
					)
				)
			)
			(symbol "CR2013-MI2120_1_1"
				(pin power_in line
					(at 0 15.24 270)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin input line
					(at -20.32 10.16 0)
					(length 2.54)
					(name "SD_CS")
					(number "10")
				)
				(pin input line
					(at -20.32 7.62 0)
					(length 2.54)
					(name "SD_MOSI")
					(number "11")
				)
				(pin output line
					(at -20.32 5.08 0)
					(length 2.54)
					(name "SD_MISO")
					(number "12")
				)
				(pin input line
					(at -20.32 2.54 0)
					(length 2.54)
					(name "SD_SCK")
					(number "13")
				)
				(pin input line
					(at -20.32 0 0)
					(length 2.54)
					(name "FLASH_CD")
					(number "14")
				)
				(pin power_in line
					(at 0 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 20.32 5.08 180)
					(length 2.54)
					(name "~{CS}")
					(number "3")
				)
				(pin input line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "RESET")
					(number "4")
				)
				(pin input line
					(at 20.32 7.62 180)
					(length 2.54)
					(name "D/~{C}")
					(number "5")
				)
				(pin input line
					(at 20.32 2.54 180)
					(length 2.54)
					(name "MOSI")
					(number "6")
				)
				(pin input line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "SCK")
					(number "7")
				)
				(pin input line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "LED")
					(number "8")
				)
				(pin output line
					(at 20.32 0 180)
					(length 2.54)
					(name "MISO")
					(number "9")
				)
			)
		)
		(symbol "PCM_Espressif:ESP32-DevKitC"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -30.48 38.1 0)
			)
			(property "Value" "ESP32-DevKitC"
				(at -30.48 35.56 0)
			)
			(property "Footprint" "PCM_Espressif:ESP32-DevKitC"
				(at 0 -43.18 0)
			)
			(property "Datasheet" "https://docs.espressif.com/projects/esp-idf/zh_CN/latest/esp32/hw-reference/esp32/get-started-devkitc.html"
				(at 0 -45.72 0)
			)
			(property "Description" "Development Kit"
				(at 0 0 0)
			)
			(property "ki_keywords" "ESP32"
				(at 0 0 0)
			)
			(symbol "ESP32-DevKitC_0_0"
				(text "ESP32-DevKitC"
					(at -2.54 -20.32 0)
				)
				(pin power_in line
					(at 0 -35.56 90)
					(length 2.54)
					(name "GND")
					(number "14")
				)
				(pin power_in line
					(at 0 35.56 270)
					(length 2.54)
					(name "5V")
					(number "19")
				)
			)
			(symbol "ESP32-DevKitC_0_1"
				(rectangle
					(start -30.48 33.02)
					(end 30.48 -33.02)
					(fill
						(type background)
					)
				)
			)
			(symbol "ESP32-DevKitC_1_1"
				(pin power_in line
					(at 2.54 35.56 270)
					(length 2.54)
					(name "3V3")
					(number "1")
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "DAC_2/ADC2_CH9/GPIO26")
					(number "10")
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "ADC2_CH7/GPIO27")
					(number "11")
				)
				(pin bidirectional line
					(at -33.02 12.7 0)
					(length 2.54)
					(name "MTMS/GPIO14/ADC2_CH6")
					(number "12")
				)
				(pin bidirectional line
					(at -33.02 17.78 0)
					(length 2.54)
					(name "MTDI/GPIO12/ADC2_CH5")
					(number "13")
				)
				(pin bidirectional line
					(at -33.02 15.24 0)
					(length 2.54)
					(name "MTCK/GPIO13/ADC2_CH4")
					(number "15")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 2.54)
					(name "SD_DATA2/GPIO9")
					(number "16")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "SD_DATA3/GPIO10")
					(number "17")
				)
				(pin bidirectional line
					(at 33.02 -25.4 180)
					(length 2.54)
					(name "CMD")
					(number "18")
				)
				(pin input line
					(at -33.02 30.48 0)
					(length 2.54)
					(name "CHIP_PU")
					(number "2")
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "SD_CLK/GPIO6")
					(number "20")
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "SD_DATA0/GPIO7")
					(number "21")
				)
				(pin bidirectional line
					(at 33.02 -17.78 180)
					(length 2.54)
					(name "SD_DATA1/GPIO8")
					(number "22")
				)
				(pin bidirectional line
					(at -33.02 10.16 0)
					(length 2.54)
					(name "MTDO/GPIO15/ADC2_CH3")
					(number "23")
				)
				(pin bidirectional line
					(at 33.02 20.32 180)
					(length 2.54)
					(name "ADC2_CH2/GPIO2")
					(number "24")
				)
				(pin bidirectional line
					(at 33.02 22.86 180)
					(length 2.54)
					(name "GPIO0/BOOT/ADC2_CH1")
					(number "25")
				)
				(pin bidirectional line
					(at 33.02 17.78 180)
					(length 2.54)
					(name "ADC2_CH0/GPIO4")
					(number "26")
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 2.54)
					(name "GPIO16")
					(number "27")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "GPIO17")
					(number "28")
				)
				(pin bidirectional line
					(at 33.02 15.24 180)
					(length 2.54)
					(name "GPIO5")
					(number "29")
				)
				(pin input line
					(at -33.02 0 0)
					(length 2.54)
					(name "SENSOR_VP/GPIO36/ADC1_CH0")
					(number "3")
				)
				(pin bidirectional line
					(at 33.02 12.7 180)
					(length 2.54)
					(name "GPIO18")
					(number "30")
				)
				(pin bidirectional line
					(at 33.02 10.16 180)
					(length 2.54)
					(name "GPIO19")
					(number "31")
				)
				(pin passive line
					(at 0 -35.56 90)
					(length 2.54) hide
					(name "GND")
					(number "32")
				)
				(pin bidirectional line
					(at 33.02 7.62 180)
					(length 2.54)
					(name "GPIO21")
					(number "33")
				)
				(pin bidirectional line
					(at 33.02 27.94 180)
					(length 2.54)
					(name "U0RXD/GPIO3")
					(number "34")
				)
				(pin bidirectional line
					(at 33.02 30.48 180)
					(length 2.54)
					(name "U0TXD/GPIO1")
					(number "35")
				)
				(pin bidirectional line
					(at 33.02 5.08 180)
					(length 2.54)
					(name "GPIO22")
					(number "36")
				)
				(pin bidirectional line
					(at 33.02 2.54 180)
					(length 2.54)
					(name "GPIO23")
					(number "37")
				)
				(pin passive line
					(at 0 -35.56 90)
					(length 2.54) hide
					(name "GND")
					(number "38")
				)
				(pin input line
					(at -33.02 -2.54 0)
					(length 2.54)
					(name "SENSOR_VN/GPIO39/ADC1_CH3")
					(number "4")
				)
				(pin input line
					(at -33.02 5.08 0)
					(length 2.54)
					(name "VDET_1/GPIO34/ADC1_CH6")
					(number "5")
				)
				(pin input line
					(at -33.02 2.54 0)
					(length 2.54)
					(name "VDET_2/GPIO35/ADC1_CH7")
					(number "6")
				)
				(pin bidirectional line
					(at -33.02 25.4 0)
					(length 2.54)
					(name "32K_XP/GPIO32/ADC1_CH4")
					(number "7")
				)
				(pin bidirectional line
					(at -33.02 22.86 0)
					(length 2.54)
					(name "32K_XN/GPIO33/ADC1_CH5")
					(number "8")
				)
				(pin bidirectional line
					(at 33.02 0 180)
					(length 2.54)
					(name "DAC_1/ADC2_CH8/GPIO25")
					(number "9")
				)
			)
		)
		(symbol "PCM_arduino-library:Arduino_Nano_33_BLE_Socket"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "A"
				(at 0 33.02 0)
			)
			(property "Value" "Arduino_Nano_33_BLE_Socket"
				(at 0 29.21 0)
			)
			(property "Footprint" "PCM_arduino-library:Arduino_Nano_Every_Socket"
				(at 0 -34.29 0)
			)
			(property "Datasheet" "https://docs.arduino.cc/hardware/nano-33-ble"
				(at 0 -30.48 0)
			)
			(property "Description" "Socket for Arduino Nano 33 BLE"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arduino MPU Shield"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Arduino_Nano_Every_Socket"
				(at 0 0 0)
			)
			(symbol "Arduino_Nano_33_BLE_Socket_0_0"
				(rectangle
					(start -17.78 26.67)
					(end 17.78 -26.67)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -7.62 6.35) (xy -6.35 6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -7.62 21.59) (xy -6.35 21.59)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -19.05) (xy 6.35 -19.05)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -11.43 -22.86) (xy -5.08 -22.86) (xy -5.08 -21.59)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 -13.97) (xy -5.08 -12.7) (xy -12.7 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -10.16 22.86) (xy -7.62 22.86) (xy -7.62 20.32) (xy -10.16 20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.89 7.62) (xy -7.62 7.62) (xy -7.62 5.08) (xy -8.89 5.08)
					)
					(fill
						(type none)
					)
				)
				(text "Analog"
					(at -2.54 2.54 900)
				)
				(text "I²C"
					(at -5.08 6.35 900)
				)
				(text "Misc."
					(at 5.08 -19.05 900)
				)
				(text "Power"
					(at -5.08 -17.78 900)
				)
				(text "Serial"
					(at -5.08 21.59 900)
				)
			)
			(symbol "Arduino_Nano_33_BLE_Socket_0_1"
				(polyline
					(pts
						(xy -13.97 12.7) (xy -2.54 12.7) (xy -2.54 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -11.43 -7.62) (xy -2.54 -7.62) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -5.08) (xy 5.08 -5.08) (xy 5.08 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 13.97 22.86) (xy 5.08 22.86) (xy 5.08 12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 10.16 -17.78) (xy 8.89 -17.78) (xy 8.89 -20.32) (xy 10.16 -20.32)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Arduino_Nano_33_BLE_Socket_1_0"
				(text "GPIO"
					(at 5.08 8.89 900)
				)
			)
			(symbol "Arduino_Nano_33_BLE_Socket_1_1"
				(pin power_in line
					(at -25.4 -17.78 0)
					(length 7.62)
					(name "3.3V")
					(number "3V3")
				)
				(pin no_connect non_logic
					(at -25.4 -15.24 0)
					(length 7.62)
					(name "5V")
					(number "5V")
				)
				(pin bidirectional line
					(at -25.4 -5.08 0)
					(length 7.62)
					(name "A0")
					(number "A0")
				)
				(pin bidirectional line
					(at -25.4 -2.54 0)
					(length 7.62)
					(name "A1")
					(number "A1")
				)
				(pin bidirectional line
					(at -25.4 0 0)
					(length 7.62)
					(name "A2")
					(number "A2")
				)
				(pin bidirectional line
					(at -25.4 2.54 0)
					(length 7.62)
					(name "A3")
					(number "A3")
				)
				(pin bidirectional line
					(at -25.4 5.08 0)
					(length 7.62)
					(name "A4/SDA")
					(number "A4")
				)
				(pin bidirectional clock
					(at -25.4 7.62 0)
					(length 7.62)
					(name "A5/SCL")
					(number "A5")
				)
				(pin input line
					(at -25.4 10.16 0)
					(length 7.62)
					(name "A6")
					(number "A6")
				)
				(pin input line
					(at -25.4 12.7 0)
					(length 7.62)
					(name "A7")
					(number "A7")
				)
				(pin input line
					(at -25.4 -7.62 0)
					(length 7.62)
					(name "AREF")
					(number "AREF")
				)
				(pin bidirectional line
					(at -25.4 22.86 0)
					(length 7.62)
					(name "D0/RX")
					(number "D0")
				)
				(pin bidirectional line
					(at -25.4 20.32 0)
					(length 7.62)
					(name "D1/TX")
					(number "D1")
				)
				(pin bidirectional line
					(at 25.4 2.54 180)
					(length 7.62)
					(name "D10")
					(number "D10")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 7.62)
					(name "D11_MOSI")
					(number "D11")
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 7.62)
					(name "D12_MISO")
					(number "D12")
				)
				(pin bidirectional clock
					(at 25.4 -5.08 180)
					(length 7.62)
					(name "D13_SCK")
					(number "D13")
				)
				(pin bidirectional line
					(at 25.4 22.86 180)
					(length 7.62)
					(name "D2")
					(number "D2")
				)
				(pin bidirectional line
					(at 25.4 20.32 180)
					(length 7.62)
					(name "D3")
					(number "D3")
				)
				(pin bidirectional line
					(at 25.4 17.78 180)
					(length 7.62)
					(name "D4")
					(number "D4")
				)
				(pin bidirectional line
					(at 25.4 15.24 180)
					(length 7.62)
					(name "D5")
					(number "D5")
				)
				(pin bidirectional line
					(at 25.4 12.7 180)
					(length 7.62)
					(name "D6")
					(number "D6")
				)
				(pin bidirectional line
					(at 25.4 10.16 180)
					(length 7.62)
					(name "D7")
					(number "D7")
				)
				(pin bidirectional line
					(at 25.4 7.62 180)
					(length 7.62)
					(name "D8")
					(number "D8")
				)
				(pin bidirectional line
					(at 25.4 5.08 180)
					(length 7.62)
					(name "D9")
					(number "D9")
				)
				(pin power_in line
					(at -25.4 -20.32 0)
					(length 7.62)
					(name "GND")
					(number "GND1")
				)
				(pin power_in line
					(at -25.4 -22.86 0)
					(length 7.62)
					(name "GND")
					(number "GND2")
				)
				(pin open_collector input_low
					(at 25.4 -17.78 180)
					(length 7.62)
					(name "RESET")
					(number "RST1")
				)
				(pin open_collector input_low
					(at 25.4 -20.32 180)
					(length 7.62)
					(name "RESET")
					(number "RST2")
				)
				(pin power_in line
					(at -25.4 -12.7 0)
					(length 7.62)
					(name "VIN")
					(number "VIN")
				)
			)
		)
		(symbol "R_1"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_1_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "power:+3.3V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3.3V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3.3V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 80.01 180.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 244.475 149.225)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 146.685)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.325 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 99.695 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 190.5 60.325)
	)
	(wire
		(pts
			(xy 40.005 84.455) (xy 46.99 84.455)
		)
	)
	(wire
		(pts
			(xy 99.695 156.845) (xy 99.695 161.29)
		)
	)
	(wire
		(pts
			(xy 113.03 74.295) (xy 120.015 74.295)
		)
	)
	(wire
		(pts
			(xy 119.38 114.3) (xy 120.65 114.3)
		)
	)
	(wire
		(pts
			(xy 40.005 64.135) (xy 46.99 64.135)
		)
	)
	(wire
		(pts
			(xy 113.03 76.835) (xy 120.015 76.835)
		)
	)
	(wire
		(pts
			(xy 210.82 38.735) (xy 210.82 45.085)
		)
	)
	(wire
		(pts
			(xy 268.605 99.695) (xy 268.605 141.605)
		)
	)
	(wire
		(pts
			(xy 236.22 103.505) (xy 236.22 102.235)
		)
	)
	(wire
		(pts
			(xy 40.005 72.39) (xy 41.91 72.39)
		)
	)
	(wire
		(pts
			(xy 244.475 146.685) (xy 244.475 149.225)
		)
	)
	(wire
		(pts
			(xy 113.03 69.215) (xy 120.015 69.215)
		)
	)
	(wire
		(pts
			(xy 80.01 161.29) (xy 80.01 167.64)
		)
	)
	(wire
		(pts
			(xy 236.22 146.685) (xy 244.475 146.685)
		)
	)
	(wire
		(pts
			(xy 119.38 117.475) (xy 113.03 117.475)
		)
	)
	(wire
		(pts
			(xy 60.325 161.29) (xy 62.865 161.29)
		)
	)
	(wire
		(pts
			(xy 41.91 76.835) (xy 46.99 76.835)
		)
	)
	(wire
		(pts
			(xy 80.01 161.29) (xy 82.55 161.29)
		)
	)
	(wire
		(pts
			(xy 113.03 71.755) (xy 120.015 71.755)
		)
	)
	(wire
		(pts
			(xy 80.01 170.18) (xy 80.01 180.34)
		)
	)
	(wire
		(pts
			(xy 231.14 55.245) (xy 236.22 55.245)
		)
	)
	(wire
		(pts
			(xy 99.695 146.685) (xy 80.01 146.685)
		)
	)
	(wire
		(pts
			(xy 236.22 106.045) (xy 236.22 107.315)
		)
	)
	(wire
		(pts
			(xy 119.38 114.935) (xy 113.03 114.935)
		)
	)
	(wire
		(pts
			(xy 80.01 122.555) (xy 80.01 127)
		)
	)
	(wire
		(pts
			(xy 40.005 76.2) (xy 41.91 76.2)
		)
	)
	(wire
		(pts
			(xy 244.475 149.225) (xy 236.22 149.225)
		)
	)
	(wire
		(pts
			(xy 41.91 80.01) (xy 41.91 81.915)
		)
	)
	(wire
		(pts
			(xy 80.01 180.34) (xy 80.01 182.245)
		)
	)
	(wire
		(pts
			(xy 40.005 80.01) (xy 41.91 80.01)
		)
	)
	(wire
		(pts
			(xy 80.01 146.685) (xy 80.01 149.225)
		)
	)
	(wire
		(pts
			(xy 41.91 72.39) (xy 41.91 74.295)
		)
	)
	(wire
		(pts
			(xy 80.01 156.845) (xy 80.01 161.29)
		)
	)
	(wire
		(pts
			(xy 113.03 81.915) (xy 120.015 81.915)
		)
	)
	(wire
		(pts
			(xy 60.325 149.225) (xy 60.325 146.685)
		)
	)
	(wire
		(pts
			(xy 99.695 161.29) (xy 99.695 167.64)
		)
	)
	(wire
		(pts
			(xy 99.695 161.29) (xy 102.235 161.29)
		)
	)
	(wire
		(pts
			(xy 185.42 55.245) (xy 190.5 55.245)
		)
	)
	(wire
		(pts
			(xy 231.14 67.945) (xy 236.22 67.945)
		)
	)
	(wire
		(pts
			(xy 244.475 153.035) (xy 244.475 149.225)
		)
	)
	(wire
		(pts
			(xy 99.695 149.225) (xy 99.695 146.685)
		)
	)
	(wire
		(pts
			(xy 231.14 60.325) (xy 236.22 60.325)
		)
	)
	(wire
		(pts
			(xy 185.42 50.165) (xy 190.5 50.165)
		)
	)
	(wire
		(pts
			(xy 236.22 131.445) (xy 240.665 131.445)
		)
	)
	(wire
		(pts
			(xy 119.38 114.3) (xy 119.38 114.935)
		)
	)
	(wire
		(pts
			(xy 41.91 74.295) (xy 46.99 74.295)
		)
	)
	(wire
		(pts
			(xy 231.14 62.865) (xy 236.22 62.865)
		)
	)
	(wire
		(pts
			(xy 60.325 170.18) (xy 60.325 180.34)
		)
	)
	(wire
		(pts
			(xy 80.01 38.735) (xy 80.01 51.435)
		)
	)
	(wire
		(pts
			(xy 268.605 141.605) (xy 236.22 141.605)
		)
	)
	(wire
		(pts
			(xy 99.695 180.34) (xy 80.01 180.34)
		)
	)
	(wire
		(pts
			(xy 119.38 118.11) (xy 119.38 117.475)
		)
	)
	(wire
		(pts
			(xy 99.695 170.18) (xy 99.695 180.34)
		)
	)
	(wire
		(pts
			(xy 181.61 144.145) (xy 185.42 144.145)
		)
	)
	(wire
		(pts
			(xy 113.03 86.995) (xy 120.015 86.995)
		)
	)
	(wire
		(pts
			(xy 40.005 89.535) (xy 46.99 89.535)
		)
	)
	(wire
		(pts
			(xy 41.91 76.2) (xy 41.91 76.835)
		)
	)
	(wire
		(pts
			(xy 80.01 142.875) (xy 80.01 146.685)
		)
	)
	(wire
		(pts
			(xy 60.325 180.34) (xy 80.01 180.34)
		)
	)
	(wire
		(pts
			(xy 236.22 107.315) (xy 238.76 107.315)
		)
	)
	(wire
		(pts
			(xy 41.91 81.915) (xy 46.99 81.915)
		)
	)
	(wire
		(pts
			(xy 248.285 131.445) (xy 253.365 131.445)
		)
	)
	(wire
		(pts
			(xy 210.82 75.565) (xy 210.82 80.645)
		)
	)
	(wire
		(pts
			(xy 60.325 161.29) (xy 60.325 167.64)
		)
	)
	(wire
		(pts
			(xy 231.14 65.405) (xy 236.22 65.405)
		)
	)
	(wire
		(pts
			(xy 113.03 84.455) (xy 120.015 84.455)
		)
	)
	(wire
		(pts
			(xy 231.14 57.785) (xy 236.22 57.785)
		)
	)
	(wire
		(pts
			(xy 236.22 102.235) (xy 238.76 102.235)
		)
	)
	(wire
		(pts
			(xy 113.03 89.535) (xy 120.015 89.535)
		)
	)
	(wire
		(pts
			(xy 60.325 156.845) (xy 60.325 161.29)
		)
	)
	(wire
		(pts
			(xy 60.325 146.685) (xy 80.01 146.685)
		)
	)
	(wire
		(pts
			(xy 185.42 57.785) (xy 190.5 57.785)
		)
	)
	(wire
		(pts
			(xy 185.42 52.705) (xy 190.5 52.705)
		)
	)
	(wire
		(pts
			(xy 231.14 52.705) (xy 236.22 52.705)
		)
	)
	(wire
		(pts
			(xy 119.38 118.11) (xy 120.015 118.11)
		)
	)
	(text "Pull Up Resistors for:\n\nWiFi Reset\nTouch Screen Calibration\nBuzzer/Beep Enable"
		(exclude_from_sim no)
		(at 29.845 163.195 0)
	)
	(text "Siren Monitor - ESP32 Dev Kit (38 pin) to Arduino Nano BLE Interfaces"
		(exclude_from_sim no)
		(at 88.265 19.685 0)
	)
	(text "Arduino Nano BLE Sense Rev 1"
		(exclude_from_sim no)
		(at 210.82 94.615 0)
	)
	(text "Please Note:\n\nDo not drive TFT Backlight Directly\nfrom a GPIO Pin"
		(exclude_from_sim no)
		(at 262.255 72.39 0)
	)
	(text "ESP32 WROOM Dev Kit"
		(exclude_from_sim no)
		(at 80.01 29.845 0)
	)
	(text "ILI9341 TFT with Integrated Touch"
		(exclude_from_sim no)
		(at 210.82 29.845 0)
	)
	(global_label "SPI-SCK"
		(shape input)
		(at 120.015 74.295 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 131.4064 74.295 0)
		)
	)
	(global_label "WIFI-RST"
		(shape input)
		(at 40.005 89.535 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 28.2507 89.535 0)
		)
	)
	(global_label "NANO-RST"
		(shape output)
		(at 40.005 64.135 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 26.9202 64.135 0)
		)
	)
	(global_label "SPI-MOSI"
		(shape input)
		(at 236.22 57.785 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 248.4581 57.785 0)
		)
	)
	(global_label "SPI-MISO"
		(shape input)
		(at 185.42 55.245 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 173.1819 55.245 0)
		)
	)
	(global_label "SPI-SCK"
		(shape input)
		(at 185.42 57.785 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 174.0286 57.785 0)
		)
	)
	(global_label "TFT-CS"
		(shape input)
		(at 120.015 71.755 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 130.0759 71.755 0)
		)
	)
	(global_label "SPI-MOSI"
		(shape input)
		(at 185.42 52.705 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 173.1819 52.705 0)
		)
	)
	(global_label "TFT-BACKLIGHT"
		(shape output)
		(at 40.005 76.2 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 22.324 76.2 0)
		)
	)
	(global_label "ESP-INT"
		(shape output)
		(at 253.365 131.445 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 264.454 131.445 0)
		)
	)
	(global_label "TFT-RST"
		(shape input)
		(at 120.015 81.915 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 131.0435 81.915 0)
		)
	)
	(global_label "BUZZER-EN"
		(shape output)
		(at 62.865 161.29 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 77.3406 161.29 0)
		)
	)
	(global_label "SPI-MISO"
		(shape input)
		(at 236.22 60.325 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 248.4581 60.325 0)
		)
	)
	(global_label "TFT-DC"
		(shape input)
		(at 236.22 52.705 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 246.3414 52.705 0)
		)
	)
	(global_label "RXD2"
		(shape output)
		(at 120.65 114.3 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 128.5942 114.3 0)
		)
	)
	(global_label "SPI-SCK"
		(shape input)
		(at 236.22 62.865 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 247.6114 62.865 0)
		)
	)
	(global_label "SPI-MISO"
		(shape input)
		(at 120.015 76.835 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 132.2531 76.835 0)
		)
	)
	(global_label "SD-CS"
		(shape input)
		(at 120.015 86.995 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 129.5316 86.995 0)
		)
	)
	(global_label "TOUCH-RST"
		(shape input)
		(at 40.005 84.455 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 25.7712 84.455 0)
		)
	)
	(global_label "ESP-INT"
		(shape input)
		(at 120.015 89.535 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 131.104 89.535 0)
		)
	)
	(global_label "SD-CS"
		(shape input)
		(at 185.42 50.165 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 175.9034 50.165 0)
		)
	)
	(global_label "TXD2"
		(shape input)
		(at 120.015 118.11 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 127.6568 118.11 0)
		)
	)
	(global_label "TFT-DC"
		(shape input)
		(at 120.015 69.215 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 130.1364 69.215 0)
		)
	)
	(global_label "TFT-RST"
		(shape input)
		(at 236.22 67.945 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 247.2485 67.945 0)
		)
	)
	(global_label "BUZZER-EN"
		(shape input)
		(at 40.005 80.01 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 25.5294 80.01 0)
		)
	)
	(global_label "TOUCH-RST"
		(shape output)
		(at 82.55 161.29 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 96.7838 161.29 0)
		)
	)
	(global_label "RXD2"
		(shape output)
		(at 238.76 107.315 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 246.7042 107.315 0)
		)
	)
	(global_label "TFT-BACKLIGHT"
		(shape input)
		(at 236.22 65.405 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 253.901 65.405 0)
		)
	)
	(global_label "NANO-RST"
		(shape input)
		(at 181.61 144.145 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 168.5252 144.145 0)
		)
	)
	(global_label "TFT-CS"
		(shape input)
		(at 236.22 55.245 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 246.2809 55.245 0)
		)
	)
	(global_label "TOUCH-CS"
		(shape input)
		(at 40.005 72.39 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 26.7388 72.39 0)
		)
	)
	(global_label "WIFI-RST"
		(shape output)
		(at 102.235 161.29 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 113.9893 161.29 0)
		)
	)
	(global_label "SPI-MOSI"
		(shape input)
		(at 120.015 84.455 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 132.2531 84.455 0)
		)
	)
	(global_label "TXD2"
		(shape input)
		(at 238.76 102.235 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 246.4018 102.235 0)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 80.01 142.875 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 80.01 146.685 0)
		)
		(property "Value" "+3.3V"
			(at 80.01 137.795 0)
		)
		(property "Footprint" ""
			(at 80.01 142.875 0)
		)
		(property "Datasheet" ""
			(at 80.01 142.875 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 80.01 142.875 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_Espressif:ESP32-DevKitC")
		(at 80.01 86.995 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 82.2041 122.555 0)
		)
		(property "Value" "ESP32-DevKitC"
			(at 82.2041 125.095 0)
		)
		(property "Footprint" "PCM_Espressif:ESP32-DevKitC"
			(at 80.01 130.175 0)
		)
		(property "Datasheet" "https://docs.espressif.com/projects/esp-idf/zh_CN/latest/esp32/hw-reference/esp32/get-started-devkitc.html"
			(at 80.01 132.715 0)
		)
		(property "Description" "Development Kit"
			(at 80.01 86.995 0)
		)
		(pin "11")
		(pin "31")
		(pin "15")
		(pin "27")
		(pin "34")
		(pin "5")
		(pin "2")
		(pin "25")
		(pin "4")
		(pin "33")
		(pin "36")
		(pin "9")
		(pin "1")
		(pin "29")
		(pin "3")
		(pin "16")
		(pin "8")
		(pin "38")
		(pin "10")
		(pin "17")
		(pin "20")
		(pin "24")
		(pin "30")
		(pin "37")
		(pin "28")
		(pin "23")
		(pin "14")
		(pin "18")
		(pin "26")
		(pin "22")
		(pin "32")
		(pin "6")
		(pin "35")
		(pin "7")
		(pin "19")
		(pin "12")
		(pin "13")
		(pin "21")
		(instances
			(project "Siren Sensor"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "Conn_01x02_Pin_2")
		(lib_id "Connector:Conn_01x02_Pin")
		(at 104.775 170.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J3"
			(at 106.045 167.6399 0)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 106.045 170.1799 0)
		)
		(property "Footprint" ""
			(at 104.775 170.18 0)
		)
		(property "Datasheet" "~"
			(at 104.775 170.18 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 104.775 170.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 80.01 153.035 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 81.915 151.7649 0)
		)
		(property "Value" "10kΩ"
			(at 81.915 154.3049 0)
		)
		(property "Footprint" ""
			(at 81.788 153.035 90)
		)
		(property "Datasheet" "~"
			(at 80.01 153.035 0)
		)
		(property "Description" "Resistor"
			(at 80.01 153.035 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 60.325 153.035 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 62.23 151.7649 0)
		)
		(property "Value" "10kΩ"
			(at 62.23 154.3049 0)
		)
		(property "Footprint" ""
			(at 62.103 153.035 90)
		)
		(property "Datasheet" "~"
			(at 60.325 153.035 0)
		)
		(property "Description" "Resistor"
			(at 60.325 153.035 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 210.82 80.645 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 210.82 86.995 0)
		)
		(property "Value" "GND"
			(at 210.82 85.09 0)
		)
		(property "Footprint" ""
			(at 210.82 80.645 0)
		)
		(property "Datasheet" ""
			(at 210.82 80.645 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 210.82 80.645 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 85.09 170.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J2"
			(at 88.9 167.6399 0)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 88.9 170.1799 0)
		)
		(property "Footprint" ""
			(at 85.09 170.18 0)
		)
		(property "Datasheet" "~"
			(at 85.09 170.18 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 85.09 170.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Driver_Display:CR2013-MI2120")
		(at 210.82 60.325 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 213.0141 43.18 0)
		)
		(property "Value" "CR2013-MI2120"
			(at 213.0141 45.72 0)
		)
		(property "Footprint" "Display:CR2013-MI2120"
			(at 210.82 78.105 0)
		)
		(property "Datasheet" "http://pan.baidu.com/s/11Y990"
			(at 194.31 47.625 0)
		)
		(property "Description" "ILI9341 controller, SPI TFT LCD Display, 9-pin breakout PCB, 4-pin SD card interface, 5V/3.3V"
			(at 210.82 60.325 0)
		)
		(pin "10")
		(pin "7")
		(pin "2")
		(pin "3")
		(pin "13")
		(pin "1")
		(pin "5")
		(pin "4")
		(pin "8")
		(pin "11")
		(pin "9")
		(pin "12")
		(pin "14")
		(pin "6")
		(instances
			(project "Siren Sensor"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 244.475 131.445 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 244.475 125.095 90)
		)
		(property "Value" "220Ω"
			(at 244.475 127.635 90)
		)
		(property "Footprint" ""
			(at 244.475 133.223 90)
		)
		(property "Datasheet" "~"
			(at 244.475 131.445 0)
		)
		(property "Description" "Resistor"
			(at 244.475 131.445 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_arduino-library:Arduino_Nano_33_BLE_Socket")
		(at 210.82 126.365 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "A1"
			(at 210.82 94.615 0)
		)
		(property "Value" "Arduino_Nano_33_BLE_Socket"
			(at 210.82 97.155 0)
		)
		(property "Footprint" "PCM_arduino-library:Arduino_Nano_Every_Socket"
			(at 210.82 160.655 0)
		)
		(property "Datasheet" "https://docs.arduino.cc/hardware/nano-33-ble"
			(at 210.82 156.845 0)
		)
		(property "Description" "Socket for Arduino Nano 33 BLE"
			(at 210.82 126.365 0)
		)
		(pin "D11")
		(pin "D1")
		(pin "D4")
		(pin "D5")
		(pin "A6")
		(pin "VIN")
		(pin "3V3")
		(pin "A7")
		(pin "GND2")
		(pin "D0")
		(pin "A5")
		(pin "D6")
		(pin "A1")
		(pin "D2")
		(pin "D3")
		(pin "A3")
		(pin "D7")
		(pin "A0")
		(pin "D10")
		(pin "D9")
		(pin "D8")
		(pin "RST1")
		(pin "RST2")
		(pin "A2")
		(pin "GND1")
		(pin "AREF")
		(pin "5V")
		(pin "A4")
		(pin "D12")
		(pin "D13")
		(instances
			(project "Siren Sensor"
				(path
					(reference "A1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 80.01 38.735 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 80.01 42.545 0)
		)
		(property "Value" "+5V"
			(at 80.01 34.29 0)
		)
		(property "Footprint" ""
			(at 80.01 38.735 0)
		)
		(property "Datasheet" ""
			(at 80.01 38.735 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 80.01 38.735 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R_1")
		(lib_id "Device:R")
		(at 99.695 153.035 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 101.6 151.7649 0)
		)
		(property "Value" "10kΩ"
			(at 101.6 154.3049 0)
		)
		(property "Footprint" ""
			(at 101.473 153.035 90)
		)
		(property "Datasheet" "~"
			(at 99.695 153.035 0)
		)
		(property "Description" "Resistor"
			(at 99.695 153.035 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 268.605 99.695 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR03"
			(at 268.605 103.505 0)
		)
		(property "Value" "+5V"
			(at 268.605 95.25 0)
		)
		(property "Footprint" ""
			(at 268.605 99.695 0)
		)
		(property "Datasheet" ""
			(at 268.605 99.695 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 268.605 99.695 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 80.01 182.245 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 80.01 188.595 0)
		)
		(property "Value" "GND"
			(at 80.01 186.69 0)
		)
		(property "Footprint" ""
			(at 80.01 182.245 0)
		)
		(property "Datasheet" ""
			(at 80.01 182.245 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 80.01 182.245 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 210.82 38.735 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 210.82 42.545 0)
		)
		(property "Value" "+3.3V"
			(at 210.82 33.655 0)
		)
		(property "Footprint" ""
			(at 210.82 38.735 0)
		)
		(property "Datasheet" ""
			(at 210.82 38.735 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 210.82 38.735 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "Conn_01x02_Pin_1")
		(lib_id "Connector:Conn_01x02_Pin")
		(at 65.405 170.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J1"
			(at 66.675 167.6399 0)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 57.785 179.07 0)
		)
		(property "Footprint" ""
			(at 65.405 170.18 0)
		)
		(property "Datasheet" "~"
			(at 65.405 170.18 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 65.405 170.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 80.01 127 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 80.01 133.35 0)
		)
		(property "Value" "GND"
			(at 80.01 131.445 0)
		)
		(property "Footprint" ""
			(at 80.01 127 0)
		)
		(property "Datasheet" ""
			(at 80.01 127 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 80.01 127 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 244.475 153.035 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 244.475 159.385 0)
		)
		(property "Value" "GND"
			(at 244.475 157.48 0)
		)
		(property "Footprint" ""
			(at 244.475 153.035 0)
		)
		(property "Datasheet" ""
			(at 244.475 153.035 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 244.475 153.035 0)
		)
		(pin "1")
		(instances
			(project "Siren Sensor"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)