(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers_Nordic/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VDD")
  (net 3 "/SDA")
  (net 4 "/SCL")
  (net 5 "/INT1")
  (net 6 "unconnected-(U1-~{RESET}-Pad3)")
  (net 7 "+5V")
  (net 8 "unconnected-(U1-NC-Pad8)")
  (net 9 "/SV1")
  (net 10 "unconnected-(U1-A2-Pad11)")
  (net 11 "unconnected-(U1-A3-Pad12)")
  (net 12 "unconnected-(U1-A4-Pad13)")
  (net 13 "unconnected-(U1-A5-Pad14)")
  (net 14 "unconnected-(U1-D2-Pad17)")
  (net 15 "unconnected-(U1-D3-Pad18)")
  (net 16 "unconnected-(U1-D4-Pad19)")
  (net 17 "unconnected-(U1-D5-Pad20)")
  (net 18 "unconnected-(U1-D6-Pad21)")
  (net 19 "unconnected-(U1-D7-Pad22)")
  (net 20 "unconnected-(U1-D8-Pad23)")
  (net 21 "unconnected-(U1-D9-Pad24)")
  (net 22 "unconnected-(U1-D10-Pad25)")
  (net 23 "unconnected-(U1-D11-Pad26)")
  (net 24 "unconnected-(U1-D12-Pad27)")
  (net 25 "unconnected-(U1-D13-Pad28)")
  (net 26 "unconnected-(U1-AREF-Pad30)")
  (net 27 "/INT2")
  (net 28 "/SV2")
  (net 29 "Net-(JBAT2-Pin_2)")
  (net 30 "Net-(JBAT1-Pin_2)")
  (net 31 "unconnected-(SW1-C-Pad3)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (at 138.017703 106.625 -90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J_SERVO1" (at 1.475 8.117703 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 4.385 7.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/SV1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Build2Together:CONN_S2B-XH-A-1LFSN_JST" (layer "F.Cu")
    (at 126.3 54.953076 180)
    (tags "S2B-XH-A-1LFSN ")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "JBAT2" (at -0.6 -5.546924 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 1.275 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.275 0 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.499999 0 180) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(JBAT2-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/Symbols/S2B-XH-A-1.STEP"
      (offset (xyz 1.2 -7.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_S5B-XH-A_1x05_P2.50mm_Horizontal" (layer "F.Cu")
    (at 150.3 56.740876 180)
    (descr "JST XH series connector, S5B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH horizontal")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1_I2C1" (at -3.9 0.140876 270) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 5 10.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5 3.45) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 2 "VDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 3 "/SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 4 "/SCL") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 5 "/INT1") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S5B-XH-A_1x05_P2.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Build2Together:1P2T_SS-12D00_CNK" (layer "F.Cu")
    (at 133.3 55.624576 180)
    (tags "SS-12D00-G 4 E ")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.4 2.824576 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SW_SPDT" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.3622 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "*" (at -2.3622 0 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.4732 0 180) (layer "F.Fab"))
    (fp_text user "*" (at -1.4732 0) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.27 1.27) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(JBAT2-Pin_2)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.27 1.27) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(JBAT1-Pin_2)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.27 1.27) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(SW1-C-Pad3)") (pinfunction "C") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/Symbols/Switch - Selector - SS12D00.wrl"
      (offset (xyz 0 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Connector_JST:JST_XH_S5B-XH-A_1x05_P2.50mm_Horizontal" (layer "F.Cu")
    (at 168.2 56.740876 180)
    (descr "JST XH series connector, S5B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH horizontal")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2_I2C1" (at -3.9 0.140876 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 5 10.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5 3.45) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 2 "VDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 3 "/SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 4 "/SCL") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 27 "/INT2") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S5B-XH-A_1x05_P2.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 122.6 65.6)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Build2Together:CONN_S2B-XH-A-1LFSN_JST" (layer "F.Cu")
    (at 147.907703 112.935676 180)
    (tags "S2B-XH-A-1LFSN ")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "JBAT1" (at -4.092297 -1.664324 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 1.275 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.275 0 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.499999 0 180) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(JBAT1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/Symbols/S2B-XH-A-1.STEP"
      (offset (xyz 1.2 -7.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 122.6 70.6)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 167.8 114.4)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Build2Together:SHIELD_NRF52840" (layer "F.Cu")
    (at 168.902703 75.045876 -90)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0 37.4 90) (layer "F.SilkS") hide)
    (fp_text value "~" (at 0 23.54 90) (layer "F.Fab"))
    (fp_text user "D8" (at 14.384 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "A1" (at 26.064 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "D6" (at 20.92175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "D2" (at 31.08175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at -0.856 3.195238 unlocked) (layer "F.SilkS"))
    (fp_text user "D1" (at 33.62175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "D10" (at 9.304 3.052381 unlocked) (layer "F.SilkS"))
    (fp_text user "D0" (at 36.16175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "5V" (at 10.824 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "AREF" (at -3.396 3.766667 unlocked) (layer "F.SilkS"))
    (fp_text user "D9" (at 11.844 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "RESET" (at 5.744 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at 13.364 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "N.C." (at 18.444 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "VDD" (at 3.204 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "VDD" (at 0.6 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "D11" (at 6.764 3.052381 unlocked) (layer "F.SilkS"))
    (fp_text user "D12" (at 4.224 3.052381 unlocked) (layer "F.SilkS"))
    (fp_text user "A3" (at 31.144 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "D4" (at 26.00175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "D13" (at 1.684 3.052381 unlocked) (layer "F.SilkS"))
    (fp_text user "A5" (at 36.224 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "D3" (at 28.54175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "A0" (at 23.524 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "SCL" (at -8.476 2.909524 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at 15.904 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "VDD" (at 8.284 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "D5" (at 23.46175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "SDA" (at -5.936 2.957143 unlocked) (layer "F.SilkS"))
    (fp_text user "A4" (at 33.684 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "D7" (at 18.38175 2.1 unlocked) (layer "F.SilkS"))
    (fp_text user "A2" (at 28.604 44.471428 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 26.08 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -13.97 46.4) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at -12.7 -1.86) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 38.1 41.32) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VDD") (pinfunction "VDD") (pintype "power_out"))
    (pad "2" thru_hole oval (at 2.54 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VDD") (pinfunction "VDD") (pintype "power_out"))
    (pad "3" thru_hole oval (at 5.08 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(U1-~{RESET}-Pad3)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "4" thru_hole oval (at 7.62 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VDD") (pinfunction "VDD") (pintype "power_out"))
    (pad "5" thru_hole oval (at 10.16 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "+5V") (pinfunction "+5V") (pintype "power_out"))
    (pad "6" thru_hole oval (at 12.7 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval (at 15.24 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 17.78 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(U1-NC-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" thru_hole oval (at 22.86 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/INT1") (pinfunction "A0") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 25.4 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/INT2") (pinfunction "A1") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 27.94 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(U1-A2-Pad11)") (pinfunction "A2") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 30.48 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(U1-A3-Pad12)") (pinfunction "A3") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 33.02 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U1-A4-Pad13)") (pinfunction "A4") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 35.56 46.4 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(U1-A5-Pad14)") (pinfunction "A5") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at 35.56 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/SV1") (pinfunction "D0") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 33.02 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/SV2") (pinfunction "D1") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 30.48 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(U1-D2-Pad17)") (pinfunction "D2") (pintype "bidirectional"))
    (pad "18" thru_hole oval (at 27.94 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(U1-D3-Pad18)") (pinfunction "D3") (pintype "bidirectional"))
    (pad "19" thru_hole oval (at 25.4 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(U1-D4-Pad19)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at 22.86 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(U1-D5-Pad20)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "21" thru_hole oval (at 20.32 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(U1-D6-Pad21)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 17.78 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(U1-D7-Pad22)") (pinfunction "D7") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 13.72 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(U1-D8-Pad23)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 11.18 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(U1-D9-Pad24)") (pinfunction "D9") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 8.64 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(U1-D10-Pad25)") (pinfunction "D10") (pintype "bidirectional"))
    (pad "26" thru_hole oval (at 6.1 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(U1-D11-Pad26)") (pinfunction "D11") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 3.56 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U1-D12-Pad27)") (pinfunction "D12") (pintype "bidirectional"))
    (pad "28" thru_hole oval (at 1.02 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U1-D13-Pad28)") (pinfunction "D13") (pintype "bidirectional"))
    (pad "29" thru_hole oval (at -1.52 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval (at -4.06 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U1-AREF-Pad30)") (pinfunction "AREF") (pintype "input"))
    (pad "31" thru_hole oval (at -6.6 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "32" thru_hole oval (at -9.14 -1.86 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/SCL") (pinfunction "SCL") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 35.6 1.9 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 17.8 -46.4 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 13.7 1.9 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 22.9 -46.4 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 -90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (at 160.417703 106.425 -90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Nordic_PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J_SERVO2" (at 1.675 -3.182297 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 4.385 7.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/SV2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 171.632703 117.115876) (end 121.632703 117.115876)
    (layer "Edge.Cuts"))
  (gr_line (start 173.632703 49.115876) (end 173.632703 115.115876)
    (layer "Edge.Cuts"))
  (gr_arc (start 119.632703 49.115876) (mid 120.218498 47.701679) (end 121.632703 47.115876)
    (layer "Edge.Cuts"))
  (gr_arc (start 173.632703 115.115876) (mid 173.046917 116.53009) (end 171.632703 117.115876)
    (layer "Edge.Cuts"))
  (gr_arc (start 121.632703 117.115876) (mid 120.218489 116.53009) (end 119.632703 115.115876)
    (layer "Edge.Cuts"))
  (gr_arc (start 171.632703 47.115876) (mid 173.046923 47.701662) (end 173.632703 49.115876)
    (layer "Edge.Cuts"))
  (gr_line (start 121.632703 47.115876) (end 171.632703 47.115876)
    (layer "Edge.Cuts"))
  (gr_line (start 119.632703 115.115876) (end 119.632703 49.115876)
    (layer "Edge.Cuts"))
  (gr_text "WayWayWay" (at 172.1 115) (layer "B.SilkS"))
  (gr_text "+" (at 146.9 114.4 180) (layer "F.SilkS"))
  (gr_text "VDD" (at 148.4 62.304762 90) (layer "F.SilkS"))
  (gr_text "VDD" (at 136.141703 104.7 90) (layer "F.SilkS"))
  (gr_text "GND" (at 156.001703 104.7 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 161.364 62.304762 90) (layer "F.SilkS"))
  (gr_text "JVic" (at 120.9 115.3) (layer "F.SilkS"))
  (gr_text "INT" (at 140.964 62.304762 90) (layer "F.SilkS"))
  (gr_text "ON" (at 130.9 61) (layer "F.SilkS"))
  (gr_text "SCL" (at 143.464 62.304762 90) (layer "F.SilkS"))
  (gr_text "SDA" (at 163.864 62.304762 90) (layer "F.SilkS"))
  (gr_text "GND" (at 133.601703 104.7 90) (layer "F.SilkS"))
  (gr_text "GND" (at 150.9 62.304762 90) (layer "F.SilkS"))
  (gr_text "BUILD2GETHER \n2.0" (at 148.175 91) (layer "F.SilkS"))
  (gr_text "PWM" (at 161.081703 104.7 90) (layer "F.SilkS"))
  (gr_text "nRF52840-DK \nSHIELD" (at 148.3 81.6) (layer "F.SilkS" knockout))
  (gr_text "PWM" (at 138.681703 104.7 90) (layer "F.SilkS"))
  (gr_text "INT" (at 158.864 62.304762 90) (layer "F.SilkS"))
  (gr_text "VDD" (at 158.541703 104.7 90) (layer "F.SilkS"))
  (gr_text "+" (at 125.2 56.2 180) (layer "F.SilkS"))
  (gr_text "GND" (at 168.8 62.304762 90) (layer "F.SilkS"))
  (gr_text "VDD" (at 166.3 62.304762 90) (layer "F.SilkS"))
  (gr_text "SDA" (at 145.964 62.304762 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "VDD") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 179.492703 39.115876)
        (xy 114.492703 39.115876)
        (xy 114.492703 129.115876)
        (xy 179.492703 129.115876)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 183.492703 35.115876)
        (xy 107.492703 35.115876)
        (xy 107.492703 137.115876)
        (xy 183.492703 137.115876)
      )
    )
  )
)
