(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "BUTTON_SMD_1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "B1" (at 0 -1.27 90))
      (property "Value" "BUTTON_SMD" (at -1.27 -1.27 90))
      (property "Footprint" "Build2Together:PTS 647 SN50 SMTR2 LFS" (at -5.08 50.8 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "Description" "6 x 6 mm, 9.5 mm Actuator Height, 100 gf, Black, Surface Mount, SPST, Tactile Switch" (at -1.27 34.29 0))
      (property "MF" "CUI Devices" (at 2.54 12.7 0))
      (property "Package" "None" (at 6.35 15.24 0))
      (property "Price" "None" (at 0 5.08 0))
      (property "Check_prices" "https://www.snapeda.com/parts/TS04-66-95-BK-100-SMT/CUI+Devices/view-part/?ref=eda" (at -1.27 24.13 0))
      (property "STANDARD" "Manufacturer Recommendations" (at 3.81 50.8 0))
      (property "PARTREV" "1.0" (at 5.08 13.97 0))
      (property "SnapEDA_Link" "" (at -1.27 50.8 0))
      (property "MP" "TS04-66-95-BK-100-SMT" (at -2.54 26.67 0))
      (property "CUI_purchase_URL" "https://www.cuidevices.com/product/switches/tactile-switches/ts04-66-95-bk-100-smt?utm_source=snapeda.com&utm_medium=referral&utm_campaign=snapedaBOM" (at 0 39.37 0))
      (property "Availability" "In Stock" (at 1.27 7.62 0))
      (property "MANUFACTURER" "CUI Devices" (at 6.35 10.16 0))
      (symbol "BUTTON_SMD_1_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "BUTTON_SMD_1_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "")
          (number "1")
        )
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "")
          (number "3")
        )
        (pin passive line (at 5.08 -2.54 180) (length 2.54)
          (name "")
          (number "4")
        )
      )
    )
    (symbol "Build2Together:MAX98357AETE_T" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -12.7 16.24 0))
      (property "Value" "MAX98357AETE_T" (at -12.7 26.67 0))
      (property "Footprint" "MAX98357AETE_T:QFN50P300X300X80-17N" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "MF" "Analog Devices" (at 0 0 0))
      (property "Description" "\nTiny, Low-Cost, PCM Class D Amplifier with Class AB Performance\n" (at 0 0 0))
      (property "Package" "TQFN-16 Maxim" (at 0 0 0))
      (property "Price" "None" (at 0 0 0))
      (property "SnapEDA_Link" "https://www.snapeda.com/parts/MAX98357AETE+T/Analog+Devices/view-part/?ref=snap" (at 0 0 0))
      (property "MP" "MAX98357AETE+T" (at 0 0 0))
      (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=48842&manufacturer=Analog Devices&part_name=MAX98357AETE+T&search_term=max9835" (at 0 0 0))
      (property "Availability" "In Stock" (at 0 0 0))
      (property "Check_prices" "https://www.snapeda.com/parts/MAX98357AETE+T/Analog+Devices/view-part/?ref=eda" (at 0 0 0))
      (symbol "MAX98357AETE_T_0_0"
        (rectangle (start -12.7 15.24) (end 12.7 -15.24)
          (fill (type background))
        )
        (pin input line (at -17.78 5.08 0) (length 5.08)
          (name "DIN")
          (number "1")
        )
        (pin output line (at 17.78 5.08 180) (length 5.08)
          (name "OUTN")
          (number "10")
        )
        (pin power_in line (at 6.35 -20.32 90) (length 5.08)
          (name "GND")
          (number "11")
        )
        (pin input clock (at -17.78 0 0) (length 5.08)
          (name "LRCLK")
          (number "14")
        )
        (pin power_in line (at 1.27 -20.32 90) (length 5.08)
          (name "GND")
          (number "15")
        )
        (pin input clock (at -17.78 7.62 0) (length 5.08)
          (name "BCLK")
          (number "16")
        )
        (pin power_in line (at 17.78 -10.16 180) (length 5.08)
          (name "EP")
          (number "17")
        )
        (pin input line (at -17.78 2.54 0) (length 5.08)
          (name "GAIN_SLOT")
          (number "2")
        )
        (pin power_in line (at -3.81 -20.32 90) (length 5.08)
          (name "GND")
          (number "3")
        )
        (pin input line (at -17.78 -2.54 0) (length 5.08)
          (name "SD_MODE")
          (number "4")
        )
        (pin power_in line (at 17.78 12.7 180) (length 5.08)
          (name "VDD")
          (number "7")
        )
        (pin power_in line (at 17.78 10.16 180) (length 5.08)
          (name "VDD")
          (number "8")
        )
        (pin output line (at 17.78 2.54 180) (length 5.08)
          (name "OUTP")
          (number "9")
        )
      )
    )
    (symbol "Build2Together:XIAO ESP32C3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -12.7 16.002 0))
      (property "Value" "XIAO ESP32C3" (at -10.16 16.51 0))
      (property "Footprint" "113991054:MODULE_113991054" (at 1.27 26.67 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "MF" "Seeed Technology Co., Ltd" (at 0 0 0))
      (property "MAXIMUM_PACKAGE_HEIGHT" "N/A" (at 0 0 0))
      (property "Package" "None" (at 0 0 0))
      (property "Price" "None" (at 0 0 0))
      (property "Check_prices" "https://www.snapeda.com/parts/113991054/Seeed+Technology+Co.%252C+Ltd/view-part/?ref=eda" (at 0 0 0))
      (property "STANDARD" "Manufacturer Recommendations" (at 0 39.37 0))
      (property "PARTREV" "23/05/2022" (at 2.54 17.78 0))
      (property "SnapEDA_Link" "https://www.snapeda.com/parts/113991054/Seeed+Technology+Co.%252C+Ltd/view-part/?ref=snap" (at 0 0 0))
      (property "MP" "113991054" (at 0 22.86 0))
      (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=12200757&manufacturer=Seeed Technology Co., Ltd&part_name=113991054&search_term=None" (at -2.54 39.37 0))
      (property "Description" "\n- ESP32-C3 Transceiver; 802.11 a/b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® Smart 4.x Low Energy (BLE) 2.4GHz Evaluation Board\n" (at 2.54 34.29 0))
      (property "SNAPEDA_PN" "113991054" (at 0 0 0))
      (property "Availability" "In Stock" (at 0 0 0))
      (property "MANUFACTURER" "Seeed Technology" (at 0 0 0))
      (symbol "XIAO ESP32C3_0_0"
        (rectangle (start -12.7 15.24) (end 12.7 -15.24)
          (fill (type background))
        )
        (text "" (at 3.81 -16.51 0))
        (pin bidirectional line (at -17.78 5.08 0) (length 5.08)
          (name "D0")
          (number "1")
        )
        (pin bidirectional line (at 17.78 -2.54 180) (length 5.08)
          (name "D9")
          (number "10")
        )
        (pin bidirectional line (at 17.78 -5.08 180) (length 5.08)
          (name "D10")
          (number "11")
        )
        (pin power_in line (at 17.78 12.7 180) (length 5.08)
          (name "VCC_3V3")
          (number "12")
        )
        (pin power_in line (at 17.78 -12.7 180) (length 5.08)
          (name "GND")
          (number "13")
        )
        (pin power_in line (at 17.78 10.16 180) (length 5.08)
          (name "VUSB")
          (number "14")
        )
        (pin bidirectional line (at -17.78 2.54 0) (length 5.08)
          (name "D1")
          (number "2")
        )
        (pin bidirectional line (at -17.78 0 0) (length 5.08)
          (name "D2")
          (number "3")
        )
        (pin bidirectional line (at -17.78 -2.54 0) (length 5.08)
          (name "D3")
          (number "4")
        )
        (pin bidirectional line (at -17.78 -5.08 0) (length 5.08)
          (name "D4")
          (number "5")
        )
        (pin bidirectional line (at -17.78 -7.62 0) (length 5.08)
          (name "D5")
          (number "6")
        )
        (pin bidirectional line (at 17.78 5.08 180) (length 5.08)
          (name "TX_D6")
          (number "7")
        )
        (pin bidirectional line (at 17.78 2.54 180) (length 5.08)
          (name "RX_D7")
          (number "8")
        )
        (pin bidirectional line (at 17.78 0 180) (length 5.08)
          (name "D8")
          (number "9")
        )
      )
      (symbol "XIAO ESP32C3_1_1"
        (pin input line (at 2.54 -17.78 90) (length 2.54)
          (name "BAT-")
          (number "21")
        )
        (pin input line (at 6.35 -17.78 90) (length 2.54)
          (name "BAT+")
          (number "22")
        )
        (pin input line (at -6.35 -17.78 90) (length 2.54)
          (name "TPAD")
          (number "23")
        )
      )
    )
    (symbol "Connector:Conn_01x02_Pin" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 2.54 0))
      (property "Value" "Conn_01x02_Pin" (at 0 -5.08 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x02_Pin_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Connector:TestPoint_2Pole" (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP1" (at 0 5.08 0))
      (property "Value" "TestPoint_2Pole" (at 0 2.54 0))
      (property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "point tp" (at 0 0 0))
      (property "ki_description" "2-polar test point" (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (at 0 0 0))
      (symbol "TestPoint_2Pole_0_1"
        (circle (center -1.778 0) (radius 0.762)
          (fill (type none))
        )
        (circle (center 1.778 0) (radius 0.762)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
      )
      (symbol "TestPoint_2Pole_1_1"
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "3")
          (number "3")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:FerriteBead_Small" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "FB" (at 1.905 1.27 0))
      (property "Value" "FerriteBead_Small" (at 1.905 -1.27 0))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "L ferrite bead inductor filter" (at 0 0 0))
      (property "ki_description" "Ferrite bead, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "Inductor_* L_* *Ferrite*" (at 0 0 0))
      (symbol "FerriteBead_Small_0_1"
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -0.7874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.889)
            (xy 0 1.2954)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.8288 0.2794)
            (xy -1.1176 1.4986)
            (xy 1.8288 -0.2032)
            (xy 1.1176 -1.4224)
            (xy -1.8288 0.2794)
          )
          (fill (type none))
        )
      )
      (symbol "FerriteBead_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Speaker" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "LS" (at 1.27 5.715 0))
      (property "Value" "Speaker" (at 1.27 3.81 0))
      (property "Footprint" "" (at 0 -5.08 0))
      (property "Datasheet" "~" (at -0.254 -1.27 0))
      (property "ki_keywords" "speaker sound" (at 0 0 0))
      (property "ki_description" "Speaker" (at 0 0 0))
      (symbol "Speaker_0_0"
        (rectangle (start -2.54 1.27) (end 1.016 -3.81)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 3.556 3.81)
            (xy 3.556 -6.35)
            (xy 1.016 -3.81)
          )
          (fill (type none))
        )
      )
      (symbol "Speaker_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin input line (at -5.08 -2.54 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Jumper:SolderJumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (at 0 2.032 0))
      (property "Value" "SolderJumper_2_Open" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "solder jumper SPST" (at 0 0 0))
      (property "ki_description" "Solder Jumper, 2-pole, open" (at 0 0 0))
      (property "ki_fp_filters" "SolderJumper*Open*" (at 0 0 0))
      (symbol "SolderJumper_2_Open_0_1"
        (arc (start -0.254 1.016) (mid -1.2656 0) (end -0.254 -1.016)
          (fill (type none))
        )
        (arc (start -0.254 1.016) (mid -1.2656 0) (end -0.254 -1.016)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -0.254 1.016)
            (xy -0.254 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.016)
            (xy 0.254 -1.016)
          )
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.2656 0) (end 0.254 1.016)
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.2656 0) (end 0.254 1.016)
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_2_Open_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "Jumper:SolderJumper_3_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (at -2.54 -2.54 0))
      (property "Value" "SolderJumper_3_Open" (at 0 2.794 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "Solder Jumper SPDT" (at 0 0 0))
      (property "ki_description" "Solder Jumper, 3-pole, open" (at 0 0 0))
      (property "ki_fp_filters" "SolderJumper*Open*" (at 0 0 0))
      (symbol "SolderJumper_3_Open_0_1"
        (arc (start -1.016 1.016) (mid -2.0276 0) (end -1.016 -1.016)
          (fill (type none))
        )
        (arc (start -1.016 1.016) (mid -2.0276 0) (end -1.016 -1.016)
          (fill (type outline))
        )
        (rectangle (start -0.508 1.016) (end 0.508 -1.016)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -2.032 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.016)
            (xy -1.016 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.016)
            (xy 1.016 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 2.032 0)
          )
          (fill (type none))
        )
        (arc (start 1.016 -1.016) (mid 2.0276 0) (end 1.016 1.016)
          (fill (type none))
        )
        (arc (start 1.016 -1.016) (mid 2.0276 0) (end 1.016 1.016)
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_3_Open_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.54)
          (name "C")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "3")
        )
      )
    )
    (symbol "Switch:SW_SPDT" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 0 4.318 0))
      (property "Value" "SW_SPDT" (at 0 -5.08 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "switch single-pole double-throw spdt ON-ON" (at 0 0 0))
      (property "ki_description" "Switch, single pole double throw" (at 0 0 0))
      (symbol "SW_SPDT_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 2.032 -2.54) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_SPDT_0_1"
        (polyline
          (pts
            (xy -1.524 0.254)
            (xy 1.651 2.286)
          )
          (fill (type none))
        )
        (circle (center 2.032 2.54) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_SPDT_1_1"
        (pin passive line (at 5.08 2.54 180) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "B")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+3V3" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 40.64 95.25) (diameter 0) (color 0 0 0 0))
  (junction (at 29.21 160.02) (diameter 0) (color 0 0 0 0))
  (junction (at 29.21 176.53) (diameter 0) (color 0 0 0 0))
  (junction (at 40.64 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 129.54 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 29.21 163.83) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 158.75) (diameter 0) (color 0 0 0 0))
  (junction (at 124.46 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 162.56) (diameter 0) (color 0 0 0 0))
  (junction (at 82.55 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 66.04) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 172.72) (diameter 0) (color 0 0 0 0))
  (junction (at 99.06 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 87.63 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 29.21 173.99) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 175.26) (diameter 0) (color 0 0 0 0))
  (no_connect (at 125.73 147.32))
  (no_connect (at 208.28 64.77))
  (wire (pts (xy 54.61 104.14) (xy 49.53 104.14)))
  (wire (pts (xy 118.11 85.09) (xy 124.46 85.09)))
  (wire (pts (xy 29.21 160.02) (xy 29.21 163.83)))
  (wire (pts (xy 35.56 50.8) (xy 35.56 60.96)))
  (wire (pts (xy 33.02 100.33) (xy 33.02 105.41)))
  (wire (pts (xy 63.5 172.72) (xy 63.5 175.26)))
  (wire (pts (xy 123.19 66.04) (xy 132.08 66.04)))
  (wire (pts (xy 107.95 147.32) (xy 107.95 154.94)))
  (wire (pts (xy 114.3 55.88) (xy 114.3 58.42)))
  (wire (pts (xy 38.1 176.53) (xy 29.21 176.53)))
  (wire (pts (xy 72.39 171.45) (xy 72.39 175.26)))
  (wire (pts (xy 38.1 172.72) (xy 38.1 176.53)))
  (wire (pts (xy 105.41 144.78) (xy 115.57 144.78)))
  (wire (pts (xy 105.41 147.32) (xy 107.95 147.32)))
  (wire (pts (xy 63.5 156.21) (xy 63.5 158.75)))
  (wire (pts (xy 114.3 55.88) (xy 132.08 55.88)))
  (wire (pts (xy 54.61 68.58) (xy 63.5 68.58)))
  (wire (pts (xy 114.3 66.04) (xy 123.19 66.04)))
  (wire (pts (xy 54.61 63.5) (xy 63.5 63.5)))
  (wire (pts (xy 99.06 66.04) (xy 105.41 66.04)))
  (wire (pts (xy 54.61 66.04) (xy 63.5 66.04)))
  (wire (pts (xy 29.21 173.99) (xy 31.75 173.99)))
  (wire (pts (xy 35.56 100.33) (xy 33.02 100.33)))
  (wire (pts (xy 35.56 71.12) (xy 63.5 71.12)))
  (wire (pts (xy 29.21 163.83) (xy 31.75 163.83)))
  (wire (pts (xy 40.64 95.25) (xy 40.64 96.52)))
  (wire (pts (xy 105.41 85.09) (xy 113.03 85.09)))
  (wire (pts (xy 63.5 175.26) (xy 63.5 176.53)))
  (wire (pts (xy 29.21 139.7) (xy 29.21 149.86)))
  (wire (pts (xy 124.46 85.09) (xy 133.35 85.09)))
  (wire (pts (xy 77.47 88.9) (xy 82.55 88.9)))
  (wire (pts (xy 72.39 175.26) (xy 63.5 175.26)))
  (wire (pts (xy 54.61 60.96) (xy 63.5 60.96)))
  (wire (pts (xy 78.74 106.68) (xy 81.28 106.68)))
  (wire (pts (xy 166.37 74.93) (xy 172.72 74.93)))
  (wire (pts (xy 45.72 100.33) (xy 49.53 100.33)))
  (wire (pts (xy 99.06 63.5) (xy 105.41 63.5)))
  (wire (pts (xy 193.04 92.71) (xy 193.04 99.06)))
  (wire (pts (xy 123.19 66.04) (xy 123.19 69.85)))
  (wire (pts (xy 105.41 80.01) (xy 114.3 80.01)))
  (wire (pts (xy 166.37 72.39) (xy 172.72 72.39)))
  (wire (pts (xy 35.56 68.58) (xy 35.56 71.12)))
  (wire (pts (xy 124.46 85.09) (xy 124.46 93.98)))
  (wire (pts (xy 99.06 55.88) (xy 114.3 55.88)))
  (wire (pts (xy 72.39 163.83) (xy 72.39 158.75)))
  (wire (pts (xy 166.37 77.47) (xy 172.72 77.47)))
  (wire (pts (xy 125.73 142.24) (xy 137.16 142.24)))
  (wire (pts (xy 132.08 55.88) (xy 132.08 58.42)))
  (wire (pts (xy 53.34 93.98) (xy 53.34 95.25)))
  (wire (pts (xy 29.21 173.99) (xy 29.21 176.53)))
  (wire (pts (xy 214.63 54.61) (xy 214.63 62.23)))
  (wire (pts (xy 63.5 158.75) (xy 63.5 162.56)))
  (wire (pts (xy 40.64 95.25) (xy 53.34 95.25)))
  (wire (pts (xy 133.35 83.82) (xy 133.35 85.09)))
  (wire (pts (xy 133.35 80.01) (xy 133.35 81.28)))
  (wire (pts (xy 63.5 162.56) (xy 66.04 162.56)))
  (wire (pts (xy 208.28 77.47) (xy 214.63 77.47)))
  (wire (pts (xy 129.54 80.01) (xy 133.35 80.01)))
  (wire (pts (xy 129.54 95.25) (xy 129.54 106.68)))
  (wire (pts (xy 72.39 158.75) (xy 63.5 158.75)))
  (wire (pts (xy 82.55 88.9) (xy 87.63 88.9)))
  (wire (pts (xy 208.28 74.93) (xy 214.63 74.93)))
  (wire (pts (xy 99.06 88.9) (xy 87.63 88.9)))
  (wire (pts (xy 208.28 87.63) (xy 208.28 91.44)))
  (wire (pts (xy 40.64 81.28) (xy 40.64 83.82)))
  (wire (pts (xy 82.55 88.9) (xy 82.55 93.98)))
  (wire (pts (xy 99.06 55.88) (xy 99.06 58.42)))
  (wire (pts (xy 40.64 83.82) (xy 40.64 86.36)))
  (wire (pts (xy 66.04 106.68) (xy 68.58 106.68)))
  (wire (pts (xy 63.5 172.72) (xy 66.04 172.72)))
  (wire (pts (xy 53.34 86.36) (xy 53.34 83.82)))
  (wire (pts (xy 208.28 62.23) (xy 214.63 62.23)))
  (wire (pts (xy 129.54 80.01) (xy 129.54 87.63)))
  (wire (pts (xy 63.5 140.97) (xy 63.5 148.59)))
  (wire (pts (xy 99.06 78.74) (xy 99.06 88.9)))
  (wire (pts (xy 40.64 93.98) (xy 40.64 95.25)))
  (wire (pts (xy 124.46 101.6) (xy 124.46 106.68)))
  (wire (pts (xy 29.21 176.53) (xy 29.21 177.8)))
  (wire (pts (xy 119.38 80.01) (xy 129.54 80.01)))
  (wire (pts (xy 49.53 100.33) (xy 49.53 104.14)))
  (wire (pts (xy 40.64 83.82) (xy 53.34 83.82)))
  (wire (pts (xy 38.1 160.02) (xy 29.21 160.02)))
  (wire (pts (xy 29.21 157.48) (xy 29.21 160.02)))
  (wire (pts (xy 196.85 99.06) (xy 196.85 92.71)))
  (wire (pts (xy 38.1 165.1) (xy 38.1 160.02)))
  (wire (pts (xy 99.06 48.26) (xy 99.06 55.88)))
  (rectangle (start 22.86 33.02) (end 153.67 116.84)
    (fill (type none))
  )
  (rectangle (start 21.59 130.81) (end 82.55 189.23)
    (fill (type none))
  )
  (text "BUTTONS\n" (at 22.86 128.27 0))
  (text "MAX98357" (at 22.86 31.75 0))
  (label "DIN" (at 54.61 63.5 0) (fields_autoplaced))
  (label "SPK_P" (at 81.28 106.68 0) (fields_autoplaced))
  (label "OUTP" (at 105.41 66.04 180) (fields_autoplaced))
  (label "OUTN" (at 105.41 63.5 180) (fields_autoplaced))
  (label "OUTP" (at 105.41 85.09 0) (fields_autoplaced))
  (label "DIN" (at 166.37 72.39 0) (fields_autoplaced))
  (label "BUTTON1" (at 214.63 74.93 0) (fields_autoplaced))
  (label "LRC" (at 166.37 77.47 0) (fields_autoplaced))
  (label "BUTTON2" (at 214.63 77.47 0) (fields_autoplaced))
  (label "SPK_N" (at 124.46 80.01 0) (fields_autoplaced))
  (label "LRC" (at 54.61 68.58 0) (fields_autoplaced))
  (label "BAT+" (at 137.16 142.24 180) (fields_autoplaced))
  (label "GAIN" (at 40.64 81.28 0) (fields_autoplaced))
  (label "OUTN" (at 105.41 80.01 0) (fields_autoplaced))
  (label "SPK_N" (at 88.9 113.03 90) (fields_autoplaced))
  (label "BCLK" (at 54.61 60.96 0) (fields_autoplaced))
  (label "GAIN" (at 54.61 66.04 0) (fields_autoplaced))
  (label "BUTTON2" (at 72.39 158.75 0) (fields_autoplaced))
  (label "BAT+" (at 196.85 99.06 90) (fields_autoplaced))
  (label "SPK_P" (at 124.46 85.09 0) (fields_autoplaced))
  (label "BCLK" (at 166.37 74.93 0) (fields_autoplaced))
  (label "SPK_N" (at 66.04 106.68 180) (fields_autoplaced))
  (label "BUTTON1" (at 38.1 160.02 0) (fields_autoplaced))
  (symbol (lib_id "power:+3V3") (at 29.21 139.7 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR09" (at 29.21 143.51 0))
    (property "Value" "+3V3" (at 29.21 134.62 0))
    (property "Footprint" "" (at 29.21 139.7 0))
    (property "Datasheet" "" (at 29.21 139.7 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 124.46 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR013" (at 124.46 113.03 0))
    (property "Value" "GND" (at 124.46 111.76 0))
    (property "Footprint" "" (at 124.46 106.68 0))
    (property "Datasheet" "" (at 124.46 106.68 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR013") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 54.61 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR06" (at 54.61 107.95 0))
    (property "Value" "+3V3" (at 54.61 99.06 0))
    (property "Footprint" "" (at 54.61 104.14 0))
    (property "Datasheet" "" (at 54.61 104.14 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 63.5 152.4 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "RB2" (at 66.04 151.13 0))
    (property "Value" "10k" (at 66.04 153.67 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (at 65.278 152.4 90))
    (property "Datasheet" "~" (at 63.5 152.4 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "RB2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "BUTTON_SMD_1") (lib_id "Build2Together:BUTTON_SMD") (at 63.5 167.64 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "B2" (at 64.77 167.64 90))
    (property "Value" "BUTTON_SMD" (at 64.77 168.91 90))
    (property "Footprint" "Build2Together:BUTTON SMD ALIEXPRESS" (at 12.7 172.72 0))
    (property "Datasheet" "" (at 63.5 167.64 0))
    (property "MF" "CUI Devices" (at 50.8 165.1 0))
    (property "Description" "6 x 6 mm, 9.5 mm Actuator Height, 100 gf, Black, Surface Mount, SPST, Tactile Switch" (at 29.21 168.91 0))
    (property "Package" "None" (at 48.26 161.29 0))
    (property "Price" "None" (at 58.42 167.64 0))
    (property "Check_prices" "https://www.snapeda.com/parts/TS04-66-95-BK-100-SMT/CUI+Devices/view-part/?ref=eda" (at 39.37 168.91 0))
    (property "STANDARD" "Manufacturer Recommendations" (at 12.7 163.83 0))
    (property "PARTREV" "1.0" (at 49.53 162.56 0))
    (property "SnapEDA_Link" "" (at 12.7 168.91 0))
    (property "MP" "TS04-66-95-BK-100-SMT" (at 36.83 170.18 0))
    (property "CUI_purchase_URL" "https://www.cuidevices.com/product/switches/tactile-switches/ts04-66-95-bk-100-smt?utm_source=snapeda.com&utm_medium=referral&utm_campaign=snapedaBOM" (at 24.13 167.64 0))
    (property "Availability" "In Stock" (at 55.88 166.37 0))
    (property "MANUFACTURER" "CUI Devices" (at 53.34 161.29 0))
    (pin "3")
    (pin "4")
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "B2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 114.3 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "CVDD1" (at 115.57 59.69 0))
    (property "Value" "0.1uF" (at 118.11 63.5 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 115.2652 66.04 0))
    (property "Datasheet" "~" (at 114.3 62.23 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "CVDD1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 129.54 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR017" (at 129.54 113.03 0))
    (property "Value" "GND" (at 129.54 111.76 0))
    (property "Footprint" "" (at 129.54 106.68 0))
    (property "Datasheet" "" (at 129.54 106.68 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR017") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 38.1 168.91 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "CB1" (at 39.37 166.37 0))
    (property "Value" "0.1uF" (at 41.91 170.18 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 39.0652 172.72 0))
    (property "Datasheet" "~" (at 38.1 168.91 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "CB1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 33.02 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 33.02 111.76 0))
    (property "Value" "GND" (at 33.02 110.49 0))
    (property "Footprint" "" (at 33.02 105.41 0))
    (property "Datasheet" "" (at 33.02 105.41 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:Speaker") (at 138.43 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "LS1" (at 143.51 81.28 0))
    (property "Value" "Speaker" (at 143.51 83.82 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical" (at 138.43 86.36 0))
    (property "Datasheet" "~" (at 138.176 82.55 0))
    (pin "1")
    (pin "2")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "LS1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 123.19 69.85 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 123.19 76.2 0))
    (property "Value" "GND" (at 123.19 74.93 0))
    (property "Footprint" "" (at 123.19 69.85 0))
    (property "Datasheet" "" (at 123.19 69.85 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 193.04 99.06 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR016" (at 193.04 105.41 0))
    (property "Value" "GND" (at 193.04 104.14 0))
    (property "Footprint" "" (at 193.04 99.06 0))
    (property "Datasheet" "" (at 193.04 99.06 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR016") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 184.15 92.71 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR015" (at 184.15 99.06 0))
    (property "Value" "GND" (at 184.15 97.79 0))
    (property "Footprint" "" (at 184.15 92.71 0))
    (property "Datasheet" "" (at 184.15 92.71 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR015") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 124.46 97.79 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "CN1" (at 119.38 95.25 0))
    (property "Value" "220 pF" (at 114.3 97.79 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 125.4252 101.6 0))
    (property "Datasheet" "~" (at 124.46 97.79 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "CN1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:FerriteBead_Small") (at 115.57 85.09 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "FBP1" (at 115.57 88.9 90))
    (property "Value" "FerriteBead_Small" (at 115.5319 81.28 90))
    (property "Footprint" "Build2Together:SMD_FERRITE" (at 115.57 86.868 90))
    (property "Datasheet" "587-1876-2-ND" (at 115.57 85.09 0))
    (property "BOM" "BLM21AG121SN1D" (at 115.57 85.09 90))
    (pin "1")
    (pin "2")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "FBP1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 132.08 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "CVDD2" (at 135.89 60.96 0))
    (property "Value" "10uF" (at 135.89 63.5 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 133.0452 66.04 0))
    (property "Datasheet" "~" (at 132.08 62.23 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "CVDD2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 63.5 176.53 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR012" (at 63.5 182.88 0))
    (property "Value" "GND" (at 63.5 181.61 0))
    (property "Footprint" "" (at 63.5 176.53 0))
    (property "Datasheet" "" (at 63.5 176.53 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR012") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 72.39 167.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "CB2" (at 73.66 165.1 0))
    (property "Value" "0.1uF" (at 76.2 168.91 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 73.3552 171.45 0))
    (property "Datasheet" "~" (at 72.39 167.64 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "CB2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 35.56 64.77 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R_SD1" (at 38.1 63.5 0))
    (property "Value" "634k" (at 38.1 66.04 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 37.338 64.77 90))
    (property "Datasheet" "~" (at 35.56 64.77 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "R_SD1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 82.55 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 82.55 100.33 0))
    (property "Value" "GND" (at 82.55 99.06 0))
    (property "Footprint" "" (at 82.55 93.98 0))
    (property "Datasheet" "" (at 82.55 93.98 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_SPDT") (at 120.65 144.78 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "SW1" (at 120.65 137.16 0))
    (property "Value" "SW_SPDT" (at 120.65 139.7 0))
    (property "Footprint" "Build2Together:SW ALIEXPRESS" (at 120.65 144.78 0))
    (property "Datasheet" "~" (at 120.65 144.78 0))
    (pin "2")
    (pin "1")
    (pin "3")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "SW1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Build2Together:MAX98357AETE_T") (at 81.28 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 81.28 48.26 0))
    (property "Value" "MAX98357AETE_T" (at 81.28 50.8 0))
    (property "Footprint" "Build2Together:MAX98357_VAR1" (at 81.28 68.58 0))
    (property "Datasheet" "" (at 81.28 68.58 0))
    (property "MF" "Analog Devices" (at 81.28 68.58 0))
    (property "Description" "\nTiny, Low-Cost, PCM Class D Amplifier with Class AB Performance\n" (at 81.28 68.58 0))
    (property "Package" "TQFN-16 Maxim" (at 81.28 68.58 0))
    (property "Price" "None" (at 81.28 68.58 0))
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/MAX98357AETE+T/Analog+Devices/view-part/?ref=snap" (at 81.28 68.58 0))
    (property "MP" "MAX98357AETE+T" (at 81.28 68.58 0))
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=48842&manufacturer=Analog Devices&part_name=MAX98357AETE+T&search_term=max9835" (at 81.28 68.58 0))
    (property "Availability" "In Stock" (at 81.28 68.58 0))
    (property "Check_prices" "https://www.snapeda.com/parts/MAX98357AETE+T/Analog+Devices/view-part/?ref=eda" (at 81.28 68.58 0))
    (pin "11")
    (pin "1")
    (pin "14")
    (pin "2")
    (pin "17")
    (pin "4")
    (pin "3")
    (pin "16")
    (pin "10")
    (pin "9")
    (pin "8")
    (pin "7")
    (pin "15")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 35.56 50.8 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 35.56 54.61 0))
    (property "Value" "+3V3" (at 35.56 45.72 0))
    (property "Footprint" "" (at 35.56 50.8 0))
    (property "Datasheet" "" (at 35.56 50.8 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Build2Together:XIAO ESP32C3") (at 190.5 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U2" (at 190.5 54.61 0))
    (property "Value" "XIAO ESP32C3" (at 190.5 57.15 0))
    (property "Footprint" "Build2Together:XIAO_ESP32_HYBRID" (at 191.77 48.26 0))
    (property "Datasheet" "" (at 190.5 74.93 0))
    (property "MF" "Seeed Technology Co., Ltd" (at 190.5 74.93 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "N/A" (at 190.5 74.93 0))
    (property "Package" "None" (at 190.5 74.93 0))
    (property "Price" "None" (at 190.5 74.93 0))
    (property "Check_prices" "https://www.snapeda.com/parts/113991054/Seeed+Technology+Co.%252C+Ltd/view-part/?ref=eda" (at 190.5 74.93 0))
    (property "STANDARD" "Manufacturer Recommendations" (at 190.5 74.93 0))
    (property "PARTREV" "23/05/2022" (at 190.5 74.93 0))
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/113991054/Seeed+Technology+Co.%252C+Ltd/view-part/?ref=snap" (at 190.5 74.93 0))
    (property "MP" "113991054" (at 190.5 52.07 0))
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=12200757&manufacturer=Seeed Technology Co., Ltd&part_name=113991054&search_term=None" (at 190.5 74.93 0))
    (property "Description" "\n- ESP32-C3 Transceiver; 802.11 a/b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® Smart 4.x Low Energy (BLE) 2.4GHz Evaluation Board\n" (at 193.04 40.64 0))
    (property "SNAPEDA_PN" "113991054" (at 190.5 74.93 0))
    (property "Availability" "In Stock" (at 190.5 74.93 0))
    (property "MANUFACTURER" "Seeed Technology" (at 190.5 74.93 0))
    (pin "6")
    (pin "8")
    (pin "2")
    (pin "4")
    (pin "7")
    (pin "1")
    (pin "5")
    (pin "9")
    (pin "14")
    (pin "13")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "3")
    (pin "23")
    (pin "21")
    (pin "22")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 29.21 153.67 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "RB1" (at 31.75 152.4 0))
    (property "Value" "10k" (at 31.75 154.94 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (at 30.988 153.67 90))
    (property "Datasheet" "~" (at 29.21 153.67 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "RB1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 107.95 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR014" (at 107.95 161.29 0))
    (property "Value" "GND" (at 107.95 160.02 0))
    (property "Footprint" "" (at 107.95 154.94 0))
    (property "Datasheet" "" (at 107.95 154.94 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR014") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 29.21 177.8 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR011" (at 29.21 184.15 0))
    (property "Value" "GND" (at 29.21 182.88 0))
    (property "Footprint" "" (at 29.21 177.8 0))
    (property "Datasheet" "" (at 29.21 177.8 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR011") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 208.28 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR08" (at 208.28 97.79 0))
    (property "Value" "GND" (at 208.28 96.52 0))
    (property "Footprint" "" (at 208.28 91.44 0))
    (property "Datasheet" "" (at 208.28 91.44 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 40.64 90.17 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R_GAIN1" (at 43.18 88.9 0))
    (property "Value" "100k" (at 43.18 91.44 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 42.418 90.17 90))
    (property "Datasheet" "~" (at 40.64 90.17 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "R_GAIN1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Jumper:SolderJumper_2_Open") (at 53.34 90.17 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "JP2" (at 55.88 88.9 90))
    (property "Value" "SolderJumper_2_Open" (at 55.88 91.44 90))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (at 53.34 90.17 0))
    (property "Datasheet" "~" (at 53.34 90.17 0))
    (pin "1")
    (pin "2")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "JP2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 129.54 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "CP1" (at 133.35 90.17 0))
    (property "Value" "220 pF" (at 133.35 92.71 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 130.5052 95.25 0))
    (property "Datasheet" "~" (at 129.54 91.44 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "CP1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x02_Pin") (at 100.33 144.78 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "JBAT1" (at 100.33 142.24 0))
    (property "Value" "Conn_01x02_Pin" (at 100.965 142.24 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Horizontal" (at 100.33 144.78 0))
    (property "Datasheet" "~" (at 100.33 144.78 0))
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "JBAT1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 63.5 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR010" (at 63.5 144.78 0))
    (property "Value" "+3V3" (at 63.5 135.89 0))
    (property "Footprint" "" (at 63.5 140.97 0))
    (property "Datasheet" "" (at 63.5 140.97 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Jumper:SolderJumper_3_Open") (at 40.64 100.33 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "JP1" (at 38.1 97.79 0))
    (property "Value" "SolderJumper_3_Open" (at 40.64 106.68 0))
    (property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels" (at 40.64 100.33 0))
    (property "Datasheet" "~" (at 40.64 100.33 0))
    (pin "3")
    (pin "1")
    (pin "2")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "JP1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 214.63 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 214.63 58.42 0))
    (property "Value" "+3V3" (at 214.63 49.53 0))
    (property "Footprint" "" (at 214.63 54.61 0))
    (property "Datasheet" "" (at 214.63 54.61 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:FerriteBead_Small") (at 116.84 80.01 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "FBN1" (at 116.84 76.2 90))
    (property "Value" "FerriteBead_Small" (at 116.8019 76.2 90))
    (property "Footprint" "Build2Together:SMD_FERRITE" (at 116.84 81.788 90))
    (property "Datasheet" "BLM21AG121SN1D" (at 116.84 80.01 0))
    (pin "1")
    (pin "2")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "FBN1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 99.06 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 99.06 52.07 0))
    (property "Value" "+3V3" (at 99.06 43.18 0))
    (property "Footprint" "" (at 99.06 48.26 0))
    (property "Datasheet" "" (at 99.06 48.26 0))
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "BUTTON_SMD_1") (lib_id "Build2Together:BUTTON_SMD") (at 29.21 168.91 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "B1" (at 33.02 168.91 90))
    (property "Value" "BUTTON_SMD" (at 30.48 170.18 90))
    (property "Footprint" "Build2Together:BUTTON SMD ALIEXPRESS" (at -21.59 173.99 0))
    (property "Datasheet" "" (at 29.21 168.91 0))
    (property "MF" "CUI Devices" (at 16.51 166.37 0))
    (property "Description" "6 x 6 mm, 9.5 mm Actuator Height, 100 gf, Black, Surface Mount, SPST, Tactile Switch" (at -5.08 170.18 0))
    (property "Package" "None" (at 13.97 162.56 0))
    (property "Price" "None" (at 24.13 168.91 0))
    (property "Check_prices" "https://www.snapeda.com/parts/TS04-66-95-BK-100-SMT/CUI+Devices/view-part/?ref=eda" (at 5.08 170.18 0))
    (property "STANDARD" "Manufacturer Recommendations" (at -21.59 165.1 0))
    (property "PARTREV" "1.0" (at 15.24 163.83 0))
    (property "SnapEDA_Link" "" (at -21.59 170.18 0))
    (property "MP" "TS04-66-95-BK-100-SMT" (at 2.54 171.45 0))
    (property "CUI_purchase_URL" "https://www.cuidevices.com/product/switches/tactile-switches/ts04-66-95-bk-100-smt?utm_source=snapeda.com&utm_medium=referral&utm_campaign=snapedaBOM" (at -10.16 168.91 0))
    (property "Availability" "In Stock" (at 21.59 167.64 0))
    (property "MANUFACTURER" "CUI Devices" (at 19.05 162.56 0))
    (pin "3")
    (pin "4")
    (pin "2")
    (pin "1")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "B1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:TestPoint_2Pole") (at 73.66 106.68 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "TP1" (at 73.66 101.6 0))
    (property "Value" "TestPoint_2Pole" (at 73.66 104.14 0))
    (property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm" (at 73.66 106.68 0))
    (property "Datasheet" "~" (at 73.66 106.68 0))
    (pin "1")
    (pin "3")
    (instances
      (project "ESP32_PCB"
        (path
          (reference "TP1") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
