(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "Capactive Touch (AC-ON/OFF)")
		(date "2024-04-18")
		(rev "V0.1")
	)
	(lib_symbols
		(symbol "Connector:Conn_ARM_SWD_TagConnect_TC2030-NL"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(property "Reference" "J"
				(at 2.54 11.43 0)
			)
			(property "Value" "Conn_ARM_SWD_TagConnect_TC2030-NL"
				(at 2.54 8.89 0)
			)
			(property "Footprint" "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
				(at 0 -17.78 0)
			)
			(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2030-CTX_1.pdf"
				(at 0 -15.24 0)
			)
			(property "Description" "Tag-Connect ARM Cortex SWD JTAG connector, 6 pin, no legs"
				(at 0 0 0)
			)
			(property "ki_keywords" "Cortex Debug Connector ARM SWD JTAG"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*TC2030*"
				(at 0 0 0)
			)
			(symbol "Conn_ARM_SWD_TagConnect_TC2030-NL_0_0"
				(pin power_in line
					(at -2.54 10.16 270)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin bidirectional line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "SWDIO")
					(number "2")
					(alternate "TMS" bidirectional line)
				)
				(pin open_collector line
					(at 7.62 5.08 180)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "SWCLK")
					(number "4")
					(alternate "TCK" output line)
				)
				(pin power_in line
					(at -2.54 -10.16 90)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin input line
					(at 7.62 -5.08 180)
					(length 2.54)
					(name "SWO")
					(number "6")
					(alternate "TDO" input line)
				)
			)
			(symbol "Conn_ARM_SWD_TagConnect_TC2030-NL_0_1"
				(rectangle
					(start -5.08 7.62)
					(end 5.08 -7.62)
					(fill
						(type background)
					)
				)
			)
		)
		(symbol "Device:C"
			(pin_numbers hide)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:LED"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Jumper:SolderJumper_2_Open"
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim yes)
			(in_bom no)
			(on_board yes)
			(property "Reference" "JP"
				(at 0 2.032 0)
			)
			(property "Value" "SolderJumper_2_Open"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Solder Jumper, 2-pole, open"
				(at 0 0 0)
			)
			(property "ki_keywords" "solder jumper SPST"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SolderJumper*Open*"
				(at 0 0 0)
			)
			(symbol "SolderJumper_2_Open_0_1"
				(arc
					(start -0.254 1.016)
					(mid -1.2656 0)
					(end -0.254 -1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.254 1.016)
					(mid -1.2656 0)
					(end -0.254 -1.016)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.254 1.016) (xy -0.254 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 1.016) (xy 0.254 -1.016)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 0.254 -1.016)
					(mid 1.2656 0)
					(end 0.254 1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start 0.254 -1.016)
					(mid 1.2656 0)
					(end 0.254 1.016)
					(fill
						(type outline)
					)
				)
			)
			(symbol "SolderJumper_2_Open_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "B")
					(number "2")
				)
			)
		)
		(symbol "LED:WS2812B"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 5.08 5.715 0)
			)
			(property "Value" "WS2812B"
				(at 1.27 -5.715 0)
			)
			(property "Footprint" "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
				(at 1.27 -7.62 0)
			)
			(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
				(at 2.54 -9.525 0)
			)
			(property "Description" "RGB LED with integrated controller"
				(at 0 0 0)
			)
			(property "ki_keywords" "RGB LED NeoPixel addressable"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*"
				(at 0 0 0)
			)
			(symbol "WS2812B_0_0"
				(text "RGB"
					(at 2.286 -4.191 0)
				)
			)
			(symbol "WS2812B_0_1"
				(polyline
					(pts
						(xy 1.27 -3.556) (xy 1.778 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 1.778 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.699 -3.556) (xy 2.667 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -2.54) (xy 1.27 -3.556) (xy 1.27 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -1.524) (xy 1.27 -2.54) (xy 1.27 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.683 -1.016) (xy 3.683 -3.556) (xy 3.683 -4.064)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.699 -1.524) (xy 2.667 -1.524) (xy 3.683 -3.556) (xy 4.699 -1.524)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.08 5.08)
					(end -5.08 -5.08)
					(fill
						(type background)
					)
				)
			)
			(symbol "WS2812B_1_1"
				(pin power_in line
					(at 0 7.62 270)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "DOUT")
					(number "2")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "VSS")
					(number "3")
				)
				(pin input line
					(at -7.62 0 0)
					(length 2.54)
					(name "DIN")
					(number "4")
				)
			)
		)
		(symbol "MCU_ST_STM32G0:STM32G030F6Px"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -17.78 19.05 0)
			)
			(property "Value" "STM32G030F6Px"
				(at 2.54 19.05 0)
			)
			(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
				(at -17.78 -17.78 0)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030f6.pdf"
				(at 0 0 0)
			)
			(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 17 GPIO, TSSOP20"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
				(at 0 0 0)
			)
			(symbol "STM32G030F6Px_0_1"
				(rectangle
					(start -17.78 -17.78)
					(end 17.78 17.78)
					(fill
						(type background)
					)
				)
			)
			(symbol "STM32G030F6Px_1_1"
				(pin bidirectional line
					(at -20.32 -2.54 0)
					(length 2.54)
					(name "PB7/PB8")
					(number "1")
					(alternate "ADC1_IN11" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "SYS_PVD_IN" bidirectional line)
					(alternate "TIM17_CH1N" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 7.62 180)
					(length 2.54)
					(name "PA3")
					(number "10")
					(alternate "ADC1_IN3" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 5.08 180)
					(length 2.54)
					(name "PA4")
					(number "11")
					(alternate "ADC1_IN4" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RTC_OUT_ALARM" bidirectional line)
					(alternate "RTC_OUT_CALIB" bidirectional line)
					(alternate "RTC_TAMP_IN1" bidirectional line)
					(alternate "RTC_TS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "SYS_WKUP2" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 2.54 180)
					(length 2.54)
					(name "PA5")
					(number "12")
					(alternate "ADC1_IN5" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 0 180)
					(length 2.54)
					(name "PA6")
					(number "13")
					(alternate "ADC1_IN6" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM1_BK" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "PA7")
					(number "14")
					(alternate "ADC1_IN7" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 2.54 0)
					(length 2.54)
					(name "PB0/PB1/PB2/PA8")
					(number "15")
					(alternate "ADC1_IN8" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "PA11/PA9")
					(number "16")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC1_IN15" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM1_BK2" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "PA12/PA10")
					(number "17")
					(alternate "ADC1_IN16" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "I2S_CKIN" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "PA13")
					(number "18")
					(alternate "ADC1_IN17" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "SYS_SWDIO" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "PA14/PA15")
					(number "19")
					(alternate "ADC1_IN18" bidirectional line)
					(alternate "SYS_SWCLK" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 10.16 0)
					(length 2.54)
					(name "PC14/PB9")
					(number "2")
					(alternate "RCC_OSC32_IN" bidirectional line)
					(alternate "RCC_OSC_IN" bidirectional line)
					(alternate "TIM1_BK2" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 0 0)
					(length 2.54)
					(name "PB3/PB4/PB5/PB6")
					(number "20")
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 7.62 0)
					(length 2.54)
					(name "PC15")
					(number "3")
					(alternate "RCC_OSC32_EN" bidirectional line)
					(alternate "RCC_OSC32_OUT" bidirectional line)
					(alternate "RCC_OSC_EN" bidirectional line)
				)
				(pin power_in line
					(at 0 20.32 270)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
				(pin power_in line
					(at 0 -20.32 90)
					(length 2.54)
					(name "VSS")
					(number "5")
				)
				(pin input line
					(at -20.32 15.24 0)
					(length 2.54)
					(name "NRST")
					(number "6")
				)
				(pin bidirectional line
					(at 20.32 15.24 180)
					(length 2.54)
					(name "PA0")
					(number "7")
					(alternate "ADC1_IN0" bidirectional line)
					(alternate "RTC_TAMP_IN2" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "SYS_WKUP1" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 12.7 180)
					(length 2.54)
					(name "PA1")
					(number "8")
					(alternate "ADC1_IN1" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 10.16 180)
					(length 2.54)
					(name "PA2")
					(number "9")
					(alternate "ADC1_IN2" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "RCC_LSCO" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "SYS_WKUP4" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
			)
		)
		(symbol "Memory_EEPROM:CAT24C128"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -6.35 6.35 0)
			)
			(property "Value" "CAT24C128"
				(at 1.27 6.35 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/CAT24C128-D.PDF"
				(at 0 0 0)
			)
			(property "Description" "128 kb CMOS Serial EEPROM, SOIC-8/TSSOP-8/DFN-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "I2C EEPROM Serial 128kb"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
				(at 0 0 0)
			)
			(symbol "CAT24C128_1_1"
				(rectangle
					(start -7.62 5.08)
					(end 7.62 -5.08)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -10.16 2.54 0)
					(length 2.54)
					(name "A0")
					(number "1")
				)
				(pin input line
					(at -10.16 0 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at -10.16 -2.54 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 10.16 2.54 180)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin input line
					(at 10.16 0 180)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "WP")
					(number "7")
				)
				(pin power_in line
					(at 0 7.62 270)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
		)
		(symbol "Relay_SolidState:MOC3063M"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.08 5.08 0)
			)
			(property "Value" "MOC3063M"
				(at 0 5.08 0)
			)
			(property "Footprint" ""
				(at -5.08 -5.08 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3163M-D.pdf"
				(at 0 0 0)
			)
			(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 5mA, DIP6"
				(at 0 0 0)
			)
			(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
				(at 0 0 0)
			)
			(symbol "MOC3063M_0_0"
				(rectangle
					(start -0.381 -2.032)
					(end 1.397 -3.048)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -2.54) (xy 1.397 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.635) (xy 1.016 -1.016) (xy 1.016 -2.032)
					)
					(fill
						(type none)
					)
				)
				(text "ZCD"
					(at 0.508 -2.54 0)
				)
			)
			(symbol "MOC3063M_0_1"
				(rectangle
					(start -5.08 3.81)
					(end 5.08 -3.81)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.175 -0.635) (xy -1.905 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.635) (xy 1.524 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 0.635) (xy 3.048 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -0.635) (xy 2.286 -2.54) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 0.635) (xy 2.286 2.54) (xy 5.08 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 2.54) (xy 0.508 2.54) (xy 0.508 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 2.54) (xy -2.54 2.54) (xy -2.54 -2.54) (xy -5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -0.635) (xy -3.175 0.635) (xy -1.905 0.635) (xy -2.54 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.889 -0.635) (xy 3.683 -0.635) (xy 3.048 0.635) (xy 2.413 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.683 0.635) (xy 0.889 0.635) (xy 1.524 -0.635) (xy 2.159 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.143 -0.508) (xy 0.127 -0.508) (xy -0.254 -0.635) (xy -0.254 -0.381) (xy 0.127 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.143 0.508) (xy 0.127 0.508) (xy -0.254 0.381) (xy -0.254 0.635) (xy 0.127 0.508)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.286 -2.54)
					(radius 0.127)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.286 2.54)
					(radius 0.127)
					(fill
						(type none)
					)
				)
			)
			(symbol "MOC3063M_1_1"
				(pin passive line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "~")
					(number "2")
				)
				(pin no_connect line
					(at -5.08 0 0)
					(length 2.54) hide
					(name "NC")
					(number "3")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "~")
					(number "4")
				)
				(pin no_connect line
					(at 5.08 0 180)
					(length 2.54) hide
					(name "NC")
					(number "5")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "~")
					(number "6")
				)
			)
		)
		(symbol "TTP223:TTP223-BA6"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 8.128 0)
			)
			(property "Value" "TTP223-BA6"
				(at -7.62 -9.906 0)
			)
			(property "Footprint" "TTP223-BA6:SOT23-6"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "MF" "tontek"
				(at 0 0 0)
			)
			(property "Description_1" "\n"
				(at 0 0 0)
			)
			(property "LIB" "CID"
				(at 0 0 0)
			)
			(property "Package" "None"
				(at 0 0 0)
			)
			(property "Price" "None"
				(at 0 0 0)
			)
			(property "SnapEDA_Link" "https://www.snapeda.com/parts/TTP223-BA6/TONTEK/view-part/?ref=snap"
				(at 0 0 0)
			)
			(property "MP" "TTP223-BA6"
				(at 0 0 0)
			)
			(property "Availability" "Not in stock"
				(at 0 0 0)
			)
			(property "Check_prices" "https://www.snapeda.com/parts/TTP223-BA6/TONTEK/view-part/?ref=eda"
				(at 0 0 0)
			)
			(symbol "TTP223-BA6_0_0"
				(rectangle
					(start -7.62 -7.62)
					(end 7.62 7.62)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "Q")
					(number "1")
				)
				(pin power_in line
					(at -10.16 -5.08 0)
					(length 2.54)
					(name "VSS")
					(number "2")
				)
				(pin bidirectional line
					(at -10.16 0 0)
					(length 2.54)
					(name "I")
					(number "3")
				)
				(pin input line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "AHLB")
					(number "4")
				)
				(pin power_in line
					(at -10.16 5.08 0)
					(length 2.54)
					(name "VDD")
					(number "5")
				)
				(pin input line
					(at 10.16 0 180)
					(length 2.54)
					(name "TOG")
					(number "6")
				)
			)
		)
		(symbol "Transistor_FET:BSS138"
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "BSS138"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
				(at 5.08 -3.81 0)
			)
			(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
				(at 0 0 0)
			)
			(property "ki_keywords" "N-Channel MOSFET"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOT?23*"
				(at 0 0 0)
			)
			(symbol "BSS138_0_1"
				(polyline
					(pts
						(xy 0.254 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 1.905) (xy 0.254 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.27) (xy 0.762 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 0) (xy 0.762 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.778) (xy 3.302 -1.778) (xy 3.302 1.778) (xy 0.762 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 0) (xy 2.032 0.381) (xy 2.032 -0.381) (xy 1.016 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 0.508) (xy 2.921 0.381) (xy 3.683 0.381) (xy 3.81 0.254)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 0.381) (xy 2.921 -0.254) (xy 3.683 -0.254) (xy 3.302 0.381)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.651 0)
					(radius 2.794)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
			)
			(symbol "BSS138_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
			)
		)
		(symbol "Triac_Thyristor:BTA16-600B"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "BTA16-600B"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
				(at 0 0 0)
			)
			(property "Description" "16A RMS, 600V Off-State Voltage, 50mA Sensitivity, Insulated, Triac, TO-220"
				(at 0 0 0)
			)
			(property "ki_keywords" "Triac"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO?220*"
				(at 0 0 0)
			)
			(symbol "BTA16-600B_0_1"
				(polyline
					(pts
						(xy -2.54 -1.27) (xy 2.54 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 1.27) (xy 2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -2.54) (xy -0.635 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 1.27) (xy -1.27 -1.27) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 1.27 1.27) (xy 2.54 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "BTA16-600B_1_1"
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "A1")
					(number "1")
				)
				(pin passive line
					(at 0 3.81 270)
					(length 2.54)
					(name "A2")
					(number "2")
				)
				(pin input line
					(at -3.81 -2.54 0)
					(length 2.54)
					(name "G")
					(number "3")
				)
			)
		)
		(symbol "power:+3.3V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3.3V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3.3V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 33.02 162.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 41.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 219.71 41.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 226.06 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 217.17 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 234.95 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 182.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 39.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 238.76 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 265.43 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 80.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 217.17 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 265.43 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 251.46 36.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 245.11 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 44.45 182.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 245.11 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 251.46 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 233.68 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 266.7 95.25)
	)
	(wire
		(pts
			(xy 238.76 21.59) (xy 238.76 22.86)
		)
	)
	(wire
		(pts
			(xy 207.01 138.43) (xy 212.09 138.43)
		)
	)
	(wire
		(pts
			(xy 109.22 102.87) (xy 109.22 118.11)
		)
	)
	(wire
		(pts
			(xy 182.88 120.65) (xy 182.88 90.17)
		)
	)
	(wire
		(pts
			(xy 251.46 33.02) (xy 251.46 36.83)
		)
	)
	(wire
		(pts
			(xy 128.27 82.55) (xy 134.62 82.55)
		)
	)
	(wire
		(pts
			(xy 48.26 161.29) (xy 48.26 163.83)
		)
	)
	(wire
		(pts
			(xy 100.33 102.87) (xy 109.22 102.87)
		)
	)
	(wire
		(pts
			(xy 238.76 46.99) (xy 238.76 53.34)
		)
	)
	(wire
		(pts
			(xy 265.43 149.86) (xy 271.78 149.86)
		)
	)
	(wire
		(pts
			(xy 266.7 41.91) (xy 267.97 41.91)
		)
	)
	(wire
		(pts
			(xy 210.82 133.35) (xy 212.09 133.35)
		)
	)
	(wire
		(pts
			(xy 72.39 182.88) (xy 44.45 182.88)
		)
	)
	(wire
		(pts
			(xy 219.71 29.21) (xy 219.71 30.48)
		)
	)
	(wire
		(pts
			(xy 219.71 41.91) (xy 219.71 49.53)
		)
	)
	(wire
		(pts
			(xy 259.08 113.03) (xy 259.08 115.57)
		)
	)
	(wire
		(pts
			(xy 128.27 69.85) (xy 134.62 69.85)
		)
	)
	(wire
		(pts
			(xy 91.44 161.29) (xy 91.44 163.83)
		)
	)
	(wire
		(pts
			(xy 106.68 105.41) (xy 106.68 120.65)
		)
	)
	(wire
		(pts
			(xy 248.92 36.83) (xy 251.46 36.83)
		)
	)
	(wire
		(pts
			(xy 135.89 48.26) (xy 154.94 48.26)
		)
	)
	(wire
		(pts
			(xy 265.43 133.35) (xy 271.78 133.35)
		)
	)
	(wire
		(pts
			(xy 72.39 168.91) (xy 72.39 182.88)
		)
	)
	(wire
		(pts
			(xy 251.46 22.86) (xy 259.08 22.86)
		)
	)
	(wire
		(pts
			(xy 104.14 64.77) (xy 134.62 64.77)
		)
	)
	(wire
		(pts
			(xy 217.17 77.47) (xy 217.17 81.28)
		)
	)
	(wire
		(pts
			(xy 72.39 166.37) (xy 72.39 168.91)
		)
	)
	(wire
		(pts
			(xy 154.94 48.26) (xy 154.94 59.69)
		)
	)
	(wire
		(pts
			(xy 128.27 72.39) (xy 134.62 72.39)
		)
	)
	(wire
		(pts
			(xy 128.27 77.47) (xy 134.62 77.47)
		)
	)
	(wire
		(pts
			(xy 226.06 87.63) (xy 226.06 81.28)
		)
	)
	(wire
		(pts
			(xy 77.47 180.34) (xy 77.47 182.88)
		)
	)
	(wire
		(pts
			(xy 234.95 90.17) (xy 234.95 95.25)
		)
	)
	(wire
		(pts
			(xy 217.17 90.17) (xy 217.17 95.25)
		)
	)
	(wire
		(pts
			(xy 77.47 171.45) (xy 77.47 172.72)
		)
	)
	(wire
		(pts
			(xy 72.39 161.29) (xy 91.44 161.29)
		)
	)
	(wire
		(pts
			(xy 182.88 90.17) (xy 175.26 90.17)
		)
	)
	(wire
		(pts
			(xy 266.7 25.4) (xy 266.7 22.86)
		)
	)
	(wire
		(pts
			(xy 266.7 33.02) (xy 266.7 41.91)
		)
	)
	(wire
		(pts
			(xy 175.26 87.63) (xy 185.42 87.63)
		)
	)
	(wire
		(pts
			(xy 219.71 36.83) (xy 219.71 41.91)
		)
	)
	(wire
		(pts
			(xy 30.48 162.56) (xy 33.02 162.56)
		)
	)
	(wire
		(pts
			(xy 233.68 149.86) (xy 245.11 149.86)
		)
	)
	(wire
		(pts
			(xy 259.08 77.47) (xy 259.08 80.01)
		)
	)
	(wire
		(pts
			(xy 227.33 138.43) (xy 233.68 138.43)
		)
	)
	(wire
		(pts
			(xy 90.17 113.03) (xy 90.17 118.11)
		)
	)
	(wire
		(pts
			(xy 217.17 95.25) (xy 220.98 95.25)
		)
	)
	(wire
		(pts
			(xy 48.26 161.29) (xy 44.45 161.29)
		)
	)
	(wire
		(pts
			(xy 104.14 97.79) (xy 104.14 64.77)
		)
	)
	(wire
		(pts
			(xy 259.08 22.86) (xy 259.08 25.4)
		)
	)
	(wire
		(pts
			(xy 265.43 140.97) (xy 265.43 142.24)
		)
	)
	(wire
		(pts
			(xy 245.11 133.35) (xy 265.43 133.35)
		)
	)
	(wire
		(pts
			(xy 248.92 41.91) (xy 266.7 41.91)
		)
	)
	(wire
		(pts
			(xy 175.26 72.39) (xy 185.42 72.39)
		)
	)
	(wire
		(pts
			(xy 228.6 39.37) (xy 226.06 39.37)
		)
	)
	(wire
		(pts
			(xy 33.02 162.56) (xy 45.72 162.56)
		)
	)
	(wire
		(pts
			(xy 135.89 54.61) (xy 135.89 55.88)
		)
	)
	(wire
		(pts
			(xy 233.68 139.7) (xy 241.3 139.7)
		)
	)
	(wire
		(pts
			(xy 238.76 22.86) (xy 251.46 22.86)
		)
	)
	(wire
		(pts
			(xy 273.05 80.01) (xy 279.4 80.01)
		)
	)
	(wire
		(pts
			(xy 90.17 85.09) (xy 90.17 92.71)
		)
	)
	(wire
		(pts
			(xy 259.08 39.37) (xy 267.97 39.37)
		)
	)
	(wire
		(pts
			(xy 33.02 162.56) (xy 33.02 166.37)
		)
	)
	(wire
		(pts
			(xy 226.06 81.28) (xy 217.17 81.28)
		)
	)
	(wire
		(pts
			(xy 44.45 182.88) (xy 44.45 171.45)
		)
	)
	(wire
		(pts
			(xy 199.39 133.35) (xy 203.2 133.35)
		)
	)
	(wire
		(pts
			(xy 44.45 185.42) (xy 44.45 182.88)
		)
	)
	(wire
		(pts
			(xy 231.14 95.25) (xy 234.95 95.25)
		)
	)
	(wire
		(pts
			(xy 226.06 39.37) (xy 226.06 22.86)
		)
	)
	(wire
		(pts
			(xy 100.33 105.41) (xy 106.68 105.41)
		)
	)
	(wire
		(pts
			(xy 109.22 118.11) (xy 180.34 118.11)
		)
	)
	(wire
		(pts
			(xy 180.34 92.71) (xy 175.26 92.71)
		)
	)
	(wire
		(pts
			(xy 48.26 171.45) (xy 52.07 171.45)
		)
	)
	(wire
		(pts
			(xy 52.07 166.37) (xy 45.72 166.37)
		)
	)
	(wire
		(pts
			(xy 245.11 149.86) (xy 265.43 149.86)
		)
	)
	(wire
		(pts
			(xy 227.33 133.35) (xy 229.87 133.35)
		)
	)
	(wire
		(pts
			(xy 259.08 80.01) (xy 265.43 80.01)
		)
	)
	(wire
		(pts
			(xy 251.46 22.86) (xy 251.46 25.4)
		)
	)
	(wire
		(pts
			(xy 33.02 173.99) (xy 33.02 182.88)
		)
	)
	(wire
		(pts
			(xy 180.34 118.11) (xy 180.34 92.71)
		)
	)
	(wire
		(pts
			(xy 237.49 133.35) (xy 245.11 133.35)
		)
	)
	(wire
		(pts
			(xy 77.47 163.83) (xy 83.82 163.83)
		)
	)
	(wire
		(pts
			(xy 175.26 69.85) (xy 185.42 69.85)
		)
	)
	(wire
		(pts
			(xy 251.46 36.83) (xy 267.97 36.83)
		)
	)
	(wire
		(pts
			(xy 44.45 161.29) (xy 44.45 157.48)
		)
	)
	(wire
		(pts
			(xy 233.68 147.32) (xy 233.68 149.86)
		)
	)
	(wire
		(pts
			(xy 154.94 100.33) (xy 154.94 109.22)
		)
	)
	(wire
		(pts
			(xy 259.08 22.86) (xy 266.7 22.86)
		)
	)
	(wire
		(pts
			(xy 226.06 22.86) (xy 238.76 22.86)
		)
	)
	(wire
		(pts
			(xy 175.26 85.09) (xy 185.42 85.09)
		)
	)
	(wire
		(pts
			(xy 175.26 74.93) (xy 185.42 74.93)
		)
	)
	(wire
		(pts
			(xy 259.08 102.87) (xy 259.08 105.41)
		)
	)
	(wire
		(pts
			(xy 238.76 22.86) (xy 238.76 31.75)
		)
	)
	(wire
		(pts
			(xy 91.44 161.29) (xy 95.25 161.29)
		)
	)
	(wire
		(pts
			(xy 228.6 36.83) (xy 219.71 36.83)
		)
	)
	(wire
		(pts
			(xy 248.92 39.37) (xy 259.08 39.37)
		)
	)
	(wire
		(pts
			(xy 234.95 95.25) (xy 251.46 95.25)
		)
	)
	(wire
		(pts
			(xy 259.08 80.01) (xy 259.08 87.63)
		)
	)
	(wire
		(pts
			(xy 128.27 80.01) (xy 134.62 80.01)
		)
	)
	(wire
		(pts
			(xy 33.02 182.88) (xy 44.45 182.88)
		)
	)
	(wire
		(pts
			(xy 154.94 46.99) (xy 154.94 48.26)
		)
	)
	(wire
		(pts
			(xy 219.71 22.86) (xy 226.06 22.86)
		)
	)
	(wire
		(pts
			(xy 45.72 166.37) (xy 45.72 162.56)
		)
	)
	(wire
		(pts
			(xy 219.71 41.91) (xy 228.6 41.91)
		)
	)
	(wire
		(pts
			(xy 214.63 95.25) (xy 217.17 95.25)
		)
	)
	(wire
		(pts
			(xy 100.33 97.79) (xy 104.14 97.79)
		)
	)
	(wire
		(pts
			(xy 52.07 161.29) (xy 48.26 161.29)
		)
	)
	(wire
		(pts
			(xy 259.08 33.02) (xy 259.08 39.37)
		)
	)
	(wire
		(pts
			(xy 217.17 81.28) (xy 217.17 82.55)
		)
	)
	(wire
		(pts
			(xy 44.45 171.45) (xy 48.26 171.45)
		)
	)
	(wire
		(pts
			(xy 106.68 120.65) (xy 182.88 120.65)
		)
	)
	(wire
		(pts
			(xy 233.68 138.43) (xy 233.68 139.7)
		)
	)
	(wire
		(pts
			(xy 77.47 182.88) (xy 72.39 182.88)
		)
	)
	(wire
		(pts
			(xy 234.95 77.47) (xy 234.95 82.55)
		)
	)
	(wire
		(pts
			(xy 245.11 140.97) (xy 245.11 149.86)
		)
	)
	(global_label "EEPROM_WP"
		(shape input)
		(at 267.97 41.91 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 282.2641 41.91 0)
		)
	)
	(global_label "LED_OUT"
		(shape output)
		(at 128.27 77.47 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 117.2415 77.47 0)
		)
	)
	(global_label "TOUCH_INPUT"
		(shape output)
		(at 95.25 161.29 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 110.9353 161.29 0)
		)
	)
	(global_label "I2C1_SCL"
		(shape bidirectional)
		(at 267.97 39.37 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 280.8355 39.37 0)
		)
	)
	(global_label "AC_CONTROL"
		(shape output)
		(at 185.42 74.93 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 200.2586 74.93 0)
		)
	)
	(global_label "I2C1_SDA"
		(shape bidirectional)
		(at 267.97 36.83 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 280.896 36.83 0)
		)
	)
	(global_label "AC_IN"
		(shape input)
		(at 271.78 149.86 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 280.0267 149.86 0)
		)
	)
	(global_label "I2C1_SCL"
		(shape bidirectional)
		(at 128.27 82.55 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 115.4045 82.55 0)
		)
	)
	(global_label "I2C2_SCL"
		(shape bidirectional)
		(at 185.42 87.63 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 198.2855 87.63 0)
		)
	)
	(global_label "TOUCH_INPUT"
		(shape input)
		(at 128.27 80.01 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 112.5847 80.01 0)
		)
	)
	(global_label "AC_LOAD"
		(shape output)
		(at 271.78 133.35 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 282.8086 133.35 0)
		)
	)
	(global_label "USART2_RX"
		(shape input)
		(at 185.42 72.39 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 198.928 72.39 0)
		)
	)
	(global_label "TOUCH_PAD"
		(shape input)
		(at 30.48 162.56 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 16.6695 162.56 0)
		)
	)
	(global_label "I2C2_SDA"
		(shape bidirectional)
		(at 185.42 85.09 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 198.346 85.09 0)
		)
	)
	(global_label "LED_OUT"
		(shape input)
		(at 214.63 95.25 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 203.6015 95.25 0)
		)
	)
	(global_label "I2C1_SDA"
		(shape bidirectional)
		(at 128.27 69.85 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 115.344 69.85 0)
		)
	)
	(global_label "AC_CONTROL"
		(shape input)
		(at 199.39 133.35 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 184.5514 133.35 0)
		)
	)
	(global_label "USART2_TX"
		(shape output)
		(at 185.42 69.85 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 198.6256 69.85 0)
		)
	)
	(global_label "EEPROM_WP"
		(shape output)
		(at 128.27 72.39 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 113.9759 72.39 0)
		)
	)
	(symbol
		(lib_id "Jumper:SolderJumper_2_Open")
		(at 87.63 163.83 180)
		(unit 1)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(property "Reference" "JP1"
			(at 87.63 166.116 0)
		)
		(property "Value" "SolderJumper_2_Open"
			(at 94.742 166.878 0)
		)
		(property "Footprint" ""
			(at 87.63 163.83 0)
		)
		(property "Datasheet" "~"
			(at 87.63 163.83 0)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 87.63 163.83 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "JP1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 265.43 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C3"
			(at 269.24 144.7799 0)
		)
		(property "Value" "0.1u"
			(at 269.24 147.3199 0)
		)
		(property "Footprint" ""
			(at 266.3952 149.86 0)
		)
		(property "Datasheet" "~"
			(at 265.43 146.05 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 265.43 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 259.08 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR015"
			(at 259.08 81.28 0)
		)
		(property "Value" "+5V"
			(at 259.08 72.39 0)
		)
		(property "Footprint" ""
			(at 259.08 77.47 0)
		)
		(property "Datasheet" ""
			(at 259.08 77.47 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 259.08 77.47 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 154.94 46.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 154.94 50.8 0)
		)
		(property "Value" "+3.3V"
			(at 154.94 41.91 0)
		)
		(property "Footprint" ""
			(at 154.94 46.99 0)
		)
		(property "Datasheet" ""
			(at 154.94 46.99 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 154.94 46.99 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 90.17 118.11 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 90.17 124.46 0)
		)
		(property "Value" "3.3V GND"
			(at 90.17 123.19 0)
		)
		(property "Footprint" ""
			(at 90.17 118.11 0)
		)
		(property "Datasheet" ""
			(at 90.17 118.11 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 90.17 118.11 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 77.47 176.53 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 81.28 176.8474 90)
		)
		(property "Value" "LED"
			(at 81.28 179.3874 90)
		)
		(property "Footprint" ""
			(at 77.47 176.53 0)
		)
		(property "Datasheet" "~"
			(at 77.47 176.53 0)
		)
		(property "Description" "Light emitting diode"
			(at 77.47 176.53 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 207.01 133.35 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R4"
			(at 206.756 131.064 90)
		)
		(property "Value" "330"
			(at 207.264 135.636 90)
		)
		(property "Footprint" ""
			(at 207.01 135.128 90)
		)
		(property "Datasheet" "~"
			(at 207.01 133.35 0)
		)
		(property "Description" "Resistor"
			(at 207.01 133.35 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 265.43 137.16 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R7"
			(at 270.002 136.144 0)
		)
		(property "Value" "100"
			(at 270.51 138.43 0)
		)
		(property "Footprint" ""
			(at 267.208 137.16 90)
		)
		(property "Datasheet" "~"
			(at 265.43 137.16 0)
		)
		(property "Description" "Resistor"
			(at 265.43 137.16 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 266.7 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 268.224 27.94 0)
		)
		(property "Value" "3.3k"
			(at 268.224 30.48 0)
		)
		(property "Footprint" ""
			(at 264.922 29.21 90)
		)
		(property "Datasheet" "~"
			(at 266.7 29.21 0)
		)
		(property "Description" "Resistor"
			(at 266.7 29.21 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 219.71 26.67 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C2"
			(at 214.884 24.892 0)
		)
		(property "Value" "100n"
			(at 214.884 27.94 0)
		)
		(property "Footprint" ""
			(at 218.7448 22.86 0)
		)
		(property "Datasheet" "~"
			(at 219.71 26.67 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 219.71 26.67 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 217.17 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR014"
			(at 217.17 81.28 0)
		)
		(property "Value" "+3.3V"
			(at 217.17 72.39 0)
		)
		(property "Footprint" ""
			(at 217.17 77.47 0)
		)
		(property "Datasheet" ""
			(at 217.17 77.47 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 217.17 77.47 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_ST_STM32G0:STM32G030F6Px")
		(at 154.94 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 170.18 60.452 0)
		)
		(property "Value" "STM32G030F6Px"
			(at 159.512 99.314 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 137.16 97.79 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030f6.pdf"
			(at 154.94 80.01 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 17 GPIO, TSSOP20"
			(at 154.94 80.01 0)
		)
		(pin "3")
		(pin "8")
		(pin "18")
		(pin "2")
		(pin "6")
		(pin "9")
		(pin "20")
		(pin "7")
		(pin "15")
		(pin "13")
		(pin "14")
		(pin "19")
		(pin "12")
		(pin "11")
		(pin "16")
		(pin "10")
		(pin "1")
		(pin "4")
		(pin "17")
		(pin "5")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 238.76 21.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 238.76 25.4 0)
		)
		(property "Value" "+3.3V"
			(at 238.76 16.51 0)
		)
		(property "Footprint" ""
			(at 238.76 21.59 0)
		)
		(property "Datasheet" ""
			(at 238.76 21.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 238.76 21.59 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 269.24 80.01 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C6"
			(at 269.24 76.454 90)
		)
		(property "Value" "104"
			(at 269.24 83.82 90)
		)
		(property "Footprint" ""
			(at 273.05 79.0448 0)
		)
		(property "Datasheet" "~"
			(at 269.24 80.01 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 269.24 80.01 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 259.08 109.22 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R11"
			(at 261.62 107.9499 0)
		)
		(property "Value" "84"
			(at 261.62 110.4899 0)
		)
		(property "Footprint" ""
			(at 257.302 109.22 90)
		)
		(property "Datasheet" "~"
			(at 259.08 109.22 0)
		)
		(property "Description" "Resistor"
			(at 259.08 109.22 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 90.17 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 90.17 88.9 0)
		)
		(property "Value" "+3.3V"
			(at 90.17 80.01 0)
		)
		(property "Footprint" ""
			(at 90.17 85.09 0)
		)
		(property "Datasheet" ""
			(at 90.17 85.09 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 90.17 85.09 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 207.01 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR010"
			(at 207.01 144.78 0)
		)
		(property "Value" "3.3V GND"
			(at 207.01 143.51 0)
		)
		(property "Footprint" ""
			(at 207.01 138.43 0)
		)
		(property "Datasheet" ""
			(at 207.01 138.43 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 207.01 138.43 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_ARM_SWD_TagConnect_TC2030-NL")
		(at 92.71 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 86.36 101.5999 0)
		)
		(property "Value" "Conn_ARM_SWD_TagConnect_TC2030-NL"
			(at 86.36 104.1399 0)
		)
		(property "Footprint" "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
			(at 92.71 120.65 0)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2030-CTX_1.pdf"
			(at 92.71 118.11 0)
		)
		(property "Description" "Tag-Connect ARM Cortex SWD JTAG connector, 6 pin, no legs"
			(at 92.71 102.87 0)
		)
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "5")
		(pin "6")
		(pin "3")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Triac_Thyristor:BTA16-600B")
		(at 245.11 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q1"
			(at 248.92 136.4741 0)
		)
		(property "Value" "BTA16-600B"
			(at 248.92 139.0141 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
			(at 250.19 139.065 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 245.11 137.16 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 50mA Sensitivity, Insulated, Triac, TO-220"
			(at 245.11 137.16 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 259.08 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR017"
			(at 259.08 121.92 0)
		)
		(property "Value" "5V GND"
			(at 259.08 120.65 0)
		)
		(property "Footprint" ""
			(at 259.08 115.57 0)
		)
		(property "Datasheet" ""
			(at 259.08 115.57 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 259.08 115.57 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR017")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 217.17 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R9"
			(at 219.71 85.0899 0)
		)
		(property "Value" "10K"
			(at 219.71 87.6299 0)
		)
		(property "Footprint" ""
			(at 215.392 86.36 90)
		)
		(property "Datasheet" "~"
			(at 217.17 86.36 0)
		)
		(property "Description" "Resistor"
			(at 217.17 86.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 219.71 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 219.71 35.56 0)
		)
		(property "Value" "3.3V GND"
			(at 219.71 34.29 0)
		)
		(property "Footprint" ""
			(at 219.71 29.21 0)
		)
		(property "Datasheet" ""
			(at 219.71 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 219.71 29.21 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 77.47 167.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R8"
			(at 80.01 166.3699 0)
		)
		(property "Value" "1K"
			(at 80.01 168.9099 0)
		)
		(property "Footprint" ""
			(at 75.692 167.64 90)
		)
		(property "Datasheet" "~"
			(at 77.47 167.64 0)
		)
		(property "Description" "Resistor"
			(at 77.47 167.64 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Memory_EEPROM:CAT24C128")
		(at 238.76 39.37 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U2"
			(at 243.332 32.512 0)
		)
		(property "Value" "CAT24C64YI"
			(at 240.284 45.974 0)
		)
		(property "Footprint" ""
			(at 238.76 39.37 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/CAT24C128-D.PDF"
			(at 238.76 39.37 0)
		)
		(property "Description" "128 kb CMOS Serial EEPROM, SOIC-8/TSSOP-8/DFN-8"
			(at 238.76 39.37 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(pin "4")
		(pin "8")
		(pin "6")
		(pin "7")
		(pin "5")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 33.02 170.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C5"
			(at 27.432 169.164 0)
		)
		(property "Value" "22p"
			(at 25.654 171.704 0)
		)
		(property "Footprint" ""
			(at 33.9852 173.99 0)
		)
		(property "Datasheet" "~"
			(at 33.02 170.18 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 33.02 170.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 219.71 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR09"
			(at 219.71 55.88 0)
		)
		(property "Value" "3.3V GND"
			(at 219.71 54.61 0)
		)
		(property "Footprint" ""
			(at 219.71 49.53 0)
		)
		(property "Datasheet" ""
			(at 219.71 49.53 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 219.71 49.53 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 234.95 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 234.95 81.28 0)
		)
		(property "Value" "+5V"
			(at 234.95 72.39 0)
		)
		(property "Footprint" ""
			(at 234.95 77.47 0)
		)
		(property "Datasheet" ""
			(at 234.95 77.47 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 234.95 77.47 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 233.68 133.35 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R5"
			(at 233.426 131.064 90)
		)
		(property "Value" "320"
			(at 233.934 135.636 90)
		)
		(property "Footprint" ""
			(at 233.68 135.128 90)
		)
		(property "Datasheet" "~"
			(at 233.68 133.35 0)
		)
		(property "Description" "Resistor"
			(at 233.68 133.35 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 279.4 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR016"
			(at 279.4 86.36 0)
		)
		(property "Value" "5V GND"
			(at 279.4 85.09 0)
		)
		(property "Footprint" ""
			(at 279.4 80.01 0)
		)
		(property "Datasheet" ""
			(at 279.4 80.01 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 279.4 80.01 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 234.95 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R10"
			(at 237.49 85.0899 0)
		)
		(property "Value" "10K"
			(at 237.49 87.6299 0)
		)
		(property "Footprint" ""
			(at 233.172 86.36 90)
		)
		(property "Datasheet" "~"
			(at 234.95 86.36 0)
		)
		(property "Description" "Resistor"
			(at 234.95 86.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 238.76 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 238.76 59.69 0)
		)
		(property "Value" "3.3V GND"
			(at 238.76 58.42 0)
		)
		(property "Footprint" ""
			(at 238.76 53.34 0)
		)
		(property "Datasheet" ""
			(at 238.76 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 238.76 53.34 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 48.26 167.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C4"
			(at 42.672 166.624 0)
		)
		(property "Value" "100n"
			(at 40.894 169.164 0)
		)
		(property "Footprint" ""
			(at 49.2252 171.45 0)
		)
		(property "Datasheet" "~"
			(at 48.26 167.64 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 48.26 167.64 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 233.68 143.51 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R6"
			(at 237.49 142.748 0)
		)
		(property "Value" "320"
			(at 237.998 144.78 0)
		)
		(property "Footprint" ""
			(at 235.458 143.51 90)
		)
		(property "Datasheet" "~"
			(at 233.68 143.51 0)
		)
		(property "Description" "Resistor"
			(at 233.68 143.51 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 259.08 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R3"
			(at 260.604 28.194 0)
		)
		(property "Value" "3.3k"
			(at 260.604 30.734 0)
		)
		(property "Footprint" ""
			(at 257.302 29.21 90)
		)
		(property "Datasheet" "~"
			(at 259.08 29.21 0)
		)
		(property "Description" "Resistor"
			(at 259.08 29.21 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 44.45 185.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR012"
			(at 44.45 191.77 0)
		)
		(property "Value" "5V GND"
			(at 44.45 190.5 0)
		)
		(property "Footprint" ""
			(at 44.45 185.42 0)
		)
		(property "Datasheet" ""
			(at 44.45 185.42 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 44.45 185.42 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 135.89 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 135.89 60.96 0)
		)
		(property "Value" "3.3V GND"
			(at 135.89 59.69 0)
		)
		(property "Footprint" ""
			(at 135.89 54.61 0)
		)
		(property "Datasheet" ""
			(at 135.89 54.61 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 135.89 54.61 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "TTP223:TTP223-BA6")
		(at 62.23 166.37 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U4"
			(at 62.23 153.67 0)
		)
		(property "Value" "TTP223-BA6"
			(at 62.23 156.21 0)
		)
		(property "Footprint" "TTP223-BA6:SOT23-6"
			(at 62.23 166.37 0)
		)
		(property "Datasheet" ""
			(at 62.23 166.37 0)
		)
		(property "Description" ""
			(at 62.23 166.37 0)
		)
		(property "MF" "tontek"
			(at 62.23 166.37 0)
		)
		(property "Description_1" "\n"
			(at 62.23 166.37 0)
		)
		(property "LIB" "CID"
			(at 62.23 166.37 0)
		)
		(property "Package" "None"
			(at 62.23 166.37 0)
		)
		(property "Price" "None"
			(at 62.23 166.37 0)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/TTP223-BA6/TONTEK/view-part/?ref=snap"
			(at 62.23 166.37 0)
		)
		(property "MP" "TTP223-BA6"
			(at 62.23 166.37 0)
		)
		(property "Availability" "Not in stock"
			(at 62.23 166.37 0)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/TTP223-BA6/TONTEK/view-part/?ref=eda"
			(at 62.23 166.37 0)
		)
		(pin "4")
		(pin "1")
		(pin "6")
		(pin "5")
		(pin "2")
		(pin "3")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "U4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 154.94 109.22 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 154.94 115.57 0)
		)
		(property "Value" "3.3V GND"
			(at 154.94 114.3 0)
		)
		(property "Footprint" ""
			(at 154.94 109.22 0)
		)
		(property "Datasheet" ""
			(at 154.94 109.22 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 154.94 109.22 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 251.46 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R2"
			(at 252.73 27.94 0)
		)
		(property "Value" "3.3k"
			(at 252.73 30.48 0)
		)
		(property "Footprint" ""
			(at 249.682 29.21 90)
		)
		(property "Datasheet" "~"
			(at 251.46 29.21 0)
		)
		(property "Description" "Resistor"
			(at 251.46 29.21 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Relay_SolidState:MOC3063M")
		(at 219.71 135.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U3"
			(at 219.71 127 0)
		)
		(property "Value" "MOC3063M"
			(at 219.71 129.54 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-6_W9.53mm_Clearance8mm"
			(at 214.63 140.97 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3163M-D.pdf"
			(at 219.71 135.89 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 5mA, DIP6"
			(at 219.71 135.89 0)
		)
		(pin "1")
		(pin "4")
		(pin "2")
		(pin "3")
		(pin "5")
		(pin "6")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "U3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:BSS138")
		(at 226.06 92.71 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q2"
			(at 223.266 90.678 90)
		)
		(property "Value" "BSS138"
			(at 226.06 99.06 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 224.155 97.79 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 222.25 97.79 0)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 226.06 92.71 0)
		)
		(pin "3")
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LED:WS2812B")
		(at 259.08 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 270.51 88.9314 0)
		)
		(property "Value" "WS2812B"
			(at 270.51 91.4714 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
			(at 260.35 102.87 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 261.62 104.775 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 259.08 95.25 0)
		)
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 135.89 52.07 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C1"
			(at 131.064 50.292 0)
		)
		(property "Value" "100n"
			(at 131.064 53.34 0)
		)
		(property "Footprint" ""
			(at 134.9248 48.26 0)
		)
		(property "Datasheet" "~"
			(at 135.89 52.07 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 135.89 52.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 44.45 157.48 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR011"
			(at 44.45 161.29 0)
		)
		(property "Value" "+5V"
			(at 44.45 152.4 0)
		)
		(property "Footprint" ""
			(at 44.45 157.48 0)
		)
		(property "Datasheet" ""
			(at 44.45 157.48 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 44.45 157.48 0)
		)
		(pin "1")
		(instances
			(project "CapacitiveSwitchV0_0"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)