(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Flextouch")
		(comment 1 "Flextouch - FFC for Ikea Pler 8 stove")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 271.4 150.9)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(footprint "FFC:FFC_10pin_1mm-pitch_wuerth"
		(layer "F.Cu")
		(at 119.15 76.975)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FFC_10pin_1mm-pitch_wuerth"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "FFC:FFC_10pin_1mm-pitch_wuerth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -4 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -3 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -2 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -1 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 1 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 2 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 3 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 4 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "FFC:FFC_10pin_1mm-pitch_wuerth"
		(layer "F.Cu")
		(at 131.375 144.575)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FFC_10pin_1mm-pitch_wuerth"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "FFC:FFC_10pin_1mm-pitch_wuerth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -4 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -3 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -2 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -1 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 1 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 2 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 3 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 4 -5.5)
			(size 0.7 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Connector_FFC-FPC:TE_1-84952-0_1x10-1MP_P1.0mm_Horizontal"
		(layer "F.Cu")
		(at 91.075 77.75 180)
		(descr "TE FPC connector, 10 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4")
		(tags "te fpc 84952")
		(property "Reference" "REF**"
			(at 0 -4 180)
			(layer "F.SilkS")
		)
		(property "Value" "TE_1-84952-0_1x10-1MP_P1.0mm_Horizontal"
			(at 0 7.7 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_FFC-FPC:TE_1-84952-0_1x10-1MP_P1.0mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.9 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd rect
			(at -3.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "3" smd rect
			(at -2.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "4" smd rect
			(at -1.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "5" smd rect
			(at -0.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 0.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "7" smd rect
			(at 1.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "8" smd rect
			(at 2.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "9" smd rect
			(at 3.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "10" smd rect
			(at 4.5 -1.8 180)
			(size 0.61 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "MP" smd rect
			(at -7.49 1 180)
			(size 2.68 3.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "MP" smd rect
			(at 7.49 1 180)
			(size 2.68 3.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/TE_1-84952-0_1x10-1MP_P1.0mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_FFC-FPC:Molex_200528-0100_1x10-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 159.425 79.915 180)
		(descr "Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0100, 10 Circuits (https://www.molex.com/pdm_docs/sd/2005280100_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex  top entry")
		(property "Reference" "REF**"
			(at 0 -2.61 180)
			(layer "F.SilkS")
		)
		(property "Value" "Molex_200528-0100_1x10-1MP_P1.00mm_Horizontal"
			(at 0 5.39 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_FFC-FPC:Molex_200528-0100_1x10-1MP_P1.00mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.39 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd rect
			(at -3.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "3" smd rect
			(at -2.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "4" smd rect
			(at -1.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "5" smd rect
			(at -0.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 0.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "7" smd rect
			(at 1.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "8" smd rect
			(at 2.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "9" smd rect
			(at 3.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "10" smd rect
			(at 4.5 -0.91 180)
			(size 0.4 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "MP" smd rect
			(at -7.3 1.79 180)
			(size 2 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "MP" smd rect
			(at 7.3 1.79 180)
			(size 2 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Molex_200528-0100_1x10-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(image
		(at 41.375 102.075)
		(layer "F.SilkS")
		(scale 0.2548)
	)
	(image
		(at 186.1 34.525)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 87.325 102.125)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 198.325 102.125)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 163.1 34.525)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 131.375 102.075)
		(layer "F.SilkS")
		(scale 0.133345)
	)
	(image
		(at 209.25 34.425)
		(layer "F.SilkS")
		(scale 0.348651)
	)
	(image
		(at 175.325 102.125)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 64.225 102.125)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 75.1 34.525)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 29.15 34.475)
		(layer "F.SilkS")
		(scale 0.2548)
	)
	(image
		(at 52 34.525)
		(layer "F.SilkS")
		(scale 0.282167)
	)
	(image
		(at 119.15 34.475)
		(layer "F.SilkS")
		(scale 0.133345)
	)
	(image
		(at 221.475 102.025)
		(layer "F.SilkS")
		(scale 0.348651)
	)
	(gr_text "-"
		(at 108.975 105.975 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 96.75 38.375 0)
		(layer "F.SilkS")
	)
	(gr_text "FlexTouch"
		(at 41.375 113.85 0)
		(layer "F.SilkS")
	)
	(gr_text "FlexTouch"
		(at 29.075 46.75 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 130.85 38.375 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 143.075 105.975 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.375 96.275) (xy 137.275 96.275) (xy 137.275 107.975) (xy 125.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 180.15 28.675) (xy 192.05 28.675) (xy 192.05 40.375) (xy 180.15 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.375 96.275) (xy 204.275 96.275) (xy 204.275 107.975) (xy 192.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.15 28.675) (xy 125.05 28.675) (xy 125.05 40.375) (xy 113.15 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.375 96.275) (xy 154.275 96.275) (xy 154.275 107.975) (xy 142.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 46.05 28.675) (xy 57.95 28.675) (xy 57.95 40.375) (xy 46.05 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 69.15 28.675) (xy 81.05 28.675) (xy 81.05 40.375) (xy 69.15 40.375) (xy 69.15 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.375 96.275) (xy 181.275 96.275) (xy 181.275 107.975) (xy 169.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 23.15 28.675) (xy 35.05 28.675) (xy 35.05 40.375) (xy 23.15 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.375 96.275) (xy 120.275 96.275) (xy 120.275 107.975) (xy 108.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 203.15 28.675) (xy 215.05 28.675) (xy 215.05 40.375) (xy 203.15 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 35.375 96.275) (xy 47.275 96.275) (xy 47.275 107.975) (xy 35.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.375 96.275) (xy 93.275 96.275) (xy 93.275 107.975) (xy 81.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.15 28.675) (xy 142.05 28.675) (xy 142.05 40.375) (xy 130.15 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 58.275 96.275) (xy 70.175 96.275) (xy 70.175 107.975) (xy 58.275 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 215.375 96.275) (xy 227.275 96.275) (xy 227.275 107.975) (xy 215.375 107.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.15 28.675) (xy 169.05 28.675) (xy 169.05 40.375) (xy 157.15 40.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.15 28.675) (xy 108.05 28.675) (xy 108.05 40.375) (xy 96.15 40.375)
			)
		)
	)
)
