(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "LED" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "LED diode" (at 0 0 0))
      (property "ki_description" "Light emitting diode" (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "MCU_Module:Arduino_UNO_R2" (in_bom yes) (on_board yes)
      (property "Reference" "A" (at -10.16 23.495 0))
      (property "Value" "Arduino_UNO_R2" (at 5.08 -26.67 0))
      (property "Footprint" "Module:Arduino_UNO_R2" (at 0 0 0))
      (property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno" (at 0 0 0))
      (property "ki_keywords" "Arduino UNO R3 Microcontroller Module Atmel AVR USB" (at 0 0 0))
      (property "ki_description" "Arduino UNO Microcontroller Module, release 2" (at 0 0 0))
      (property "ki_fp_filters" "Arduino*UNO*R2*" (at 0 0 0))
      (symbol "Arduino_UNO_R2_0_1"
        (rectangle (start -10.16 22.86) (end 10.16 -25.4)
          (fill (type background))
        )
      )
      (symbol "Arduino_UNO_R2_1_1"
        (pin no_connect line (at -10.16 -20.32 0) (length 2.54) hide
          (name "NC")
          (number "1")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "A1")
          (number "10")
        )
        (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
          (name "A2")
          (number "11")
        )
        (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
          (name "A3")
          (number "12")
        )
        (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
          (name "SDA/A4")
          (number "13")
        )
        (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
          (name "SCL/A5")
          (number "14")
        )
        (pin bidirectional line (at -12.7 15.24 0) (length 2.54)
          (name "D0/RX")
          (number "15")
        )
        (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
          (name "D1/TX")
          (number "16")
        )
        (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
          (name "D2")
          (number "17")
        )
        (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
          (name "D3")
          (number "18")
        )
        (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
          (name "D4")
          (number "19")
        )
        (pin output line (at 12.7 10.16 180) (length 2.54)
          (name "IOREF")
          (number "2")
        )
        (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
          (name "D5")
          (number "20")
        )
        (pin bidirectional line (at -12.7 0 0) (length 2.54)
          (name "D6")
          (number "21")
        )
        (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
          (name "D7")
          (number "22")
        )
        (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
          (name "D8")
          (number "23")
        )
        (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
          (name "D9")
          (number "24")
        )
        (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
          (name "D10")
          (number "25")
        )
        (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
          (name "D11")
          (number "26")
        )
        (pin bidirectional line (at -12.7 -15.24 0) (length 2.54)
          (name "D12")
          (number "27")
        )
        (pin bidirectional line (at -12.7 -17.78 0) (length 2.54)
          (name "D13")
          (number "28")
        )
        (pin power_in line (at -2.54 -27.94 90) (length 2.54)
          (name "GND")
          (number "29")
        )
        (pin input line (at 12.7 15.24 180) (length 2.54)
          (name "~{RESET}")
          (number "3")
        )
        (pin input line (at 12.7 5.08 180) (length 2.54)
          (name "AREF")
          (number "30")
        )
        (pin power_out line (at 2.54 25.4 270) (length 2.54)
          (name "3V3")
          (number "4")
        )
        (pin power_out line (at 5.08 25.4 270) (length 2.54)
          (name "+5V")
          (number "5")
        )
        (pin power_in line (at 0 -27.94 90) (length 2.54)
          (name "GND")
          (number "6")
        )
        (pin power_in line (at 2.54 -27.94 90) (length 2.54)
          (name "GND")
          (number "7")
        )
        (pin power_in line (at -2.54 25.4 270) (length 2.54)
          (name "VIN")
          (number "8")
        )
        (pin bidirectional line (at 12.7 0 180) (length 2.54)
          (name "A0")
          (number "9")
        )
      )
    )
    (symbol "power:PWR_FLAG" (power) (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "#FLG" (at 0 1.905 0))
      (property "Value" "PWR_FLAG" (at 0 3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "flag power" (at 0 0 0))
      (property "ki_description" "Special symbol for telling ERC where power comes from" (at 0 0 0))
      (symbol "PWR_FLAG_0_0"
        (pin power_out line (at 0 0 90) (length 0)
          (name "pwr")
          (number "1")
        )
      )
      (symbol "PWR_FLAG_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 1.27)
            (xy -1.016 1.905)
            (xy 0 2.54)
            (xy 1.016 1.905)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
    )
    (symbol "rfid-rc522-module:RFID-RC522-MODULE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "P" (at 0 1.27 0))
      (property "Value" "RFID-RC522-MODULE" (at -1.27 3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "RFID-RC522-MODULE_0_1"
        (rectangle (start -16.51 7.62) (end 15.24 -6.35)
          (fill (type none))
        )
      )
      (symbol "RFID-RC522-MODULE_1_1"
        (pin input line (at -13.97 -13.97 90) (length 7.62)
          (name "SDA")
          (number "1")
        )
        (pin input line (at -10.16 -13.97 90) (length 7.62)
          (name "SCK")
          (number "2")
        )
        (pin input line (at -6.35 -13.97 90) (length 7.62)
          (name "MOSI")
          (number "3")
        )
        (pin input line (at -2.54 -13.97 90) (length 7.62)
          (name "MISO")
          (number "4")
        )
        (pin input line (at 1.27 -13.97 90) (length 7.62)
          (name "IRQ")
          (number "5")
        )
        (pin input line (at 5.08 -13.97 90) (length 7.62)
          (name "GND")
          (number "6")
        )
        (pin input line (at 8.89 -13.97 90) (length 7.62)
          (name "RST")
          (number "7")
        )
        (pin input line (at 12.7 -13.97 90) (length 7.62)
          (name "3.3V")
          (number "8")
        )
      )
    )
  )
  (junction (at 102.87 173.99) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 151.13) (diameter 0) (color 0 0 0 0))
  (junction (at 100.33 152.4) (diameter 0) (color 0 0 0 0))
  (no_connect (at 113.03 106.68))
  (no_connect (at 113.03 116.84))
  (no_connect (at 113.03 134.62))
  (no_connect (at 87.63 114.3))
  (no_connect (at 113.03 132.08))
  (no_connect (at 113.03 111.76))
  (no_connect (at 113.03 129.54))
  (no_connect (at 87.63 109.22))
  (no_connect (at 87.63 124.46))
  (no_connect (at 87.63 106.68))
  (no_connect (at 149.86 86.36))
  (no_connect (at 87.63 139.7))
  (no_connect (at 87.63 111.76))
  (no_connect (at 87.63 121.92))
  (no_connect (at 113.03 124.46))
  (no_connect (at 87.63 119.38))
  (no_connect (at 113.03 121.92))
  (no_connect (at 87.63 116.84))
  (no_connect (at 97.79 96.52))
  (no_connect (at 113.03 127))
  (no_connect (at 102.87 149.86))
  (wire (pts (xy 213.36 101.6) (xy 213.36 40.64)))
  (wire (pts (xy 134.62 86.36) (xy 134.62 104.14)))
  (wire (pts (xy 60.96 132.08) (xy 87.63 132.08)))
  (wire (pts (xy 153.67 86.36) (xy 153.67 92.71)))
  (wire (pts (xy 127 138.43) (xy 128.27 138.43)))
  (wire (pts (xy 163.83 138.43) (xy 163.83 121.92)))
  (wire (pts (xy 55.88 40.64) (xy 55.88 134.62)))
  (wire (pts (xy 207.01 96.52) (xy 207.01 45.72)))
  (wire (pts (xy 55.88 134.62) (xy 87.63 134.62)))
  (wire (pts (xy 46.99 137.16) (xy 87.63 137.16)))
  (wire (pts (xy 46.99 38.1) (xy 46.99 137.16)))
  (wire (pts (xy 130.81 121.92) (xy 130.81 85.09)))
  (wire (pts (xy 138.43 101.6) (xy 213.36 101.6)))
  (wire (pts (xy 142.24 86.36) (xy 142.24 99.06)))
  (wire (pts (xy 82.55 127) (xy 87.63 127)))
  (wire (pts (xy 191.77 57.15) (xy 102.87 57.15)))
  (wire (pts (xy 97.79 151.13) (xy 97.79 149.86)))
  (wire (pts (xy 102.87 57.15) (xy 102.87 96.52)))
  (wire (pts (xy 139.7 173.99) (xy 102.87 173.99)))
  (wire (pts (xy 127 152.4) (xy 127 138.43)))
  (wire (pts (xy 153.67 92.71) (xy 200.66 92.71)))
  (wire (pts (xy 162.56 152.4) (xy 162.56 180.34)))
  (wire (pts (xy 69.85 49.53) (xy 69.85 165.1)))
  (wire (pts (xy 100.33 149.86) (xy 100.33 152.4)))
  (wire (pts (xy 142.24 99.06) (xy 210.82 99.06)))
  (wire (pts (xy 105.41 90.17) (xy 127 90.17)))
  (wire (pts (xy 163.83 121.92) (xy 130.81 121.92)))
  (wire (pts (xy 146.05 86.36) (xy 146.05 96.52)))
  (wire (pts (xy 146.05 96.52) (xy 207.01 96.52)))
  (wire (pts (xy 95.25 165.1) (xy 95.25 151.13)))
  (wire (pts (xy 60.96 43.18) (xy 60.96 132.08)))
  (wire (pts (xy 217.17 104.14) (xy 217.17 38.1)))
  (wire (pts (xy 200.66 49.53) (xy 69.85 49.53)))
  (wire (pts (xy 162.56 180.34) (xy 102.87 180.34)))
  (wire (pts (xy 210.82 99.06) (xy 210.82 43.18)))
  (wire (pts (xy 101.6 156.21) (xy 101.6 173.99)))
  (wire (pts (xy 200.66 92.71) (xy 200.66 49.53)))
  (wire (pts (xy 100.33 152.4) (xy 100.33 156.21)))
  (wire (pts (xy 138.43 86.36) (xy 138.43 101.6)))
  (wire (pts (xy 105.41 85.09) (xy 105.41 90.17)))
  (wire (pts (xy 213.36 40.64) (xy 55.88 40.64)))
  (wire (pts (xy 96.52 151.13) (xy 97.79 151.13)))
  (wire (pts (xy 130.81 85.09) (xy 105.41 85.09)))
  (wire (pts (xy 82.55 53.34) (xy 82.55 127)))
  (wire (pts (xy 210.82 43.18) (xy 60.96 43.18)))
  (wire (pts (xy 134.62 104.14) (xy 217.17 104.14)))
  (wire (pts (xy 64.77 45.72) (xy 64.77 129.54)))
  (wire (pts (xy 104.14 90.17) (xy 105.41 90.17)))
  (wire (pts (xy 157.48 90.17) (xy 196.85 90.17)))
  (wire (pts (xy 154.94 138.43) (xy 156.21 138.43)))
  (wire (pts (xy 207.01 45.72) (xy 64.77 45.72)))
  (wire (pts (xy 95.25 151.13) (xy 96.52 151.13)))
  (wire (pts (xy 102.87 180.34) (xy 102.87 173.99)))
  (wire (pts (xy 104.14 90.17) (xy 104.14 96.52)))
  (wire (pts (xy 196.85 53.34) (xy 82.55 53.34)))
  (wire (pts (xy 104.14 96.52) (xy 105.41 96.52)))
  (wire (pts (xy 101.6 173.99) (xy 102.87 173.99)))
  (wire (pts (xy 127 123.19) (xy 127 90.17)))
  (wire (pts (xy 139.7 152.4) (xy 139.7 173.99)))
  (wire (pts (xy 64.77 129.54) (xy 87.63 129.54)))
  (wire (pts (xy 157.48 86.36) (xy 157.48 90.17)))
  (wire (pts (xy 132.08 152.4) (xy 127 152.4)))
  (wire (pts (xy 135.89 138.43) (xy 135.89 123.19)))
  (wire (pts (xy 191.77 86.36) (xy 191.77 57.15)))
  (wire (pts (xy 196.85 90.17) (xy 196.85 53.34)))
  (wire (pts (xy 135.89 123.19) (xy 127 123.19)))
  (wire (pts (xy 69.85 165.1) (xy 95.25 165.1)))
  (wire (pts (xy 154.94 152.4) (xy 154.94 138.43)))
  (wire (pts (xy 161.29 86.36) (xy 191.77 86.36)))
  (wire (pts (xy 100.33 156.21) (xy 101.6 156.21)))
  (wire (pts (xy 217.17 38.1) (xy 46.99 38.1)))
  (symbol (lib_id "power:PWR_FLAG") (at 100.33 152.4 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#FLG02" (at 100.33 150.495 0))
    (property "Value" "PWR_FLAG" (at 100.33 147.32 0))
    (property "Footprint" "" (at 100.33 152.4 0))
    (property "Datasheet" "~" (at 100.33 152.4 0))
    (pin "1")
    (instances
      (project "a new"
        (path
          (reference "#FLG02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 135.89 152.4 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D1" (at 137.4775 144.78 0))
    (property "Value" "LED" (at 137.4775 147.32 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 135.89 152.4 0))
    (property "Datasheet" "~" (at 135.89 152.4 0))
    (pin "1")
    (pin "2")
    (instances
      (project "a new"
        (path
          (reference "D1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 160.02 138.43 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R2" (at 160.02 132.08 90))
    (property "Value" "100" (at 160.02 134.62 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal" (at 160.02 140.208 90))
    (property "Datasheet" "~" (at 160.02 138.43 0))
    (pin "1")
    (pin "2")
    (instances
      (project "a new"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "rfid-rc522-module:RFID-RC522-MODULE") (at 148.59 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "P1" (at 165.1 70.485 0))
    (property "Value" "RFID-RC522-MODULE" (at 165.1 73.025 0))
    (property "Footprint" "RFID-RC522:RFID-RC522" (at 148.59 72.39 0))
    (property "Datasheet" "" (at 148.59 72.39 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "a new"
        (path
          (reference "P1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 158.75 152.4 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D2" (at 160.3375 144.78 0))
    (property "Value" "LED" (at 160.3375 147.32 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 158.75 152.4 0))
    (property "Datasheet" "~" (at 158.75 152.4 0))
    (pin "1")
    (pin "2")
    (instances
      (project "a new"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:PWR_FLAG") (at 96.52 151.13 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#FLG01" (at 96.52 149.225 0))
    (property "Value" "PWR_FLAG" (at 96.52 146.05 0))
    (property "Footprint" "" (at 96.52 151.13 0))
    (property "Datasheet" "~" (at 96.52 151.13 0))
    (pin "1")
    (instances
      (project "a new"
        (path
          (reference "#FLG01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 132.08 138.43 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 132.08 132.08 90))
    (property "Value" "100" (at 132.08 134.62 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal" (at 132.08 136.652 90))
    (property "Datasheet" "~" (at 132.08 138.43 0))
    (pin "1")
    (pin "2")
    (instances
      (project "a new"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "MCU_Module:Arduino_UNO_R2") (at 100.33 121.92 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "A1" (at 107.6041 93.98 0))
    (property "Value" "Arduino_UNO_R2" (at 107.6041 96.52 0))
    (property "Footprint" "Module:Arduino_UNO_R2" (at 100.33 121.92 0))
    (property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno" (at 100.33 121.92 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "a new"
        (path
          (reference "A1") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
