(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.52)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.18)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.18)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(A1-Pad1)")
	(net 3 "/nRF9151_SiP/GPS_RF5")
	(net 4 "VDD_5V")
	(net 5 "VDD")
	(net 6 "VBAT_PWR")
	(net 7 "/nRF9151_Power_Supply/VSYS")
	(net 8 "VDD_3V0")
	(net 9 "VDD_3V3")
	(net 10 "Net-(M1A-VDD)")
	(net 11 "/nRF9151_SiP/DEC0")
	(net 12 "Net-(M1C-nRESET)")
	(net 13 "/nRF9151_SiP/GPS_RF1")
	(net 14 "/nRF9151_SiP/GPS_RF2")
	(net 15 "Net-(C20-Pad2)")
	(net 16 "VDD_GNSS")
	(net 17 "Net-(U3-VEN)")
	(net 18 "/nRF9151_SiP/ANT")
	(net 19 "/nRF9151_SiP/GPS_RF3")
	(net 20 "Net-(C26-Pad2)")
	(net 21 "Net-(U3-VCC)")
	(net 22 "Net-(U5A-VBUS)")
	(net 23 "/nRF5340_Interface_MCU/DECR")
	(net 24 "/nRF5340_Interface_MCU/DECUSB")
	(net 25 "/nRF5340_Interface_MCU/DECN")
	(net 26 "Net-(U5A-DECD)")
	(net 27 "/nRF5340_Interface_MCU/DECA")
	(net 28 "/nRF5340_Interface_MCU/IMCU_RESET")
	(net 29 "Net-(U6-GND)")
	(net 30 "SIM_1V8")
	(net 31 "Net-(D2-VCC)")
	(net 32 "VBUS'")
	(net 33 "unconnected-(D1-NC-Pad4)")
	(net 34 "SIM_RST")
	(net 35 "Net-(D1-DATA2_OUT)")
	(net 36 "SIM_CLK")
	(net 37 "Net-(D1-CLK_OUT)")
	(net 38 "SIM_IO")
	(net 39 "Net-(D1-DATA1_OUT)")
	(net 40 "IMCU_USB_D_N")
	(net 41 "IMCU_USB_D_P")
	(net 42 "/nRF9151_SiP/LTE_RF1")
	(net 43 "unconnected-(J3-Pad6)")
	(net 44 "unconnected-(J3-Pad9)")
	(net 45 "/nRF5340_Interface_MCU/IMCU_SWDIO")
	(net 46 "/nRF5340_Interface_MCU/IMCU_SWDCLK")
	(net 47 "unconnected-(J3-Pad7)")
	(net 48 "unconnected-(J3-Pad8)")
	(net 49 "Net-(J4-X)")
	(net 50 "Net-(J5-CC1)")
	(net 51 "unconnected-(J5-SBU1-PadA8)")
	(net 52 "unconnected-(J5-SBU2-PadB8)")
	(net 53 "Net-(J5-CC2)")
	(net 54 "unconnected-(J6-SIMVPP-PadC6)")
	(net 55 "Net-(J6-PadCD)")
	(net 56 "TRACE_DATA2")
	(net 57 "TRACE_CLK")
	(net 58 "unconnected-(J7-Pad10)")
	(net 59 "TRACE_DATA0")
	(net 60 "DBG_CMD")
	(net 61 "TRACE_DATA3")
	(net 62 "TRACE_DATA1")
	(net 63 "/nRF9151_Power_Supply/SW1")
	(net 64 "/nRF9151_Power_Supply/SW2")
	(net 65 "Net-(U3-AMP_IN)")
	(net 66 "Net-(U3-FIL_OUT)")
	(net 67 "/nRF9151_SiP/GPS_RF4")
	(net 68 "Net-(LED1-A)")
	(net 69 "Net-(LED1-C)")
	(net 70 "unconnected-(M1C-MAGPIO2-Pad23)")
	(net 71 "unconnected-(M1B-P0.07-Pad64)")
	(net 72 "unconnected-(M1D-RESERVED-Pad94)")
	(net 73 "unconnected-(M1C-SDATA-Pad27)")
	(net 74 "unconnected-(M1C-SIM_DET-Pad26)")
	(net 75 "unconnected-(M1D-RESERVED-Pad99)")
	(net 76 "unconnected-(M1D-RESERVED-Pad98)")
	(net 77 "nRF91_SWD_SWDCLK")
	(net 78 "FLAME_SENSE")
	(net 79 "FLAME_SENSE_D1")
	(net 80 "TWI_SCL")
	(net 81 "unconnected-(M1D-RESERVED-Pad100)")
	(net 82 "unconnected-(M1D-RESERVED-Pad103)")
	(net 83 "TWI1_SCL")
	(net 84 "unconnected-(M1D-RESERVED-Pad89)")
	(net 85 "unconnected-(M1D-RESERVED-Pad83)")
	(net 86 "EXT_MEM_CS")
	(net 87 "CO_SENSE")
	(net 88 "unconnected-(M1C-MAGPIO0-Pad21)")
	(net 89 "EXT_MEM_SCK")
	(net 90 "FLAME_SENSE_D2")
	(net 91 "unconnected-(M1D-RESERVED-Pad96)")
	(net 92 "NO2_SENSE")
	(net 93 "unconnected-(M1D-RESERVED-Pad33)")
	(net 94 "unconnected-(M1C-MAGPIO1-Pad22)")
	(net 95 "UART2_RXD")
	(net 96 "unconnected-(M1D-RESERVED-Pad90)")
	(net 97 "Net-(SB1-1)")
	(net 98 "unconnected-(M1D-RESERVED-Pad93)")
	(net 99 "TWI1_SDA")
	(net 100 "unconnected-(M1D-RESERVED-Pad85)")
	(net 101 "FLAME_SENSE_D4")
	(net 102 "FLAME_SENSE_D5")
	(net 103 "/nRF9151_SiP/COEX0")
	(net 104 "unconnected-(M1D-RESERVED-Pad88)")
	(net 105 "BAT_SENSE_A1")
	(net 106 "SMOKE_SENSE")
	(net 107 "unconnected-(M1D-RESERVED-Pad97)")
	(net 108 "unconnected-(M1D-RESERVED-Pad87)")
	(net 109 "unconnected-(M1D-RESERVED-Pad104)")
	(net 110 "unconnected-(M1D-RESERVED-Pad92)")
	(net 111 "unconnected-(M1C-SCLK-Pad28)")
	(net 112 "unconnected-(M1D-RESERVED-Pad81)")
	(net 113 "nRF91_SWD_SWDIO")
	(net 114 "unconnected-(M1A-AUX-Pad37)")
	(net 115 "EXT_MEM_MISO")
	(net 116 "unconnected-(M1C-VIO-Pad29)")
	(net 117 "PANEL_SEN0_A5")
	(net 118 "unconnected-(M1D-RESERVED-Pad102)")
	(net 119 "unconnected-(M1D-RESERVED-Pad82)")
	(net 120 "UART1_TXD")
	(net 121 "TWI_SDA")
	(net 122 "/nRF9151_SiP/COEX2")
	(net 123 "Net-(M1A-ENABLE)")
	(net 124 "unconnected-(M1D-RESERVED-Pad31)")
	(net 125 "unconnected-(M1D-RESERVED-Pad84)")
	(net 126 "unconnected-(M1D-RESERVED-Pad95)")
	(net 127 "PANEL_SEN1_A6")
	(net 128 "unconnected-(M1D-RESERVED-Pad91)")
	(net 129 "unconnected-(M1B-P0.08-Pad67)")
	(net 130 "VDD_3V3_EN")
	(net 131 "EXT_MEM_MOSI")
	(net 132 "VOC_SENSE")
	(net 133 "UART2_TXD")
	(net 134 "unconnected-(M1D-RESERVED-Pad86)")
	(net 135 "unconnected-(M1C-COEX1-Pad53)")
	(net 136 "unconnected-(M1D-RESERVED-Pad32)")
	(net 137 "UART1_RXD")
	(net 138 "TWI_SCL_3V3")
	(net 139 "TWI_SDA_3V3")
	(net 140 "unconnected-(P6-Pad8)")
	(net 141 "nRF91_SWD_RESET")
	(net 142 "unconnected-(P6-Pad7)")
	(net 143 "unconnected-(P7-Pad11)")
	(net 144 "unconnected-(P7-Pad13)")
	(net 145 "SWD0_SWDCLK")
	(net 146 "unconnected-(P8-Pad8)")
	(net 147 "SWD0_SWO")
	(net 148 "unconnected-(P8-Pad7)")
	(net 149 "unconnected-(P8-Pad9)")
	(net 150 "SWD0_SWDIO")
	(net 151 "SWD0_SELECT")
	(net 152 "SWD0_RESET")
	(net 153 "unconnected-(P14-A2-Pad3)")
	(net 154 "unconnected-(P14-A1-Pad1)")
	(net 155 "VBUS")
	(net 156 "Net-(Q1A-G1)")
	(net 157 "Net-(Q2A-G1)")
	(net 158 "VBAT")
	(net 159 "VBAT'")
	(net 160 "Net-(Q3A-D1)")
	(net 161 "USB_DETECT")
	(net 162 "Net-(Q7B-S2)")
	(net 163 "Net-(Q7A-D1)")
	(net 164 "/nRF9151_SiP/nRESET")
	(net 165 "/nRF5340_Interface_MCU/IMCU_LED")
	(net 166 "PMIC_TWI_SDA")
	(net 167 "VBAT_IN")
	(net 168 "PMIC_TWI_SCL")
	(net 169 "Net-(U1-VSET1)")
	(net 170 "Net-(U1-VSET2)")
	(net 171 "RESET_IN")
	(net 172 "/nRF5340_Interface_MCU/SWD_CTRL")
	(net 173 "Net-(U7-OE)")
	(net 174 "TWI1_SDA_3V3")
	(net 175 "TWI1_SCL_3V3")
	(net 176 "/nRF9151_Power_Supply/VBUSOUT")
	(net 177 "unconnected-(U1-GPIO3-Pad10)")
	(net 178 "unconnected-(U1-GPIO2-Pad9)")
	(net 179 "unconnected-(U1-SHPHLD-Pad15)")
	(net 180 "unconnected-(U1-LED2-Pad27)")
	(net 181 "unconnected-(U1-CC2-Pad24)")
	(net 182 "unconnected-(U1-GPIO0-Pad7)")
	(net 183 "unconnected-(U1-GPIO1-Pad8)")
	(net 184 "unconnected-(U1-GPIO4-Pad11)")
	(net 185 "unconnected-(U1-CC1-Pad23)")
	(net 186 "unconnected-(U1-LED0-Pad25)")
	(net 187 "unconnected-(U1-LED1-Pad26)")
	(net 188 "unconnected-(U2-NC-Pad4)")
	(net 189 "unconnected-(U4-IO2-Pad3)")
	(net 190 "unconnected-(U4-IO3-Pad7)")
	(net 191 "unconnected-(U5B-P0.08{slash}TRACEDATA[3]-PadAH2)")
	(net 192 "/nRF5340_Interface_MCU/SWD3_IO")
	(net 193 "unconnected-(U5A-DCCD-PadB10)")
	(net 194 "unconnected-(U5B-P0.20-PadAK16)")
	(net 195 "unconnected-(U5D-N.C.-PadA1)")
	(net 196 "/nRF5340_Interface_MCU/SWD3_SWO")
	(net 197 "unconnected-(U5B-P0.21-PadAL15)")
	(net 198 "unconnected-(U5B-P0.12{slash}TRACECLK-PadAK6)")
	(net 199 "unconnected-(U5D-N.C.-PadA31)")
	(net 200 "unconnected-(U5B-P0.11{slash}TRACEDATA[0]-PadAK4)")
	(net 201 "/nRF5340_Interface_MCU/SWD3_CLK")
	(net 202 "unconnected-(U5B-P0.28{slash}AIN7-PadAE31)")
	(net 203 "unconnected-(U5C-P1.09-PadAK26)")
	(net 204 "unconnected-(U5C-P1.01-PadP2)")
	(net 205 "unconnected-(U5B-P0.22-PadAK18)")
	(net 206 "unconnected-(U5A-DCCH-PadJ1)")
	(net 207 "/nRF5340_Interface_MCU/XC1")
	(net 208 "unconnected-(U5C-P1.13-PadA17)")
	(net 209 "unconnected-(U5D-N.C.-PadD2)")
	(net 210 "unconnected-(U5D-N.C.-PadAL31)")
	(net 211 "unconnected-(U5B-P0.16{slash}QSPI[3]-PadAL9)")
	(net 212 "unconnected-(U5A-DCC-PadA21)")
	(net 213 "unconnected-(U5D-N.C.-PadAL1)")
	(net 214 "unconnected-(U5C-P1.00-PadM2)")
	(net 215 "unconnected-(U5C-P1.10-PadR31)")
	(net 216 "unconnected-(U5C-P1.05-PadAK22)")
	(net 217 "unconnected-(U5B-P0.04{slash}AIN0-PadV2)")
	(net 218 "unconnected-(U5D-N.C.-PadF2)")
	(net 219 "unconnected-(U5B-P0.19-PadAL13)")
	(net 220 "unconnected-(U5B-P0.10{slash}TRACEDATA[1]-PadAK2)")
	(net 221 "unconnected-(U5B-P0.23-PadAK20)")
	(net 222 "unconnected-(U5D-N.C.-PadT2)")
	(net 223 "unconnected-(U5D-N.C.-PadAG31)")
	(net 224 "unconnected-(U5B-P0.25{slash}AIN4-PadAK28)")
	(net 225 "unconnected-(U5C-P1.15-PadB14)")
	(net 226 "unconnected-(U5C-P1.07-PadAK24)")
	(net 227 "unconnected-(U5B-P0.07{slash}AIN3-PadAD2)")
	(net 228 "unconnected-(U5B-P0.18{slash}QSPI_CS-PadAK14)")
	(net 229 "/nRF5340_Interface_MCU/SWD3_RESET")
	(net 230 "unconnected-(U5B-P0.27{slash}AIN6-PadAK30)")
	(net 231 "unconnected-(U5B-P0.13{slash}QSPI[0]-PadAL5)")
	(net 232 "unconnected-(U5B-P0.09{slash}TRACEDATA[2]-PadAJ1)")
	(net 233 "unconnected-(U5B-P0.14{slash}QSPI[1]-PadAK8)")
	(net 234 "/nRF5340_Interface_MCU/XC2")
	(net 235 "unconnected-(U6-NO3-Pad7)")
	(net 236 "unconnected-(U6-NO4-Pad11)")
	(net 237 "unconnected-(U6-NO2-Pad3)")
	(net 238 "unconnected-(P14-A5-Pad9)")
	(net 239 "unconnected-(P14-D3-Pad6)")
	(net 240 "unconnected-(P14-A4-Pad7)")
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 186.31 80.96 -90)
		(property "Reference" "C11"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C_NC"
		(layer "F.Cu")
		(at 165.48 71.19 90)
		(property "Reference" "R37"
			(at -1.45186 -0.01543 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -1.976311 -0.1397 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C_NC"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-N.C."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100107"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100107"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.0608 -1.825409 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "RESET_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 172.48 86.85)
		(property "Reference" "C38"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/nRF5340_Interface_MCU/DECN")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 207.7 74.47)
		(property "Reference" "C20"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-N.C."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Cap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200001"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200001"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C_NC*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(C20-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 156.755 79.52 -90)
		(property "Reference" "C4"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "VBAT_PWR")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:INDC1005X04L_NC"
		(layer "F.Cu")
		(at 209.62 64.92 180)
		(property "Reference" "L8"
			(at 0.10867 -0.82555 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -0.6985 2.91719 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC1005X04L_NC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0402-N.C."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-11-24"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-11-24"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300037"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300037"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC1005X04L_NC*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.06759 -0.014391 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.475 0 270)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "/nRF9151_SiP/GPS_RF4")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.475 0 270)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "FP:RESC1005X04L"
		(layer "F.Cu")
		(at 210.08 63.53 90)
		(property "Reference" "R28"
			(at 0.08966 0.80339 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0R"
			(at -3.1431 -0.113 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC1005X04L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±5%, 0.063W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0402-0R"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-070RL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2009-11-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2009-05-08"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "0R"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 5%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Farnell"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "146-9661"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "27049000"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007128"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100109"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100109"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.04792 0.010821 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.5 0 180)
			(size 0.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "/nRF9151_SiP/GPS_RF4")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.5 0 180)
			(size 0.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/nRF9151_SiP/GPS_RF5")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0402-1.step"
			(offset
				(xyz 0.00006 0.00006 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:DSGP.1575.18.4.C.02"
		(layer "F.Cu")
		(at 198.325 62.05 90)
		(property "Reference" "A2"
			(at 0.08232 -10.275 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DSGP.1575.18"
			(at -9.9441 11.526711 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:DSGP.1575.18.4.C.02"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "18 x 18 mm Low Profile GPS L1 / GALILEO E1 Passive Patch Antenna"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "DSGP.1575.18.4.C.02"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Taoglas"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "DSGP.1575.18.4.C.02"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://www.taoglas.com/datasheets/DSGP.1575.18.4.A.02.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/product-detail/en/taoglas-limited/DSGP.1575.18.4.A.02/931-1511-1-ND/8275289"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.taoglas.com/product/18184mm-dsgp-1575-184-gps-l1-galileo-e1-ceramic-patch-copy/?compare=16929"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "DSGP.1575.18.4.C.02"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-01-01"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-01-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "DSGP.1575.18"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007687"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Antennas"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100700073"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100700073"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSGP.1575.18.4.C.02*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "COPPER KEEPOUT"
			(at -1.6755 9.64998 180)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "${REFERENCE}"
			(at -1.942565 -3.86126 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at 0 8.55 270)
			(size 2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/nRF9151_SiP/GPS_RF5")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.3)
			(solder_paste_margin -0.25)
		)
		(pad "2" smd rect
			(at -6.75001 -6.75 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(pad "2" smd rect
			(at -6.75001 0 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(pad "2" smd rect
			(at -6.75001 6.75 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(pad "2" smd rect
			(at 0 -6.75 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(pad "2" smd rect
			(at 6.75 -6.75 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(pad "2" smd rect
			(at 6.75 0 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(pad "2" smd rect
			(at 6.75 6.75 270)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1)
			(solder_paste_margin -0.6)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 204.825 64.05002) (xy 208.325 64.05) (xy 208.325 60.05) (xy 204.825 60.05002)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 204.980381 60.208107) (xy 204.983087 60.205401) (xy 204.986913 60.205401) (xy 204.989619 60.208107)
					(xy 204.99 60.21002) (xy 204.99 63.89001) (xy 204.989619 63.891923) (xy 204.986913 63.894629) (xy 204.983087 63.894629)
					(xy 204.980381 63.891923) (xy 204.98 63.89001) (xy 204.98 60.21002)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 208.160371 60.208107) (xy 208.163077 60.205401) (xy 208.166903 60.205401) (xy 208.169609 60.208107)
					(xy 208.16999 60.21002) (xy 208.16999 60.79001) (xy 208.169609 60.791923) (xy 208.166903 60.794629)
					(xy 208.163077 60.794629) (xy 208.160371 60.791923) (xy 208.15999 60.79001) (xy 208.15999 60.21002)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 208.160371 63.308097) (xy 208.163077 63.305391) (xy 208.166903 63.305391) (xy 208.169609 63.308097)
					(xy 208.16999 63.31001) (xy 208.16999 63.89001) (xy 208.169609 63.891923) (xy 208.166903 63.894629)
					(xy 208.163077 63.894629) (xy 208.160371 63.891923) (xy 208.15999 63.89001) (xy 208.15999 63.31001)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 208.166903 60.205401) (xy 208.169609 60.208107) (xy 208.169609 60.211933) (xy 208.166903 60.214639)
					(xy 208.16499 60.21502) (xy 204.985 60.21502) (xy 204.983087 60.214639) (xy 204.980381 60.211933)
					(xy 204.980381 60.208107) (xy 204.983087 60.205401) (xy 204.985 60.20502) (xy 208.16499 60.20502)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 208.166903 63.885391) (xy 208.169609 63.888097) (xy 208.169609 63.891923) (xy 208.166903 63.894629)
					(xy 208.16499 63.89501) (xy 204.985 63.89501) (xy 204.983087 63.894629) (xy 204.980381 63.891923)
					(xy 204.980381 63.888097) (xy 204.983087 63.885391) (xy 204.985 63.88501) (xy 208.16499 63.88501)
				)
			)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/SGGP.18A v5.step"
			(offset
				(xyz -0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 211.45 64.22 90)
		(property "Reference" "C30"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U3-VCC)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 161.955 79.52 -90)
		(property "Reference" "C10"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "VDD_3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:AMPHENOL_10114829-10102LF"
		(layer "F.Cu")
		(at 174.4625 53.525 180)
		(property "Reference" "P1"
			(at 0.05 -3.985 180)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x2, Angled"
			(at 12.75 2.965 180)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:AMPHENOL_10114829-10102LF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "10114829-10102LF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "10114829-10102LF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x2, Angled"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "10114829-10102LF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -0.625 0 180)
			(size 1.108 1.108)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VBAT_PWR")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0.625 0 180)
			(size 1.108 1.108)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:HDR_2x10-SMD-1.27mm-K-SWD"
		(layer "F.Cu")
		(at 182.65 66.5 -90)
		(property "Reference" "P7"
			(at 0.125 3.76767 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin Header 2x10, 1.27mm, SWD"
			(at -8.96239 -3.0353 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:HDR_2x10-SMD-1.27mm-K-SWD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header 2x10, 1.27mm (50mil), SMD, Keying Shroud, Removed Pin 7"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin Header 2x10 SMD, 1.27mm, KS, SWD (Cabcon)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "WCON"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "3132-20MS0BK00R3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-12-14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-12-14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin Header 2x10, 1.27mm, SWD"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "HDR_2x10-SMD-1.27mm-SWD"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not Mounted"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "3132-20MS0BK00R3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500841"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "19"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "kod1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500841,100500280"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*HDR_2x10-SMD-1.27mm-K-SWD*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "1"
			(at -5.875 4.57446 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.03527 0.037331 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -5.715 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -5.715 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "nRF91_SWD_SWDIO")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -4.445 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -4.445 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "nRF91_SWD_SWDCLK")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -3.175 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -3.175 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "TRACE_DATA0")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -1.905 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "DBG_CMD")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -0.635 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -0.635 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "nRF91_SWD_RESET")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0.635 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 143 "unconnected-(P7-Pad11)")
			(pinfunction "11")
			(pintype "passive+no_connect")
		)
		(pad "12" smd rect
			(at 0.635 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "TRACE_CLK")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 1.905 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 144 "unconnected-(P7-Pad13)")
			(pinfunction "13")
			(pintype "passive+no_connect")
		)
		(pad "14" smd rect
			(at 1.905 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "TRACE_DATA0")
			(pinfunction "14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 3.175 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 3.175 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "TRACE_DATA1")
			(pinfunction "16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 4.445 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 4.445 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "TRACE_DATA2")
			(pinfunction "18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 5.715 1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 5.715 -1.95 270)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "TRACE_DATA3")
			(pinfunction "20")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/FTSH-110-01-L-DV-007-K-TR.stp"
			(offset
				(xyz 0.00012 0.00007 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "FP:AMPHENOL_G800W305018EU"
		(layer "F.Cu")
		(at 142.0625 94.99 180)
		(property "Reference" "P11"
			(at -0.885 -3.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x3, Straight"
			(at 9.91 3.135 0)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:AMPHENOL_G800W305018EU"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol ICC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "G800W305018EU"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x3, Straight"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "VOC_SENSE")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "VDD_3V3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 181.72 85.55)
		(property "Reference" "R45"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 174 "TWI1_SDA_3V3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "VDD_3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 161.275 89.96)
		(property "Reference" "R35"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "120R"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-120"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-07120RL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "120R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000000880"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100028"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107076"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100028"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "Net-(LED1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "VDD_3V0")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 207.73 73.11)
		(property "Reference" "C21"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "39pF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±1%, 25V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-39p"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM0335C1E390FA01"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "39pF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "25V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001668"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200039"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200039"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C_NC*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "VDD_GNSS")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 164.6 80.15 90)
		(property "Reference" "C44"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 162.24 82.97 180)
		(property "Reference" "C48"
			(at -1.404825 -0.13896 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:INDC1005X04L_NC"
		(layer "F.Cu")
		(at 209.38 74.46 180)
		(property "Reference" "L3"
			(at 0.10867 -0.82555 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -0.6985 2.91719 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC1005X04L_NC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0402-N.C."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-11-24"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-11-24"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300037"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300037"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC1005X04L_WW*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.06759 -0.014391 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.475 0 270)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/nRF9151_SiP/GPS_RF2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.475 0 270)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(C20-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 164.25 61.75 90)
		(property "Reference" "R43"
			(at -0.94747 -0.02966 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5k1"
			(at -3.42519 -0.1905 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-5k1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100565"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-075K1L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-04-20"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-04-20"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "5k1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26192285"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100565"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "Net-(J5-CC1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:SOT95P285X140-5N"
		(layer "F.Cu")
		(at 159.355 80.12)
		(property "Reference" "U2"
			(at 0.66442 -2.53029 0)
			(layer "F.SilkS")
		)
		(property "Value" "AP2112K-3.3TRG1 "
			(at 5.96176 2.45355 0)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:SOT95P285X140-5N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra low capacitance double rail-to-rail ESD protection diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "AP2112K-3.3TRG1 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Diodes Incorporated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "AP2112K-3.3TRG1 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2012-06-11"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "AP2112K-3.3TRG1 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "10069015"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SOT-143B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009951"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.farnell.com/datasheets/109718.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "568-4140-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Farnell"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "152-4157"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300082"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26313940"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300082"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOT190P230X110-4L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.185 -0.95)
			(size 1.35 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.075)
			(net 6 "VBAT_PWR")
			(pinfunction "IN")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -1.185 0)
			(size 1.35 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.075)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -1.185 0.95)
			(size 1.35 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.075)
			(net 130 "VDD_3V3_EN")
			(pinfunction "EN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at 1.185 0.95)
			(size 1.35 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.075)
			(net 188 "unconnected-(U2-NC-Pad4)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at 1.185 -0.95)
			(size 1.35 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.075)
			(net 9 "VDD_3V3")
			(pinfunction "OUT")
			(pintype "power_out")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 154 64.3 -90)
		(property "Reference" "R2"
			(at -0.94747 -0.02966 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M0"
			(at -3.42519 -0.1905 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1M0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1M0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-071ML"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001418"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100093"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107108"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100093"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "VBAT'")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:HDR_2x5-SMD-1.27mm-K"
		(layer "F.Cu")
		(at 174.26 63.12)
		(property "Reference" "P8"
			(at 3.68665 0.038825 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin Header 2x5, 1.27mm"
			(at -3.0607 7.08279 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:HDR_2x5-SMD-1.27mm-K"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header 2x5, 1.27mm (50mil), SMD, Keying Shroud"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin Header 2x5 SMD, 1.27mm, KS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "WCON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "3132-10MS0BK00R1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "HDR_2x5-SMD-1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-04-21"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-01-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin Header 2x5, 1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "55010009"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009968"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not Mounted"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "~{\\}hiz~{z}pr~{o}app971~{7}Datashee~{t}connector~{s}W-CO~{N}3132-XXMXXBK00XX.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "3132-10MS0BK00R1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "FTSH-105-01-F-DV-K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500261"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500261"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*HDR_2x5-SMD-1.27mm-K*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "1"
			(at -2.41291 3.688415 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd rect
			(at -2.54 1.95001)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.54 -1.95)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "SWD0_SWDIO")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.27 1.95001)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 151 "SWD0_SELECT")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.27 -1.95)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 145 "SWD0_SWDCLK")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 1.95001)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0 -1.95)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "SWD0_SWO")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 1.27 1.95001)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 148 "unconnected-(P8-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 1.27 -1.95)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "unconnected-(P8-Pad8)")
			(pinfunction "8")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at 2.54 1.95001)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 149 "unconnected-(P8-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
		)
		(pad "10" smd rect
			(at 2.54 -1.95)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 152 "SWD0_RESET")
			(pinfunction "10")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/Samtec-FTSH-105-01-F-DV-K.step"
			(offset
				(xyz 0.00008 0.00008 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 187.03 80.96 -90)
		(property "Reference" "C13"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 169.04 80.15 90)
		(property "Reference" "C46"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1608X06L"
		(layer "F.Cu")
		(at 148.44 89.78 -90)
		(property "Reference" "C7"
			(at -1.16796 -1.27709 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10µF"
			(at -1.35891 2.306511 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1608X06L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7T, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0603-10µ-10V-X7T-GRM188D71A106MA73"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200414"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM188D71A106MA73"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://no.mouser.com/datasheet/2/281/murata_03052018_GRM_Series_1-1310166.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-22"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-09-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10µF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10VDC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-7200-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-GRM188D71A106MA3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004696"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200414"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.25 -0.162338 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Capacitor 0603.step"
			(offset
				(xyz -0.00005 -0.43011 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 215.25 64.30251 -90)
		(property "Reference" "R27"
			(at -0.94747 -0.02966 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at -3.42519 -0.1905 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1k0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-071KL"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1k"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000005786"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100043"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100043"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "/nRF9151_SiP/COEX0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U3-VEN)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 182.54 58.98 180)
		(property "Reference" "R20"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2k"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "ERJ-1GNF2001C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-072KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "2k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "PANEL_SEN1_A6")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 175.9125 86.96 90)
		(property "Reference" "C52"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1608X06L"
		(layer "F.Cu")
		(at 155.805 91.74 -90)
		(property "Reference" "C8"
			(at -1.16796 -1.27709 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10µF"
			(at -1.35891 2.306511 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1608X06L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7T, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0603-10µ-10V-X7T-GRM188D71A106MA73"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200414"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM188D71A106MA73"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://no.mouser.com/datasheet/2/281/murata_03052018_GRM_Series_1-1310166.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-22"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-09-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10µF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10VDC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-7200-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-GRM188D71A106MA3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004696"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200414"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.25 -0.162338 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "VDD_3V0")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Capacitor 0603.step"
			(offset
				(xyz -0.00005 -0.43011 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1608X06L"
		(layer "F.Cu")
		(at 153.115 80.42 -90)
		(property "Reference" "C9"
			(at -1.16796 -1.27709 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10µF"
			(at -1.35891 2.306511 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1608X06L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7T, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0603-10µ-10V-X7T-GRM188D71A106MA73"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200414"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM188D71A106MA73"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://no.mouser.com/datasheet/2/281/murata_03052018_GRM_Series_1-1310166.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-22"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-09-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10µF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10VDC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-7200-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-GRM188D71A106MA3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004696"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200414"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.25 -0.162338 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/nRF9151_Power_Supply/VSYS")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Capacitor 0603.step"
			(offset
				(xyz -0.00005 -0.43011 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 160.25 61.75 90)
		(property "Reference" "C54"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-10n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GMD033R61A103KA01D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000003480"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200067"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26621779"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200067"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1005X04L*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(D2-VCC)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CONN_BM04B-SRSS-TB_SPK"
		(layer "F.Cu")
		(at 182.21995 101.21315 180)
		(tags "PRT-16766 ")
		(property "Reference" "P3"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x4, Angled"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:CONN_BM04B-SRSS-TB_SPK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Sparkfun"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "PRT-16766"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x4, Angled"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "TWI_SDA_3V3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "TWI_SCL_3V3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 204.83 77.78 180)
		(property "Reference" "R24"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M0"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1M0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-071ML"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1M0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001418"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100093"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107108"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100093"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "/nRF9151_SiP/COEX0")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 172.68 81.39)
		(property "Reference" "R33"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "ERJ-1GNF2001C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-072KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "2k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(U5A-VBUS)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "VBUS")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 190.64 77.6 180)
		(property "Reference" "C18"
			(at -1.404825 -0.13896 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(M1C-nRESET)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 219.86 68.96)
		(property "Reference" "C28"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.5pF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±0.1pF, 25V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-3.5p"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GJM0335C1H3R5BB01E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-02-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-02-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "3.5pF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "25V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001469"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200023"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200023"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(C26-Pad2)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(A1-Pad1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 177.01 75.8 -90)
		(property "Reference" "C32"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 157.435 83.59)
		(property "Reference" "R17"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "150k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-150k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100082"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-07150KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "150k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001422"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100082"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 170 "Net-(U1-VSET2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 172.48 86.07)
		(property "Reference" "C33"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 172.48 85.27)
		(property "Reference" "C40"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U5A-DECD)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:SKY65943-11"
		(layer "F.Cu")
		(at 211.72 67.13 -90)
		(property "Reference" "U3"
			(at -0.18593 -1.77435 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SKY65943-11"
			(at 0.3429 2.44221 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SKY65943-11"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "GNSS Low-Noise Amplifier Front-End Module with Integrated Pre-Filter and Post-Filter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "SKY65943-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Skyworks"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "SKY65943-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "MCM-10"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "SKY65943-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "http://www.skyworksinc.com/uploads/documents/SKY65943_11_204404F.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/product-detail/en/skyworks-solutions-inc/SKY65943-11/863-2032-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.skyworksinc.com/Product/3579/SKY65943-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "863-2032-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "873-SKY65943-11"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000002997"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101900584"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Misc_ICs"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "10"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101900584"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SKY65943-11*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.060309 -0.07815 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -1.1875 -1.1435 270)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at -1.1875 -0.5 270)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U3-VEN)")
			(pinfunction "VEN")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at -1.1875 0 270)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U3-VCC)")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at -1.1875 0.5 270)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at -1.1875 1.1435 270)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "/nRF9151_SiP/GPS_RF4")
			(pinfunction "RF_IN")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at 1.18751 1.1435 270)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at 1.18751 0.5 270)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U3-FIL_OUT)")
			(pinfunction "FIL_OUT")
			(pintype "output")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at 1.18751 0 270)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U3-AMP_IN)")
			(pinfunction "AMP_IN")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "9" smd rect
			(at 1.18751 -0.5 270)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "10" smd rect
			(at 1.18751 -1.1435 270)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/nRF9151_SiP/GPS_RF3")
			(pinfunction "RF_OUT")
			(pintype "output")
			(solder_mask_margin 0.05)
		)
		(pad "11" smd rect
			(at 0 0 270)
			(size 1.45 2.802)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin -5)
			(solder_paste_margin -2)
		)
	)
	(footprint "FP:CAPC1608X06L"
		(layer "F.Cu")
		(at 185.31 80.89 90)
		(property "Reference" "C15"
			(at -1.16796 -1.27709 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10µF"
			(at -1.35891 2.306511 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1608X06L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7T, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0603-10µ-10V-X7T-GRM188D71A106MA73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200414"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM188D71A106MA73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://no.mouser.com/datasheet/2/281/murata_03052018_GRM_Series_1-1310166.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-22"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-09-11"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10µF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10VDC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-7200-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-GRM188D71A106MA3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004696"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200414"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.25 -0.162338 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0 180)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0 180)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Capacitor 0603.step"
			(offset
				(xyz -0.00005 -0.43011 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 154.705 81.04 90)
		(property "Reference" "R16"
			(at -0.94747 -0.02966 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47k"
			(at -3.42519 -0.1905 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-47k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100076"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-0747KL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "47k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100076"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "Net-(U1-VSET1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 168.19 64.27 90)
		(property "Reference" "R31"
			(at -0.94747 -0.02966 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at -3.42519 -0.1905 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D10KL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001255"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100065"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107101"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100065"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "Net-(Q7B-S2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 154.26 63.35)
		(property "Reference" "R13"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "Net-(Q2A-G1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 156.092505 66.51)
		(property "Reference" "R3"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M0"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1M0"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-071ML"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1M0"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001418"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100093"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107108"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100093"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "Net-(Q3A-D1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1005X04L"
		(layer "F.Cu")
		(at 172.89 83.1)
		(property "Reference" "C37"
			(at -0.16053 -1.29174 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7µF"
			(at -0.7239 2.89179 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1005X04L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, 10V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0402-4µ7-10V-X5R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM155R61A475MEAAD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R61A475MEAA-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM155R61A475MEAAD/490-14306-1-ND/6234742"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/capacitor/product/GRM155R61A475MEAA%23.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-10-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-10-04"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4.7µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-14306-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200415"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200415"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.4318 0.189738 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/nRF5340_Interface_MCU/DECUSB")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0402(1005M) Cap.step"
			(offset
				(xyz 0.00007 0.00007 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 153.12 58.29 90)
		(property "Reference" "R34"
			(at -0.94747 -0.02966 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "/nRF5340_Interface_MCU/IMCU_RESET")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 149.66 64.01 180)
		(property "Reference" "R5"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "VBAT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:INDC0603X03L_C"
		(layer "F.Cu")
		(at 217.56 68.98)
		(property "Reference" "L5"
			(at 0.128005 0.67094 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5nH"
			(at -0.7239 2.89179 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, 1000mA, ±0.1ｎH, 50mOhm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0201-1n5-HQ-Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "LQP03HQ1N5B02"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/P02/JELF243C-0021.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/inductor/product/LQP03HQ1N5B02%23.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2018-10-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-10-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.5nH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "-55°C ~ 125°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13881-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300202"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300202"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.047615 -0.484389 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28492 -0.00008 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/nRF9151_SiP/ANT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28507 -0.00008 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(C26-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-smt_inductor-0201.step"
			(offset
				(xyz 0.00017 0.00017 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 169.31 89.25 -90)
		(property "Reference" "C43"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CONN_BM04B-SRSS-TB_SPK"
		(layer "F.Cu")
		(at 152.03995 101.18315 180)
		(tags "PRT-16766 ")
		(property "Reference" "P5"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x4, Angled"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:CONN_BM04B-SRSS-TB_SPK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Sparkfun"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "PRT-16766"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x4, Angled"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "VDD_3V3")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "TWI_SDA_3V3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "TWI_SCL_3V3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
	)
	(footprint "FP:LGA50P1210X1110X130-113N"
		(layer "F.Cu")
		(at 198.04 78.526005 -90)
		(property "Reference" "M1"
			(at -6.37527 3.950005 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "nRF9151-LACAA0A"
			(at 10.480802 2.22361 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:LGA50P1210X1110X130-113N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low power System-in-Package with integrated LTE-M/NB-IoT modem and GPS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "nRF9151-LACAA0A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Nordic_Devices"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "kod1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Nordic Semiconductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "nRF9151-LACAA0A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2024-04-29"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2024-04-29"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "113"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LGA-113"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "nRF9151-LACAA0A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Nordic Semiconductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "nRF9151-LACAA0A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LGA50P1210X1110X130-113N*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${VALUE}"
			(at 0.15 0.0318 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "${REFERENCE}"
			(at 0.149995 0.0318 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "" smd custom
			(at -5.35 5.15)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -0.7 0) (xy -0.7 0.69999) (xy -0.25 0.69999) (xy -0.00001 0.45)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd rect
			(at -5 5.625 90)
			(size 0.7 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin -5)
			(solder_paste_margin -2147.483637)
		)
		(pad "2" smd rect
			(at -4.25037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "FLAME_SENSE")
			(pinfunction "P0.20")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at -3.75037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "nRF91_SWD_SWDCLK")
			(pinfunction "SWDCLK")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at -3.25037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "nRF91_SWD_SWDIO")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at -2.75037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "TRACE_CLK")
			(pinfunction "P0.21")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at -2.25037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "TRACE_DATA0")
			(pinfunction "P0.22")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at -1.75037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at -1.25037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "TRACE_DATA1")
			(pinfunction "P0.23")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "9" smd rect
			(at -0.75037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(M1C-nRESET)")
			(pinfunction "nRESET")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "10" smd rect
			(at -0.25037 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "Net-(M1A-ENABLE)")
			(pinfunction "ENABLE")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "11" smd rect
			(at 0.24963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "TRACE_DATA2")
			(pinfunction "P0.24")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "12" smd rect
			(at 0.74963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "TRACE_DATA3")
			(pinfunction "P0.25")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "13" smd rect
			(at 1.24963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "14" smd rect
			(at 1.74963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(M1A-VDD)")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "15" smd rect
			(at 2.24963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "16" smd rect
			(at 2.74963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "SIM_RST")
			(pinfunction "SIM_RST")
			(pintype "output")
			(solder_mask_margin 0.05)
		)
		(pad "17" smd rect
			(at 3.24963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "SIM_IO")
			(pinfunction "SIM_IO")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "18" smd rect
			(at 3.74963 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "SIM_CLK")
			(pinfunction "SIM_CLK")
			(pintype "output")
			(solder_mask_margin 0.05)
		)
		(pad "19" smd rect
			(at 4.24999 5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "SIM_1V8")
			(pinfunction "SIM_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "20" smd rect
			(at 5 5.5)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "21" smd rect
			(at 5.125 4.75 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "unconnected-(M1C-MAGPIO0-Pad21)")
			(pinfunction "MAGPIO0")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "22" smd rect
			(at 5.125 4.25 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "unconnected-(M1C-MAGPIO1-Pad22)")
			(pinfunction "MAGPIO1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "23" smd rect
			(at 5.125 3.74997 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "unconnected-(M1C-MAGPIO2-Pad23)")
			(pinfunction "MAGPIO2")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "24" smd rect
			(at 5.125 3.24997 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/nRF9151_SiP/DEC0")
			(pinfunction "DEC0")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "25" smd rect
			(at 5.125 2.74997 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "26" smd rect
			(at 5.125 2.24997 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "unconnected-(M1C-SIM_DET-Pad26)")
			(pinfunction "SIM_DET")
			(pintype "input+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "27" smd rect
			(at 5.125 1.74997 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "unconnected-(M1C-SDATA-Pad27)")
			(pinfunction "SDATA")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "28" smd rect
			(at 5.125 1.25 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "unconnected-(M1C-SCLK-Pad28)")
			(pinfunction "SCLK")
			(pintype "output+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "29" smd rect
			(at 5.125 0.75 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "unconnected-(M1C-VIO-Pad29)")
			(pinfunction "VIO")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "30" smd rect
			(at 5.125 0.25 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "31" smd rect
			(at 5.125 -0.25 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "unconnected-(M1D-RESERVED-Pad31)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "32" smd rect
			(at 5.125 -0.75 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 136 "unconnected-(M1D-RESERVED-Pad32)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "33" smd rect
			(at 5.125 -1.25002 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "unconnected-(M1D-RESERVED-Pad33)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "34" smd rect
			(at 5.125 -1.75003 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "35" smd rect
			(at 5.125 -2.25003 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "/nRF9151_SiP/LTE_RF1")
			(pinfunction "ANT")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "36" smd rect
			(at 5.125 -2.75003 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "37" smd rect
			(at 5.125 -3.25003 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "unconnected-(M1A-AUX-Pad37)")
			(pinfunction "AUX")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "38" smd rect
			(at 5.125 -3.75002 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "39" smd rect
			(at 5.125 -4.25003 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "40" smd rect
			(at 5.125 -4.75003 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "41" smd rect
			(at 5 -5.5)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "42" smd rect
			(at 4.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/nRF9151_SiP/GPS_RF1")
			(pinfunction "GPS")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "43" smd rect
			(at 3.75 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "44" smd rect
			(at 3.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 137 "UART1_RXD")
			(pinfunction "P0.26")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "45" smd rect
			(at 2.75 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "UART1_TXD")
			(pinfunction "P0.27")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "46" smd rect
			(at 2.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "47" smd rect
			(at 1.75 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "UART2_RXD")
			(pinfunction "P0.28")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "48" smd rect
			(at 1.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "UART2_TXD")
			(pinfunction "P0.29")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "49" smd rect
			(at 0.75 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "TWI_SDA")
			(pinfunction "P0.30")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "50" smd rect
			(at 0.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "TWI_SCL")
			(pinfunction "P0.31")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "51" smd rect
			(at -0.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "52" smd rect
			(at -0.75001 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "/nRF9151_SiP/COEX0")
			(pinfunction "COEX0")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "53" smd rect
			(at -1.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "unconnected-(M1C-COEX1-Pad53)")
			(pinfunction "COEX1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "54" smd rect
			(at -1.75 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 122 "/nRF9151_SiP/COEX2")
			(pinfunction "COEX2")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "55" smd rect
			(at -2.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "56" smd rect
			(at -2.75 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 130 "VDD_3V3_EN")
			(pinfunction "P0.00")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "57" smd rect
			(at -3.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "FLAME_SENSE_D1")
			(pinfunction "P0.01")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "58" smd rect
			(at -3.75 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "FLAME_SENSE_D2")
			(pinfunction "P0.02")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "59" smd rect
			(at -4.25 -5.625)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "FLAME_SENSE_D4")
			(pinfunction "P0.03")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "60" smd rect
			(at -5 -5.5)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "61" smd rect
			(at -5.12501 -4.75 90)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "TWI1_SCL")
			(pinfunction "P0.04")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "62" smd rect
			(at -5.12501 -4.25 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "TWI1_SDA")
			(pinfunction "P0.05")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "63" smd rect
			(at -5.12501 -3.74997 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "FLAME_SENSE_D5")
			(pinfunction "P0.06")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "64" smd rect
			(at -5.12501 -3.24997 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "unconnected-(M1B-P0.07-Pad64)")
			(pinfunction "P0.07")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "65" smd rect
			(at -5.12501 -2.74997 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD_GPIO")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "66" smd rect
			(at -5.12501 -2.24997 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "67" smd rect
			(at -5.12501 -1.74998 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 129 "unconnected-(M1B-P0.08-Pad67)")
			(pinfunction "P0.08")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "68" smd rect
			(at -5.12501 -1.24997 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "EXT_MEM_SCK")
			(pinfunction "P0.09")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "69" smd rect
			(at -5.12501 -0.75 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "EXT_MEM_CS")
			(pinfunction "P0.10")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "70" smd rect
			(at -5.12501 -0.25 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 131 "EXT_MEM_MOSI")
			(pinfunction "P0.11")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "71" smd rect
			(at -5.12501 0.25 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "72" smd rect
			(at -5.12501 0.75 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "EXT_MEM_MISO")
			(pinfunction "P0.12")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "73" smd rect
			(at -5.12501 1.25 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "CO_SENSE")
			(pinfunction "P0.13")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "74" smd rect
			(at -5.12501 1.75 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "BAT_SENSE_A1")
			(pinfunction "P0.14")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "75" smd rect
			(at -5.12501 2.25 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "NO2_SENSE")
			(pinfunction "P0.15")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "76" smd rect
			(at -5.12501 2.75 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "77" smd rect
			(at -5.12501 3.25 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 132 "VOC_SENSE")
			(pinfunction "P0.16")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "78" smd rect
			(at -5.12501 3.75 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 106 "SMOKE_SENSE")
			(pinfunction "P0.17")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "79" smd rect
			(at -5.12501 4.25 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "PANEL_SEN0_A5")
			(pinfunction "P0.18")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "80" smd rect
			(at -5.12501 4.75 270)
			(size 0.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "PANEL_SEN1_A6")
			(pinfunction "P0.19")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "81" smd rect
			(at -3.40001 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "unconnected-(M1D-RESERVED-Pad81)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "82" smd rect
			(at -2.85 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 119 "unconnected-(M1D-RESERVED-Pad82)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "83" smd rect
			(at -2.30001 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "unconnected-(M1D-RESERVED-Pad83)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "84" smd rect
			(at -0.55 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 125 "unconnected-(M1D-RESERVED-Pad84)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "85" smd rect
			(at 0 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 100 "unconnected-(M1D-RESERVED-Pad85)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "86" smd rect
			(at 0.54999 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "unconnected-(M1D-RESERVED-Pad86)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "87" smd rect
			(at 2.3 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "unconnected-(M1D-RESERVED-Pad87)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "88" smd rect
			(at 2.84999 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 104 "unconnected-(M1D-RESERVED-Pad88)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "89" smd rect
			(at 3.4 4.1 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "unconnected-(M1D-RESERVED-Pad89)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "90" smd rect
			(at 2.15 0.55 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "unconnected-(M1D-RESERVED-Pad90)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "91" smd rect
			(at 2.15 0 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "unconnected-(M1D-RESERVED-Pad91)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "92" smd rect
			(at 2.15 -0.55 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "unconnected-(M1D-RESERVED-Pad92)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "93" smd rect
			(at 3.4 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "unconnected-(M1D-RESERVED-Pad93)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "94" smd rect
			(at 2.84999 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "unconnected-(M1D-RESERVED-Pad94)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "95" smd rect
			(at 2.3 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 126 "unconnected-(M1D-RESERVED-Pad95)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "96" smd rect
			(at 0.54999 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "unconnected-(M1D-RESERVED-Pad96)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "97" smd rect
			(at 0 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "unconnected-(M1D-RESERVED-Pad97)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "98" smd rect
			(at -0.55 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "unconnected-(M1D-RESERVED-Pad98)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "99" smd rect
			(at -2.30001 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "unconnected-(M1D-RESERVED-Pad99)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "100" smd rect
			(at -2.85 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "unconnected-(M1D-RESERVED-Pad100)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "101" smd rect
			(at -3.40001 -4.1 90)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "Net-(SB1-1)")
			(pinfunction "RESERVED")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "102" smd rect
			(at -2.15001 -0.55 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 118 "unconnected-(M1D-RESERVED-Pad102)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "103" smd rect
			(at -2.15001 0 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "unconnected-(M1D-RESERVED-Pad103)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "104" smd rect
			(at -2.15001 0.55 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "unconnected-(M1D-RESERVED-Pad104)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "105" smd rect
			(at -2.85 2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "106" smd rect
			(at 0 2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "107" smd rect
			(at 2.84999 2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "108" smd rect
			(at 3.57499 0)
			(size 1.6 1.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "109" smd rect
			(at 2.84999 -2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "110" smd rect
			(at 0 -2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "111" smd rect
			(at -2.85 -2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "112" smd rect
			(at -3.57501 0)
			(size 1.6 1.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "113" smd rect
			(at 0 0)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 181.81 58.08 90)
		(property "Reference" "R18"
			(at -0.94747 -0.02966 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1E"
			(at -3.42519 -0.1905 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "RL0402FR-070R1L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RL0402FR-070R1L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "0.1E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "PANEL_SEN1_A6")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "PANEL_SEN0_A5")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C_NC"
		(layer "F.Cu")
		(at 167.44 64.27 90)
		(property "Reference" "R32"
			(at -1.45186 -0.01543 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -1.976311 -0.1397 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C_NC"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-N.C."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100107"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100107"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.0608 -1.825409 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "nRF91_SWD_RESET")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "/nRF9151_SiP/nRESET")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 152.45 58.29 90)
		(property "Reference" "C42"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-10n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GMD033R61A103KA01D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000003480"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200067"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26621779"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200067"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1005X04L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "/nRF5340_Interface_MCU/IMCU_RESET")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 209.87 75.82 -90)
		(property "Reference" "C19"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "39pF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±1%, 25V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-39p"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM0335C1E390FA01"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "39pF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "25V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001668"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200039"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200039"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/nRF9151_SiP/GPS_RF2")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/nRF9151_SiP/GPS_RF1")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:INDC1005X04L_WW"
		(layer "F.Cu")
		(at 209.38 73.11)
		(property "Reference" "L4"
			(at 1.35725 0.12072 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "68nH"
			(at 0.1651 -3.45059 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC1005X04L_WW"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, 140mA, ±2%, 1960mΩ, Q=20"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0402-68n-Wirewound-Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "LQW15AN68NG00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/P02/JELF243A-0050.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/inductor/product/LQW15AN68NG00%23.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "68nH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "-55°C ~ 125°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-6837-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000002494"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300389"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300389"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC1005X04L_WW*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.06759 -0.014391 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.475 0 90)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "VDD_GNSS")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.475 0 90)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/nRF9151_SiP/GPS_RF2")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-INDC1005X50-MURATA_LQW15A.STEP"
			(offset
				(xyz 0.00008 0.00007 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:AMPHENOL_G800W305018EU"
		(layer "F.Cu")
		(at 142.0625 100.93 180)
		(property "Reference" "P10"
			(at -0.885 -3.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x3, Straight"
			(at 9.91 3.135 0)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:AMPHENOL_G800W305018EU"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol ICC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "G800W305018EU"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x3, Straight"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "NO2_SENSE")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "VDD_3V3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 172.48 84.56)
		(property "Reference" "C41"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "/nRF5340_Interface_MCU/DECA")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 182.13 56.38)
		(property "Reference" "R8"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "BAT_SENSE_A1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 167 "VBAT_IN")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 181.7125 87.16 180)
		(property "Reference" "R40"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D10KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001255"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100065"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107101"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100065"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "Net-(U7-OE)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 175.7125 85.96 180)
		(property "Reference" "R46"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 175 "TWI1_SCL_3V3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "VDD_3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 167.69 65.27 180)
		(property "Reference" "R30"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "Net-(Q7B-S2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "nRF91_SWD_RESET")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 154.17 70.63)
		(property "Reference" "R10"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 156 "Net-(Q1A-G1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 181.7125 87.76)
		(property "Reference" "R42"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "TWI1_SDA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 180.89 57.14)
		(property "Reference" "R15"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "ERJ-1GNF2001C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-072KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "2k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "PANEL_SEN0_A5")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:DFN65P200X200X80_HS-6N"
		(layer "F.Cu")
		(at 151.94 74.08 180)
		(property "Reference" "Q5"
			(at 0.075 -1.48232 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MCM2301"
			(at -0.8883 -2.615146 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:DFN65P200X200X80_HS-6N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual P-Channel MOFET, 3.8A, 90mOhm max, 1.4W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Micro Commercial Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://www.mccsemi.com/pdf/Products/MCM2301(DFN2020-6L).pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/en/products/detail/micro-commercial-co/MCM2301-TP/9655971"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.mccsemi.com/product-detail/MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "VDFN-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "MCM2301-TPMSCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "833-MCM2301-TP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DFN65P200X200X80_HS-6N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.89 -1.87 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.90499 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "2" smd rect
			(at -0.90499 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at -0.90499 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "VBUS")
			(pinfunction "D2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at 0 0.47501 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "VBUS")
			(pinfunction "D2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "4" smd rect
			(at 0.905 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "S2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "5" smd rect
			(at 0.905 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 156 "Net-(Q1A-G1)")
			(pinfunction "G2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0 -0.475 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0.905 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/QFN65P200X200X65-6N.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:SOTFL50P162X60-6N"
		(layer "F.Cu")
		(at 156.342505 64.76 -90)
		(property "Reference" "Q4"
			(at 0.14772 -1.50125 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DMC2400UV"
			(at -1.4097 3.88239 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SOTFL50P162X60-6N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual N & P Ch MOFET, 1.03A/0.7A, 480mOhm, 450mW"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "DMC2400UV"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Diodes Incorporated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "DMC2400UV"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-01-18"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-01-18"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "DMC2400UV"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Dual N & P Channel Digital FET"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SOT-563"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007803"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.diodes.com/_files/datasheets/DMC2400UV.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "DMC2400UV-7DICT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300117"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300117"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOTFL50P162X60-6N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.04781 -1.166609 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.775 -0.5)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd rect
			(at -0.775 0)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "3" smd rect
			(at -0.775 0.5)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "USB_DETECT")
			(pinfunction "D2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.775 0.5)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "S2")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.775 0)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "Net-(Q3A-D1)")
			(pinfunction "G2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.775 -0.5)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/SOTFL50P162X60-6N.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:INDC1005X04L_WW"
		(layer "F.Cu")
		(at 211.11 69.41 180)
		(property "Reference" "L6"
			(at 1.35725 0.12072 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "9.1nH"
			(at 0.1651 -3.45059 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC1005X04L_WW"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, 540mA, ±2%, 140mΩ, Q=25"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0402-9n1-Wirewound-Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "LQW15AN9N1G00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/P02/JELF243A-0050.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/inductor/product/LQW15AN9N1G00%23.html"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "9.1nH"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "-55°C ~ 125°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-6854-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000002497"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300357"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300357"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC1005X04L_WW*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.06759 -0.014391 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.475 0 270)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U3-AMP_IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.475 0 270)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U3-FIL_OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-INDC1005X50-MURATA_LQW15A.STEP"
			(offset
				(xyz 0.00008 0.00007 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:SOP50P310X90-8N"
		(layer "F.Cu")
		(at 178.6325 86.89)
		(property "Reference" "U7"
			(at 0.925 -2.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "TXS0102DCUR"
			(at 7.275 2.135 0)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:SOP50P310X90-8N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra low capacitance double rail-to-rail ESD protection diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "TXS0102DCUR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "TI"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "TXS0102DCUR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2012-06-11"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "TXS0102DCUR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "10069015"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SOT-143B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009951"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.farnell.com/datasheets/109718.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "568-4140-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Farnell"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "152-4157"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300082"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26313940"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300082"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOT190P230X110-4L*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.405 -0.75)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 175 "TWI1_SCL_3V3")
			(pinfunction "B2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -1.405 -0.25)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -1.405 0.25)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 5 "VDD")
			(pinfunction "VCCA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -1.405 0.75)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 83 "TWI1_SCL")
			(pinfunction "A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at 1.405 0.75)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 99 "TWI1_SDA")
			(pinfunction "A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at 1.405 0.25)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 173 "Net-(U7-OE)")
			(pinfunction "OE")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at 1.405 -0.25)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 9 "VDD_3V3")
			(pinfunction "VCCB")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at 1.405 -0.75)
			(size 1.12 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 174 "TWI1_SDA_3V3")
			(pinfunction "B1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:DFN65P100X40-3L"
		(layer "F.Cu")
		(at 158.955 91.22 180)
		(property "Reference" "Q9"
			(at 0.125 0.94266 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RV2C010UNT2L"
			(at 3.59918 1.573746 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:DFN65P100X40-3L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel MOSFET, 20V, 1A, 470mOhm, 400mW"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "RV2C010UNT2L"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Rohm Semiconductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RV2C010UNT2L"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/transistor/mosfet/rv2c010unt2l-e.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "DFN-3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-08-09"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-08-09"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "RV2C010UNT2L"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "RV2C010UNT2LCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "755-RV2C010UNT2L"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "35010020"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009976"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300132"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26320026"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300132"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DFN65P100X40-3L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.07346 -0.014229 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.35 -0.225 270)
			(size 0.25 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/nRF5340_Interface_MCU/IMCU_LED")
			(pinfunction "G")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at -0.35 0.225 270)
			(size 0.25 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at 0.35 0 180)
			(size 0.4 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "Net-(LED1-C)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.065)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/DFN65P100X40-3L.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:AMPHENOL_G800W305018EU"
		(layer "F.Cu")
		(at 142.0625 89.05 180)
		(property "Reference" "P12"
			(at -0.885 -3.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x3, Straight"
			(at 9.91 3.135 0)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:AMPHENOL_G800W305018EU"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol ICC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "G800W305018EU"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x3, Straight"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "SMOKE_SENSE")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VDD_5V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:CAPC1005X04L"
		(layer "F.Cu")
		(at 149.69 73.83 -90)
		(property "Reference" "C1"
			(at -0.16053 -1.29174 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7µF"
			(at -0.7239 2.89179 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1005X04L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0402-4µ7-10V-X5R"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM155R61A475MEAAD"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R61A475MEAA-01.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM155R61A475MEAAD/490-14306-1-ND/6234742"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/capacitor/product/GRM155R61A475MEAA%23.html"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-10-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-10-04"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4.7µF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-14306-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200415"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200415"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.4318 0.189738 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0402(1005M) Cap.step"
			(offset
				(xyz 0.00007 0.00007 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "FP:BT-XTAL_2016"
		(layer "F.Cu")
		(at 170.76 90.93)
		(property "Reference" "X1"
			(at 1.712385 -0.14275 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "32MHz"
			(at -9.4212 30.27613 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:BT-XTAL_2016"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "XTAL SMD 2016, 32MHz, Cl=8pF, Tot: ±40ppm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "XTAL_SMD2016_32MHz_8pF_Kyocera"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "32MHz"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "XTAL_2016"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Oscillators"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101600039"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Kyocera"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "CX2016DB32000D0WZRC1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://media.digikey.com/pdf/Data%20Sheets/AVX%20PDFs/CX2016DB32000D0WZRC1_Spec.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-06-02"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-10-15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "XTAL SMD 32.000MHz"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1253-1586-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "22010022"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007827"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26511136"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101600039"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BT-XTAL_2016*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.028181 0.087805 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.725 0.575)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "/nRF5340_Interface_MCU/XC1")
			(pinfunction "inp")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.725 0.575)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.725 -0.575)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 234 "/nRF5340_Interface_MCU/XC2")
			(pinfunction "out")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.725 -0.575)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-GeyerElectronics_KX5.step"
			(offset
				(xyz 0.00011 0.00009 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1608X06L"
		(layer "F.Cu")
		(at 190.61 81.05 90)
		(property "Reference" "C16"
			(at -1.16796 -1.27709 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10µF"
			(at -1.35891 2.306511 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1608X06L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7T, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0603-10µ-10V-X7T-GRM188D71A106MA73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200414"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM188D71A106MA73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://no.mouser.com/datasheet/2/281/murata_03052018_GRM_Series_1-1310166.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-22"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-09-11"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10µF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10VDC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-7200-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-GRM188D71A106MA3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004696"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200414"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.25 -0.162338 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0 180)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0 180)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(M1A-VDD)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Capacitor 0603.step"
			(offset
				(xyz -0.00005 -0.43011 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:DFN65P200X200X80_HS-6N"
		(layer "F.Cu")
		(at 151.93 66.84 180)
		(property "Reference" "Q6"
			(at 0.075 -1.48232 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MCM2301"
			(at -0.8883 -2.615146 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:DFN65P200X200X80_HS-6N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual P-Channel MOFET, 3.8A, 90mOhm max, 1.4W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Micro Commercial Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://www.mccsemi.com/pdf/Products/MCM2301(DFN2020-6L).pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/en/products/detail/micro-commercial-co/MCM2301-TP/9655971"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.mccsemi.com/product-detail/MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "VDFN-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "MCM2301-TPMSCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "833-MCM2301-TP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DFN65P200X200X80_HS-6N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.85 -1.85 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.90499 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "2" smd rect
			(at -0.90499 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at -0.90499 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "VBAT")
			(pinfunction "D2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at 0 0.47501 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "VBAT")
			(pinfunction "D2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "4" smd rect
			(at 0.905 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "S2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "5" smd rect
			(at 0.905 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "Net-(Q2A-G1)")
			(pinfunction "G2")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0 -0.475 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0.905 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/QFN65P200X200X65-6N.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C_NC"
		(layer "F.Cu")
		(at 217 67.47 -90)
		(property "Reference" "C23"
			(at 1.45183 -0.00265 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -2.31521 1.6383 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C_NC"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-N.C."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Cap"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.03145 -0.549581 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/nRF9151_SiP/ANT")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "FP:SOT190P230X110-4L"
		(layer "F.Cu")
		(at 163 64 180)
		(property "Reference" "D2"
			(at -3.25093 -0.98165 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PRTR5V0U2X"
			(at 2.992202 -8.05912 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SOT190P230X110-4L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra low capacitance double rail-to-rail ESD protection diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "PRTR5V0U2X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "NXP Semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "PRTR5V0U2X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2012-06-11"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "PRTR5V0U2X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "10069015"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SOT-143B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009951"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.farnell.com/datasheets/109718.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "568-4140-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Farnell"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "152-4157"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300082"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26313940"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300082"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOT190P230X110-4L*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.024791 -0.08173 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -1.025 -0.75 270)
			(size 1 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.025 0.95 270)
			(size 0.6 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "IMCU_USB_D_N")
			(pinfunction "IO1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.025 0.95 270)
			(size 0.6 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "IMCU_USB_D_P")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.025 -0.95 270)
			(size 0.6 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(D2-VCC)")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-sot143.step"
			(offset
				(xyz -0.00012 -0.00007 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 90)
			)
		)
	)
	(footprint "FP:CONN_BM04B-SRSS-TB_SPK"
		(layer "F.Cu")
		(at 172.15995 101.22315 180)
		(tags "PRT-16766 ")
		(property "Reference" "P9"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x4, Angled"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:CONN_BM04B-SRSS-TB_SPK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Sparkfun"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "PRT-16766"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x4, Angled"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "VDD_3V3")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "TWI_SDA_3V3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "TWI_SCL_3V3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 148.385 85.03 180)
		(property "Reference" "R21"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0R"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±5%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-0R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100001"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-070RL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "0R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 5%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000003245"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100001"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "VDD_3V0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "VDD_GNSS")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:COAXIAL RF U.FL-R-SMT-1"
		(layer "F.Cu")
		(at 167.86 94.11 180)
		(property "Reference" "J4"
			(at -3.00232 -1.095 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MHF I Receptacle"
			(at 4.59359 1.8161 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:COAXIAL RF U.FL-R-SMT-1"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultraminiature Coaxial Connector, 50 Ohm, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "20279-001E-03"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Wellshow"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "20279-001E-03"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "~{\\}hiz~{z}pr~{o}app971~{7}Datashee~{t}connector~{s}Wellsho~{w}20279C18.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "COAXIAL RF MHFI"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-28"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2020-01-07"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "MHF I Receptacle"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "20279-001E-03"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "H11891DKR-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004436"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500636"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500636"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*COAXIAL RF U.FL-R-SMT-1*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.77811 -1.638111 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at 0 1.52501 180)
			(size 1 1.05)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "Net-(J4-X)")
			(pinfunction "X")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.475 0 180)
			(size 1.05 2.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Y")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.475 0 180)
			(size 1.05 2.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Y")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 167.01 95.22) (xy 168.71 95.22) (xy 168.71 92.39499) (xy 167.01 92.39499)
				)
			)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/U.FL-R-SMT-1.stp"
			(offset
				(xyz 55.23893 1.05009 22.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -180)
			)
		)
	)
	(footprint "FP:SON50P210X160X65_HS-9N"
		(layer "F.Cu")
		(at 199.257525 86.191245 90)
		(property "Reference" "D1"
			(at 0.558985 2.363254 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TPD3F303DPVR"
			(at -2.86891 -2.411946 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SON50P210X160X65_HS-9N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Protection and EMI Filter for SIM Card Interface"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "TPD3F303DPVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "TPD3F303DPVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "USON-8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-10-19"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-10-19"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "TPD3F303DPVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://www.ti.com/lit/ds/symlink/tpd3f303.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/en/products/detail/texas-instruments/TPD3F303DPVR/2605055"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.ti.com/product/TPD3F303/part-details/TPD3F303DPVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "296-28299-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "595-TPD3F303DPVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101900729"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Misc_ICs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101900729"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SON50P210X160X65_HS-9N*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text_box "${REFERENCE}"
			(start 0.437616 -1.901158)
			(end -0.478686 1.816208)
			(angle -90)
			(layer "User.7")
			(border no)
		)
		(pad "1" smd rect
			(at -0.725 -0.75 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(D1-DATA1_OUT)")
			(pinfunction "DATA1_OUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at -0.725 -0.25 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(D1-CLK_OUT)")
			(pinfunction "CLK_OUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at -0.725 0.25 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(D1-DATA2_OUT)")
			(pinfunction "DATA2_OUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at -0.725 0.75 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "unconnected-(D1-NC-Pad4)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at 0.725 0.75 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "SIM_1V8")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at 0.725 0.25 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "SIM_IO")
			(pinfunction "DATA2_IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at 0.725 -0.25 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "SIM_CLK")
			(pinfunction "CLK_IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at 0.725 -0.75 180)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "SIM_RST")
			(pinfunction "DATA1_IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "9" smd rect
			(at 0 0 180)
			(size 1.7 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin -2)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/SON50P160X65_HS-9N.step"
			(offset
				(xyz -0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 181.39 58.97 180)
		(property "Reference" "R19"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "PANEL_SEN1_A6")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "VBAT'")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:COAXIAL-SWF"
		(layer "F.Cu")
		(at 207.52 84.62 90)
		(property "Reference" "J2"
			(at -2.11767 0.071295 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MM8130-2600"
			(at -1.2319 4.00939 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:COAXIAL-SWF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Coaxial Connector with Switch"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "MM8130-2600"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "MM8130-2600"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-04-24"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-04-24"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "MM8130-2600"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "55029011"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "COAXIAL-SWF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009955"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.murata.com/products/catalog/pdf/o33e.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-4981-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-MM8130-2600RA2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500400"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26030338"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500400"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*COAXIAL-SWF*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.836819 1.737805 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at 0 -1.16 90)
			(size 0.5 0.58)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "/nRF9151_SiP/LTE_RF1")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.025 -0.95 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.025 0.95 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.02499 -0.95 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.02499 0.95 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 1.16 90)
			(size 0.5 0.58)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/nRF9151_SiP/ANT")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 206.97 85.27001) (xy 206.97 83.97) (xy 206.17 83.97) (xy 206.17 85.27001)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 208.06999 83.97) (xy 208.06999 85.27001) (xy 208.87 85.27001) (xy 208.87 83.97)
				)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 175.7125 87.96 180)
		(property "Reference" "R44"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "TWI1_SCL")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:TESTPAD-TH"
		(layer "F.Cu")
		(at 142.28 56.66)
		(property "Reference" "TP1"
			(at -0.242075 1.92675 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at -0.8763 3.60299 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:TESTPAD-TH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Testpoint, through hole"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Testpoint TH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "TESTPAD-TH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "TP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500464"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500464"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TESTPAD-TH*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.05316 -1.364229 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 153.92 71.63 -90)
		(property "Reference" "R1"
			(at -0.94747 -0.02966 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "VBUS'")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:Fiducial"
		(layer "F.Cu")
		(at 139.57 54.51)
		(property "Reference" "Fid2"
			(at 0.148815 -1.89595 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial mark"
			(at -0.7493 3.47599 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:Fiducial"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fiducial Mark"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Fid-Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "Fiducial"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500073"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500073"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fiducial*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(pad "0" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.5)
			(thermal_bridge_angle 90)
		)
		(pad "0" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(solder_mask_margin 0.5)
			(thermal_bridge_angle 90)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 139.766066 53.524311) (xy 139.954597 53.581501) (xy 140.128348 53.674373) (xy 140.280642 53.799358)
					(xy 140.405627 53.951652) (xy 140.498499 54.125403) (xy 140.555689 54.313934) (xy 140.575 54.51)
					(xy 140.555689 54.706066) (xy 140.498499 54.894597) (xy 140.405627 55.068348) (xy 140.280642 55.220642)
					(xy 140.128348 55.345627) (xy 139.954597 55.438499) (xy 139.766066 55.495689) (xy 139.57 55.515)
					(xy 139.373934 55.495689) (xy 139.185403 55.438499) (xy 139.011652 55.345627) (xy 138.859358 55.220642)
					(xy 138.734373 55.068348) (xy 138.641501 54.894597) (xy 138.584311 54.706066) (xy 138.565 54.51)
					(xy 138.570186 54.51) (xy 138.589397 54.705054) (xy 138.646292 54.892612) (xy 138.738685 55.065467)
					(xy 138.863025 55.216975) (xy 139.014533 55.341315) (xy 139.187388 55.433708) (xy 139.374946 55.490603)
					(xy 139.57 55.509814) (xy 139.765054 55.490603) (xy 139.952612 55.433708) (xy 140.125467 55.341315)
					(xy 140.276975 55.216975) (xy 140.401315 55.065467) (xy 140.493708 54.892612) (xy 140.550603 54.705054)
					(xy 140.569814 54.51) (xy 140.550603 54.314946) (xy 140.493708 54.127388) (xy 140.401315 53.954533)
					(xy 140.276975 53.803025) (xy 140.125467 53.678685) (xy 139.952612 53.586292) (xy 139.765054 53.529397)
					(xy 139.57 53.510186) (xy 139.374946 53.529397) (xy 139.187388 53.586292) (xy 139.014533 53.678685)
					(xy 138.863025 53.803025) (xy 138.738685 53.954533) (xy 138.646292 54.127388) (xy 138.589397 54.314946)
					(xy 138.570186 54.51) (xy 138.565 54.51) (xy 138.584311 54.313934) (xy 138.641501 54.125403) (xy 138.734373 53.951652)
					(xy 138.859358 53.799358) (xy 139.011652 53.674373) (xy 139.185403 53.581501) (xy 139.373934 53.524311)
					(xy 139.57 53.505)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 139.766066 53.524311) (xy 139.954597 53.581501) (xy 140.128348 53.674373) (xy 140.280642 53.799358)
					(xy 140.405627 53.951652) (xy 140.498499 54.125403) (xy 140.555689 54.313934) (xy 140.575 54.51)
					(xy 140.555689 54.706066) (xy 140.498499 54.894597) (xy 140.405627 55.068348) (xy 140.280642 55.220642)
					(xy 140.128348 55.345627) (xy 139.954597 55.438499) (xy 139.766066 55.495689) (xy 139.57 55.515)
					(xy 139.373934 55.495689) (xy 139.185403 55.438499) (xy 139.011652 55.345627) (xy 138.859358 55.220642)
					(xy 138.734373 55.068348) (xy 138.641501 54.894597) (xy 138.584311 54.706066) (xy 138.565 54.51)
					(xy 138.570186 54.51) (xy 138.589397 54.705054) (xy 138.646292 54.892612) (xy 138.738685 55.065467)
					(xy 138.863025 55.216975) (xy 139.014533 55.341315) (xy 139.187388 55.433708) (xy 139.374946 55.490603)
					(xy 139.57 55.509814) (xy 139.765054 55.490603) (xy 139.952612 55.433708) (xy 140.125467 55.341315)
					(xy 140.276975 55.216975) (xy 140.401315 55.065467) (xy 140.493708 54.892612) (xy 140.550603 54.705054)
					(xy 140.569814 54.51) (xy 140.550603 54.314946) (xy 140.493708 54.127388) (xy 140.401315 53.954533)
					(xy 140.276975 53.803025) (xy 140.125467 53.678685) (xy 139.952612 53.586292) (xy 139.765054 53.529397)
					(xy 139.57 53.510186) (xy 139.374946 53.529397) (xy 139.187388 53.586292) (xy 139.014533 53.678685)
					(xy 138.863025 53.803025) (xy 138.738685 53.954533) (xy 138.646292 54.127388) (xy 138.589397 54.314946)
					(xy 138.570186 54.51) (xy 138.565 54.51) (xy 138.584311 54.313934) (xy 138.641501 54.125403) (xy 138.734373 53.951652)
					(xy 138.859358 53.799358) (xy 139.011652 53.674373) (xy 139.185403 53.581501) (xy 139.373934 53.524311)
					(xy 139.57 53.505)
				)
			)
		)
	)
	(footprint "FP:CAPC1005X04L_NC"
		(layer "F.Cu")
		(at 210.58 62.06)
		(property "Reference" "C31"
			(at 0.160045 -0.79325 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -0.0381 3.01879 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1005X04L_NC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0402-N.C."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2009-05-08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2009-05-08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Cap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200105"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200105"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.050265 0.010821 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/nRF9151_SiP/GPS_RF5")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "FP:CONN14_901522114_MOL"
		(layer "F.Cu")
		(at 139.74565 61.4634 90)
		(tags "901522114 ")
		(property "Reference" "P14"
			(at -7.3266 9.49435 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 7x2, Right Angle"
			(at -7.62 3.81 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:CONN14_901522114_MOL"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Molex"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "90152-2114"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 7x2, Right Angle"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -7.62 3.81 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "unconnected-(P14-A1-Pad1)")
			(pinfunction "A1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 7.62 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "FLAME_SENSE_D1")
			(pinfunction "D1")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -2.54 0 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 153 "unconnected-(P14-A2-Pad3)")
			(pinfunction "A2")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole circle
			(at -2.54 7.62 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "FLAME_SENSE_D2")
			(pinfunction "D2")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -5.08 0 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "FLAME_SENSE")
			(pinfunction "A3")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -5.08 7.62 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 239 "unconnected-(P14-D3-Pad6)")
			(pinfunction "D3")
			(pintype "passive+no_connect")
		)
		(pad "7" thru_hole circle
			(at -7.62 0 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 240 "unconnected-(P14-A4-Pad7)")
			(pinfunction "A4")
			(pintype "passive+no_connect")
		)
		(pad "8" thru_hole circle
			(at -7.62 7.62 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "FLAME_SENSE_D4")
			(pinfunction "D4")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -10.16 0 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 238 "unconnected-(P14-A5-Pad9)")
			(pinfunction "A5")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole circle
			(at -10.16 7.62 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "FLAME_SENSE_D5")
			(pinfunction "D5")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -12.7 0 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VDD_5V")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -12.7 7.62 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VDD_5V")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -15.24 0 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -15.24 7.62 90)
			(size 1.397 1.397)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
	)
	(footprint "FP:DFN65P100X40-3L"
		(layer "F.Cu")
		(at 168.39 68.97)
		(property "Reference" "Q8"
			(at 0.125 0.94266 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RV2C010UNT2L"
			(at 3.59918 1.573746 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:DFN65P100X40-3L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel MOSFET, 20V, 1A, 470mOhm, 400mW"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "RV2C010UNT2L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Rohm Semiconductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RV2C010UNT2L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/transistor/mosfet/rv2c010unt2l-e.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "DFN-3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-08-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-08-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "RV2C010UNT2L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "RV2C010UNT2LCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "755-RV2C010UNT2L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "35010020"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009976"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300132"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26320026"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300132"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DFN65P100X40-3L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.07346 -0.014229 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.35 -0.225 90)
			(size 0.25 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 163 "Net-(Q7A-D1)")
			(pinfunction "G")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at -0.35 0.225 90)
			(size 0.25 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at 0.35 0)
			(size 0.4 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "/nRF9151_SiP/nRESET")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.065)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/DFN65P100X40-3L.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:AMPHENOL_G800W305018EU"
		(layer "F.Cu")
		(at 142.0625 83.11 180)
		(property "Reference" "P13"
			(at -0.885 -3.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x3, Straight"
			(at 9.91 3.135 0)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:AMPHENOL_G800W305018EU"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol ICC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "G800W305018EU"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x3, Straight"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "CO_SENSE")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VDD_5V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 2.54 0 180)
			(size 1.605 1.605)
			(drill 1.07)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:INDC0603X03L_C"
		(layer "F.Cu")
		(at 220.39 67.48 -90)
		(property "Reference" "L7"
			(at 0.128005 0.67094 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22nH"
			(at -0.7239 2.89179 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Chip Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0201-22n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "LQP03TQ22NH02D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-08-29"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2013-04-10"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "22nH"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "High frequency chip inductor ±10%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001478"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300034"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300034"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.047615 -0.484389 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28492 -0.00008)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28507 -0.00008)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(A1-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-smt_inductor-0201.step"
			(offset
				(xyz 0.00017 0.00017 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 166.18 71.19 90)
		(property "Reference" "C51"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U6-GND)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:SOTFL50P162X60-6N"
		(layer "F.Cu")
		(at 167.44 67.02 90)
		(property "Reference" "Q7"
			(at 0.14772 -1.50125 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DMC2400UV"
			(at -1.4097 3.88239 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SOTFL50P162X60-6N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual N & P Ch MOFET, 1.03A/0.7A, 480mOhm, 450mW"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "DMC2400UV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Diodes Incorporated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "DMC2400UV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.diodes.com/_files/datasheets/DMC2400UV.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SOT-563"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-01-18"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-01-18"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "DMC2400UV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Dual N & P Channel Digital FET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "DMC2400UV-7DICT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007803"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300117"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300117"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOTFL50P162X60-6N*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.04781 -1.166609 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.775 -0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "S1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.775 0 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "nRF91_SWD_RESET")
			(pinfunction "G1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.775 0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 163 "Net-(Q7A-D1)")
			(pinfunction "D2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.775 0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "Net-(Q7B-S2)")
			(pinfunction "S2")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.775 0 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "nRF91_SWD_RESET")
			(pinfunction "G2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.775 -0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 163 "Net-(Q7A-D1)")
			(pinfunction "D1")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/SOTFL50P162X60-6N.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:INDC1005X04L"
		(layer "F.Cu")
		(at 212.99 63.89 90)
		(property "Reference" "FB2"
			(at -1.35565 -0.12476 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "120R/1.2A"
			(at 1.997202 -6.6398 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC1005X04L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite Bead, 120 Ohm @ 100MHz, 1200mA, 75 mOhm Max"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "FB0402-120R@100M-1200mA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300416"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "masi"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "BLM15EX121SN1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://no.mouser.com/datasheet/2/281/ENFA0023-1915680.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.murata.com/en-eu/products/productdetail?partno=BLM15EX121SN1%23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-05-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-05-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "120R/1.2A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-16509-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-BLM15EX121SN1D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300416"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC1005X04L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.10079 -0.010771 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.47501 0 180)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U3-VCC)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Inductor 0402.step"
			(offset
				(xyz -0.00009 -0.27509 0.25)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:Shunt_2.54mm_Horizontal"
		(layer "F.Cu")
		(at 392.07 136.93)
		(property "Reference" "Y1"
			(at 4.558275 3.44535 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Shunt 2.54mm"
			(at 5.0165 -4.033711 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:Shunt_2.54mm_Horizontal"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Shunt Jumper 2.54mm Black"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "SHUNT JUMPER 2.54mm BLACK GOLD Horizontal (Obsolete)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Placed on P30"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "3M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "969102-0000-DA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.digikey.com/product-detail/en/969102-0000-DA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SHUNT JUMPER 2.54mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-06-28"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-09-04"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Shunt 2.54mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "SHUNT JUMPER .1\" BLACK GOLD, h=6.00mm, w=5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "3M9580-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "56099001"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001916"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500644"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Obsolete"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500644"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Shunt_2.54mm_Horizontal*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Control System_FCI_68786-102LF.STEP"
			(offset
				(xyz 2.51464 -2.53989 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C_NC"
		(layer "F.Cu")
		(at 218.1 67.47 -90)
		(property "Reference" "C26"
			(at 1.45183 -0.00265 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -2.31521 1.6383 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C_NC"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-N.C."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Cap"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.03145 -0.549581 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(C26-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "FP:SON127P800X80_HS-9N"
		(layer "F.Cu")
		(at 180.76 78.94 90)
		(property "Reference" "U4"
			(at 4.83234 0.125 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "GD25WB256E"
			(at -2.62116 -3.758146 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SON127P800X80_HS-9N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad Serial Flash, 256Mbit, 104MHz, 1.65V - 3.6V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "GD25WB256EYIG"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "GigaDevice"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GD25WB256EYIG"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "WSON-8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-27"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-27"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "GD25WB256E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://www.gigadevice.com.cn/Public/Uploads/uploadfile/files/20220714/DS-00863-GD25WB256E-Rev1.1.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.gigadevice.com/product/flash/product-series/spi-nor-flash/gd25wb256e.html"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Misc_ICs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101900774"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101900774"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SON127P800X80_HS-9N*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.010761 0.0508 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -3.87 -1.90501 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "EXT_MEM_CS")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.87 -0.635 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "EXT_MEM_MISO")
			(pinfunction "IO1/SO")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.87 0.635 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 189 "unconnected-(U4-IO2-Pad3)")
			(pinfunction "IO2")
			(pintype "passive+no_connect")
		)
		(pad "4" smd rect
			(at -3.87 1.905 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 3.87 1.905 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 131 "EXT_MEM_MOSI")
			(pinfunction "IO0/SI")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 3.87 0.635 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "EXT_MEM_SCK")
			(pinfunction "SCLK")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 3.87 -0.635 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 190 "unconnected-(U4-IO3-Pad7)")
			(pinfunction "IO3")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 3.87 -1.90501 180)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 180)
			(size 4.3 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
			(solder_paste_margin -1.7)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 167.02 89.44 -90)
		(property "Reference" "C47"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C_NC"
		(layer "F.Cu")
		(at 219.32 67.44 -90)
		(property "Reference" "C27"
			(at 1.45183 -0.00265 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "N.C."
			(at -2.31521 1.6383 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C_NC"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not mounted"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-N.C."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.C."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Cap"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.03145 -0.549581 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(C26-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 162.11 86.49 180)
		(property "Reference" "C45"
			(at -1.404825 -0.13896 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 182.13 57.17)
		(property "Reference" "R14"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "PANEL_SEN0_A5")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 167 "VBAT_IN")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:COAXIAL RF U.FL-R-SMT-1"
		(layer "F.Cu")
		(at 212.82251 74.51 -90)
		(property "Reference" "J1"
			(at -3.00232 -1.095 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MHF I Receptacle"
			(at 4.59359 1.8161 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:COAXIAL RF U.FL-R-SMT-1"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultraminiature Coaxial Connector, 50 Ohm, SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "20279-001E-03"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Wellshow"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "20279-001E-03"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "~{\\}hiz~{z}pr~{o}app971~{7}Datashee~{t}connector~{s}Wellsho~{w}20279C18.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "COAXIAL RF MHFI"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-28"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2020-01-07"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "MHF I Receptacle"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "20279-001E-03"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "H11891DKR-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004436"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500636"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500636"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*COAXIAL RF U.FL-R-SMT-1*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.77811 -1.638111 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at 0 1.52501 270)
			(size 1 1.05)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/nRF9151_SiP/GPS_RF2")
			(pinfunction "X")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.475 0 270)
			(size 1.05 2.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Y")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.475 0 270)
			(size 1.05 2.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Y")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 213.90752 75.38) (xy 213.90752 73.68) (xy 211.08251 73.68) (xy 211.08251 75.38)
				)
			)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/U.FL-R-SMT-1.stp"
			(offset
				(xyz 55.23893 1.05009 22.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -180)
			)
		)
	)
	(footprint "FP:CAPC1005X04L"
		(layer "F.Cu")
		(at 172.9 82.17)
		(property "Reference" "C35"
			(at -0.16053 -1.29174 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7µF"
			(at -0.7239 2.89179 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1005X04L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, 10V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0402-4µ7-10V-X5R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM155R61A475MEAAD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R61A475MEAA-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM155R61A475MEAAD/490-14306-1-ND/6234742"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/capacitor/product/GRM155R61A475MEAA%23.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-10-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-10-04"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4.7µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-14306-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200415"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200415"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.4318 0.189738 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(U5A-VBUS)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0402(1005M) Cap.step"
			(offset
				(xyz 0.00007 0.00007 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "FP:SD-80259-001"
		(layer "F.Cu")
		(at 162.9 57.455 180)
		(property "Reference" "J5"
			(at -5.08132 1.47859 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "USB-C 2.0"
			(at 6.493002 -5.166805 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SD-80259-001"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB-C Receptacle, 16 Pin, USB 2.0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "80259-1021"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500830"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "getr"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Bellweather Electronic Corp."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "80259-1021"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "~{\\}hiz~{z}pr~{o}app971~{7}Datashee~{t}connector~{s}Bellwethe~{r}SD-80259-001_C.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2024-03-26"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-10-30"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "16"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SD-80259-001"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "USB-C 2.0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "80259-1021"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500830"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SD-80259-001*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.026974 1.8464 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(fp_text_box "Board Edge"
			(start -2.375473 2.46678)
			(end 3.879513 4.67027)
			(layer "Eco1.User")
			(border no)
		)
		(pad "" np_thru_hole circle
			(at -2.89 -1.315 90)
			(size 0.6 0.6)
			(drill 0.6)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "" np_thru_hole circle
			(at 2.89 -1.315 180)
			(size 0.6 0.6)
			(drill 0.6)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "13" thru_hole oval
			(at -4.325 -1.795 180)
			(size 0.9 2)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole oval
			(at -4.325 2.385 180)
			(size 0.9 1.7)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole oval
			(at 4.325 -1.795 180)
			(size 0.9 2)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole oval
			(at 4.325 2.385 180)
			(size 0.9 1.7)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "A1" smd rect
			(at -3.2 -2.385)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A4" smd rect
			(at -2.4 -2.385)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(D2-VCC)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "A5" smd rect
			(at -1.25 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "Net-(J5-CC1)")
			(pinfunction "CC1")
			(pintype "passive")
		)
		(pad "A6" smd rect
			(at -0.25 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "IMCU_USB_D_P")
			(pinfunction "DP1")
			(pintype "passive")
		)
		(pad "A7" smd rect
			(at 0.25 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "IMCU_USB_D_N")
			(pinfunction "DN1")
			(pintype "passive")
		)
		(pad "A8" smd rect
			(at 1.25 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "unconnected-(J5-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "passive+no_connect")
		)
		(pad "A9" smd rect
			(at 2.4 -2.385)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(D2-VCC)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "A12" smd rect
			(at 3.2 -2.385)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B5" smd rect
			(at 1.75 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "Net-(J5-CC2)")
			(pinfunction "CC2")
			(pintype "passive")
		)
		(pad "B6" smd rect
			(at 0.75 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "IMCU_USB_D_P")
			(pinfunction "DP2")
			(pintype "passive")
		)
		(pad "B7" smd rect
			(at -0.75 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "IMCU_USB_D_N")
			(pinfunction "DN2")
			(pintype "passive")
		)
		(pad "B8" smd rect
			(at -1.75 -2.385)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "unconnected-(J5-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "passive+no_connect")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/CM-80259-1020_20191104.stp"
			(offset
				(xyz 0 -6.3796 3.26)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 90)
			)
		)
	)
	(footprint "FP:INDC1608X06L"
		(layer "F.Cu")
		(at 188.7 80.37)
		(property "Reference" "FB1"
			(at -0.45214 -0.82438 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22R@100M/6A"
			(at -0.6985 2.91719 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC1608X06L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite Bead, 22 Ohm @ 100MHz, 6000mA, 8 mOhm Max"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "FB0603-22R@100MHz-6000mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "kod1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "BLM18SD220SN1D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.murata.com/en-us/products/productdata/8796738650142/ENFA0003.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.murata.com/en-global/products/productdata/8796733767710/S0580E.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2024-01-25"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2024-01-25"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "22R@100M/6A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip EMIFIL Inductor Type Chip Ferrite Bead"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-15633-2-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.45 0.237338 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0 90)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0 90)
			(size 0.8 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(M1A-VDD)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Inductor.step"
			(offset
				(xyz -0.00008 -0.47508 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 181.7125 86.56)
		(property "Reference" "C56"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "VDD_3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 159.75 63.25)
		(property "Reference" "C55"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "VBUS'")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:INDC2016X10N"
		(layer "F.Cu")
		(at 153.839995 91.540005 90)
		(property "Reference" "L2"
			(at 2.10724 0.24154 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2µH"
			(at -0.72389 2.76635 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC2016X10N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, Irms=2.5A, Isat=2.9A, ±20%, DCR=73mΩ"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0806-2µ2-2500mA-73mOhm-CIGT201610EH2R2MNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300400"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samsung Electro-Mechanics America"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "CIGT201610EH2R2MNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://media.digikey.com/pdf/Data%20Sheets/Samsung%20PDFs/CIGT201610EH2R2MNE_Spec.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CIGT201610EH2R2MNE/7041223?s=N4IgTCBcDaIMIEkDiAVMAGAjANk%2BgogBJgBKYAsgHL4gC6AvkA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://product.samsungsem.com/pi/CIGT201610EH2R2MN.do"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-09-07"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2021-02-03"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0806"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "2.2µH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Unshielded Thin Film Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1276-6901-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "187-CIGT201610EH2R2M"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26521789"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300400"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC2016X10N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text_box "${REFERENCE}"
			(start 0.458166 -1.883678)
			(end -0.458136 1.833688)
			(angle -90)
			(layer "User.7")
			(border no)
		)
		(pad "1" smd rect
			(at -0.88499 0 180)
			(size 1.82 1.13)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "VDD_3V0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.885 0 180)
			(size 1.82 1.13)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "/nRF9151_Power_Supply/SW2")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/INDC2016X10N.step"
			(offset
				(xyz -0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 161 61.75 90)
		(property "Reference" "R41"
			(at -0.94747 -0.02966 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5k1"
			(at -3.42519 -0.1905 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-5k1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100565"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-075K1L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-04-20"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-04-20"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "5k1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26192285"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100565"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "Net-(J5-CC2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:INDC2016X10N"
		(layer "F.Cu")
		(at 150.805 91.07)
		(property "Reference" "L1"
			(at 2.10724 0.24154 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2µH"
			(at -0.72389 2.76635 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC2016X10N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, Irms=2.5A, Isat=2.9A, ±20%, DCR=73mΩ"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L0806-2µ2-2500mA-73mOhm-CIGT201610EH2R2MNE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300400"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samsung Electro-Mechanics America"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "CIGT201610EH2R2MNE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://media.digikey.com/pdf/Data%20Sheets/Samsung%20PDFs/CIGT201610EH2R2MNE_Spec.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CIGT201610EH2R2MNE/7041223?s=N4IgTCBcDaIMIEkDiAVMAGAjANk%2BgogBJgBKYAsgHL4gC6AvkA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://product.samsungsem.com/pi/CIGT201610EH2R2MN.do"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-09-07"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2021-02-03"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0806"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "2.2µH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Unshielded Thin Film Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1276-6901-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "187-CIGT201610EH2R2M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26521789"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300400"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC2016X10N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text_box "${REFERENCE}"
			(start 0.458166 -1.883678)
			(end -0.458136 1.833688)
			(angle 270)
			(layer "User.7")
			(border no)
		)
		(pad "1" smd rect
			(at -0.88499 0 90)
			(size 1.82 1.13)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.885 0 90)
			(size 1.82 1.13)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/nRF9151_Power_Supply/SW1")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/INDC2016X10N.step"
			(offset
				(xyz -0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1005X04L"
		(layer "F.Cu")
		(at 194.8 85.32 -90)
		(property "Reference" "C17"
			(at -0.16053 -1.29174 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7µF"
			(at -0.7239 2.89179 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1005X04L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0402-4µ7-10V-X5R"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM155R61A475MEAAD"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R61A475MEAA-01.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM155R61A475MEAAD/490-14306-1-ND/6234742"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/capacitor/product/GRM155R61A475MEAA%23.html"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-10-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-10-04"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4.7µF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-14306-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200415"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200415"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.4318 0.189738 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/nRF9151_SiP/DEC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0402(1005M) Cap.step"
			(offset
				(xyz 0.00007 0.00007 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 157.43501 85.03)
		(property "Reference" "R7"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 166 "PMIC_TWI_SDA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 190.64 78.22)
		(property "Reference" "R25"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1k0"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-071KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000005786"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100043"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100043"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "/nRF9151_SiP/nRESET")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(M1C-nRESET)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 149.66 66.84)
		(property "Reference" "R12"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D10KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001255"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100065"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107101"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100065"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "VBUS'")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "Net-(Q2A-G1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:XQFN40P180X260X50-16N"
		(layer "F.Cu")
		(at 165.93 73.91)
		(property "Reference" "U6"
			(at 1.67601 -0.125005 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FSA2466UMX"
			(at 0.3683 2.417889 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:XQFN40P180X260X50-16N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Data / Audio Low-Voltage Dual DPDT Analog Switch"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "FSA2466UMX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "ON Semiconductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "FSA2466UMX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.onsemi.com/pub/Collateral/FSA2466-D.PDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "UFQFN-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-05-15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-05-18"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "FSA2466UMX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "FSA2466UMXCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "512-FSA2466UMX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "15070069"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009986"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Misc_ICs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101900422"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26500608"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101900422"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*XQFN40P180X260X50-16N*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.026699 -0.05277 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd oval
			(at -0.825 -0.60001 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 229 "/nRF5340_Interface_MCU/SWD3_RESET")
			(pinfunction "NC1")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "2" smd oval
			(at -0.825 -0.2 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "/nRF5340_Interface_MCU/SWD_CTRL")
			(pinfunction "IN_1-2")
			(pintype "input")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "3" smd oval
			(at -0.825 0.2 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 237 "unconnected-(U6-NO2-Pad3)")
			(pinfunction "NO2")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "4" smd oval
			(at -0.825 0.59999 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "TRACE_DATA0")
			(pinfunction "COM2")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "5" smd oval
			(at -0.6 1.225)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 196 "/nRF5340_Interface_MCU/SWD3_SWO")
			(pinfunction "NC2")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "6" smd oval
			(at -0.2 1.225)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U6-GND)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "7" smd oval
			(at 0.2 1.225)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 235 "unconnected-(U6-NO3-Pad7)")
			(pinfunction "NO3")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "8" smd oval
			(at 0.6 1.225)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "nRF91_SWD_SWDCLK")
			(pinfunction "COM3")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "9" smd oval
			(at 0.825 0.59999 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 201 "/nRF5340_Interface_MCU/SWD3_CLK")
			(pinfunction "NC3")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "10" smd oval
			(at 0.825 0.2 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "/nRF5340_Interface_MCU/SWD_CTRL")
			(pinfunction "IN_3-4")
			(pintype "input")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "11" smd oval
			(at 0.825 -0.2 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 236 "unconnected-(U6-NO4-Pad11)")
			(pinfunction "NO4")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "12" smd oval
			(at 0.825 -0.60001 90)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "nRF91_SWD_SWDIO")
			(pinfunction "COM4")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "13" smd oval
			(at 0.6 -1.22501)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 192 "/nRF5340_Interface_MCU/SWD3_IO")
			(pinfunction "NC4")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "14" smd oval
			(at 0.2 -1.22501)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "15" smd oval
			(at -0.2 -1.22501)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "RESET_IN")
			(pinfunction "NO1")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(pad "16" smd oval
			(at -0.6 -1.22501)
			(size 0.22 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "nRF91_SWD_RESET")
			(pinfunction "COM1")
			(pintype "bidirectional")
			(solder_mask_margin 0.04)
			(solder_paste_margin -0.02)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-XQFN-16-1.step"
			(offset
				(xyz -0.00001 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "FP:INDC1005X04L"
		(layer "F.Cu")
		(at 159.25 62 -90)
		(property "Reference" "FB3"
			(at -1.35565 -0.12476 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "120R/0.55A"
			(at 1.997202 -6.6398 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:INDC1005X04L"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite Bead, 120 Ohm @ 100MHz, 500mA, 250 mOhm Max"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "FB0402-120R@100M-500mA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "BLM15AG121SN1D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-01-10"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2011-11-14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "120R/0.55A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip EMIFIL Inductor Type Chip Ferrite Bead"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "33029317"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009954"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0110S0100BLM15A_SN.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-1005-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Farnell"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "151-5760"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100300099"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Inductors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "265230631"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100300099"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*INDC1005X04L*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.10079 -0.010771 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.47501 0)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(D2-VCC)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.5 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "VBUS'")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Inductor 0402.step"
			(offset
				(xyz -0.00009 -0.27509 0.25)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 205.55 87.19 -90)
		(property "Reference" "R47"
			(at -0.94747 -0.02966 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M0"
			(at -3.42519 -0.1905 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1M0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-071ML"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1M0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001418"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100093"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107108"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100093"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(J6-PadCD)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 177.07 82.49 -90)
		(property "Reference" "R29"
			(at -0.94747 -0.02966 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "EXT_MEM_CS")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 168.65 89.25 -90)
		(property "Reference" "C39"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7R, ±10%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-2n2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "2.2nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200060"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A222KA01D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001778"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26470002"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200060"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/nRF5340_Interface_MCU/DECR")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 180.88 56.38)
		(property "Reference" "R9"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "ERJ-1GNF2001C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-072KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "2k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "BAT_SENSE_A1")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:KLS1-SIM-066"
		(layer "F.Cu")
		(at 198.2525 88.762505)
		(property "Reference" "J6"
			(at 9.525 0.26766 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KLS1-SIM-066"
			(at 7.557755 -1.700746 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:KLS1-SIM-066"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Nano SIM Card Connector, Push-Push, 6-Pin, H1.37mm, with CD Pin"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L-KLS1-SIM-066-(6+1)P-H1.37-R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "KLS Electronic"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "L-KLS1-SIM-066-(6+1)P-H1.37-R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "KLS1-SIM-066"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-01-01"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-01-01"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "KLS1-SIM-066"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://klsele.com/admin/product_upload/20190123133741L-KLS1-SIM-066-(6+1)P-H1.37-R--.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://klsele.com/products/connectors/SIM-card-connectors-Micro-SIM-card-connectors-Nano-SIM-Card-Connectors/4918.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "L-KLS1-SIM-066-(6+1)P-H1.37-R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500776"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500776"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*KLS1-SIM-066*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 6.1423 7.611551 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "" np_thru_hole circle
			(at -0.17 12.3 180)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "" np_thru_hole circle
			(at 8.33 12.3 180)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "0" smd rect
			(at -1.67 1.54999 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "power_in")
		)
		(pad "0" smd rect
			(at -1.67 13.55 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "power_in")
		)
		(pad "0" smd rect
			(at 11.32 1.54999 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "power_in")
		)
		(pad "0" smd rect
			(at 11.32 13.55 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "power_in")
		)
		(pad "C1" smd rect
			(at 5.08 0)
			(size 0.75 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "SIM_1V8")
			(pinfunction "VSIM")
			(pintype "passive")
		)
		(pad "C2" smd rect
			(at 2.54 0)
			(size 0.75 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(D1-DATA1_OUT)")
			(pinfunction "SIMRST")
			(pintype "passive")
		)
		(pad "C3" smd rect
			(at 0 0)
			(size 0.75 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(D1-CLK_OUT)")
			(pinfunction "SIMCLK")
			(pintype "passive")
		)
		(pad "C5" smd rect
			(at 6.35 0)
			(size 0.75 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "C6" smd rect
			(at 3.81 0)
			(size 0.75 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "unconnected-(J6-SIMVPP-PadC6)")
			(pinfunction "SIMVPP")
			(pintype "passive+no_connect")
		)
		(pad "C7" smd rect
			(at 1.27 0)
			(size 0.75 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(D1-DATA2_OUT)")
			(pinfunction "SIMDATA")
			(pintype "passive")
		)
		(pad "CD" smd rect
			(at 7.3 0)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(J6-PadCD)")
			(pinfunction "CD")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 200.0025 95.262505) (xy 198.8025 95.262495) (xy 198.8025 91.462495) (xy 200.0025 91.462495)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 200.0025 102.162505) (xy 198.8025 102.162495) (xy 198.8025 98.362495) (xy 200.0025 98.362495)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 202.5425 95.262505) (xy 201.3425 95.262495) (xy 201.3425 91.462495) (xy 202.5425 91.462495)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 202.5425 102.162505) (xy 201.3425 102.162495) (xy 201.3425 98.362495) (xy 202.5425 98.362495)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 205.0825 95.262505) (xy 203.8825 95.262495) (xy 203.8825 91.462495) (xy 205.0825 91.462495)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 205.0825 102.162505) (xy 203.8825 102.162495) (xy 203.8825 98.362495) (xy 205.0825 98.362495)
				)
			)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/SIM8066-6-1-14-01-A--3DModel-STEP-56544.STEP"
			(offset
				(xyz 4.82191 -7.55 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "FP:L-KLS7-TS6616B-2.5-160-T"
		(layer "F.Cu")
		(at 160.97 71.2 90)
		(property "Reference" "SW1"
			(at -3.61766 0.125 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PB SW"
			(at -7.28599 -3.0353 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:L-KLS7-TS6616B-2.5-160-T"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tactile Switch, SPNO, SMD, 160gf, 6.2x6.4x2.5mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "L-KLS7-TS6616B-2.5-160-T"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "KLS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "L-KLS7-TS6616B-2.5-160-T"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "L-KLS7-TS6616B-2.5-160-T"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-02"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2021-07-02"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "PB SW"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "~{\\}hiz~{z}pr~{o}app971~{7}Datashee~{t}switche~{s}KL~{S}L-KLS7-TS6616B-2.5-160-T.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "L-KLS7-TS6616B-2.5-160-T"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101500133"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Switches"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "masi"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101500133, 101500001"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*L-KLS7-TS6616B-2.5-160-T*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.05844 0.058219 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -3.025 -2 90)
			(size 2.75 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.O")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 3.025 -2 90)
			(size 2.75 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.O")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.025 2 90)
			(size 2.75 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "RESET_IN")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.025 2 90)
			(size 2.75 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "RESET_IN")
			(pinfunction "COM")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/L-KLS7-TS6616B-2.5-160-T-BLACK.step"
			(offset
				(xyz -0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 151.935 80.4 90)
		(property "Reference" "C2"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:Fiducial"
		(layer "F.Cu")
		(at 214 102)
		(property "Reference" "Fid3"
			(at 0.148815 -1.89595 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial mark"
			(at -0.7493 3.47599 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:Fiducial"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fiducial Mark"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Fid-Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "Fiducial"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500073"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500073"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fiducial*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(pad "0" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.5)
			(thermal_bridge_angle 90)
		)
		(pad "0" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(solder_mask_margin 0.5)
			(thermal_bridge_angle 90)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 214.196066 101.014311) (xy 214.384597 101.071501) (xy 214.558348 101.164373) (xy 214.710642 101.289358)
					(xy 214.835627 101.441652) (xy 214.928499 101.615403) (xy 214.985689 101.803934) (xy 215.005 102)
					(xy 214.985689 102.196066) (xy 214.928499 102.384597) (xy 214.835627 102.558348) (xy 214.710642 102.710642)
					(xy 214.558348 102.835627) (xy 214.384597 102.928499) (xy 214.196066 102.985689) (xy 214 103.005)
					(xy 213.803934 102.985689) (xy 213.615403 102.928499) (xy 213.441652 102.835627) (xy 213.289358 102.710642)
					(xy 213.164373 102.558348) (xy 213.071501 102.384597) (xy 213.014311 102.196066) (xy 212.995 102)
					(xy 213.000186 102) (xy 213.019397 102.195054) (xy 213.076292 102.382612) (xy 213.168685 102.555467)
					(xy 213.293025 102.706975) (xy 213.444533 102.831315) (xy 213.617388 102.923708) (xy 213.804946 102.980603)
					(xy 214 102.999814) (xy 214.195054 102.980603) (xy 214.382612 102.923708) (xy 214.555467 102.831315)
					(xy 214.706975 102.706975) (xy 214.831315 102.555467) (xy 214.923708 102.382612) (xy 214.980603 102.195054)
					(xy 214.999814 102) (xy 214.980603 101.804946) (xy 214.923708 101.617388) (xy 214.831315 101.444533)
					(xy 214.706975 101.293025) (xy 214.555467 101.168685) (xy 214.382612 101.076292) (xy 214.195054 101.019397)
					(xy 214 101.000186) (xy 213.804946 101.019397) (xy 213.617388 101.076292) (xy 213.444533 101.168685)
					(xy 213.293025 101.293025) (xy 213.168685 101.444533) (xy 213.076292 101.617388) (xy 213.019397 101.804946)
					(xy 213.000186 102) (xy 212.995 102) (xy 213.014311 101.803934) (xy 213.071501 101.615403) (xy 213.164373 101.441652)
					(xy 213.289358 101.289358) (xy 213.441652 101.164373) (xy 213.615403 101.071501) (xy 213.803934 101.014311)
					(xy 214 100.995)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 214.196066 101.014311) (xy 214.384597 101.071501) (xy 214.558348 101.164373) (xy 214.710642 101.289358)
					(xy 214.835627 101.441652) (xy 214.928499 101.615403) (xy 214.985689 101.803934) (xy 215.005 102)
					(xy 214.985689 102.196066) (xy 214.928499 102.384597) (xy 214.835627 102.558348) (xy 214.710642 102.710642)
					(xy 214.558348 102.835627) (xy 214.384597 102.928499) (xy 214.196066 102.985689) (xy 214 103.005)
					(xy 213.803934 102.985689) (xy 213.615403 102.928499) (xy 213.441652 102.835627) (xy 213.289358 102.710642)
					(xy 213.164373 102.558348) (xy 213.071501 102.384597) (xy 213.014311 102.196066) (xy 212.995 102)
					(xy 213.000186 102) (xy 213.019397 102.195054) (xy 213.076292 102.382612) (xy 213.168685 102.555467)
					(xy 213.293025 102.706975) (xy 213.444533 102.831315) (xy 213.617388 102.923708) (xy 213.804946 102.980603)
					(xy 214 102.999814) (xy 214.195054 102.980603) (xy 214.382612 102.923708) (xy 214.555467 102.831315)
					(xy 214.706975 102.706975) (xy 214.831315 102.555467) (xy 214.923708 102.382612) (xy 214.980603 102.195054)
					(xy 214.999814 102) (xy 214.980603 101.804946) (xy 214.923708 101.617388) (xy 214.831315 101.444533)
					(xy 214.706975 101.293025) (xy 214.555467 101.168685) (xy 214.382612 101.076292) (xy 214.195054 101.019397)
					(xy 214 101.000186) (xy 213.804946 101.019397) (xy 213.617388 101.076292) (xy 213.444533 101.168685)
					(xy 213.293025 101.293025) (xy 213.168685 101.444533) (xy 213.076292 101.617388) (xy 213.019397 101.804946)
					(xy 213.000186 102) (xy 212.995 102) (xy 213.014311 101.803934) (xy 213.071501 101.615403) (xy 213.164373 101.441652)
					(xy 213.289358 101.289358) (xy 213.441652 101.164373) (xy 213.615403 101.071501) (xy 213.803934 101.014311)
					(xy 214 100.995)
				)
			)
		)
	)
	(footprint "FP:SOTFL50P162X60-6N"
		(layer "F.Cu")
		(at 156.342505 68.26 90)
		(property "Reference" "Q3"
			(at 0.14772 -1.50125 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DMC2400UV"
			(at -1.4097 3.88239 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:SOTFL50P162X60-6N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual N & P Ch MOFET, 1.03A/0.7A, 480mOhm, 450mW"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "DMC2400UV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Diodes Incorporated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "DMC2400UV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-01-18"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-01-18"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "DMC2400UV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Dual N & P Channel Digital FET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "SOT-563"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007803"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.diodes.com/_files/datasheets/DMC2400UV.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "DMC2400UV-7DICT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300117"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300117"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOTFL50P162X60-6N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.04781 -1.166609 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.775 -0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "S1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.775 0 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "VBUS")
			(pinfunction "G1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.775 0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "4" smd rect
			(at 0.775 0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "5" smd rect
			(at 0.775 0 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 0.775 -0.5 180)
			(size 0.35 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "Net-(Q3A-D1)")
			(pinfunction "D1")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/SOTFL50P162X60-6N.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 168.18 74.12 180)
		(property "Reference" "R38"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M0"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1M0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-071ML"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1M0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001418"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100093"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107108"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100093"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "/nRF5340_Interface_MCU/SWD_CTRL")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 164.25 89.25 -90)
		(property "Reference" "C49"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CONN_BM04B-SRSS-TB_SPK"
		(layer "F.Cu")
		(at 162.09995 101.21315 180)
		(tags "PRT-16766 ")
		(property "Reference" "P4"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x4, Angled"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:CONN_BM04B-SRSS-TB_SPK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Sparkfun"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "PRT-16766"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "LIST_ANG_1x4-SMD-2.54MM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x4, Angled"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "1125B-1104S0Z135CR02"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.4216 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "VDD_3V3")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.499999 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "TWI_SDA_3V3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 1.4216 180)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "TWI_SCL_3V3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 2.799999 -1.103399 180)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 156.092505 63.01 180)
		(property "Reference" "R6"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47k"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-47k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-0747KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "47k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001423"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100076"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100076"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "USB_DETECT")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 157.43501 84.31)
		(property "Reference" "R11"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-074K7L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4k7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001706"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100061"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "PMIC_TWI_SCL")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 156.545 85.88 -90)
		(property "Reference" "C3"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 172.48 87.69)
		(property "Reference" "C36"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/nRF5340_Interface_MCU/DECR")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:TC2050-IDC-NLFP"
		(layer "F.Cu")
		(at 149.93 55.14 180)
		(property "Reference" "J3"
			(at 0.125 1.51767 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TC2050-IDC"
			(at 6.196546 -1.4404 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:TC2050-IDC-NLFP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CBL PLUG-OF-NAILS 10-PIN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "TC2050-IDC-NLFP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Tag-Connect LLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "TC2050-IDC-NLFP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2012-11-21"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2012-11-21"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "TC2050-IDC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "TC2050-IDC-NLFP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.tag-connect.com/Materials/TC2050-IDC%20Datasheet.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "TC2050-IDC-NL-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500463"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "10"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500463"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TC2050-IDC-NLFP*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.606731 0.04353 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "" np_thru_hole circle
			(at -3.81 0 180)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "" np_thru_hole circle
			(at 3.81 -1.016 180)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "" np_thru_hole circle
			(at 3.81 1.016 180)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "1" smd circle
			(at -2.54 0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "2" smd circle
			(at -1.27 0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/nRF5340_Interface_MCU/IMCU_SWDIO")
			(pinfunction "2")
			(pintype "passive")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "3" smd circle
			(at 0 0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "4" smd circle
			(at 1.27 0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/nRF5340_Interface_MCU/IMCU_SWDCLK")
			(pinfunction "4")
			(pintype "passive")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "5" smd circle
			(at 2.54 0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "VBUS'")
			(pinfunction "5")
			(pintype "passive")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "6" smd circle
			(at 2.54 -0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "unconnected-(J3-Pad6)")
			(pinfunction "6")
			(pintype "passive+no_connect")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "7" smd circle
			(at 1.27 -0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "unconnected-(J3-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "8" smd circle
			(at 0 -0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "unconnected-(J3-Pad8)")
			(pinfunction "8")
			(pintype "passive+no_connect")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "9" smd circle
			(at -1.27 -0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "unconnected-(J3-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(pad "10" smd circle
			(at -2.54 -0.635 270)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "/nRF5340_Interface_MCU/IMCU_RESET")
			(pinfunction "10")
			(pintype "passive")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 152.45 55.78) (xy 152.45 54.51) (xy 147.37 54.51) (xy 147.37 55.78)
				)
			)
		)
	)
	(footprint "FP:DFN65P200X200X80_HS-6N"
		(layer "F.Cu")
		(at 151.92 70.63 180)
		(property "Reference" "Q1"
			(at 0.075 -1.48232 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MCM2301"
			(at -0.8883 -2.615146 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:DFN65P200X200X80_HS-6N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual P-Channel MOFET, 3.8A, 90mOhm max, 1.4W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Micro Commercial Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://www.mccsemi.com/pdf/Products/MCM2301(DFN2020-6L).pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/en/products/detail/micro-commercial-co/MCM2301-TP/9655971"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.mccsemi.com/product-detail/MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "VDFN-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "MCM2301-TPMSCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "833-MCM2301-TP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DFN65P200X200X80_HS-6N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.09924 -0.089209 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.90499 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "VBUS'")
			(pinfunction "S1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "2" smd rect
			(at -0.90499 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 156 "Net-(Q1A-G1)")
			(pinfunction "G1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at -0.90499 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at 0 0.47501 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "4" smd rect
			(at 0.905 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "5" smd rect
			(at 0.905 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0 -0.475 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "VBUS")
			(pinfunction "D1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0.905 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "VBUS")
			(pinfunction "D1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/QFN65P200X200X65-6N.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 204.83 76.78 180)
		(property "Reference" "R26"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M0"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-1M0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201JR-071ML"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1M0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001418"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100093"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107108"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100093"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 122 "/nRF9151_SiP/COEX2")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 166.66 80.15 90)
		(property "Reference" "C50"
			(at -1.404825 -0.13896 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 203.31 87.36 -90)
		(property "Reference" "C53"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-10n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GMD033R61A103KA01D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000003480"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200067"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26621779"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200067"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1005X04L*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "SIM_1V8")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:TP_SMD_D1.5mm"
		(layer "F.Cu")
		(at 151.5 77.57 90)
		(property "Reference" "TP2"
			(at 0.11354 -1.37305 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Ø1.5mm,SMD"
			(at -0.5715 3.29819 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:TP_SMD_D1.5mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.5mm circular SMD testpad"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "TP_SMD_Ø1.5MM"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Nordic Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "TP_SMD_Ø1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-03-05"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-06-02"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Ø1.5mm,SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500477"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500477"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TP_SMD_D1.5mm*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.03363 0.008421 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 176 "/nRF9151_Power_Supply/VBUSOUT")
			(pinfunction "1")
			(pintype "passive")
			(solder_paste_margin -5)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "FP:P822601"
		(locked yes)
		(layer "F.Cu")
		(at 227.59 77.66 -90)
		(property "Reference" "A1"
			(at -25.88625 -0.204225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "P822601"
			(at -40.91419 -1.7579 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:P822601"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ANTENNA PRESTTA OCTABAND LTE"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "P822601"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Ethertronics"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "P822601"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "P822601"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-07-28"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2017-07-28"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "P822601"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "http://www.ethertronics.com/wp-content/uploads/2016/11/Prestta-P822601-P822602-Standard-Cellular-Octa-Band-20160904.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "moreelectronics.dk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "P822601"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Digi-Key"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "939-1057-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100700043"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Antennas"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100700043"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*P822601*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(pad "" smd custom
			(at -24.19553 2.54626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.30447) (xy 0.5 -0.30447) (xy 0.5 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -22.5 0.54626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2) (xy 4.3 -2) (xy 4.3 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -22.5 1.04626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.3) (xy 0.5 -0.3) (xy 0.5 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -22.5 2.04626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2) (xy 1 -2) (xy 1 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -22.5 3.54626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2) (xy 1 -2) (xy 1 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -22.5 5.04626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2) (xy 1 -2) (xy 1 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -22.4 0.84626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2.1) (xy 1.7 -2.1) (xy 1.7 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -21.6 -1.25374)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2.9) (xy 2.5 -2.9) (xy 2.5 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -21.6 3.74626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2.9) (xy 2.5 -2.9) (xy 2.5 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -21 3.54626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 2.5 -1) (xy 2.5 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -10.45 7.9961)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2) (xy 1.5 -2) (xy 1.49984 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -10.45 11.29627)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -14.2) (xy 3.30017 -14.2) (xy 3.30001 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.59999 9.19626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.20002) (xy 0.6 -0.20002) (xy 0.6 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.59999 11.29627)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.20002) (xy 0.40001 -0.20002) (xy 0.40001 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 7.09626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 7.49626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 8.19626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 8.59626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 9.39626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 9.79626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 10.49626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.45 10.89626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -9.20002 6.49626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -3.24998) (xy 0.5 -3.24998) (xy 0.5 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.59998 6.89626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.20002) (xy 1.2 -0.20002) (xy 1.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 7.09626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 7.29626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.50001) (xy 0.2 -1.50001) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 7.49626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 8.19626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 8.39626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.50001) (xy 0.2 -1.50001) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 8.59626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 9.39626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 9.59626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.50001) (xy 0.2 -1.50001) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 9.79626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 10.49626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 10.69626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.50001) (xy 0.2 -1.50001) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.44999 10.89626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.5) (xy 0.2 -0.5) (xy 0.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -8.19997 5.69626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.00005) (xy 1.9 -1.00005) (xy 1.9 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.29999 3.79626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -3.10001) (xy 3.2 -3.10001) (xy 3.2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -3.86 7.99626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -8.59) (xy 2 -8.59) (xy 2 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -3.67001 3.82626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2.7291) (xy 3.26 -2.72999) (xy 3.26 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -3.67001 5.99626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2.03999) (xy 2.17 -2.03999) (xy 2.17 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -3.67001 7.99126)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -4.37996) (xy 1.995 -4.37996) (xy 1.995 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 4.7 5.79626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 2.05 -1) (xy 2.05 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 6.2 5.79626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 2.05 -1) (xy 2.05 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.7 4.59626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 0.85 -1) (xy 0.85 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.7 5.79626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 0.9 -1) (xy 0.9 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 9.2 4.59626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 0.85 -1) (xy 0.85 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 9.2 5.79626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 0.9 -1) (xy 0.9 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 10.7 4.59626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 0.85 -1) (xy 0.85 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 10.7 5.79626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 0.9 -1) (xy 0.9 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 13.2 4.59626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2) (xy 0.85 -2) (xy 0.85 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 13.2 4.89626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -6.5) (xy 0.3 -6.5) (xy 0.3 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 13.2 5.79626)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2) (xy 0.9 -2) (xy 0.9 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 24.6 2.04626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -2.9) (xy 5.8 -2.9) (xy 5.8 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 24.6 5.79626)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -12.55) (xy 3.75 -12.55) (xy 3.75 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 24.75 11.29627)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -32.79997) (xy 3.29501 -32.79997) (xy 3.29501 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 24.75157 11.29627)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -49.39927) (xy 3.30001 -49.40157) (xy 3.30001 -0.00157)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd rect
			(at -8.89 2.286 270)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(A1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -5.08 2.286 270)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 232.59 38.66) (xy 232.59 117.66) (xy 219.5139 117.66) (xy 219.5139 38.66)
				)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 156.555 81.12 180)
		(property "Reference" "R22"
			(at -0.94747 -0.02966 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at -3.42519 -0.1905 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-100k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D100KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100k"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001419"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100080"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26108487"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100080"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 130 "VDD_3V3_EN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 270)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:AMPHENOL_10114829-10102LF"
		(layer "F.Cu")
		(at 181.6375 53.525 180)
		(property "Reference" "P2"
			(at -3.8625 -2.225 180)
			(layer "F.SilkS")
		)
		(property "Value" "Pin List 1x2, Angled"
			(at 12.75 2.965 180)
			(layer "F.Fab")
		)
		(property "Footprint" "FP:AMPHENOL_10114829-10102LF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin List 1x4, 2.54mm (100mil), Right Angled, SMD"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin List Ang 1x4 SMD, 2.54mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "10114829-10102LF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "10114829-10102LF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-04-29"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2015-01-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin List 1x2, Angled"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "10114829-10102LF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "TSM-104-01-L-SH-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004780"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500358"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LIST_ANG_1x4-SMD-2.54MM*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -0.625 0 180)
			(size 1.108 1.108)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 167 "VBAT_IN")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0.625 0 180)
			(size 1.108 1.108)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 190.67 78.94)
		(property "Reference" "R23"
			(at -0.94747 -0.02966 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at -3.42519 -0.1905 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-7D10KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001255"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100065"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26107101"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100065"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(M1A-VDD)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "Net-(M1A-ENABLE)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 172.48 83.89)
		(property "Reference" "C34"
			(at -1.404825 -0.13896 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.0µF"
			(at 3.01879 0.0381 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±20%, 10V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-1µ0-10V-X5R-GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61A105ME15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R61A105ME15-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.murata.com/en-us/products/productdetail?partno=GRM033R61A105ME15%23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2023-03-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "1.0µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-13226-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200545"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 214.54 64.29 -90)
		(property "Reference" "C22"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U3-VEN)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 213.83 64.29 -90)
		(property "Reference" "C25"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100pF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±2%, 25V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100p"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM0335C1E101GA01"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100pF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "25V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007853"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200044"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200044"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U3-VEN)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:AQFN40P700X700X85_HS-99N"
		(layer "F.Cu")
		(at 166.85 84.76 -90)
		(property "Reference" "U5"
			(at -2.6 -4.22332 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "nRF5340-QKAA"
			(at -0.05209 4.799546 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:AQFN40P700X700X85_HS-99N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multi-protocol Bluetooth Low Energy, IEEE 802.15.4, ANT and 2.4GHz proprietary system-on-chip"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "nRF5340-QKAAD0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "102000216"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Nordic_Devices"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Nordic Semiconductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "nRF5340-QKAAD0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "AQFN-98"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-12-02"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "98"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2020-12-02"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "nRF5340-QKAA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Nordic Semiconductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "nRF5340-QKAAD0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "NOD26470035"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "102000216"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*AQFN40P700X700X85_HS-99N*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "AL17"
			(at 0.05563 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A21"
			(at 0.89828 -3.3502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AJ31"
			(at 3.32234 2.6498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A5"
			(at -2.27219 -3.35089 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AG1"
			(at -3.54071 2.2498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "C1"
			(at -3.4688 -2.5502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "L1"
			(at -3.48853 -0.9502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "C31"
			(at 3.32234 -2.5502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK30"
			(at 2.66221 3.04911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK4"
			(at -2.50826 3.04911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "J31"
			(at 3.32234 -1.3502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "N31"
			(at 3.32234 -0.55019 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AH2"
			(at -3.20803 2.4498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL11"
			(at -1.14437 3.44917 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK20"
			(at 0.66221 3.0498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A13"
			(at -0.70172 -3.3502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK18"
			(at 0.26221 3.049 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B16"
			(at -0.09846 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B22"
			(at 1.10154 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK10"
			(at -1.33779 3.0498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "F2"
			(at -3.12806 -1.9502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A23"
			(at 1.29828 -3.3502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AD2"
			(at -3.20803 1.6498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B30"
			(at 2.70154 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "L31"
			(at 3.32234 -0.9502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "E1"
			(at -3.44919 -2.1502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AC31"
			(at 3.32234 1.4498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL15"
			(at -0.34437 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AF2"
			(at -3.20803 2.04981 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK22"
			(at 1.0622 3.04911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "R31"
			(at 3.32234 -0.1502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AB2"
			(at -3.20803 1.2498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK2"
			(at -2.90826 3.02325 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "P2"
			(at -3.12806 -0.3502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A27"
			(at 2.09828 -3.35089 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "R1"
			(at -3.45565 -0.1502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B26"
			(at 1.90154 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B12"
			(at -0.89846 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL5"
			(at -2.31484 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK28"
			(at 2.2622 3.049 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL7"
			(at -1.91484 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AA1"
			(at -3.5342 1.0498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AA31"
			(at 3.32234 1.0498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "E31"
			(at 3.32234 -2.1502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "T2"
			(at -3.12806 0.0498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B8"
			(at -1.66893 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "M2"
			(at -3.12806 -0.7502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B6"
			(at -2.06893 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK8"
			(at -1.70826 3.049 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AC1"
			(at -3.54071 1.4498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "D2"
			(at -3.12806 -2.3502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "K2"
			(at -3.12806 -1.1502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL25"
			(at 1.65563 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A25"
			(at 1.69828 -3.35089 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL21"
			(at 0.85563 3.44917 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL29"
			(at 2.45563 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B14"
			(at -0.49846 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "J1"
			(at -3.4688 -1.3502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK14"
			(at -0.53779 3.04911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B28"
			(at 2.30154 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B2"
			(at -2.85316 -2.93741 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK24"
			(at 1.46221 3.04911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A19"
			(at 0.49828 -3.35089 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AE1"
			(at -3.5211 1.8498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "W31"
			(at 3.32234 0.64981 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B10"
			(at -1.29846 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A17"
			(at 0.09829 -3.35089 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL3"
			(at -2.71484 3.44917 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "G1"
			(at -3.4688 -1.75019 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL27"
			(at 2.05563 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "V2"
			(at -3.12806 0.4498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "U31"
			(at 3.32234 0.2498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK6"
			(at -2.10826 3.049 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "U1"
			(at -3.4688 0.2498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B20"
			(at 0.70154 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "N1"
			(at -3.44919 -0.55019 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AJ1"
			(at -3.54071 2.6498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL9"
			(at -1.54437 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK26"
			(at 1.86221 3.049 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B24"
			(at 1.50154 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "H2"
			(at -3.12806 -1.5502 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AG31"
			(at 3.32234 2.2498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "A15"
			(at -0.30172 -3.35089 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK16"
			(at -0.1378 3.049 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "G31"
			(at 3.32234 -1.75019 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "W1"
			(at -3.4688 0.64981 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "Y2"
			(at -3.12806 0.84981 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B18"
			(at 0.30154 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL13"
			(at -0.74437 3.44917 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AK12"
			(at -0.93779 3.04911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "B4"
			(at -2.46893 -2.95109 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL23"
			(at 1.25563 3.44917 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AE31"
			(at 3.32234 1.8498 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "AL19"
			(at 0.45563 3.44911 -90)
			(unlocked yes)
			(layer "User.5")
		)
		(fp_text user "${REFERENCE}"
			(at -0.00077 0.010781 -90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "104" smd rect
			(at 0.2 0 270)
			(size 5.4 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS_PAD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin -5)
		)
		(pad "A1" smd circle
			(at -3.2 -3.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 195 "unconnected-(U5D-N.C.-PadA1)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A5" smd circle
			(at -2.2 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(U5A-VBUS)")
			(pinfunction "VBUS")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A13" smd circle
			(at -0.6 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "/nRF5340_Interface_MCU/DECA")
			(pinfunction "DECA")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A15" smd circle
			(at -0.2 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U5A-DECD)")
			(pinfunction "DECD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A17" smd circle
			(at 0.2 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 208 "unconnected-(U5C-P1.13-PadA17)")
			(pinfunction "P1.13")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A19" smd circle
			(at 0.6 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A21" smd circle
			(at 1 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 212 "unconnected-(U5A-DCC-PadA21)")
			(pinfunction "DCC")
			(pintype "output+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A23" smd circle
			(at 1.4 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/nRF5340_Interface_MCU/DECN")
			(pinfunction "DECN")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A25" smd circle
			(at 1.8 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.C.")
			(pintype "passive")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A27" smd circle
			(at 2.2 -3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/nRF5340_Interface_MCU/DECR")
			(pinfunction "DECR")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "A31" smd circle
			(at 3.2 -3.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 199 "unconnected-(U5D-N.C.-PadA31)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AA1" smd circle
			(at -3.2 1 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 229 "/nRF5340_Interface_MCU/SWD3_RESET")
			(pinfunction "P0.03/NFC2")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AA31" smd circle
			(at 3.2 1 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/nRF5340_Interface_MCU/IMCU_SWDIO")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AB2" smd circle
			(at -2.8 1.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "/nRF5340_Interface_MCU/SWD_CTRL")
			(pinfunction "P0.06/AIN2")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AC1" smd circle
			(at -3.2 1.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AC31" smd circle
			(at 3.2 1.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "/nRF5340_Interface_MCU/IMCU_RESET")
			(pinfunction "~{RESET}")
			(pintype "input")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AD2" smd circle
			(at -2.8 1.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 227 "unconnected-(U5B-P0.07{slash}AIN3-PadAD2)")
			(pinfunction "P0.07/AIN3")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AE1" smd circle
			(at -3.2 1.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 166 "PMIC_TWI_SDA")
			(pinfunction "P1.02/TWI")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AE31" smd circle
			(at 3.2 1.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 202 "unconnected-(U5B-P0.28{slash}AIN7-PadAE31)")
			(pinfunction "P0.28/AIN7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AF2" smd circle
			(at -2.8 2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "PMIC_TWI_SCL")
			(pinfunction "P1.03/TWI")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AG1" smd circle
			(at -3.2 2.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AG31" smd circle
			(at 3.2 2.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 223 "unconnected-(U5D-N.C.-PadAG31)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AH2" smd circle
			(at -2.8 2.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 191 "unconnected-(U5B-P0.08{slash}TRACEDATA[3]-PadAH2)")
			(pinfunction "P0.08/TRACEDATA[3]")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AJ1" smd circle
			(at -3.2 2.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "unconnected-(U5B-P0.09{slash}TRACEDATA[2]-PadAJ1)")
			(pinfunction "P0.09/TRACEDATA[2]")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AJ31" smd circle
			(at 3.2 2.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK2" smd circle
			(at -2.8 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 220 "unconnected-(U5B-P0.10{slash}TRACEDATA[1]-PadAK2)")
			(pinfunction "P0.10/TRACEDATA[1]")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK4" smd circle
			(at -2.4 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 200 "unconnected-(U5B-P0.11{slash}TRACEDATA[0]-PadAK4)")
			(pinfunction "P0.11/TRACEDATA[0]")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK6" smd circle
			(at -2 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 198 "unconnected-(U5B-P0.12{slash}TRACECLK-PadAK6)")
			(pinfunction "P0.12/TRACECLK")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK8" smd circle
			(at -1.6 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 233 "unconnected-(U5B-P0.14{slash}QSPI[1]-PadAK8)")
			(pinfunction "P0.14/QSPI[1]")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK10" smd circle
			(at -1.2 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "TWI_SDA")
			(pinfunction "P0.15/QSPI[2]")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK12" smd circle
			(at -0.8 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "TWI_SCL")
			(pinfunction "P0.17/QSPI_CLK")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK14" smd circle
			(at -0.4 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 228 "unconnected-(U5B-P0.18{slash}QSPI_CS-PadAK14)")
			(pinfunction "P0.18/QSPI_CS")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK16" smd circle
			(at 0 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 194 "unconnected-(U5B-P0.20-PadAK16)")
			(pinfunction "P0.20")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK18" smd circle
			(at 0.4 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 205 "unconnected-(U5B-P0.22-PadAK18)")
			(pinfunction "P0.22")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK20" smd circle
			(at 0.8 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 221 "unconnected-(U5B-P0.23-PadAK20)")
			(pinfunction "P0.23")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK22" smd circle
			(at 1.2 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 216 "unconnected-(U5C-P1.05-PadAK22)")
			(pinfunction "P1.05")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK24" smd circle
			(at 1.6 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 226 "unconnected-(U5C-P1.07-PadAK24)")
			(pinfunction "P1.07")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK26" smd circle
			(at 2 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 203 "unconnected-(U5C-P1.09-PadAK26)")
			(pinfunction "P1.09")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK28" smd circle
			(at 2.4 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 224 "unconnected-(U5B-P0.25{slash}AIN4-PadAK28)")
			(pinfunction "P0.25/AIN4")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AK30" smd circle
			(at 2.8 2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 230 "unconnected-(U5B-P0.27{slash}AIN6-PadAK30)")
			(pinfunction "P0.27/AIN6")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL1" smd circle
			(at -3.2 3.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "unconnected-(U5D-N.C.-PadAL1)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL3" smd circle
			(at -2.6 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL5" smd circle
			(at -2.2 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 231 "unconnected-(U5B-P0.13{slash}QSPI[0]-PadAL5)")
			(pinfunction "P0.13/QSPI[0]")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL7" smd circle
			(at -1.8 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL9" smd circle
			(at -1.4 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "unconnected-(U5B-P0.16{slash}QSPI[3]-PadAL9)")
			(pinfunction "P0.16/QSPI[3]")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL11" smd circle
			(at -1 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL13" smd circle
			(at -0.6 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 219 "unconnected-(U5B-P0.19-PadAL13)")
			(pinfunction "P0.19")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL15" smd circle
			(at -0.2 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "unconnected-(U5B-P0.21-PadAL15)")
			(pinfunction "P0.21")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL17" smd circle
			(at 0.2 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL19" smd circle
			(at 0.6 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "UART1_TXD")
			(pinfunction "P1.04")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL21" smd circle
			(at 1 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "UART2_TXD")
			(pinfunction "P1.06")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL23" smd circle
			(at 1.4 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "UART2_RXD")
			(pinfunction "P1.08")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL25" smd circle
			(at 1.8 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL27" smd circle
			(at 2.2 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "RESET_IN")
			(pinfunction "P0.24")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL29" smd circle
			(at 2.6 3.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/nRF5340_Interface_MCU/IMCU_LED")
			(pinfunction "P0.26/AIN5")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "AL31" smd circle
			(at 3.2 3.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 210 "unconnected-(U5D-N.C.-PadAL31)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B2" smd circle
			(at -2.8 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "IMCU_USB_D_P")
			(pinfunction "D+")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B4" smd circle
			(at -2.4 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "IMCU_USB_D_N")
			(pinfunction "D-")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B6" smd circle
			(at -2 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/nRF5340_Interface_MCU/DECUSB")
			(pinfunction "DECUSB")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B8" smd circle
			(at -1.6 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B10" smd circle
			(at -1.2 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 193 "unconnected-(U5A-DCCD-PadB10)")
			(pinfunction "DCCD")
			(pintype "power_in+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B12" smd circle
			(at -0.8 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.C.")
			(pintype "passive")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B14" smd circle
			(at -0.4 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 225 "unconnected-(U5C-P1.15-PadB14)")
			(pinfunction "P1.15")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B16" smd circle
			(at 0 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "SWD0_SWDIO")
			(pinfunction "P1.14")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B18" smd circle
			(at 0.4 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 145 "SWD0_SWDCLK")
			(pinfunction "P1.12")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B20" smd circle
			(at 0.8 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "SWD0_SWO")
			(pinfunction "P1.11")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B22" smd circle
			(at 1.2 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 152 "SWD0_RESET")
			(pinfunction "P0.31")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B24" smd circle
			(at 1.6 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 151 "SWD0_SELECT")
			(pinfunction "P0.30")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B26" smd circle
			(at 2 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.C.")
			(pintype "passive")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B28" smd circle
			(at 2.4 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "B30" smd circle
			(at 2.8 -2.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 234 "/nRF5340_Interface_MCU/XC2")
			(pinfunction "XC2")
			(pintype "output")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "C1" smd circle
			(at -3.2 -2.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "C31" smd circle
			(at 3.2 -2.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "/nRF5340_Interface_MCU/XC1")
			(pinfunction "XC1")
			(pintype "input")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "D2" smd circle
			(at -2.8 -2.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 209 "unconnected-(U5D-N.C.-PadD2)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "E1" smd circle
			(at -3.2 -2.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDDH")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "E31" smd circle
			(at 3.2 -2.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "F2" smd circle
			(at -2.8 -2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "unconnected-(U5D-N.C.-PadF2)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "G1" smd circle
			(at -3.2 -1.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.C.")
			(pintype "passive")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "G31" smd circle
			(at 3.2 -1.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/nRF5340_Interface_MCU/DECR")
			(pinfunction "DECRF")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "H2" smd circle
			(at -2.8 -1.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.C.")
			(pintype "passive")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "J1" smd circle
			(at -3.2 -1.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 206 "unconnected-(U5A-DCCH-PadJ1)")
			(pinfunction "DCCH")
			(pintype "power_in+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "J31" smd circle
			(at 3.2 -1.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "N.C.")
			(pintype "passive")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "K2" smd circle
			(at -2.8 -1.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "L1" smd circle
			(at -3.2 -1 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "L31" smd circle
			(at 3.2 -1 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "Net-(J4-X)")
			(pinfunction "ANT")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "M2" smd circle
			(at -2.8 -0.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 214 "unconnected-(U5C-P1.00-PadM2)")
			(pinfunction "P1.00")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "N1" smd circle
			(at -3.2 -0.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 192 "/nRF5340_Interface_MCU/SWD3_IO")
			(pinfunction "P0.00/XL1")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "N31" smd circle
			(at 3.2 -0.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "P2" smd circle
			(at -2.8 -0.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 204 "unconnected-(U5C-P1.01-PadP2)")
			(pinfunction "P1.01")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "R1" smd circle
			(at -3.2 -0.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 201 "/nRF5340_Interface_MCU/SWD3_CLK")
			(pinfunction "P0.01/XL2")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "R31" smd circle
			(at 3.2 -0.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 215 "unconnected-(U5C-P1.10-PadR31)")
			(pinfunction "P1.10")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "T2" smd circle
			(at -2.8 0 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 222 "unconnected-(U5D-N.C.-PadT2)")
			(pinfunction "N.C.")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "U1" smd circle
			(at -3.2 0.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "U31" smd circle
			(at 3.2 0.2 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 137 "UART1_RXD")
			(pinfunction "P0.29")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "V2" smd circle
			(at -2.8 0.4 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 217 "unconnected-(U5B-P0.04{slash}AIN0-PadV2)")
			(pinfunction "P0.04/AIN0")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "W1" smd circle
			(at -3.2 0.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 196 "/nRF5340_Interface_MCU/SWD3_SWO")
			(pinfunction "P0.02/NFC1")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "W31" smd circle
			(at 3.2 0.6 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/nRF5340_Interface_MCU/IMCU_SWDCLK")
			(pinfunction "SWDCLK")
			(pintype "input")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(pad "Y2" smd circle
			(at -2.8 0.8 270)
			(size 0.225 0.225)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "USB_DETECT")
			(pinfunction "P0.05/AIN1")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.0125)
			(thermal_bridge_angle 90)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/aQFN-94 (7x7).sldprt"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "FP:HDR_2x5-SMD-1.27mm-K"
		(layer "F.Cu")
		(at 174.35 71.15 180)
		(property "Reference" "P6"
			(at 3.68665 0.038825 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Pin Header 2x5, 1.27mm"
			(at -3.0607 7.08279 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:HDR_2x5-SMD-1.27mm-K"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header 2x5, 1.27mm (50mil), SMD, Keying Shroud"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Pin Header 2x5 SMD, 1.27mm, KS"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "WCON"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "3132-10MS0BK00R1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "HDR_2x5-SMD-1.27mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2016-04-21"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2016-01-22"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Pin Header 2x5, 1.27mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "55010009"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000009968"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not Mounted"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "~{\\}hiz~{z}pr~{o}app971~{7}Datashee~{t}connector~{s}W-CO~{N}3132-XXMXXBK00XX.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Cabcon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "3132-10MS0BK00R1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "FTSH-105-01-F-DV-K"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100500261"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "10"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500261"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*HDR_2x5-SMD-1.27mm-K*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "1"
			(at -2.41291 3.688415 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd rect
			(at -2.54 1.95001 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.54 -1.95 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "nRF91_SWD_SWDIO")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.27 1.95001 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.27 -1.95 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "nRF91_SWD_SWDCLK")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 1.95001 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0 -1.95 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "TRACE_DATA0")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 1.27 1.95001 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 142 "unconnected-(P6-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 1.27 -1.95 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 140 "unconnected-(P6-Pad8)")
			(pinfunction "8")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at 2.54 1.95001 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 2.54 -1.95 180)
			(size 0.76 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "nRF91_SWD_RESET")
			(pinfunction "10")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/Samtec-FTSH-105-01-F-DV-K.step"
			(offset
				(xyz 0.00008 0.00008 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "FP:Nordic_QFN50P500X500X90-33N"
		(layer "F.Cu")
		(at 152.865 85.34 90)
		(property "Reference" "U1"
			(at -1.925 -3.71767 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "nPM1300-QEAA"
			(at -5.89589 -5.1534 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:Nordic_QFN50P500X500X90-33N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Li-Ion/Li-Polymer USB-C battery charger with high efficiency buck regulators, LDOs or load switches, LED drivers, TWI and VBUSOUT"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "nPM1300-QEAA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "102000291"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Nordic_Devices"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "eisk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Nordic Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "nPM1300-QEAA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2023-05-25"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-02-17"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "33"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "QFN-32"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "nPM1300-QEAA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Nordic Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "nPM1300-QEAA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "102000291"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Nordic_QFN50P500X500X90-33N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.48501 -0.046094 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd oval
			(at -2.45001 -1.75001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VOUT1")
			(pintype "power_in")
		)
		(pad "2" smd oval
			(at -2.45001 -1.25001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PVSS1")
			(pintype "power_in")
		)
		(pad "3" smd oval
			(at -2.45001 -0.75002 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/nRF9151_Power_Supply/SW1")
			(pinfunction "SW1")
			(pintype "power_in")
		)
		(pad "4" smd oval
			(at -2.45001 -0.24999 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/nRF9151_Power_Supply/VSYS")
			(pinfunction "PVDD")
			(pintype "power_in")
		)
		(pad "5" smd oval
			(at -2.45001 0.24998 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "/nRF9151_Power_Supply/SW2")
			(pinfunction "SW2")
			(pintype "power_in")
		)
		(pad "6" smd oval
			(at -2.45001 0.75001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PVSS2")
			(pintype "power_in")
		)
		(pad "7" smd oval
			(at -2.45001 1.25001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 182 "unconnected-(U1-GPIO0-Pad7)")
			(pinfunction "GPIO0")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" smd oval
			(at -2.45001 1.75 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 183 "unconnected-(U1-GPIO1-Pad8)")
			(pinfunction "GPIO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd oval
			(at -1.75001 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 178 "unconnected-(U1-GPIO2-Pad9)")
			(pinfunction "GPIO2")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" smd oval
			(at -1.25001 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 177 "unconnected-(U1-GPIO3-Pad10)")
			(pinfunction "GPIO3")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd oval
			(at -0.75001 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 184 "unconnected-(U1-GPIO4-Pad11)")
			(pinfunction "GPIO4")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd oval
			(at -0.24999 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD")
			(pinfunction "VDDIO")
			(pintype "power_in")
		)
		(pad "13" smd oval
			(at 0.24999 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 166 "PMIC_TWI_SDA")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "14" smd oval
			(at 0.75001 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "PMIC_TWI_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "15" smd oval
			(at 1.25001 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 179 "unconnected-(U1-SHPHLD-Pad15)")
			(pinfunction "SHPHLD")
			(pintype "input+no_connect")
		)
		(pad "16" smd oval
			(at 1.75001 2.45 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 170 "Net-(U1-VSET2)")
			(pinfunction "VSET2")
			(pintype "input")
		)
		(pad "17" smd oval
			(at 2.45001 1.75 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "Net-(U1-VSET1)")
			(pinfunction "VSET1")
			(pintype "input")
		)
		(pad "18" smd oval
			(at 2.45001 1.25001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "NTC")
			(pintype "input")
		)
		(pad "19" smd oval
			(at 2.45001 0.75001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "VBAT_PWR")
			(pinfunction "VBAT")
			(pintype "passive")
		)
		(pad "20" smd oval
			(at 2.45001 0.24998 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/nRF9151_Power_Supply/VSYS")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "21" smd oval
			(at 2.45001 -0.24999 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_5V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "22" smd oval
			(at 2.45001 -0.75002 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 176 "/nRF9151_Power_Supply/VBUSOUT")
			(pinfunction "VBUSOUT")
			(pintype "power_in")
		)
		(pad "23" smd oval
			(at 2.45001 -1.25001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "unconnected-(U1-CC1-Pad23)")
			(pinfunction "CC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" smd oval
			(at 2.45001 -1.75001 180)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 181 "unconnected-(U1-CC2-Pad24)")
			(pinfunction "CC2")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd oval
			(at 1.75001 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 186 "unconnected-(U1-LED0-Pad25)")
			(pinfunction "LED0")
			(pintype "output+no_connect")
		)
		(pad "26" smd oval
			(at 1.25001 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 187 "unconnected-(U1-LED1-Pad26)")
			(pinfunction "LED1")
			(pintype "output+no_connect")
		)
		(pad "27" smd oval
			(at 0.75001 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 180 "unconnected-(U1-LED2-Pad27)")
			(pinfunction "LED2")
			(pintype "output+no_connect")
		)
		(pad "28" smd oval
			(at 0.24999 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "VDD_3V0")
			(pinfunction "LSIN1/VINLDO1")
			(pintype "power_in")
		)
		(pad "29" smd oval
			(at -0.24999 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "VDD_GNSS")
			(pinfunction "LSOUT1/VOUTLDO1")
			(pintype "power_in")
		)
		(pad "30" smd oval
			(at -0.75001 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "LSIN2/VINLDO2")
			(pintype "power_in")
		)
		(pad "31" smd oval
			(at -1.25001 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "LSOUT2/VOUTLDO2")
			(pintype "power_in")
		)
		(pad "32" smd oval
			(at -1.75001 -2.45001 90)
			(size 0.3 0.85001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "VDD_3V0")
			(pinfunction "VOUT2")
			(pintype "power_in")
		)
		(pad "33" smd rect
			(at 0 0 90)
			(size 3.5 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "AVSS")
			(pintype "power_in")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/QFN50P500X500X90_HS-33N.step"
			(offset
				(xyz -0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:RESC0603X03L_C"
		(layer "F.Cu")
		(at 153.96 73.71 90)
		(property "Reference" "R4"
			(at -0.94747 -0.02966 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "150k"
			(at -3.42519 -0.1905 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:RESC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, ±1%, 0.05W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "R0201-150k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Yageo"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "RC0201FR-07150KL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "150k"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "Chip Res 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001422"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100100082"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100100082"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC0603X03L_C*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.72123 0.010761 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.285 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.28499 0 180)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "VBUS")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-res0201-1.step"
			(offset
				(xyz 0.00008 0.00011 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:LED_0603_G"
		(layer "F.Cu")
		(at 159.295 89.96)
		(property "Reference" "LED1"
			(at 0 -2.0131 0)
			(unlocked yes)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "L0603G"
			(at -2.84861 1.4859 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:LED_0603_G"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LED, Green, 0603, 573nm, Vf=2.0V, 24mcd, - 40 to +85°C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "VS 25C7M5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Victory Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "VS 25C7M5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-10-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2017-08-21"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "L0603G"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "13019193"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001274, 00000009961"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "~{\\}hiz~{z}pr~{o}app971~{7}Datashee~{t}optoelectronic~{s}Victory Electronic~{s}VS 25C7M5.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "EC Partner"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101400097"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Optoelectronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "26313411"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101400097"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED_0603_G*")
		(sheetname "nRF5340_Interface_MCU")
		(sheetfile "nRF5340_Interface_MCU.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.050805 -0.889219 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.6985 0 180)
			(size 0.762 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "Net-(LED1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.6985 0 180)
			(size 0.762 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-led_0603_green.step"
			(offset
				(xyz 0.00646 -0.00005 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 212.18 64.22 -90)
		(property "Reference" "C29"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100pF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±2%, 25V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100p"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM0335C1E101GA01"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100pF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "25V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000007853"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200044"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200044"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U3-VCC)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "F.Cu")
		(at 209.86 71.85 -90)
		(property "Reference" "C24"
			(at -1.404825 -0.13896 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "39pF"
			(at 3.01879 0.0381 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±1%, 25V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-39p"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM0335C1E390FA01"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2019-04-16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "39pF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "25V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001668"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "100200039"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200039"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 -0.010781 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/nRF9151_SiP/GPS_RF3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0)
			(size 0.3 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/nRF9151_SiP/GPS_RF2")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(footprint "FP:DFN65P200X200X80_HS-6N"
		(layer "F.Cu")
		(at 151.98 63.36 180)
		(property "Reference" "Q2"
			(at 0.075 -1.48232 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MCM2301"
			(at -0.8883 -2.615146 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:DFN65P200X200X80_HS-6N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual P-Channel MOFET, 3.8A, 90mOhm max, 1.4W"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Micro Commercial Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "https://www.mccsemi.com/pdf/Products/MCM2301(DFN2020-6L).pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/en/products/detail/micro-commercial-co/MCM2301-TP/9655971"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.mccsemi.com/product-detail/MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "VDFN-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2022-12-27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "MCM2301"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "MCM2301-TPMSCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "833-MCM2301-TP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rubr"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTID" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "101300199"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DFN65P200X200X80_HS-6N*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.09924 -0.089209 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.90499 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "VBAT'")
			(pinfunction "S1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "2" smd rect
			(at -0.90499 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "Net-(Q2A-G1)")
			(pinfunction "G1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at -0.90499 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "3" smd rect
			(at 0 0.47501 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "4" smd rect
			(at 0.905 0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "5" smd rect
			(at 0.905 0 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0 -0.475 180)
			(size 0.92 0.71)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "VBAT")
			(pinfunction "D1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(pad "6" smd rect
			(at 0.905 -0.65 270)
			(size 0.42 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "VBAT")
			(pinfunction "D1")
			(pintype "passive")
			(solder_mask_margin 0.055)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/QFN65P200X200X65-6N.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:Molex_502774-0891"
		(layer "B.Cu")
		(at 191.64999 87.83)
		(property "Reference" "J7"
			(at 12.32752 -1.60475 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "microSD Card Connector"
			(at -7.0993 -10.33399 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:Molex_502774-0891"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.10mm Pitch microSD Memory Card Connector, Reverse Mount Surface Mount, Push-Push Type"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Molex_502774-0891"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Molex"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "502774-0891"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "http://www.molex.com/pdm_docs/sd/5027740891_sd.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://www.molex.com/molex/products/part-detail/memory_card_socket/5027740891"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "Molex 502774-0891"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-02-06"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2017-11-08"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "microSD Card Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "WM24066CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Elfa"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "300-76-403"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001284"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTID" "100500509"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "14"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500509"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Molex_502774-0891*")
		(sheetname "Connectors")
		(sheetfile "Connectors.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 5.629925 7.116572 0)
			(unlocked yes)
			(layer "User.8")
		)
		(pad "0" smd rect
			(at -0.75 14.77 180)
			(size 1.5 1.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "0" smd rect
			(at -0.21 0 180)
			(size 1.6 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "0" smd rect
			(at 12.45 0 180)
			(size 1.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "0" smd rect
			(at 12.75 14.77 180)
			(size 1.5 1.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "1" smd rect
			(at 8.9 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 56 "TRACE_DATA2")
			(pinfunction "DAT2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 7.8 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 61 "TRACE_DATA3")
			(pinfunction "CD/DAT3")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at 6.70001 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "DBG_CMD")
			(pinfunction "CMD")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at 5.60001 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at 4.50001 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 57 "TRACE_CLK")
			(pinfunction "CLK")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at 3.40001 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at 2.30001 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 59 "TRACE_DATA0")
			(pinfunction "DAT0")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at 1.2 0.08 180)
			(size 0.8 1.68)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 62 "TRACE_DATA1")
			(pinfunction "DAT1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "9" smd rect
			(at -0.96 1.6 180)
			(size 1.29 1.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "10" smd rect
			(at -0.96 8.97 180)
			(size 1.29 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 58 "unconnected-(J7-Pad10)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/5027740891.stp"
			(offset
				(xyz 2.49994 6.59991 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -180 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1608X06L"
		(layer "B.Cu")
		(at 154.115 89.14 180)
		(property "Reference" "C5"
			(at -1.16796 1.27709 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "10µF"
			(at -1.35891 -2.306511 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1608X06L"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7T, ±20%, 10V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0603-10µ-10V-X7T-GRM188D71A106MA73"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTID" "100200414"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM188D71A106MA73"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://no.mouser.com/datasheet/2/281/murata_03052018_GRM_Series_1-1310166.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-22"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-09-11"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "NOTE" "10VDC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-7200-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-GRM188D71A106MA3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004696"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200414"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.25 0.162338 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0 90)
			(size 0.8 0.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0 90)
			(size 0.8 0.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "/nRF9151_Power_Supply/VSYS")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Capacitor 0603.step"
			(offset
				(xyz -0.00005 -0.43011 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1608X06L"
		(layer "B.Cu")
		(at 151.095 89.14)
		(property "Reference" "C6"
			(at -1.16796 1.27709 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "10µF"
			(at -1.35891 -2.306511 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1608X06L"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X7T, ±20%, 10V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0603-10µ-10V-X7T-GRM188D71A106MA73"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTID" "100200414"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM188D71A106MA73"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://no.mouser.com/datasheet/2/281/murata_03052018_GRM_Series_1-1310166.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2021-07-22"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-09-11"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10µF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "NOTE" "10VDC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-7200-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "81-GRM188D71A106MA3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000004696"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200414"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_Power_Supply")
		(sheetfile "nRF9151_Power_Supply.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0.25 0.162338 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.675 0 270)
			(size 0.8 0.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0 270)
			(size 0.8 0.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "/nRF9151_Power_Supply/VSYS")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-Chip Capacitor 0603.step"
			(offset
				(xyz -0.00005 -0.43011 0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "FP:CAPC1005X04L"
		(layer "B.Cu")
		(at 200.57 74.13 180)
		(property "Reference" "C14"
			(at -0.16053 1.29174 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "4.7µF"
			(at -0.7239 -2.89179 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC1005X04L"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, 10V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0402-4µ7-10V-X5R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM155R61A475MEAAD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R61A475MEAA-01.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "https://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM155R61A475MEAAD/490-14306-1-ND/6234742"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HELPURL" "https://psearch.en.murata.com/capacitor/product/GRM155R61A475MEAA%23.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2020-10-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2018-10-04"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "4.7µF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "NOTE" "10V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "Digi-Key"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "490-14306-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTID" "100200415"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200415"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1608X06L*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.4318 -0.189738 0)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0402(1005M) Cap.step"
			(offset
				(xyz 0.00007 0.00007 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "FP:Solderbridge"
		(layer "B.Cu")
		(at 199.4 84.37 90)
		(property "Reference" "SB1"
			(at -1.903965 0.12356 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Solderbridge"
			(at 3.69443 -0.3429 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:Solderbridge"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solderbridge"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Solderbridge"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2009-12-14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2009-12-14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "Solderbridge"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "Solderbridge"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTID" "100500458"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500458"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Solderbridge*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -0.057185 -1.126334 90)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "" smd custom
			(at -0.190168 0.491816)
			(size 0.000001 0.000001)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 0.0762)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(arc
							(start 0 0)
							(mid -0.171708 0.293949)
							(end -0.491803 0.409832)
						)
						(arc
							(start -0.491806 0.409832)
							(mid -0.811897 0.293949)
							(end -0.983609 0.000008)
						)
						(arc
							(start -0.983613 0.000001)
							(mid -0.96716 -0.062682)
							(end -0.908472 -0.090168)
						)
						(xy -0.908466 -0.090168)
						(arc
							(start -0.075138 -0.090168)
							(mid -0.016457 -0.062682)
							(end -0.00001 -0.000004)
						)
						(xy -0.000006 0.000002)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 0.190168 -0.491806)
			(size 0.000001 0.000001)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 0.0762)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(arc
							(start 0 0)
							(mid 0.171708 -0.293949)
							(end 0.491803 -0.409832)
						)
						(arc
							(start 0.491806 -0.409822)
							(mid 0.811897 -0.293939)
							(end 0.983609 0.000002)
						)
						(arc
							(start 0.983613 -0.000001)
							(mid 0.96716 0.062682)
							(end 0.908472 0.090168)
						)
						(xy 0.908466 0.090168)
						(arc
							(start 0.075138 0.090168)
							(mid 0.016457 0.062682)
							(end 0.00001 0.000004)
						)
						(xy -0.000004 0.000008)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd circle
			(at -0.35 0 90)
			(size 0.0254 0.0254)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "DBG_CMD")
			(pinfunction "0")
			(pintype "passive")
			(solder_paste_margin -2147.483637)
			(thermal_bridge_angle 90)
		)
		(pad "2" smd circle
			(at 0.35 0 270)
			(size 0.0254 0.0254)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "Net-(SB1-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_paste_margin -2147.483637)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "FP:Fiducial"
		(layer "B.Cu")
		(at 214 53.5 180)
		(property "Reference" "Fid1"
			(at 0.148815 1.89595 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial mark"
			(at -0.7493 -3.47599 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:Fiducial"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Fiducial Mark"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "Fid-Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2009-12-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "NOTE" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "Fiducial"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" "Not mounted"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTID" "100500073"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100500073"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SYSTEM" "Connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fiducial*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(pad "0" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.5)
			(thermal_bridge_angle 90)
		)
		(pad "0" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(solder_mask_margin 0.5)
			(thermal_bridge_angle 90)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 213.803934 52.514311) (xy 213.615403 52.571501) (xy 213.441652 52.664373) (xy 213.289358 52.789358)
					(xy 213.164373 52.941652) (xy 213.071501 53.115403) (xy 213.014311 53.303934) (xy 212.995 53.5)
					(xy 213.014311 53.696066) (xy 213.071501 53.884597) (xy 213.164373 54.058348) (xy 213.289358 54.210642)
					(xy 213.441652 54.335627) (xy 213.615403 54.428499) (xy 213.803934 54.485689) (xy 214 54.505) (xy 214.196066 54.485689)
					(xy 214.384597 54.428499) (xy 214.558348 54.335627) (xy 214.710642 54.210642) (xy 214.835627 54.058348)
					(xy 214.928499 53.884597) (xy 214.985689 53.696066) (xy 215.005 53.5) (xy 214.999814 53.5) (xy 214.980603 53.695054)
					(xy 214.923708 53.882612) (xy 214.831315 54.055467) (xy 214.706975 54.206975) (xy 214.555467 54.331315)
					(xy 214.382612 54.423708) (xy 214.195054 54.480603) (xy 214 54.499814) (xy 213.804946 54.480603)
					(xy 213.617388 54.423708) (xy 213.444533 54.331315) (xy 213.293025 54.206975) (xy 213.168685 54.055467)
					(xy 213.076292 53.882612) (xy 213.019397 53.695054) (xy 213.000186 53.5) (xy 213.019397 53.304946)
					(xy 213.076292 53.117388) (xy 213.168685 52.944533) (xy 213.293025 52.793025) (xy 213.444533 52.668685)
					(xy 213.617388 52.576292) (xy 213.804946 52.519397) (xy 214 52.500186) (xy 214.195054 52.519397)
					(xy 214.382612 52.576292) (xy 214.555467 52.668685) (xy 214.706975 52.793025) (xy 214.831315 52.944533)
					(xy 214.923708 53.117388) (xy 214.980603 53.304946) (xy 214.999814 53.5) (xy 215.005 53.5) (xy 214.985689 53.303934)
					(xy 214.928499 53.115403) (xy 214.835627 52.941652) (xy 214.710642 52.789358) (xy 214.558348 52.664373)
					(xy 214.384597 52.571501) (xy 214.196066 52.514311) (xy 214 52.495)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 213.803934 52.514311) (xy 213.615403 52.571501) (xy 213.441652 52.664373) (xy 213.289358 52.789358)
					(xy 213.164373 52.941652) (xy 213.071501 53.115403) (xy 213.014311 53.303934) (xy 212.995 53.5)
					(xy 213.014311 53.696066) (xy 213.071501 53.884597) (xy 213.164373 54.058348) (xy 213.289358 54.210642)
					(xy 213.441652 54.335627) (xy 213.615403 54.428499) (xy 213.803934 54.485689) (xy 214 54.505) (xy 214.196066 54.485689)
					(xy 214.384597 54.428499) (xy 214.558348 54.335627) (xy 214.710642 54.210642) (xy 214.835627 54.058348)
					(xy 214.928499 53.884597) (xy 214.985689 53.696066) (xy 215.005 53.5) (xy 214.999814 53.5) (xy 214.980603 53.695054)
					(xy 214.923708 53.882612) (xy 214.831315 54.055467) (xy 214.706975 54.206975) (xy 214.555467 54.331315)
					(xy 214.382612 54.423708) (xy 214.195054 54.480603) (xy 214 54.499814) (xy 213.804946 54.480603)
					(xy 213.617388 54.423708) (xy 213.444533 54.331315) (xy 213.293025 54.206975) (xy 213.168685 54.055467)
					(xy 213.076292 53.882612) (xy 213.019397 53.695054) (xy 213.000186 53.5) (xy 213.019397 53.304946)
					(xy 213.076292 53.117388) (xy 213.168685 52.944533) (xy 213.293025 52.793025) (xy 213.444533 52.668685)
					(xy 213.617388 52.576292) (xy 213.804946 52.519397) (xy 214 52.500186) (xy 214.195054 52.519397)
					(xy 214.382612 52.576292) (xy 214.555467 52.668685) (xy 214.706975 52.793025) (xy 214.831315 52.944533)
					(xy 214.923708 53.117388) (xy 214.980603 53.304946) (xy 214.999814 53.5) (xy 215.005 53.5) (xy 214.985689 53.303934)
					(xy 214.928499 53.115403) (xy 214.835627 52.941652) (xy 214.710642 52.789358) (xy 214.558348 52.664373)
					(xy 214.384597 52.571501) (xy 214.196066 52.514311) (xy 214 52.495)
				)
			)
		)
	)
	(footprint "FP:CAPC0603X03L_C"
		(layer "B.Cu")
		(at 200.51 73.37 180)
		(property "Reference" "C12"
			(at -1.404825 0.13896 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 3.01879 -0.0381 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "FP:CAPC0603X03L_C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, X5R, ±10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER" "C0201-100n"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "FOOTPRINT DOC" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ASSEMBLY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT CLASS" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AUTHOR" "rsk"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PAD COUNT" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTID" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER PART NUMBER" "GRM033R61C104KE14D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK1DESCRIPTION" "Datasheet"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2URL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENTLINK2DESCRIPTION" "Supplier link"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HELPURL" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LATESTREVISIONDATE" "2017-11-09"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PUBLISHED" "2014-11-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "NOTE" "16V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 1" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SUPPLIER PART NUMBER 2" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ARTIKKELNR NOCA" "N.A."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER IPS" "00000001248, 00000002505"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NORAUTRON" "262071862"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "COMPONENT STATUS" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PART NUMBER NEMS" "100200078"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC0603X03L_C*")
		(sheetname "nRF9151_SiP")
		(sheetfile "nRF9151_SiP.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at -1.028785 0.010781 180)
			(unlocked yes)
			(layer "User.7")
		)
		(pad "1" smd rect
			(at -0.28499 0 90)
			(size 0.3 0.27)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "VDD")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0.285 0 90)
			(size 0.3 0.27)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0201(0603M) Cap.step"
			(offset
				(xyz 0.00009 0.0001 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 0)
			)
		)
	)
	(gr_rect
		(start 137.08 51.71)
		(end 232.08 103.71)
		(fill none)
		(layer "Edge.Cuts")
	)
	(zone
		(net 158)
		(net_name "VBAT")
		(layer "F.Cu")
		(hatch none 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.85 63.8) (xy 151.3 63.8) (xy 151.52 63.58) (xy 151.52 63.48) (xy 152.44 63.48) (xy 152.44 64.40222)
				(xy 152.797145 64.68) (xy 152.99 64.68) (xy 153.05999 64.74) (xy 153.05999 66.4) (xy 152.60999 66.4)
				(xy 152.39 66.61999) (xy 152.39 66.71999) (xy 151.47 66.71999) (xy 151.47 65.42) (xy 150.85 64.8)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 203.97 83.11) (xy 202.64 82.92) (xy 202.16 83.36) (xy 202.16 83.97) (xy 203.91 83.91)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.31 51.71) (xy 232.08 51.72) (xy 232.08 103.61) (xy 137.08 103.7) (xy 137.01 51.72)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.13 51.71) (xy 232.01 51.75) (xy 232.07 103.71) (xy 137.09 103.7)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.26 51.85) (xy 231.98 51.79) (xy 231.97 103.59) (xy 137.19 103.53) (xy 137.25 51.86)
			)
		)
	)
)
