(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.611)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" power)
		(6 "In2.Cu" signal)
		(8 "In3.Cu" signal)
		(10 "In4.Cu" power)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.025)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "#808080FF")
				(thickness 0.069)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.03)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.075)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.03)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.109)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02) addsublayer
				(color "FR4 natural")
				(thickness 0.865)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02) addsublayer
				(color "FR4 natural")
				(thickness 0.109)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.03)
			)
			(layer "dielectric 4"
				(type "core")
				(color "FR4 natural")
				(thickness 0.075)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.03)
			)
			(layer "dielectric 5"
				(type "prepreg")
				(thickness 0.069)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.025)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting none)
		(grid_origin 50.1 186.2)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/PWR_nRF91")
	(net 3 "/nRF9151 - Power + RF/nRF91_VDD_GPIO")
	(net 4 "/nRF9151 - Power + RF/nRF91_VDD")
	(net 5 "Net-(U1A-DEC0)")
	(net 6 "/nRF9151 - Power + RF/LNA_EN_FILT")
	(net 7 "/nRF9151 - Power + RF/LNA_VCC_IN")
	(net 8 "/nRF9151 - GPIO + UICC/nRESET_FILT")
	(net 9 "VCC")
	(net 10 "/USB/PWR_USB_5V0_IN")
	(net 11 "/Power Management/ACDRV1_S")
	(net 12 "/Power Management/ACDRV1_G")
	(net 13 "/Power Management/ACDRV2_G")
	(net 14 "/Power Management/ACDRV2_S")
	(net 15 "/Power Management/PWR_VBUS")
	(net 16 "/Power Management/PMID")
	(net 17 "/PWR_USB_IN")
	(net 18 "/Power Management/REGN")
	(net 19 "/PWR_PANEL")
	(net 20 "/PWR_USB")
	(net 21 "/Power Management/BTST2")
	(net 22 "/Power Management/SW2")
	(net 23 "/Power Management/BTST1")
	(net 24 "/Power Management/SW1")
	(net 25 "/nRF52833/XC2")
	(net 26 "/PWR_3V3")
	(net 27 "/Power Management/CT")
	(net 28 "/Power Management/SDRV")
	(net 29 "/nRF52833/DEC3")
	(net 30 "/nRF52833/XC1")
	(net 31 "/nRF52833/ANT_MATCH")
	(net 32 "/PWR_nRF52")
	(net 33 "/nRF52833/DEC4_6")
	(net 34 "/USB/USB_CMC_D_P")
	(net 35 "/USB/USB_CC1")
	(net 36 "/USB/USB_CC2")
	(net 37 "/BAT_N")
	(net 38 "/USB/USB_CMC_D_N")
	(net 39 "Net-(U10-DEC1)")
	(net 40 "/nRF9151 - GPIO + UICC/LED_GREEN")
	(net 41 "/nRF9151 - GPIO + UICC/LED_RED")
	(net 42 "/nRF9151 - GPIO + UICC/LED_YELLOW")
	(net 43 "/nRF9151 - Power + RF/LTE_ANT")
	(net 44 "/nRF9151 - GPIO + UICC/APP_SIM_DETECT")
	(net 45 "/nRF9151 - GPIO + UICC/SIM_CLK_EXT")
	(net 46 "/nRF9151 - GPIO + UICC/SIM_RST_EXT")
	(net 47 "/nRF9151 - GPIO + UICC/SIM_IO_EXT")
	(net 48 "/PWR_BAT_IN")
	(net 49 "/PANEL_DETECT")
	(net 50 "/PWR_PANEL_IN")
	(net 51 "Net-(U10-P0.18{slash}RESET)")
	(net 52 "Net-(U10-DECUSB)")
	(net 53 "unconnected-(CN1-SBU2-PadB8)")
	(net 54 "unconnected-(CN1-SBU1-PadA8)")
	(net 55 "/I2C_SBUS.SDA")
	(net 56 "/I2C_SBUS.SCL")
	(net 57 "/nRF52833/nRF_GPIO0")
	(net 58 "unconnected-(J12-NC-Pad8)")
	(net 59 "/nRF52833/nRF52_SWCLK")
	(net 60 "/nRF52833/nRF91_SWD.nRESET")
	(net 61 "/nRF52_nRESET")
	(net 62 "/nRF52833/nRF52_SWDIO")
	(net 63 "unconnected-(J12-KEY-Pad7)")
	(net 64 "/nRF9151 - GPIO + UICC/SWO_UNUSED")
	(net 65 "unconnected-(J13-VPP{slash}SWP-PadC6)")
	(net 66 "/PWR_3V3_LS_OUT")
	(net 67 "/nRF9151 - Power + RF/FIL_OUT")
	(net 68 "/nRF9151 - Power + RF/AMP_IN")
	(net 69 "unconnected-(J15-NC-Pad8)")
	(net 70 "/nRF52833/ANT_BLE")
	(net 71 "/nRF52833/DCC_L")
	(net 72 "/nRF52833/DCC")
	(net 73 "Net-(U1A-ENABLE)")
	(net 74 "/nRF9151 - Power + RF/LTE_ANT_TUNED")
	(net 75 "/nRF9151 - GPIO + UICC/LNA_EN")
	(net 76 "unconnected-(J15-KEY-Pad7)")
	(net 77 "Net-(U6-LX2)")
	(net 78 "Net-(U6-LX1)")
	(net 79 "/Power Management/I2C_PMIC.SCL")
	(net 80 "/USB/USB_D_N")
	(net 81 "/USB/USB_D_P")
	(net 82 "/Power Management/ACDRV1")
	(net 83 "/Power Management/ACDRV2")
	(net 84 "/Power Management/PROG")
	(net 85 "/BOOST_PWM_EN")
	(net 86 "/Power Management/BATP")
	(net 87 "/nRF52833/RADIO")
	(net 88 "/nRF9151 - GPIO + UICC/SPI_FLASH_SCLK")
	(net 89 "/Power Management/TS")
	(net 90 "/Power Management/FB")
	(net 91 "/Power Management/ILIM_HIZ")
	(net 92 "unconnected-(U1C-COEX2-Pad54)")
	(net 93 "unconnected-(U1D-RESERVED-Pad82)")
	(net 94 "/Power Management/I2C_PMIC.SDA")
	(net 95 "unconnected-(U1D-RESERVED-Pad99)")
	(net 96 "/nRF9151 - GPIO + UICC/SPI_FLASH_SIO1")
	(net 97 "unconnected-(U1D-RESERVED-Pad31)")
	(net 98 "unconnected-(U1C-COEX1-Pad53)")
	(net 99 "unconnected-(U1C-MAGPIO0-Pad21)")
	(net 100 "/nRF9151 - GPIO + UICC/SIM_RST_IN")
	(net 101 "unconnected-(U1D-RESERVED-Pad103)")
	(net 102 "/nRF52833/nRF_GPIO2")
	(net 103 "unconnected-(U1C-SIM_DET-Pad26)")
	(net 104 "unconnected-(U1D-RESERVED-Pad101)")
	(net 105 "unconnected-(U1D-RESERVED-Pad32)")
	(net 106 "unconnected-(U1D-RESERVED-Pad33)")
	(net 107 "/nRF52833/UART0.TX")
	(net 108 "unconnected-(U1D-RESERVED-Pad90)")
	(net 109 "/nRF52833/BLE_SPI.MOSI")
	(net 110 "/nRF9151 - GPIO + UICC/SPI_FLASH_nHOLD{slash}SIO3")
	(net 111 "unconnected-(U1D-RESERVED-Pad92)")
	(net 112 "unconnected-(U1D-RESERVED-Pad100)")
	(net 113 "/nRF52833/BLE_SPI.nCS")
	(net 114 "unconnected-(U1D-RESERVED-Pad98)")
	(net 115 "/nRF52833/nRF_GPIO1")
	(net 116 "unconnected-(U1D-RESERVED-Pad84)")
	(net 117 "unconnected-(U1D-RESERVED-Pad86)")
	(net 118 "unconnected-(U1C-MAGPIO1-Pad22)")
	(net 119 "unconnected-(U1D-RESERVED-Pad91)")
	(net 120 "unconnected-(U1C-SDATA-Pad27)")
	(net 121 "unconnected-(U1C-MAGPIO2-Pad23)")
	(net 122 "unconnected-(U1C-SCLK-Pad28)")
	(net 123 "unconnected-(U1D-RESERVED-Pad96)")
	(net 124 "/nRF9151 - GPIO + UICC/SPI_FLASH_nWP{slash}SIO2")
	(net 125 "unconnected-(U1D-RESERVED-Pad81)")
	(net 126 "unconnected-(U1D-RESERVED-Pad104)")
	(net 127 "/nRF52833/nRF91_SWD.IO")
	(net 128 "/nRF9151 - GPIO + UICC/SIM_CLK_IN")
	(net 129 "unconnected-(U1C-VIO-Pad29)")
	(net 130 "/nRF52833/UART0.RX")
	(net 131 "unconnected-(U1D-RESERVED-Pad93)")
	(net 132 "unconnected-(U1D-RESERVED-Pad85)")
	(net 133 "/nRF52833/BLE_SPI.MISO")
	(net 134 "unconnected-(U1D-RESERVED-Pad97)")
	(net 135 "/nRF52833/BLE_SPI.CLK")
	(net 136 "unconnected-(U5-D+-Pad6)")
	(net 137 "unconnected-(U1D-RESERVED-Pad89)")
	(net 138 "unconnected-(U1D-RESERVED-Pad87)")
	(net 139 "unconnected-(U1D-RESERVED-Pad102)")
	(net 140 "/nRF9151 - Power + RF/GNSS_LNA_RF")
	(net 141 "/nRF9151 - GPIO + UICC/SIM_IO_IN")
	(net 142 "unconnected-(U1D-RESERVED-Pad94)")
	(net 143 "unconnected-(U1D-RESERVED-Pad83)")
	(net 144 "/nRF9151 - GPIO + UICC/SPI_FLASH_SI{slash}SIO0")
	(net 145 "/nRF9151 - GPIO + UICC/SPI_FLASH_nCS")
	(net 146 "/SBUS_EN")
	(net 147 "/nRF9151 - Power + RF/GNSS_RF")
	(net 148 "unconnected-(U1D-RESERVED-Pad88)")
	(net 149 "unconnected-(U1D-RESERVED-Pad95)")
	(net 150 "unconnected-(U5-D--Pad7)")
	(net 151 "unconnected-(U10-DEC5-Pad21)")
	(net 152 "/Power Management/nQON")
	(net 153 "/nRF52833/nRF_GPIO3")
	(net 154 "/nRF52833/nRF91_SWD.CLK")
	(net 155 "unconnected-(J15-SWO-Pad6)")
	(net 156 "/nRF52833/UART1.RX")
	(net 157 "/nRF52833/nRF91_SWD.SWO")
	(net 158 "/nRF52833/UART1.TX")
	(net 159 "/nRF52833/nRF_GPIO4")
	(net 160 "/BQ_nINT")
	(net 161 "/BQ_nCE")
	(net 162 "/Power Management/PWR_SYS")
	(net 163 "/Power Management/PWR_TPS63_VIN")
	(net 164 "/PWR_3V3_LS")
	(net 165 "/Battery Protection/VDD")
	(net 166 "/PWR_BATT")
	(net 167 "/nRF52833/RADIO_MATCH")
	(net 168 "Net-(D1-K)")
	(net 169 "Net-(D2-K)")
	(net 170 "Net-(D3-K)")
	(net 171 "/nRF9151 - GPIO + UICC/SCLK_TERM")
	(net 172 "/Battery Protection/CTR")
	(net 173 "/BAT_P")
	(net 174 "/Battery Protection/BAT_P_POL")
	(net 175 "/Battery Protection/CHG")
	(net 176 "/Battery Protection/DSG")
	(net 177 "/Battery Protection/BAT")
	(net 178 "/Battery Protection/PACK")
	(net 179 "/Power Management/STAT")
	(net 180 "unconnected-(U9-I{slash}O2-Pad3)")
	(net 181 "unconnected-(U9-I{slash}O1-Pad1)")
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 100.7 163)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/17/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10000 pF ±10% 25V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CC0402KRX7R8BB103"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "17"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/nRF9151 - GPIO + UICC/nRESET_FILT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 87.4 170.3 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at -2 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "590"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/133/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "590 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF5900X"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "133"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 169 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/nRF9151 - GPIO + UICC/LED_RED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:JAE_SF72S006VBDR2500"
		(layer "F.Cu")
		(at 115.18 145.685 180)
		(descr "SIM Card, Push-Push, https://www.jae.com/direct/topics/topics_file_download/topics_id=68892&ext_no=06&index=0&_lang=en&v=202003111511468456809")
		(tags "SIM Card with Detect Switch")
		(property "Reference" "J13"
			(at -4.667 -6.541 0)
			(layer "F.SilkS")
		)
		(property "Value" "SF72S006VBDR2500"
			(at -0.98 -6.485 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/10/info"
			(at -2 4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8 (6 + 2) Position Card Connector NANO SIM Surface Mount, Right Angle Gold"
			(at -2 4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Memory Card Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SF72S006VBDR2500"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "JAE Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "10"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "JAE*SIM*Card*SF72S006*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1 2.3 90)
			(layer "F.Fab")
		)
		(pad "C1" smd rect
			(at 0.54 6.46 180)
			(size 0.9 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "C2" smd rect
			(at -2 6.46 180)
			(size 0.9 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "/nRF9151 - GPIO + UICC/SIM_RST_EXT")
			(pinfunction "RST")
			(pintype "input")
		)
		(pad "C3" smd rect
			(at -4.54 6.46 180)
			(size 0.9 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/nRF9151 - GPIO + UICC/SIM_CLK_EXT")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "C5" smd rect
			(at 0.54 3.29 180)
			(size 0.9 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "C6" smd rect
			(at -2 3.29 180)
			(size 0.9 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "unconnected-(J13-VPP{slash}SWP-PadC6)")
			(pinfunction "VPP/SWP")
			(pintype "bidirectional+no_connect")
		)
		(pad "C7" smd rect
			(at -4.54 3.29 180)
			(size 0.9 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/nRF9151 - GPIO + UICC/SIM_IO_EXT")
			(pinfunction "I/O")
			(pintype "bidirectional")
		)
		(pad "CSW" smd rect
			(at -6.27 -0.04 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "CSW")
			(pintype "passive")
		)
		(pad "DSW" smd rect
			(at -2.55 -3.715 180)
			(size 1.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/nRF9151 - GPIO + UICC/APP_SIM_DETECT")
			(pinfunction "DSW")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at -6.595 2.31 180)
			(size 0.45 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at -6.595 7.16 180)
			(size 0.45 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at -6.095 -1.84 180)
			(size 0.75 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at -4.22 -4.79 180)
			(size 1.4 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at -3.22 8.31 180)
			(size 0.3 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at -0.78 8.31 180)
			(size 0.3 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at 0.2 -4.79 180)
			(size 1.4 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at 4.555 -2.84 180)
			(size 0.45 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at 4.555 2.31 180)
			(size 0.45 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at 4.555 7.16 180)
			(size 0.45 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/JAE_SF72S006VBDR2500.STEP"
			(offset
				(xyz -2 2.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 180 180)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 115.99 161.3 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 2.1 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/15/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1002X"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "15"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "/BOOST_PWM_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:L_0402_1005Metric"
		(layer "F.Cu")
		(at 84.635 147.425)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 1.665 0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "9n1"
			(at -0.7 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/23/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "9.1 nH Unshielded Drum Core, Wirewound Inductor 540 mA 140mOhm Max 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Inductors/RF Inductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LQW15AN9N1J00D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/nRF9151 - Power + RF/AMP_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/nRF9151 - Power + RF/FIL_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 82.45 152.275 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 6.75 -0.125 0)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/19/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2GE0R00X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "19"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/nRF9151 - Power + RF/LNA_VCC_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 68.6 163.5 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 2.1 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "47n"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/111/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.047 µF ±10% 10V Ceramic Capacitor X7S 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C0603X7S1A473K030BC"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TDK Corporation"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "111"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/nRF52833/DEC4_6")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 84.22 152.675)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at -7.02 0.225 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/nRF9151 - Power + RF/LNA_VCC_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 100.7 161.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/8/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1001X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "8"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/nRF52833/nRF91_SWD.nRESET")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/nRF9151 - GPIO + UICC/nRESET_FILT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:KOA_TEST_POINT_1206"
		(layer "F.Cu")
		(at 110.6 161.2 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TP5"
			(at 0 -1.82 90)
			(layer "F.SilkS")
		)
		(property "Value" "RCWCTE"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/130/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PC Test Point Plating Surface Mount Mounting Type"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RCWCTE"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KOA Speer Electronics, Inc."
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "130"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 4.2 1.749995)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KOA_RCWCTE.step"
			(offset
				(xyz 0 0 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "footprints:L_0402_1005Metric"
		(layer "F.Cu")
		(at 71.3 162.5 -90)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L6"
			(at 0 -1.17 90)
			(layer "F.SilkS")
		)
		(property "Value" "15n"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/116/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "15 nH Unshielded Multilayer Inductor 450 mA 320mOhm Max 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Inductors/Fixed Inductors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LQG15HS15NJ02D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "116"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/nRF52833/DCC_L")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/nRF52833/DEC4_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:L_0603_1608Metric"
		(layer "F.Cu")
		(at 69.2 161.9)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L7"
			(at 1.1 -1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/115/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10 µH Shielded Multilayer Inductor 300 mA 600mOhm 0603 (1608 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Inductors/Fixed Inductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MLZ1608N100LT000"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TDK Corporation"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0603 (1608 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "115"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/nRF52833/DCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/nRF52833/DCC_L")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 69.8 170.1 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at 0 -1.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "12p"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/104/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "12 pF ±2% 50V Ceramic Capacitor C0G, NP0 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM0335C1H120GA01D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "104"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/nRF52833/XC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 100.7 160.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -1.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/15/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1002X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "15"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/nRF9151 - Power + RF/nRF91_VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Net-(U1A-ENABLE)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:QFN-40-1EP_5x5mm_P0.4mm_EP3.6x3.6mm"
		(layer "F.Cu")
		(at 63.7 164.2 -90)
		(descr "QFN, 40 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=297), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U10"
			(at 3.65 -2.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "NRF52833-QDAA-B-R7"
			(at 0 3.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/122/info"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC RF TxRx + MCU 802.15.4, Bluetooth Bluetooth v5.3, Thread, Zigbee® 2.4GHz 40-VFQFN Exposed Pad"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/RF and Wireless"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NRF52833-QDAA-B-R7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Nordic Semiconductor ASA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "40-QFN (5x5)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "122"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.2 -1.2 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1.2 0 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1.2 1.2 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 -1.2 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 1.2 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.2 -1.2 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.2 0 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.2 1.2 270)
			(size 0.97 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.4375 -1.8 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "Net-(U10-DEC1)")
			(pinfunction "DEC1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.4375 -1.4 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "/nRF52833/BLE_SPI.nCS")
			(pinfunction "P.0.00/XL1")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.4375 -1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/nRF52833/nRF_GPIO0")
			(pinfunction "P0.01/XL2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.4375 -0.6 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/nRF52833/nRF_GPIO1")
			(pinfunction "P0.04/AIN2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -2.4375 -0.2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/nRF52833/nRF_GPIO2")
			(pinfunction "P0.05/AIN3")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -2.4375 0.2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/nRF52833/nRF91_SWD.nRESET")
			(pinfunction "P1.09")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -2.4375 0.6 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "/nRF52833/nRF_GPIO3")
			(pinfunction "P0.11")
			(pintype "passive+no_connect")
		)
		(pad "8" smd roundrect
			(at -2.4375 1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -2.4375 1.4 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pinfunction "VDDH")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at -2.4375 1.8 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/PWR_USB")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -1.8 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(U10-DECUSB)")
			(pinfunction "DECUSB")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at -1.4 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "/USB/USB_D_N")
			(pinfunction "D-")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at -1 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/USB/USB_D_P")
			(pinfunction "D+")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at -0.6 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "/nRF52833/UART1.RX")
			(pinfunction "P0.15")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at -0.2 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "/nRF52833/UART1.TX")
			(pinfunction "P0.17")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 0.2 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(U10-P0.18{slash}RESET)")
			(pinfunction "P0.18/RESET")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at 0.6 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "/nRF52833/nRF_GPIO4")
			(pinfunction "P0.20")
			(pintype "passive+no_connect")
		)
		(pad "18" smd roundrect
			(at 1 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at 1.4 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/nRF52833/nRF52_SWDIO")
			(pinfunction "SWDIO")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at 1.8 2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/nRF52833/nRF52_SWCLK")
			(pinfunction "SWDCLK")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at 2.4375 1.8 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "unconnected-(U10-DEC5-Pad21)")
			(pinfunction "DEC5")
			(pintype "passive+no_connect")
		)
		(pad "22" smd roundrect
			(at 2.4375 1.4 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/nRF52833/UART0.RX")
			(pinfunction "P0.09/NFC1")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at 2.4375 1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/nRF52833/UART0.TX")
			(pinfunction "P0.10/NFC2")
			(pintype "passive")
		)
		(pad "24" smd roundrect
			(at 2.4375 0.6 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "/nRF52833/RADIO")
			(pinfunction "ANT")
			(pintype "passive")
		)
		(pad "25" smd roundrect
			(at 2.4375 0.2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "26" smd roundrect
			(at 2.4375 -0.2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/nRF52833/DEC4_6")
			(pinfunction "DEC6")
			(pintype "passive")
		)
		(pad "27" smd roundrect
			(at 2.4375 -0.6 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/nRF52833/DEC3")
			(pinfunction "DEC3")
			(pintype "passive")
		)
		(pad "28" smd roundrect
			(at 2.4375 -1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/nRF52833/XC1")
			(pinfunction "XC1")
			(pintype "passive")
		)
		(pad "29" smd roundrect
			(at 2.4375 -1.4 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/nRF52833/XC2")
			(pinfunction "XC2")
			(pintype "passive")
		)
		(pad "30" smd roundrect
			(at 2.4375 -1.8 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "31" smd roundrect
			(at 1.8 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/nRF52833/BLE_SPI.MOSI")
			(pinfunction "P0.08")
			(pintype "passive")
		)
		(pad "32" smd roundrect
			(at 1.4 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/nRF52833/BLE_SPI.MISO")
			(pinfunction "P0.29")
			(pintype "passive")
		)
		(pad "33" smd roundrect
			(at 1 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "/nRF52833/BLE_SPI.CLK")
			(pinfunction "P0.30")
			(pintype "passive")
		)
		(pad "34" smd roundrect
			(at 0.6 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "/nRF52833/nRF91_SWD.SWO")
			(pinfunction "P0.28")
			(pintype "passive")
		)
		(pad "35" smd roundrect
			(at 0.2 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "/nRF52833/nRF91_SWD.CLK")
			(pinfunction "P0.03/AIN1")
			(pintype "passive")
		)
		(pad "36" smd roundrect
			(at -0.2 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "/nRF52833/nRF91_SWD.IO")
			(pinfunction "P0.02/AIN0")
			(pintype "passive")
		)
		(pad "37" smd roundrect
			(at -0.6 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "38" smd roundrect
			(at -1 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/nRF52833/DEC4_6")
			(pinfunction "DEC4")
			(pintype "passive")
		)
		(pad "39" smd roundrect
			(at -1.4 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/nRF52833/DCC")
			(pinfunction "DCC")
			(pintype "passive")
		)
		(pad "40" smd roundrect
			(at -1.8 -2.4375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at 0 0 270)
			(size 3.6 3.6)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-40-1EP_5x5mm_P0.4mm_EP3.6x3.6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 63.3 171.1)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C58"
			(at -1.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1p2"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/106/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.2 pF ±0.05pF 50V Ceramic Capacitor C0G, NP0 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM0335C1H1R2WA01D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "106"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "/nRF52833/RADIO_MATCH")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 85.2 170.3 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at -2 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "590"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/133/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "590 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF5900X"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "133"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 170 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/nRF9151 - GPIO + UICC/LED_YELLOW")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 83.646 167.55545)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -1.896 -0.00545 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:XTAL_MP06003_SMD_2016-4Pin_2.0x1.6mm"
		(layer "F.Cu")
		(at 68 170.1 180)
		(descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "XTAL1"
			(at -0.3 -2.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "32M"
			(at 0 2 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/147/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32 MHz ±10ppm Crystal 8pF 50 Ohms 4-SMD, No Lead"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Miscellaneous/Crystals"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MP06003"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Golledge Electronics Ltd"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "4-SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "147"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.725 0.575 180)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/nRF52833/XC2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.725 0.575 180)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.725 -0.575 180)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/nRF52833/XC1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.725 -0.575 180)
			(size 0.95 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/FA-128_32.0000MF20X-K5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 105 160)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 84.22 151.875)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -6.72 -0.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "100p 50V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/109/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100 pF ±5% 50V Ceramic Capacitor C0G, NP0 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM0335C1H101JA01D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "109"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/nRF9151 - Power + RF/LNA_VCC_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 63.3 168.7)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at -1.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1p"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/105/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 pF ±0.05pF 50V Ceramic Capacitor C0G, NP0 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM0335C1H1R0WA01D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "105"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "/nRF52833/RADIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.6 166.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/32/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF4701X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "32"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/Power Management/I2C_PMIC.SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 57.5 165.4 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 1.9 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/17/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10000 pF ±10% 25V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CC0402KRX7R8BB103"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "17"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(U10-P0.18{slash}RESET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:L_0201_0603Metric"
		(layer "F.Cu")
		(at 62.98 172.3 -90)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L9"
			(at 0 -1.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "2n2"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/135/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2 nH Unshielded Thick Film Inductor 600 mA 150mOhm Max 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Inductors/RF Inductors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LQP03TN2N2B02D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "135"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "/nRF52833/RADIO_MATCH")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/nRF52833/ANT_MATCH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0201_0603Metric"
		(layer "F.Cu")
		(at 62.98 178.3 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/134/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0201 (0603 Metric) Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-1GN0R00C"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "134"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "/nRF52833/ANT_BLE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/nRF52833/ANT_MATCH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 84.4 161.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/32/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF4701X"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "32"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/I2C_SBUS.SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0201_0603Metric"
		(layer "F.Cu")
		(at 63.3 177.1 180)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at -1.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/134/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0201 (0603 Metric) Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-1GN0R00C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "134"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/nRF52833/ANT_MATCH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "F.Cu")
		(at 123.475 169.65)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 3.475 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "/Power Management/PWR_SYS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 83.75 168.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -1.7 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/19/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2GE0R00X"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "19"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/nRF9151 - GPIO + UICC/SPI_FLASH_SCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "/nRF9151 - GPIO + UICC/SCLK_TERM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 89.6 167.5)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -1.35 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/nRF9151 - Power + RF/nRF91_VDD_GPIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:MX_8USON"
		(layer "F.Cu")
		(at 82.5 165.4 -90)
		(property "Reference" "U4"
			(at 0 1.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MX25V8035FZUI"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/60/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "FLASH - NOR Memory IC 8Mbit SPI 104 MHz 8-USON (2x3)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/Memory"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MX25V8035FZUI"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Macronix"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "8-USON (2x3)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "60"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOP*3.9x4.9mm*P1.27mm*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.2 -0.75 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "/nRF9151 - GPIO + UICC/SPI_FLASH_nCS")
			(pinfunction "n~{CS}")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at -1.2 -0.25 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "/nRF9151 - GPIO + UICC/SPI_FLASH_SIO1")
			(pinfunction "SO/SIO1")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at -1.2 0.25 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "/nRF9151 - GPIO + UICC/SPI_FLASH_nWP{slash}SIO2")
			(pinfunction "n~{WP}/SIO2")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at -1.2 0.75 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at 1.2 0.75 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "/nRF9151 - GPIO + UICC/SPI_FLASH_SI{slash}SIO0")
			(pinfunction "SI/SIO0")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at 1.2 0.25 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "/nRF9151 - GPIO + UICC/SPI_FLASH_SCLK")
			(pinfunction "SCLK")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at 1.2 -0.25 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "/nRF9151 - GPIO + UICC/SPI_FLASH_nHOLD{slash}SIO3")
			(pinfunction "n~{HOLD}/SIO3")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at 1.2 -0.75 270)
			(size 0.3 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/PWR_nRF91")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.05)
		)
		(pad "GND" smd roundrect
			(at 0 0 270)
			(size 0.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0)
			(chamfer_ratio 0.4)
			(chamfer top_left)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/MX_8USON.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 56.4 165.4 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 1.9 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/8/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1001X"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "8"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(U10-P0.18{slash}RESET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/nRF52_nRESET")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 84.4 162.9)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/32/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF4701X"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "32"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/I2C_SBUS.SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0603_1608Metric"
		(layer "F.Cu")
		(at 58.975 160.225 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at -0.025 -2.925 0)
			(layer "F.SilkS")
		)
		(property "Value" "4u7"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/108/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 µF ±10% 6.3V Ceramic Capacitor X7R 0603 (1608 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10B475KQ8NQNC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "108"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/PWR_USB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 66.1 160.5)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100n 16V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "Net-(U10-DEC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0201_0603Metric"
		(layer "F.Cu")
		(at 90.555 147.4)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 1.445 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/134/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0201 (0603 Metric) Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-1GN0R00C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "134"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/nRF9151 - Power + RF/LTE_ANT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 59.5 165.4 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 0 -1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SKY_MCM-10"
		(layer "F.Cu")
		(at 83.9 149.8 90)
		(property "Reference" "U2"
			(at 0.4 2.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SKY65943-11"
			(at 0 2.6 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/9/info"
			(at -1.2 -1.1435 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RF Front End 1.559GHz ~ 1.606GHz Galileo, GLONASS, GNSS, GPS 10-MCM (2.5x2.5)"
			(at -1.2 -1.1435 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/RF and Wireless"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SKY65943-11"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Skyworks Solutions Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "10-MCM (2.5x2.5)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(solder_mask_margin 0.05)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.2 -1.1435 90)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -1.2 -0.5 90)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/nRF9151 - Power + RF/LNA_EN_FILT")
			(pinfunction "VEN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -1.2 0 90)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/nRF9151 - Power + RF/LNA_VCC_IN")
			(pinfunction "VCC")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -1.2 0.5 90)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -1.2 1.1435 90)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "/nRF9151 - Power + RF/GNSS_RF")
			(pinfunction "RF_IN")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 1.175 1.1435 90)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 1.175 0.5 90)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "/nRF9151 - Power + RF/FIL_OUT")
			(pinfunction "FIL_OUT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 1.175 0 90)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "/nRF9151 - Power + RF/AMP_IN")
			(pinfunction "AMP_IN")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 1.175 -0.5 90)
			(size 0.425 0.275)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 1.175 -1.1435 90)
			(size 0.425 0.515)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "/nRF9151 - Power + RF/GNSS_LNA_RF")
			(pinfunction "RF_OUT")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd custom
			(at 0 -0.8 90)
			(size 1.45 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
			(solder_paste_margin_ratio -0.05)
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.239 -0.054) (xy 0.175 0.098) (xy -0.106 0.098) (xy -0.106 -0.102) (xy 0.239 -0.102)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "11" smd custom
			(at 0 0 90)
			(size 1.45 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
			(solder_paste_margin_ratio -0.05)
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.239 -0.054) (xy 0.175 0.098) (xy -0.106 0.098) (xy -0.106 -0.102) (xy 0.239 -0.102)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "11" smd custom
			(at 0 0.8 90)
			(size 1.45 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
			(solder_paste_margin_ratio -0.05)
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.239 -0.054) (xy 0.175 0.098) (xy -0.106 0.098) (xy -0.106 -0.102) (xy 0.239 -0.102)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/SKY_MCM-10.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 68.3 160.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 -1.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/110/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 µF ±10% 10V Ceramic Capacitor X7S 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GCM155C71A105KE38D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "110"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:L_0402_1005Metric"
		(layer "F.Cu")
		(at 100.7 159.45 180)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at -1.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R / 2A"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/39/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "120 Ohms @ 100 MHz 1 Power Line Ferrite Bead 0402 (1005 Metric) 2A 55mOhm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Filters/Ferrite Beads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "BLM15PX121SN1D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "39"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/nRF9151 - Power + RF/nRF91_VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 69.5 163.7 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 1.9 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/110/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 µF ±10% 10V Ceramic Capacitor X7S 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GCM155C71A105KE38D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "110"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/nRF52833/DEC4_6")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0603_1608Metric"
		(layer "F.Cu")
		(at 59 161.825 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 0 -2.325 0)
			(layer "F.SilkS")
		)
		(property "Value" "4u7"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/108/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 µF ±10% 6.3V Ceramic Capacitor X7R 0603 (1608 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10B475KQ8NQNC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "108"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(U10-DECUSB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 66.2 170.1 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C57"
			(at -1.85 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "12p"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/104/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "12 pF ±2% 50V Ceramic Capacitor C0G, NP0 0201 (0603 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM0335C1H120GA01D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "104"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/nRF52833/XC1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 105 158.8)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u 10V"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/40/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 µF ±10% 10V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155Z71A105KE01D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "40"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0201_0603Metric"
		(layer "F.Cu")
		(at 90.875 148.55 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 1.325 90)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/134/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0201 (0603 Metric) Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-1GN0R00C"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "134"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "/nRF9151 - Power + RF/LTE_ANT_TUNED")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/nRF9151 - Power + RF/LTE_ANT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 86.3 170.3 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at -2 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "590"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/133/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "590 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF5900X"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "133"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/nRF9151 - GPIO + UICC/LED_GREEN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "F.Cu")
		(at 123.475 167.45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 3.475 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "/Power Management/PWR_SYS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 83.9 154.9 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0.6 7.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100p 50V"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/109/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100 pF ±5% 50V Ceramic Capacitor C0G, NP0 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM0335C1H101JA01D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "109"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/nRF9151 - Power + RF/LNA_EN_FILT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TI_ANT_TRACE_AN043"
		(locked yes)
		(layer "F.Cu")
		(at 65.53 180 180)
		(property "Reference" "REF**"
			(at 0 1.15 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TI_ANT_TRACE_AN043"
			(at 0 2.95 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 6.45 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 6.45 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 4.45 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 2.55 -0.25 180)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 70 "/nRF52833/ANT_BLE")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0.45 -0.25 180)
			(size 1.2 0.5)
			(layers "F.Cu")
			(net 1 "GND")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:TE_CONN_MHF1_SMD"
		(layer "F.Cu")
		(at 90.9 144.3 180)
		(descr "Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)")
		(tags "mcrf hirose ufl u.fl microcoaxial")
		(property "Reference" "J11"
			(at 0 2.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONMHF1-SMD-G-T"
			(at 0 -3.302 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/48/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "U.FL (UMCC) Connector Jack, Male Pin 50 Ohms Surface Mount Solder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Coaxial Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CONMHF1-SMD-G-T"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TE Connectivity Linx"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "48"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -1.525)
			(size 1 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/nRF9151 - Power + RF/LTE_ANT")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.475 0)
			(size 1.05 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 1.525)
			(size 1 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.475 0)
			(size 1.05 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/TE_HF1-SMD-G-T-A.STEP"
			(offset
				(xyz 0 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:NORDIC_LGA-113"
		(locked yes)
		(layer "F.Cu")
		(at 92.1 161.2 180)
		(descr "LACA-R7")
		(tags "NSMD")
		(property "Reference" "U1"
			(at 5.7 -6.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "nRF9151-LACA"
			(at 0 6.8 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/7/info"
			(at -4.8 -5.1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Transceiver Module"
			(at -4.8 -5.1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/RF and Wireless"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NRF9151-LACA-R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Nordic Semiconductor ASA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "113 LGA (12.1 x 11.1)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VSSOP*3x3mm*P0.65mm*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(solder_mask_margin 0.05)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.5 -5 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0)
			(chamfer_ratio 0.355)
			(chamfer bottom_right)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -5.625 -4.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "/Power Management/I2C_PMIC.SCL")
			(pinfunction "P0.20")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -5.625 -3.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "/nRF52833/nRF91_SWD.CLK")
			(pinfunction "SWDCLK")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -5.625 -3.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "/nRF52833/nRF91_SWD.IO")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -5.625 -2.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "/Power Management/I2C_PMIC.SDA")
			(pinfunction "P0.21")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at -5.625 -2.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "/BQ_nINT")
			(pinfunction "P0.22")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at -5.625 -1.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at -5.625 -1.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "/SBUS_EN")
			(pinfunction "P0.23")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at -5.625 -0.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/nRF9151 - GPIO + UICC/nRESET_FILT")
			(pinfunction "nRESET")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at -5.625 -0.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "Net-(U1A-ENABLE)")
			(pinfunction "ENABLE")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "11" smd rect
			(at -5.625 0.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "/BOOST_PWM_EN")
			(pinfunction "P0.24")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "12" smd rect
			(at -5.625 0.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/nRF9151 - GPIO + UICC/APP_SIM_DETECT")
			(pinfunction "P0.25")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "13" smd rect
			(at -5.625 1.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "14" smd rect
			(at -5.625 1.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/nRF9151 - Power + RF/nRF91_VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "15" smd rect
			(at -5.625 2.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "16" smd rect
			(at -5.625 2.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/nRF9151 - GPIO + UICC/SIM_RST_IN")
			(pinfunction "SIM_RST")
			(pintype "output")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "17" smd rect
			(at -5.625 3.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "/nRF9151 - GPIO + UICC/SIM_IO_IN")
			(pinfunction "SIM_IO")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "18" smd rect
			(at -5.625 3.75 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "/nRF9151 - GPIO + UICC/SIM_CLK_IN")
			(pinfunction "SIM_CLK")
			(pintype "output")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "19" smd rect
			(at -5.625 4.25 270)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "VCC")
			(pinfunction "SIM_1V8")
			(pintype "power_out")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "20" smd rect
			(at -5.5 5 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "21" smd rect
			(at -4.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "unconnected-(U1C-MAGPIO0-Pad21)")
			(pinfunction "MAGPIO0")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "22" smd rect
			(at -4.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "unconnected-(U1C-MAGPIO1-Pad22)")
			(pinfunction "MAGPIO1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "23" smd rect
			(at -3.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "unconnected-(U1C-MAGPIO2-Pad23)")
			(pinfunction "MAGPIO2")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "24" smd rect
			(at -3.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(U1A-DEC0)")
			(pinfunction "DEC0")
			(pintype "passive")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "25" smd rect
			(at -2.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "26" smd rect
			(at -2.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "unconnected-(U1C-SIM_DET-Pad26)")
			(pinfunction "SIM_DET")
			(pintype "input+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "27" smd rect
			(at -1.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "unconnected-(U1C-SDATA-Pad27)")
			(pinfunction "SDATA")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "28" smd rect
			(at -1.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "unconnected-(U1C-SCLK-Pad28)")
			(pinfunction "SCLK")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "29" smd rect
			(at -0.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "unconnected-(U1C-VIO-Pad29)")
			(pinfunction "VIO")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "30" smd rect
			(at -0.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "31" smd rect
			(at 0.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "unconnected-(U1D-RESERVED-Pad31)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "32" smd rect
			(at 0.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "unconnected-(U1D-RESERVED-Pad32)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "33" smd rect
			(at 1.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "unconnected-(U1D-RESERVED-Pad33)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "34" smd rect
			(at 1.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "35" smd rect
			(at 2.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/nRF9151 - Power + RF/LTE_ANT_TUNED")
			(pinfunction "ANT")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "36" smd rect
			(at 2.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "37" smd rect
			(at 3.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "/nRF9151 - Power + RF/GNSS_RF")
			(pinfunction "AUX")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "38" smd rect
			(at 3.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "39" smd rect
			(at 4.25 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "40" smd rect
			(at 4.75 5.125)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "41" smd rect
			(at 5.5 5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "42" smd rect
			(at 5.625 4.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "/nRF9151 - Power + RF/GNSS_LNA_RF")
			(pinfunction "GPS")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "43" smd rect
			(at 5.625 3.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "44" smd rect
			(at 5.625 3.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "/nRF52833/nRF_GPIO2")
			(pinfunction "P0.26")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "45" smd rect
			(at 5.625 2.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "/nRF52833/nRF_GPIO1")
			(pinfunction "P0.27")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "46" smd rect
			(at 5.625 2.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "47" smd rect
			(at 5.625 1.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "/nRF52833/nRF_GPIO0")
			(pinfunction "P0.28")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "48" smd rect
			(at 5.625 1.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "/nRF52833/BLE_SPI.nCS")
			(pinfunction "P0.29")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "49" smd rect
			(at 5.625 0.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "/I2C_SBUS.SDA")
			(pinfunction "P0.30")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "50" smd rect
			(at 5.625 0.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/I2C_SBUS.SCL")
			(pinfunction "P0.31")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "51" smd rect
			(at 5.625 -0.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "52" smd rect
			(at 5.625 -0.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "/nRF9151 - GPIO + UICC/LNA_EN")
			(pinfunction "COEX0")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "53" smd rect
			(at 5.625 -1.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "unconnected-(U1C-COEX1-Pad53)")
			(pinfunction "COEX1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "54" smd rect
			(at 5.625 -1.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "unconnected-(U1C-COEX2-Pad54)")
			(pinfunction "COEX2")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "55" smd rect
			(at 5.625 -2.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "56" smd rect
			(at 5.625 -2.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "/nRF9151 - GPIO + UICC/SPI_FLASH_nCS")
			(pinfunction "P0.00")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "57" smd rect
			(at 5.625 -3.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "/nRF9151 - GPIO + UICC/SPI_FLASH_SIO1")
			(pinfunction "P0.01")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "58" smd rect
			(at 5.625 -3.75 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "/nRF9151 - GPIO + UICC/SPI_FLASH_nWP{slash}SIO2")
			(pinfunction "P0.02")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "59" smd rect
			(at 5.625 -4.25 90)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "/nRF9151 - GPIO + UICC/SPI_FLASH_nHOLD{slash}SIO3")
			(pinfunction "P0.03")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "60" smd rect
			(at 5.5 -5)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "61" smd rect
			(at 4.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "/nRF9151 - GPIO + UICC/SCLK_TERM")
			(pinfunction "P0.04")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "62" smd rect
			(at 4.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "/nRF9151 - GPIO + UICC/SPI_FLASH_SI{slash}SIO0")
			(pinfunction "P0.05")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "63" smd rect
			(at 3.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/nRF9151 - GPIO + UICC/LED_YELLOW")
			(pinfunction "P0.06")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "64" smd rect
			(at 3.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/nRF9151 - GPIO + UICC/LED_GREEN")
			(pinfunction "P0.07")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "65" smd rect
			(at 2.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/nRF9151 - Power + RF/nRF91_VDD_GPIO")
			(pinfunction "VDD_GPIO")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "66" smd rect
			(at 2.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "67" smd rect
			(at 1.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/nRF9151 - GPIO + UICC/LED_RED")
			(pinfunction "P0.08")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "68" smd rect
			(at 1.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "/nRF52833/BLE_SPI.CLK")
			(pinfunction "P0.09")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "69" smd rect
			(at 0.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "/nRF52833/BLE_SPI.MISO")
			(pinfunction "P0.10")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "70" smd rect
			(at 0.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "/nRF52833/BLE_SPI.MOSI")
			(pinfunction "P0.11")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "71" smd rect
			(at -0.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "72" smd rect
			(at -0.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "/nRF52833/UART1.RX")
			(pinfunction "P0.12")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "73" smd rect
			(at -1.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "/nRF52833/UART1.TX")
			(pinfunction "P0.13")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "74" smd rect
			(at -1.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "/nRF52833/UART0.RX")
			(pinfunction "P0.14")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "75" smd rect
			(at -2.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "/nRF52833/UART0.TX")
			(pinfunction "P0.15")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "76" smd rect
			(at -2.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "77" smd rect
			(at -3.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/nRF52_nRESET")
			(pinfunction "P0.16")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "78" smd rect
			(at -3.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "/nRF52833/nRF91_SWD.SWO")
			(pinfunction "P0.17")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "79" smd rect
			(at -4.25 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "/PANEL_DETECT")
			(pinfunction "P0.18")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "80" smd rect
			(at -4.75 -5.125 180)
			(size 0.3 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "/BQ_nCE")
			(pinfunction "P0.19")
			(pintype "bidirectional")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "81" smd rect
			(at -4.1 -3.4 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "unconnected-(U1D-RESERVED-Pad81)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "82" smd rect
			(at -4.1 -2.85 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "unconnected-(U1D-RESERVED-Pad82)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "83" smd rect
			(at -4.1 -2.3 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "unconnected-(U1D-RESERVED-Pad83)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "84" smd rect
			(at -4.1 -0.55 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "unconnected-(U1D-RESERVED-Pad84)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "85" smd rect
			(at -4.1 0 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "unconnected-(U1D-RESERVED-Pad85)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "86" smd rect
			(at -4.1 0.55 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "unconnected-(U1D-RESERVED-Pad86)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "87" smd rect
			(at -4.1 2.3 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "unconnected-(U1D-RESERVED-Pad87)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "88" smd rect
			(at -4.1 2.85 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "unconnected-(U1D-RESERVED-Pad88)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "89" smd rect
			(at -4.1 3.4 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "unconnected-(U1D-RESERVED-Pad89)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "90" smd rect
			(at -0.55 2.15 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "unconnected-(U1D-RESERVED-Pad90)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "91" smd rect
			(at 0 2.15 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "unconnected-(U1D-RESERVED-Pad91)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "92" smd rect
			(at 0.55 2.15 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "unconnected-(U1D-RESERVED-Pad92)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "93" smd rect
			(at 4.1 3.4)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "unconnected-(U1D-RESERVED-Pad93)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "94" smd rect
			(at 4.1 2.85)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "unconnected-(U1D-RESERVED-Pad94)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "95" smd rect
			(at 4.1 2.3)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "unconnected-(U1D-RESERVED-Pad95)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "96" smd rect
			(at 4.1 0.55)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "unconnected-(U1D-RESERVED-Pad96)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "97" smd rect
			(at 4.1 0)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "unconnected-(U1D-RESERVED-Pad97)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "98" smd rect
			(at 4.1 -0.55)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "unconnected-(U1D-RESERVED-Pad98)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "99" smd rect
			(at 4.1 -2.3)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "unconnected-(U1D-RESERVED-Pad99)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "100" smd rect
			(at 4.1 -2.85)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "unconnected-(U1D-RESERVED-Pad100)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "101" smd rect
			(at 4.1 -3.4)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "unconnected-(U1D-RESERVED-Pad101)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "102" smd rect
			(at 0.55 -2.15 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "unconnected-(U1D-RESERVED-Pad102)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "103" smd rect
			(at 0 -2.15 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "unconnected-(U1D-RESERVED-Pad103)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "104" smd rect
			(at -0.55 -2.15 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "unconnected-(U1D-RESERVED-Pad104)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 45)
		)
		(pad "105" smd rect
			(at -2.85 -2.85 180)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "106" smd rect
			(at -2.85 0 180)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "107" smd rect
			(at -2.85 2.85 180)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "108" smd rect
			(at 0 3.575 180)
			(size 1.6 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "109" smd rect
			(at 2.85 2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "110" smd rect
			(at 2.85 0)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "111" smd rect
			(at 2.85 -2.85)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "112" smd rect
			(at 0 -3.575 180)
			(size 1.6 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(pad "113" smd rect
			(at 0 0 180)
			(size 1.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.05)
			(zone_connect 1)
			(thermal_bridge_width 0.25)
			(thermal_gap 0.25)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/NRF_LGA_9151_12.1x11.1mm.STEP"
			(offset
				(xyz 0 0 0.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 119.675 172.05)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "47n 25V"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/85/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.047 µF ±10% 25V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71E473KA88D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "85"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/Power Management/BTST2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/Power Management/SW2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 84.4 153.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 7.2 -0.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/19/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2GE0R00X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "19"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "/nRF9151 - GPIO + UICC/LNA_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/nRF9151 - Power + RF/LNA_EN_FILT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 83 154.9 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0.7 7.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/nRF9151 - Power + RF/LNA_EN_FILT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:RIBBIT_LOGO"
		(layer "F.Cu")
		(at 60.2 140.2)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via"
		(locked yes)
		(layer "F.Cu")
		(at 54.1 140.2)
		(descr "Mounting Hole 2.7mm")
		(tags "mounting hole 2.7mm")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5_Pad_Via"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.025 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.431891 -1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.431891 1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.025)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.4 5.4)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole circle
			(at 0 2.025)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.431891 -1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.431891 1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.025 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 119.675 175.85)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "47n 25V"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/85/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.047 µF ±10% 25V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71E473KA88D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "85"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/Power Management/BTST1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Management/SW1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0201_0603Metric"
		(layer "F.Cu")
		(at 90.555 149.7)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 1.445 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/134/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0201 (0603 Metric) Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-1GN0R00C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "134"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "/nRF9151 - Power + RF/LTE_ANT_TUNED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 89.3 170 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -1.8 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/19/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2GE0R00X"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "19"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/nRF9151 - Power + RF/nRF91_VDD_GPIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 65.1 170.1 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C55"
			(at 1.8 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/109/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100 pF ±5% 50V Ceramic Capacitor C0G, NP0 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM0335C1H101JA01D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "109"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/nRF52833/DEC3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Symbol_8.9x8mm_SilkScreen"
		(layer "F.Cu")
		(at 128 161.336177)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Symbol_8.9x8mm_SilkScreen"
			(at 0.75 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(footprint "footprints:C_0603_1608Metric"
		(layer "F.Cu")
		(at 62.1 159.3 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 -1.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "4u7"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/108/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 µF ±10% 6.3V Ceramic Capacitor X7R 0603 (1608 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10B475KQ8NQNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "108"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.1 154.8)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -1.7 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4u7 10V"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/37/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 µF ±20% 10V Ceramic Capacitor X5R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R61A475MEAAD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "37"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1A-DEC0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:L_0201_0603Metric"
		(layer "F.Cu")
		(at 62.98 169.9 -90)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L8"
			(at 0 1.88 90)
			(layer "F.SilkS")
		)
		(property "Value" "4n7"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/113/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 nH Unshielded Thick Film Inductor 600 mA 140mOhm Max 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Inductors/RF Inductors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LQP03PN4N7J02D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "113"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "/nRF52833/RADIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "/nRF52833/RADIO_MATCH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 84.9 155.1375 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0.0625 7.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/20/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 MOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1004X"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "20"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "/nRF9151 - GPIO + UICC/LNA_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 98.9 159.77 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.42 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/nRF9151 - Power + RF/nRF91_VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.6 164.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at -2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/15/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1002X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "15"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "/BQ_nINT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ST_UFDFN-8"
		(layer "F.Cu")
		(at 102.88 152.7)
		(property "Reference" "U3"
			(at 0 -1.85 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EMIF03-SIM02M8"
			(at 0.05 1.95 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/13/info"
			(at -0.75 -0.6 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RC (Pi) EMI Filter 2nd Order Low Pass 3 Channel R = 47Ohms, 100Ohms, C = 17pF 8-UFDFN Exposed Pad"
			(at -0.75 -0.6 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Filters/EMI/RFI Filters"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "EMIF03-SIM02M8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "STMicroelectronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "8-UFDFN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 -0.6 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -0.75 -0.2 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/nRF9151 - GPIO + UICC/SIM_RST_IN")
			(pinfunction "RST_IN")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -0.75 0.2 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "/nRF9151 - GPIO + UICC/SIM_CLK_IN")
			(pinfunction "CLK_IN")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -0.75 0.6 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "/nRF9151 - GPIO + UICC/SIM_IO_IN")
			(pinfunction "DATA_IN")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0.75 0.6 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/nRF9151 - GPIO + UICC/SIM_IO_EXT")
			(pinfunction "DATA_EXT")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0.75 0.2 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/nRF9151 - GPIO + UICC/SIM_CLK_EXT")
			(pinfunction "CLK_EXT")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0.75 -0.2 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "/nRF9151 - GPIO + UICC/SIM_RST_EXT")
			(pinfunction "RST_EXT")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0.75 -0.6 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "GND" smd rect
			(at 0 0 270)
			(size 1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/ST_UFDFN-8.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via"
		(locked yes)
		(layer "F.Cu")
		(at 130.1 140.2)
		(descr "Mounting Hole 2.7mm")
		(tags "mounting hole 2.7mm")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5_Pad_Via"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.025 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.431891 -1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.431891 1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.025)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.4 5.4)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole circle
			(at 0 2.025)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.431891 -1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.431891 1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.025 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.6 165.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/32/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF4701X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "32"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/Power Management/I2C_PMIC.SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "F.Cu")
		(at 119.525 167.45 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "3K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/87/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF3001X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "87"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "/Power Management/PROG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "F.Cu")
		(at 89.8 168.4)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -1.55 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4u7 10V"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/37/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.7 µF ±20% 10V Ceramic Capacitor X5R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R61A475MEAAD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "37"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/nRF9151 - Power + RF/nRF91_VDD_GPIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "F.Cu")
		(at 67.72 167.1)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at 2.13 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/PWR_nRF52")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via"
		(locked yes)
		(layer "F.Cu")
		(at 130.1 182.2)
		(descr "Mounting Hole 2.7mm")
		(tags "mounting hole 2.7mm")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5_Pad_Via"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.025 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.431891 -1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.431891 1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.025)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.4 5.4)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole circle
			(at 0 2.025)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.431891 -1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.431891 1.431891)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.025 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "F.Cu")
		(at 100.75 157.1 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -2.5 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "47u 10V"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/38/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47 µF ±20% 10V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61A476ME15K"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "38"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "F.Cu")
		(at 102.85 157.1 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -2.5 -0.005 90)
			(layer "F.SilkS")
		)
		(property "Value" "47u 10V"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/38/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47 µF ±20% 10V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61A476ME15K"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "38"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - Power + RF/")
		(sheetfile "nrf9151_power_rf.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0201_0603Metric"
		(layer "F.Cu")
		(at 63.3 179.5)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 1.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0R"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/134/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0201 (0603 Metric) Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-1GN0R00C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "134"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "/nRF52833/ANT_BLE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 104.1 147.065 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at -0.435 -1.9 90)
			(layer "B.SilkS")
		)
		(property "Value" "300"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/141/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "300 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF3000X"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "141"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 174 "/Battery Protection/BAT_P_POL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 165 "/Battery Protection/VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 113.24 161.3)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at -0.39 1.75 0)
			(layer "B.SilkS")
		)
		(property "Value" "47u 10V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/38/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "47 µF ±20% 10V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61A476ME15K"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "38"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 120.175 169.025 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1 0)
			(layer "B.SilkS")
		)
		(property "Value" "1n 50V"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/95/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "1000 pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM1555C1H102JA01D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "95"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/Power Management/SDRV")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/PWR_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SW_Tactile_SPST_NO_Straight_CK_ PTS636SM50JSMTR LFS"
		(layer "B.Cu")
		(at 75.1 160.2 90)
		(descr "Tactile switch, SPST, 6.0x3.5 mm, H2.5 mm, straight, NO, gull wing leads: https://www.ckswitches.com/media/2779/pts636.pdf")
		(tags "switch tactile SPST 1P1T straight NO SMTR C&K")
		(property "Reference" "SW1"
			(at 0 3 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "PTS636SM50JSMTR LFS"
			(at 0 -3 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/42/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Tactile Switch SPST-NO Top Actuated Surface Mount"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Switches/Tactile Switches"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "C&K"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "PTS636SM50JSMTR LFS"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "42"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -3.25 0 90)
			(size 0.9 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "/nRF52833/nRF91_SWD.nRESET")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.25 0 90)
			(size 0.9 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Tactile_SPST_NO_Straight_CK_PTS636Sx25SMTRLFS.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TestPoint_Pad_1.0x1.0mm"
		(layer "B.Cu")
		(at 122.8 184.7)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP8"
			(at -1.45 0 270)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint_Small"
			(at 0 -1.55 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/144/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "144"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 179 "/Power Management/STAT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 104.7 148.565 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C61"
			(at 0 -1.035 0)
			(layer "B.SilkS")
		)
		(property "Value" "100n 50V"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 165 "/Battery Protection/VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/BAT_N")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:L_1206_3216Metric"
		(layer "B.Cu")
		(at 85.7 175.3)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L5"
			(at 0 1.9 0)
			(layer "B.SilkS")
		)
		(property "Value" "50R / 3.5A"
			(at 0 -1.9 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/72/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "50 Ohms 1 Power Line Ferrite Bead 1206 (3216 Metric) 3.5A 15mOhm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Filters/Ferrite Beads"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "BLM31PG500SN1L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "72"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.575 0)
			(size 1.05 1.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.238095)
			(net 10 "/USB/PWR_USB_5V0_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.575 0)
			(size 1.05 1.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.238095)
			(net 17 "/PWR_USB_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SAM_MICRO-IDC_FTSH-105-01-L-DV-K_SMD"
		(layer "B.Cu")
		(at 54.6 168.7 90)
		(descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x05 1.27mm double row")
		(property "Reference" "J15"
			(at 0 4.235 90)
			(layer "B.SilkS")
		)
		(property "Value" "FTSH-105-01-L-DV-K"
			(at -0.1 -6.1 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/145/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 10 position 0.050\" (1.27mm)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "FTSH-105-01-L-DV-K"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Samtec Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "145"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.6 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.075 2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/PWR_nRF52")
			(pinfunction "VREF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.075 2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "/nRF52833/nRF52_SWDIO")
			(pinfunction "SWDIO")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.075 1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.075 1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 59 "/nRF52833/nRF52_SWCLK")
			(pinfunction "SWDCLK")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.075 0 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.075 0 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 155 "unconnected-(J15-SWO-Pad6)")
			(pinfunction "SWO")
			(pintype "passive+no_connect")
		)
		(pad "7" smd rect
			(at -2.075 -1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 76 "unconnected-(J15-KEY-Pad7)")
			(pinfunction "KEY")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 2.075 -1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 69 "unconnected-(J15-NC-Pad8)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at -2.075 -2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 2.075 -2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "/nRF52_nRESET")
			(pinfunction "nRST")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/FTSH-105-01-L-DV-K.step"
			(offset
				(xyz 0 0 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
	)
	(footprint "footprints:DI_DFN2020-6"
		(layer "B.Cu")
		(at 110.75 181.07)
		(property "Reference" "Q4"
			(at 0 2.03 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DMN1019UFDE-7"
			(at 0 -2.4 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/76/info"
			(at 0 0.25 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 12 V 11A (Ta) 690mW (Ta) Surface Mount U-DFN2020-6 (Type E)"
			(at 0 0.25 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Transistors/FETs"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "DMN1019UFDE-7"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "U-DFN2020-6 (Type E)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "76"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 0 0.325 90)
			(size 1.05 1.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "/Power Management/PWR_VBUS")
			(pinfunction "D")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.525 1.15) (xy -0.125 1.15) (xy -0.125 0.8) (xy 0.125 0.8) (xy 0.125 1.15) (xy 0.525 1.15)
						(xy 0.525 -1.15) (xy 0.125 -1.15) (xy 0.125 -0.8) (xy -0.125 -0.8) (xy -0.125 -1.15) (xy -0.525 -1.15)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd rect
			(at -0.9 -0.65 90)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "/Power Management/ACDRV2_G")
			(pinfunction "G")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 -0.65 90)
			(size 0.285 0.92)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "/Power Management/ACDRV2_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0.9 -0.65 90)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "/Power Management/ACDRV2_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/DI_U-DFN2020-6.stp"
			(offset
				(xyz 0 0 0.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 123.475 165.25)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 3.125 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 162 "/Power Management/PWR_SYS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 123.475 167.45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 3.125 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 162 "/Power Management/PWR_SYS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "B.Cu")
		(at 110.875 165.05 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at -0.025 1 0)
			(layer "B.SilkS")
		)
		(property "Value" "1n"
			(at 0 -1.05 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/81/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "1000 pF ±10% 25V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033R71E102KA01D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "81"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.68 0)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/Power Management/CT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 118.275 177.7)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "4u7 10V"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/37/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4.7 µF ±20% 10V Ceramic Capacitor X5R 0402 (1005 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R61A475MEAAD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "37"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Power Management/REGN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 108.7 181.47 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0.23 1.16 270)
			(layer "B.SilkS")
		)
		(property "Value" "294R"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/80/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "294 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF2940X"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "80"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/Power Management/ACDRV2_G")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/Power Management/ACDRV2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 115.875 178.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 1 0)
			(layer "B.SilkS")
		)
		(property "Value" "215k"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/120/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "215 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-07215KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "120"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Power Management/REGN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/Power Management/ILIM_HIZ")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PANASONIC_EXCX4CE"
		(layer "B.Cu")
		(at 79.1 175.825 90)
		(property "Reference" "U8"
			(at 2.375 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "EXC-34CE121U"
			(at 0 -2 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/67/info"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "2 Line Common Mode Choke Surface Mount 120 Ohms @ 100 MHz 200mA DCR 1Ohm"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Filters/EMI/RFI Filters"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "EXC-34CE121U"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "67"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L_* L_CommonMode*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -3.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.925 0.4 90)
			(size 0.75 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "/USB/USB_CMC_D_N")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -0.925 -0.4 90)
			(size 0.75 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "/USB/USB_CMC_D_P")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0.925 -0.4 90)
			(size 0.75 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 81 "/USB/USB_D_P")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 0.925 0.4 90)
			(size 0.75 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 80 "/USB/USB_D_N")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/PANASONIC_EXCX4CE.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Symbol:Symbol_Barrel_Polarity"
		(layer "B.Cu")
		(at 92.3 175.375)
		(descr "Barrel connector polarity indicator")
		(tags "barrel polarity")
		(property "Reference" "REF**"
			(at 0 2 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Symbol_Barrel_Polarity"
			(at 0 -2 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 122.675 172.45 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.125 270)
			(layer "B.SilkS")
		)
		(property "Value" "100n 50V"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 162 "/Power Management/PWR_SYS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 115.875 181.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 -1.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "30k1"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/98/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "30.1 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0730K1L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "98"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 89 "/Power Management/TS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "B.Cu")
		(at 113.7 138.4)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -1.8 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 -1.05 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/34/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 16V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033Z71C104KE14J"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "34"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.68 0)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DI_DFN2020-6"
		(layer "B.Cu")
		(at 110.75 178.295 180)
		(property "Reference" "Q2"
			(at -2.05 1.245 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DMN1019UFDE-7"
			(at 0 -2.4 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/76/info"
			(at 0 0.25 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 12 V 11A (Ta) 690mW (Ta) Surface Mount U-DFN2020-6 (Type E)"
			(at 0 0.25 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Transistors/FETs"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "DMN1019UFDE-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "U-DFN2020-6 (Type E)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "76"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 0 0.325 270)
			(size 1.05 1.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "/PWR_PANEL")
			(pinfunction "D")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.525 1.15) (xy -0.125 1.15) (xy -0.125 0.8) (xy 0.125 0.8) (xy 0.125 1.15) (xy 0.525 1.15)
						(xy 0.525 -1.15) (xy 0.125 -1.15) (xy 0.125 -0.8) (xy -0.125 -0.8) (xy -0.125 -1.15) (xy -0.525 -1.15)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd rect
			(at -0.9 -0.65 270)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "/Power Management/ACDRV2_G")
			(pinfunction "G")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 -0.65 270)
			(size 0.285 0.92)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "/Power Management/ACDRV2_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0.9 -0.65 270)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "/Power Management/ACDRV2_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/DI_U-DFN2020-6.stp"
			(offset
				(xyz 0 0 0.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 108.7 177.87 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at -0.07 1.16 270)
			(layer "B.SilkS")
		)
		(property "Value" "100n 50V"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/PWR_PANEL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:KEYSTONE_254"
		(layer "B.Cu")
		(at 62.8745 149.0325 180)
		(property "Reference" "J2"
			(at -4.1125 10.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "KEYSTONE_254"
			(at -0.7925 -11 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/128/info"
			(at -0.1425 0.3 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Battery Contact Clip 18650 1 Cell SMD (SMT) Tab"
			(at -0.1425 0.3 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "254"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Keystone Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "128"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.4925 -9.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -8.005 0 180)
			(size 4.24 5.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "/BAT_N")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 8.005 0 180)
			(size 4.24 3.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "/BAT_N")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KEYSTONE_254TR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 119.475 165.25 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C59"
			(at 0 2.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/PWR_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:KEYSTONE_254"
		(layer "B.Cu")
		(at 121.3245 149.0325)
		(property "Reference" "J1"
			(at 4.9255 6.9175 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "KEYSTONE_254"
			(at -0.7925 -11 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/128/info"
			(at -0.1425 0.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Battery Contact Clip 18650 1 Cell SMD (SMT) Tab"
			(at -0.1425 0.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "254"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Keystone Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "128"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.4925 -9.5 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -8.005 0)
			(size 4.24 5.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 173 "/BAT_P")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 8.005 0)
			(size 4.24 3.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 173 "/BAT_P")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KEYSTONE_254TR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 81.7 175.8 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 2.05 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "5k1"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/74/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "5.1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF5101X"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "74"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/USB/USB_CC1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:L_Taiyo-Yuden_MD-3030"
		(layer "B.Cu")
		(at 115.14 166.05 180)
		(descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-3030, 3.0mmx3.0mm")
		(tags "inductor taiyo-yuden md smd")
		(property "Reference" "L4"
			(at -0.96 -2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at 0 -3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/89/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "1 µH Shielded Wirewound Inductor 2.1 A 36mOhm Max 1212 (3030 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Inductors/Fixed Inductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "LSXND3030QKT1R0NNG"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Taiyo Yuden"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1212"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "89"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0 180)
			(size 0.8 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 78 "Net-(U6-LX1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0 180)
			(size 0.8 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "Net-(U6-LX2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/L_TAIYO_YUDEN_LSX_3030.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 113.4 171)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 1.95 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/15/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1002X"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "15"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 179 "/Power Management/STAT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:KOA_TEST_POINT_1206"
		(layer "B.Cu")
		(at 108.2 163.1 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TP4"
			(at 0 -1.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "RCWCTE"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/130/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "PC Test Point Plating Surface Mount Mounting Type"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RCWCTE"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KOA Speer Electronics, Inc."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "130"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 4.2 1.749995)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/PWR_3V3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KOA_RCWCTE.step"
			(offset
				(xyz 0 0 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 119.475 180.45 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at -0.025 -3.7 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/Power Management/PWR_VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 104.1 142.665 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 1.965 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/96/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-07100KL"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "96"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 172 "/Battery Protection/CTR")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 115.375 180.4 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 1.875 270)
			(layer "B.SilkS")
		)
		(property "Value" "59k"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/119/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "59 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0759KL"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "119"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/Power Management/ILIM_HIZ")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 123.475 178.25)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 2.575 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/Power Management/PMID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 122.675 175.45 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 1.16 270)
			(layer "B.SilkS")
		)
		(property "Value" "100n 50V"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/Power Management/PMID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 83.8 173 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 -1 90)
			(layer "B.SilkS")
		)
		(property "Value" "10n"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/17/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10000 pF ±10% 25V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CC0402KRX7R8BB103"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "17"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/USB/PWR_USB_5V0_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 102.5 142.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C62"
			(at 0 1.16 0)
			(layer "B.SilkS")
		)
		(property "Value" "100n 50V"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 172 "/Battery Protection/CTR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 86.3 170.3 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 1.75 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "Green LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/47/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Green 572nm LED Indication - Discrete 2.2V 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Diodes/LEDs"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "HSMG-C280"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Broadcom Limited"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "47"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 113.4 173.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 2 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/15/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1002X"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "15"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 161 "/BQ_nCE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 100.2 149.0325 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 1.17 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/100/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "NTC Thermistor 10k 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Sensors/Thermistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "NTCG103JF103FT1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TDK Corporation"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "100"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*NTC* *Thermistor* PIN?ARRAY* bornier* *Terminal?Block* R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 89 "/Power Management/TS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 102.5 175.233333 180)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left")
		(property "Reference" "J6"
			(at 0 3.6 180)
			(layer "B.SilkS")
		)
		(property "Value" "10129380-902001BLF"
			(at 0 -3.6 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/129/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 2 position 0.100\" (2.54mm)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Amphenol ICC (FCI)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "129"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "/PWR_USB")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 -1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "/PWR_USB_IN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ST_SOT-23-6"
		(layer "B.Cu")
		(at 72.9 174.5)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U9"
			(at 0 2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "USBLC6-4SC6"
			(at 0 -3.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/26/info"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "17V Clamp 5A (8/20µs) Ipp Tvs Diode Surface Mount SOT-23-6"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Diodes/TVS"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "USBLC6-4SC6"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "STMicroelectronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "SOT-23-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "26"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0.95)
			(size 1.2 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 181 "unconnected-(U9-I{slash}O1-Pad1)")
			(pinfunction "I/O1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -1.15 0)
			(size 1.2 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.15 -0.95)
			(size 1.2 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 180 "unconnected-(U9-I{slash}O2-Pad3)")
			(pinfunction "I/O2")
			(pintype "passive+no_connect")
		)
		(pad "4" smd rect
			(at 1.15 -0.95)
			(size 1.2 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 80 "/USB/USB_D_N")
			(pinfunction "I/O3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.15 0)
			(size 1.2 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "/USB/PWR_USB_5V0_IN")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.15 0.95)
			(size 1.2 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 81 "/USB/USB_D_P")
			(pinfunction "I/O4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 76.5 175.8 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 2.1 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "5k1"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/74/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "5.1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF5101X"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "74"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/USB/USB_CC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 123.475 182.65)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 2.575 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/Power Management/PMID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 118.075 169.025)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at -0.025 1 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/88/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF1000X"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "88"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 86 "/Power Management/BATP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/PWR_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 77.6 175.8 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 2.05 0.1 90)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/19/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2GE0R00X"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "19"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/USB/USB_CMC_D_P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/USB/USB_D_P")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 108.6525 175.23 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0.22 1.1125 270)
			(layer "B.SilkS")
		)
		(property "Value" "294R"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/80/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "294 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF2940X"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "80"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/Power Management/ACDRV1_G")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/Power Management/ACDRV1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TestPoint_Pad_1.0x1.0mm"
		(layer "B.Cu")
		(at 106.2 140.7 90)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP7"
			(at 0 1.448 90)
			(layer "B.SilkS")
		)
		(property "Value" "PACK_RESET"
			(at 0 -1.55 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/144/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "144"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 172 "/Battery Protection/CTR")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:L_Taiyo-Yuden_MD-3030"
		(layer "B.Cu")
		(at 127.075 173.95 90)
		(descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-3030, 3.0mmx3.0mm")
		(tags "inductor taiyo-yuden md smd")
		(property "Reference" "L3"
			(at -2.5 0.025 90)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at 0 -3 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/89/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "1 µH Shielded Wirewound Inductor 2.1 A 36mOhm Max 1212 (3030 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Inductors/Fixed Inductors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "LSXND3030QKT1R0NNG"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Taiyo Yuden"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1212"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "89"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0 90)
			(size 0.8 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/Power Management/SW1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0 90)
			(size 0.8 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "/Power Management/SW2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/L_TAIYO_YUDEN_LSX_3030.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 80.9 160.7)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left")
		(property "Reference" "J7"
			(at 0 3.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "10129380-902001BLF"
			(at 0 -3.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/129/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 2 position 0.100\" (2.54mm)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Amphenol ICC (FCI)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "129"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 1.27)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/PWR_nRF52")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 -1.27)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/PWR_3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 105.2 147.065 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at -0.435 -2.05 90)
			(layer "B.SilkS")
		)
		(property "Value" "20"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/138/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "20 Ohms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF20R0X"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "138"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 174 "/Battery Protection/BAT_P_POL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 177 "/Battery Protection/BAT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TI_DSBGA-8"
		(layer "B.Cu")
		(at 115.14 163.35 90)
		(descr "Texas Instruments, DSBGA, area grid, NSMD, YBJ0008 pad definition, 0.705x1.468mm, 8 Ball, 2x4 Layout, 0.4mm Pitch, https://www.ti.com/lit/gpn/ina234")
		(tags "BGA 8 0.4")
		(property "Reference" "U6"
			(at 0 1.96 270)
			(layer "B.SilkS")
		)
		(property "Value" "TPS631010YBGR"
			(at 0 -1.734 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/77/info"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Buck-Boost Switching Regulator IC Positive Adjustable 1.2V 1 Output 1.5A 8-XFBGA, DSBGA"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/PMIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "TPS631010YBGR"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "8-DSBGA (1.6x1.1)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "77"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(solder_mask_margin 0.05)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "A1" smd circle
			(at -0.2 0.6 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 163 "/Power Management/PWR_TPS63_VIN")
			(pinfunction "VIN")
			(pintype "passive")
		)
		(pad "A2" smd circle
			(at 0.2 0.6 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 163 "/Power Management/PWR_TPS63_VIN")
			(pinfunction "EN")
			(pintype "passive")
		)
		(pad "B1" smd circle
			(at -0.2 0.2 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 78 "Net-(U6-LX1)")
			(pinfunction "LX1")
			(pintype "passive")
		)
		(pad "B2" smd circle
			(at 0.2 0.2 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 85 "/BOOST_PWM_EN")
			(pinfunction "MODE")
			(pintype "passive")
		)
		(pad "C1" smd circle
			(at -0.2 -0.2 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "Net-(U6-LX2)")
			(pinfunction "LX2")
			(pintype "passive")
		)
		(pad "C2" smd circle
			(at 0.2 -0.2 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "D1" smd circle
			(at -0.2 -0.6 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/PWR_3V3")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "D2" smd circle
			(at 0.2 -0.6 90)
			(size 0.23 0.23)
			(property pad_prop_bga)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 90 "/Power Management/FB")
			(pinfunction "FB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-8_0.705x1.468mm_Layout2x4_P0.4mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 85.2 170.3 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 1.75 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "Yellow LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/44/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yellow 586nm LED Indication - Discrete 2.1V 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Diodes/LEDs"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "HSMY-C280"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Broadcom Limited"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "44"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 170 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 102.4 182.5 180)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left")
		(property "Reference" "J5"
			(at 0 3.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "10129380-902001BLF"
			(at 0 -3.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/129/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 2 position 0.100\" (2.54mm)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Amphenol ICC (FCI)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "129"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "/PWR_PANEL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 -1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "/PWR_PANEL_IN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOT-23"
		(layer "B.Cu")
		(at 107.6 148.7275 -90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q5"
			(at 0 -2.25 90)
			(layer "B.SilkS")
		)
		(property "Value" "SSM3J355R,LF"
			(at 0 -2.7 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/63/info"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "P-Channel 20 V 6A (Ta) 1W (Ta) Surface Mount SOT-23F"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Transistors/FETs"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SSM3J355R,LF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Toshiba Semiconductor and Storage"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "SOT-23F"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "63"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 174 "/Battery Protection/BAT_P_POL")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/BAT_N")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 173 "/BAT_P")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal"
		(layer "B.Cu")
		(at 96.2 141.3)
		(descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J16"
			(at 0 5.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "S2B-PH-SM4-TB"
			(at 0 -5.8 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/125/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount, Right Angle 2 position 0.079\" (2.00mm)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Power Connectors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "S2B-PH-SM4-TB"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "JST Sales America Inc."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "125"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 2.85)
			(size 1 3.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/BAT_N")
			(pinfunction "NEG")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at 1 2.85)
			(size 1 3.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 173 "/BAT_P")
			(pinfunction "POS")
			(pintype "input")
		)
		(pad "G1" smd roundrect
			(at -3.35 -2.9)
			(size 1.5 3.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.166667)
			(net 1 "GND")
			(pintype "input")
		)
		(pad "G2" smd roundrect
			(at 3.35 -2.9)
			(size 1.5 3.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.166667)
			(net 1 "GND")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/S2B-PH-SM4-TB.step"
			(offset
				(xyz 0 -4.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 108.7025 171.63 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at -0.13 1.1625 270)
			(layer "B.SilkS")
		)
		(property "Value" "100n 50V"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/PWR_USB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:KOA_TEST_POINT_1206"
		(layer "B.Cu")
		(at 98.9 180.1 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TP2"
			(at -3.4 0 270)
			(layer "B.SilkS")
		)
		(property "Value" "RCWCTE"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/130/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "PC Test Point Plating Surface Mount Mounting Type"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RCWCTE"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KOA Speer Electronics, Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "130"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 4.2 1.749995)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "/PWR_PANEL_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KOA_RCWCTE.step"
			(offset
				(xyz 0 0 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "footprints:ON_6-WLCSP_1.77x3.05"
		(layer "B.Cu")
		(at 108.6 143.9 -90)
		(property "Reference" "Q6"
			(at 0 -1.85 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "EFC3J018NUZTDG"
			(at 0 -3.1 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/123/info"
			(at -0.1 2.4 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Mosfet Array 20V 23A (Ta) 2.5W (Ta) Surface Mount 6-WLCSP (1.77x3.05)"
			(at -0.1 2.4 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Transistors/FETs"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "onsemi"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "EFC3J018NUZTDG"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "6-WLCSP (1.77x3.05)"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "123"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.6 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.88 -0.4 270)
			(size 1.005 0.36)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.5)
			(net 48 "/PWR_BAT_IN")
			(pinfunction "S1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd circle
			(at 0 -0.4 270)
			(size 0.25 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 176 "/Battery Protection/DSG")
			(pinfunction "G1")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd roundrect
			(at 0.88 -0.4 270)
			(size 1.005 0.36)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.5)
			(net 48 "/PWR_BAT_IN")
			(pinfunction "S1")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd roundrect
			(at 0.88 0.4 270)
			(size 1.005 0.36)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.5)
			(net 174 "/Battery Protection/BAT_P_POL")
			(pinfunction "S2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd circle
			(at 0 0.4 270)
			(size 0.25 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 175 "/Battery Protection/CHG")
			(pinfunction "G2")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd roundrect
			(at -0.88 0.4 270)
			(size 1.005 0.36)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.5)
			(net 174 "/Battery Protection/BAT_P_POL")
			(pinfunction "S2")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/ON_6-WLCSP.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 120.275 177.7 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "100n 50V"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/Power Management/PWR_VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 86.4 173 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 -1 270)
			(layer "B.SilkS")
		)
		(property "Value" "100n 16V"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/132/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1 µF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R71H104KE14D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "132"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/PWR_USB_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 116.94 161.3 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at -0.66 1.55 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 10V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/92/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 10V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "C0805C106K8PACTU"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "92"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 163 "/Power Management/PWR_TPS63_VIN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TI_VQFN-HR-29"
		(layer "B.Cu")
		(at 119.275 173.95 90)
		(property "Reference" "U5"
			(at 2.9 1.875 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "BQ25798"
			(at 0 -3.3 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/73/info"
			(at -1.775 1.55 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Charger IC Lithium Ion/Polymer 29-VQFN-HR (4x4)"
			(at -1.775 1.55 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/PMIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "BQ25798RQMR"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "29-VQFN-HR (4x4)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "73"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VQFN*4x4mm*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(solder_mask_margin 0.05)
		(attr smd allow_soldermask_bridges)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.725 1.6 90)
			(size 0.95 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer bottom_right)
			(net 179 "/Power Management/STAT")
			(pinfunction "STAT")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -1.35 1.95 180)
			(size 0.5 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 179 "/Power Management/STAT")
			(pinfunction "STAT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.9 1.2 90)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/Power Management/PWR_VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.9 0.8 90)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/Power Management/PWR_VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.9 0.4 90)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/Power Management/BTST1")
			(pinfunction "BTST1")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -1.9 0 90)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Power Management/REGN")
			(pinfunction "REGN")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -1.9 -0.4 90)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 136 "unconnected-(U5-D+-Pad6)")
			(pinfunction "D+")
			(pintype "passive+no_connect")
		)
		(pad "7" smd roundrect
			(at -1.9 -0.8 90)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 150 "unconnected-(U5-D--Pad7)")
			(pinfunction "D-")
			(pintype "passive+no_connect")
		)
		(pad "8" smd roundrect
			(at -1.9 -1.2 90)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/PWR_PANEL")
			(pinfunction "VAC2")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -1.75 -1.6 90)
			(size 0.9 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right)
			(net 20 "/PWR_USB")
			(pinfunction "VAC1")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -1.4 -1.95)
			(size 0.5 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 20 "/PWR_USB")
			(pinfunction "VAC1")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at -1 -1.9)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/Power Management/ACDRV2")
			(pinfunction "ACDRV2")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -0.6 -1.9)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/Power Management/ACDRV1")
			(pinfunction "ACDRV1")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at -0.2 -1.9)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 152 "/Power Management/nQON")
			(pinfunction "nQON")
			(pintype "passive+no_connect")
		)
		(pad "13" smd roundrect
			(at 0.2 -1.9)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 161 "/BQ_nCE")
			(pinfunction "nCE")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 0.6 -1.9)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/Power Management/I2C_PMIC.SCL")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 1 -1.9)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/Power Management/I2C_PMIC.SDA")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 1.4 -1.95 180)
			(size 0.5 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_left bottom_left)
			(net 89 "/Power Management/TS")
			(pinfunction "TS")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 1.75 -1.6 90)
			(size 0.9 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_left)
			(net 89 "/Power Management/TS")
			(pinfunction "TS")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at 1.85 -1.2 90)
			(size 0.7 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/Power Management/ILIM_HIZ")
			(pinfunction "ILIM_HIZ")
			(pintype "passive")
		)
		(pad "18" smd roundrect
			(at 1.875 -0.8 90)
			(size 0.65 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 86 "/Power Management/BATP")
			(pinfunction "BATP")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at 1.86 -0.4 90)
			(size 0.68 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/Power Management/BTST2")
			(pinfunction "BTST2")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at 1.9 0 270)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 84 "/Power Management/PROG")
			(pinfunction "PROG")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at 1.9 0.4 270)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 160 "/BQ_nINT")
			(pinfunction "nINT")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 1.9 0.8 270)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/PWR_BATT")
			(pinfunction "BAT")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at 1.9 1.2 270)
			(size 0.6 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/PWR_BATT")
			(pinfunction "BAT")
			(pintype "passive")
		)
		(pad "24" smd roundrect
			(at 1.35 1.95)
			(size 0.5 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_left bottom_left)
			(net 28 "/Power Management/SDRV")
			(pinfunction "SDRV")
			(pintype "passive")
		)
		(pad "24" smd roundrect
			(at 1.725 1.6 90)
			(size 0.95 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer bottom_left)
			(net 28 "/Power Management/SDRV")
			(pinfunction "SDRV")
			(pintype "passive")
		)
		(pad "25" smd roundrect
			(at 0.9 1.7)
			(size 1 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 162 "/Power Management/PWR_SYS")
			(pinfunction "SYS")
			(pintype "passive")
		)
		(pad "26" smd roundrect
			(at 0.45 1.7)
			(size 1 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/Power Management/SW2")
			(pinfunction "SW2")
			(pintype "passive")
		)
		(pad "27" smd roundrect
			(at 0 1.7)
			(size 1 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "28" smd roundrect
			(at -0.45 1.7)
			(size 1 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Management/SW1")
			(pinfunction "SW1")
			(pintype "passive")
		)
		(pad "29" smd roundrect
			(at -0.9 1.725)
			(size 0.95 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/Power Management/PMID")
			(pinfunction "PMID")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/TI_VQFN-HR-29.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:KOA_TEST_POINT_1206"
		(layer "B.Cu")
		(at 131 173.95 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TP1"
			(at 0 1.65 270)
			(layer "B.SilkS")
		)
		(property "Value" "RCWCTE"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/130/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "PC Test Point Plating Surface Mount Mounting Type"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RCWCTE"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KOA Speer Electronics, Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "130"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 4.2 1.749995)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "/PWR_BAT_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KOA_RCWCTE.step"
			(offset
				(xyz 0 0 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "footprints:DI_DFN2020-6"
		(layer "B.Cu")
		(at 110.7525 174.83)
		(property "Reference" "Q3"
			(at 2.0475 0.97 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DMN1019UFDE-7"
			(at 0 -2.4 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/76/info"
			(at 0 0.25 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 12 V 11A (Ta) 690mW (Ta) Surface Mount U-DFN2020-6 (Type E)"
			(at 0 0.25 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Transistors/FETs"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "DMN1019UFDE-7"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "U-DFN2020-6 (Type E)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "76"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 0 0.325 90)
			(size 1.05 1.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "/Power Management/PWR_VBUS")
			(pinfunction "D")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.525 1.15) (xy -0.125 1.15) (xy -0.125 0.8) (xy 0.125 0.8) (xy 0.125 1.15) (xy 0.525 1.15)
						(xy 0.525 -1.15) (xy 0.125 -1.15) (xy 0.125 -0.8) (xy -0.125 -0.8) (xy -0.125 -1.15) (xy -0.525 -1.15)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd rect
			(at -0.9 -0.65 90)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "/Power Management/ACDRV1_G")
			(pinfunction "G")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 -0.65 90)
			(size 0.285 0.92)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/Power Management/ACDRV1_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0.9 -0.65 90)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/Power Management/ACDRV1_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/DI_U-DFN2020-6.stp"
			(offset
				(xyz 0 0 0.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "footprints:KOA_TEST_POINT_1206"
		(layer "B.Cu")
		(at 70.1 182.2 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TP6"
			(at 0 2 90)
			(layer "B.SilkS")
		)
		(property "Value" "RCWCTE"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/130/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "PC Test Point Plating Surface Mount Mounting Type"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RCWCTE"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KOA Speer Electronics, Inc."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "130"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 4.2 1.749995)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KOA_RCWCTE.step"
			(offset
				(xyz 0 0 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 80.6 175.8 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 2.05 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/19/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0 Ohms Jumper Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2GE0R00X"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "19"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/USB/USB_CMC_D_N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 80 "/USB/USB_D_N")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 102.755 160.7)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left")
		(property "Reference" "J9"
			(at 0 -3.7 0)
			(layer "B.SilkS")
		)
		(property "Value" "10129380-902001BLF"
			(at 0 -3.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/129/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 2 position 0.100\" (2.54mm)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Amphenol ICC (FCI)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "129"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 1.27)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "/PWR_nRF91")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 -1.27)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/PWR_3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 87.4 170.3 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 1.75 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "Red LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/46/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Red 626nm LED Indication - Discrete 2.1V 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Diodes/LEDs"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "HSMS-C280"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Broadcom Limited"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "46"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 169 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/PWR_nRF91")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 119.475 167.45 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C60"
			(at 0 3.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/PWR_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:JST_SH_BM04B-SRSS-TB"
		(layer "B.Cu")
		(at 92.15 161.7 180)
		(descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH vertical")
		(property "Reference" "J10"
			(at 3.05 -2.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "BM04B-SRSS-TB"
			(at 0 -3.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/102/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 4 position 0.039\" (1.00mm)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "BM04B-SRSS-TB"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "JST Sales America Inc."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "102"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.25 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -1.325 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -1.325 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/PWR_3V3_LS_OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -1.325 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/I2C_SBUS.SDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -1.325 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/I2C_SBUS.SCL")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "G1" smd roundrect
			(at -2.8 1.2 180)
			(size 1.2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "G1")
			(pintype "passive")
		)
		(pad "G2" smd roundrect
			(at 2.8 1.2 180)
			(size 1.2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "G2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/JST_BM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 0.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:DI_DFN2020-6"
		(layer "B.Cu")
		(at 110.7525 172.055 180)
		(property "Reference" "Q1"
			(at 0.0025 2.005 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DMN1019UFDE-7"
			(at 0 -2.4 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/76/info"
			(at 0 0.25 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 12 V 11A (Ta) 690mW (Ta) Surface Mount U-DFN2020-6 (Type E)"
			(at 0 0.25 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Transistors/FETs"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "DMN1019UFDE-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "U-DFN2020-6 (Type E)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "76"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 0 0.325 270)
			(size 1.05 1.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "/PWR_USB")
			(pinfunction "D")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.525 1.15) (xy -0.125 1.15) (xy -0.125 0.8) (xy 0.125 0.8) (xy 0.125 1.15) (xy 0.525 1.15)
						(xy 0.525 -1.15) (xy 0.125 -1.15) (xy 0.125 -0.8) (xy -0.125 -0.8) (xy -0.125 -1.15) (xy -0.525 -1.15)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd rect
			(at -0.9 -0.65 270)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "/Power Management/ACDRV1_G")
			(pinfunction "G")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 -0.65 270)
			(size 0.285 0.92)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/Power Management/ACDRV1_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0.9 -0.65 270)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/Power Management/ACDRV1_S")
			(pinfunction "S")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/DI_U-DFN2020-6.stp"
			(offset
				(xyz 0 0 0.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "footprints:TENSILITY_54-00125"
		(locked yes)
		(layer "B.Cu")
		(at 92.1 181.7 90)
		(property "Reference" "J3"
			(at -2.1 5.4 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "3.5mm/1.1mm"
			(at 0 -5.5 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/101/info"
			(at 3.5 -3.75 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Power Barrel Connector Jack 1.10mm ID (0.043\"), 3.50mm OD (0.138\") Through Hole, Right Angle"
			(at 3.5 -3.75 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Power Connectors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "54-00125"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Tensility International Corp"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "101"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.5 0.25 90)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "A" thru_hole oval
			(at 3.5 -3.75 90)
			(size 2.3 1.1)
			(drill oval 1.8 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/PWR_PANEL_IN")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "B" thru_hole oval
			(at 3.5 3.75 90)
			(size 2.3 1.1)
			(drill oval 1.8 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "C" thru_hole oval
			(at 3.5 0.25 90)
			(size 2.3 1.1)
			(drill oval 1.8 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/PANEL_DETECT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/54-00125.STEP"
			(offset
				(xyz -4.5 -1.5 2.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 119.475 182.65 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -2.55 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/Power Management/PWR_VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0805_2012Metric"
		(layer "B.Cu")
		(at 102.5 144.865 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at -0.015 1.45 90)
			(layer "B.SilkS")
		)
		(property "Value" "3m"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/143/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "3 mOhms ±1% 0.5W, 1/2W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Current Sense Metal Element"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Rohm Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "PMR10EZPFV3L00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "143"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 37 "/BAT_N")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "B.Cu")
		(at 108.8 179.67 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at -0.08 -1.26 270)
			(layer "B.SilkS")
		)
		(property "Value" "1n"
			(at 0 -1.05 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/81/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "1000 pF ±10% 25V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033R71E102KA01D"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "81"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.68 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/Power Management/ACDRV2_G")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/Power Management/ACDRV2_S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 113.24 169.1)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at -2.74 -0.45 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SAM_MICRO-IDC_FTSH-105-01-L-DV-K_SMD"
		(layer "B.Cu")
		(at 75.1 168.4 90)
		(descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x05 1.27mm double row")
		(property "Reference" "J12"
			(at 0 4.235 90)
			(layer "B.SilkS")
		)
		(property "Value" "FTSH-105-01-L-DV-K"
			(at -0.1 -6.1 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/145/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 10 position 0.050\" (1.27mm)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "FTSH-105-01-L-DV-K"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Samtec Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "145"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/nRF9151 - GPIO + UICC/")
		(sheetfile "nrf9151_gpio_uicc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.6 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.075 2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "/PWR_nRF91")
			(pinfunction "VREF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.075 2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 127 "/nRF52833/nRF91_SWD.IO")
			(pinfunction "SWDIO")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.075 1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.075 1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 154 "/nRF52833/nRF91_SWD.CLK")
			(pinfunction "SWDCLK")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.075 0 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.075 0 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "/nRF9151 - GPIO + UICC/SWO_UNUSED")
			(pinfunction "SWO")
			(pintype "passive+no_connect")
		)
		(pad "7" smd rect
			(at -2.075 -1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "unconnected-(J12-KEY-Pad7)")
			(pinfunction "KEY")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 2.075 -1.27 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "unconnected-(J12-NC-Pad8)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at -2.075 -2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 2.075 -2.54 90)
			(size 2.65 0.74)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "/nRF52833/nRF91_SWD.nRESET")
			(pinfunction "nRST")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/FTSH-105-01-L-DV-K.step"
			(offset
				(xyz 0 0 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
	)
	(footprint "footprints:GCT_USB4105-XX"
		(locked yes)
		(layer "B.Cu")
		(at 79.1 182.5 180)
		(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
		(tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
		(property "Reference" "CN1"
			(at 6.45 4.3 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "USB4105-GF-A"
			(at 0 -5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/27/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "USB-C (USB TYPE-C) USB 2.0 Receptacle Connector 24 (16+8 Dummy) Position Surface Mount, Right Angle; Through Hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/USB Connectors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "USB4105-GF-A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GCT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "27"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "PCB Edge"
			(at 0 -3.1 0)
			(unlocked yes)
			(layer "User.1")
		)
		(pad "" np_thru_hole circle
			(at -2.89 2.605 180)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 2.605 180)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "A1" smd roundrect
			(at -3.2 3.73 180)
			(size 0.6 1.05)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" smd roundrect
			(at -2.4 3.68 180)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/USB/PWR_USB_5V0_IN")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd roundrect
			(at -1.25 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/USB/USB_CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd roundrect
			(at -0.25 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/USB/USB_CMC_D_P")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd roundrect
			(at 0.25 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/USB/USB_CMC_D_N")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd roundrect
			(at 1.25 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(CN1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A9" smd roundrect
			(at 2.4 3.68 180)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/USB/PWR_USB_5V0_IN")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd roundrect
			(at 3.2 3.73 180)
			(size 0.6 1.05)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd roundrect
			(at 3.2 3.73 180)
			(size 0.6 1.05)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" smd roundrect
			(at 2.4 3.68 180)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/USB/PWR_USB_5V0_IN")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd roundrect
			(at 1.75 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/USB/USB_CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd roundrect
			(at 0.75 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/USB/USB_CMC_D_P")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd roundrect
			(at -0.75 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/USB/USB_CMC_D_N")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd roundrect
			(at -1.75 3.68 180)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(CN1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B9" smd roundrect
			(at -2.4 3.68 180)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/USB/PWR_USB_5V0_IN")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd roundrect
			(at -3.2 3.73 180)
			(size 0.6 1.05)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -1.075 180)
			(size 1.1 1.9)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 3.105 180)
			(size 1.1 2.2)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -1.075 180)
			(size 1.1 1.9)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 3.105 180)
			(size 1.1 2.2)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 130.2 167.967 180)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left")
		(property "Reference" "J4"
			(at 0 3.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "10129380-902001BLF"
			(at 0 -3.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/129/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 2 position 0.100\" (2.54mm)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Amphenol ICC (FCI)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "129"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 166 "/PWR_BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 -1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "/PWR_BAT_IN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 123.475 169.65)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 2.675 1.35 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 162 "/Power Management/PWR_SYS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 115.09 159.7)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.15 0)
			(layer "B.SilkS")
		)
		(property "Value" "91k"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/94/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "91 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF9102X"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "94"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/Power Management/FB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 112.47 159.7)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.15 0)
			(layer "B.SilkS")
		)
		(property "Value" "511k"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/93/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "511 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CRCW0402511KFKEDC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "93"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/Power Management/FB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TI_X2QFN-8"
		(layer "B.Cu")
		(at 104.7 144.865 90)
		(tags "BQ298000RUGR ")
		(property "Reference" "U11"
			(at 0.315 1.55 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "BQ298000"
			(at 0 -4.4 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/137/info"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Battery Battery Protection IC Lithium Ion/Polymer 8-X2QFN (1.5x1.5)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/PMIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "BQ298000RUGT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "8-X2QFN (1.5x1.5)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "137"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(solder_mask_margin 0.05)
		(fp_text user "${REFERENCE}"
			(at 0.05 -2.35 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.635 0.5 270)
			(size 0.58 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 177 "/Battery Protection/BAT")
			(pinfunction "BAT")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at -0.635 0 270)
			(size 0.58 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 165 "/Battery Protection/VDD")
			(pinfunction "VDD")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at -0.635 -0.5 270)
			(size 0.58 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "/BAT_N")
			(pinfunction "VSS")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at 0 -0.435 270)
			(size 0.35 0.63)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "CS")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at 0.635 -0.5 270)
			(size 0.58 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 172 "/Battery Protection/CTR")
			(pinfunction "CTR")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at 0.635 0 270)
			(size 0.58 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 178 "/Battery Protection/PACK")
			(pinfunction "PACK")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at 0.635 0.5 270)
			(size 0.58 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 176 "/Battery Protection/DSG")
			(pinfunction "DSG")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at 0 0.435 270)
			(size 0.35 0.63)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 175 "/Battery Protection/CHG")
			(pinfunction "CHG")
			(pintype "passive")
			(solder_mask_margin 0.05)
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/TI_X2QFN-8.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 105.3 142.665 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at -1.965 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/140/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ERJ-2RKF2001X"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "140"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Battery Protection/")
		(sheetfile "battery-protection.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/PWR_BAT_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 178 "/Battery Protection/PACK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0201_0603Metric"
		(layer "B.Cu")
		(at 108.8025 173.43 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0.05 1.2625 270)
			(layer "B.SilkS")
		)
		(property "Value" "1n"
			(at 0 -1.05 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/81/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "1000 pF ±10% 25V Ceramic Capacitor X7R 0201 (0603 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM033R71E102KA01D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "81"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.68 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/Power Management/ACDRV1_S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/Power Management/ACDRV1_G")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 130.2 160.700333 180)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left")
		(property "Reference" "J14"
			(at 0.95 3.550333 180)
			(layer "B.SilkS")
		)
		(property "Value" "10129380-902001BLF"
			(at 0 -3.6 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/129/info"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 2 position 0.100\" (2.54mm)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Amphenol ICC (FCI)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "129"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 163 "/Power Management/PWR_TPS63_VIN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 -1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 162 "/Power Management/PWR_SYS")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_0402_1005Metric"
		(layer "B.Cu")
		(at 116.475 180.4 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 2.075 270)
			(layer "B.SilkS")
		)
		(property "Value" "5k23"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/99/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "5.23 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Resistors/Thick Film"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-075K23L"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "YAGEO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "99"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Power Management/REGN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 89 "/Power Management/TS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:KOA_TEST_POINT_1206"
		(layer "B.Cu")
		(at 86 183.2 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TP3"
			(at -3.5 -0.85 90)
			(layer "B.SilkS")
		)
		(property "Value" "RCWCTE"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/130/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "PC Test Point Plating Surface Mount Mounting Type"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Test Points"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RCWCTE"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KOA Speer Electronics, Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "130"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 4.2 1.749995)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "/PWR_USB_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${HTTP_LIBRARY_3D_DIR}/KOA_RCWCTE.step"
			(offset
				(xyz 0 0 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "footprints:C_0805_2012Metric"
		(layer "B.Cu")
		(at 123.475 180.45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 2.575 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u 25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/86/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "10 µF ±10% 25V Ceramic Capacitor X5R 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61E106KA73L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "86"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/Power Management/PMID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_0402_1005Metric"
		(layer "B.Cu")
		(at 87.6 173 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 1.1 270)
			(layer "B.SilkS")
		)
		(property "Value" "4u7 10V"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/37/info"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4.7 µF ±20% 10V Ceramic Capacitor X5R 0402 (1005 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage - Rated" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Capacitors/Ceramic Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM155R61A475MEAAD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "37"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/PWR_USB_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SW_Tactile_SPST_NO_Straight_CK_ PTS636SM50JSMTR LFS"
		(layer "B.Cu")
		(at 54.6 160.2 -90)
		(descr "Tactile switch, SPST, 6.0x3.5 mm, H2.5 mm, straight, NO, gull wing leads: https://www.ckswitches.com/media/2779/pts636.pdf")
		(tags "switch tactile SPST 1P1T straight NO SMTR C&K")
		(property "Reference" "SW2"
			(at 0 3 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "PTS636SM50JSMTR LFS"
			(at 0 -3 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/42/info"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Tactile Switch SPST-NO Top Actuated Surface Mount"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Switches/Tactile Switches"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "C&K"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "PTS636SM50JSMTR LFS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "42"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/nRF52833/")
		(sheetfile "nrf52833.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -3.25 0 270)
			(size 0.9 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.25 0 270)
			(size 0.9 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "/nRF52_nRESET")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Tactile_SPST_NO_Straight_CK_PTS636Sx25SMTRLFS.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 102.6 167.966667)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left")
		(property "Reference" "J8"
			(at 0 -3.566667 0)
			(layer "B.SilkS")
		)
		(property "Value" "10129380-902001BLF"
			(at 0 -3.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/129/info"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 2 position 0.100\" (2.54mm)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Connectors/Rectangular Connectors/Male Pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Amphenol ICC (FCI)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "129"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "solar-ribbit.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 1.27)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 66 "/PWR_3V3_LS_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 -1.27)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 164 "/PWR_3V3_LS")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TI_WQFN-6"
		(layer "B.Cu")
		(at 110.9 166.6 180)
		(property "Reference" "U7"
			(at 1.8 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TPS22995RZFR"
			(at 0 -2.35 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://parts.djgood.ca/en/part/78/info"
			(at -0.35 0.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Power Switch/Driver 1:1 N-Channel 3.8A 6-WQFN-HR (1.25x0.85)"
			(at -0.35 0.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits/Load Switches"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "TPS22995RZFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturing Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB Footprint" "6-WQFN-HR (1.25x0.85)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part-DB ID" "78"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Management/")
		(sheetfile "power_management.kicad_sch")
		(solder_mask_margin 0.05)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.2 0.6 90)
			(size 0.45 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PWR_3V3")
			(pinfunction "VBIAS")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -0.375 0 180)
			(size 0.5 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PWR_3V3")
			(pinfunction "VIN")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -0.2 -0.6 90)
			(size 0.45 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 146 "/SBUS_EN")
			(pinfunction "ON")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 0.2 -0.6 90)
			(size 0.45 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 0.375 0 180)
			(size 0.5 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 164 "/PWR_3V3_LS")
			(pinfunction "VOUT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.2 0.6 90)
			(size 0.45 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/Power Management/CT")
			(pinfunction "CT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "/Users/dgood/Projects/kicad-library/3d/TI_WQFN-6.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 54.1 136.2)
		(end 130.1 136.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.1 140.2)
		(end 134.1 182.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 130.1 136.2)
		(mid 132.928427 137.371573)
		(end 134.1 140.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 50.1 186.2)
		(end 50.1 140.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 50.1 140.2)
		(mid 51.271573 137.371573)
		(end 54.1 136.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.1 186.2)
		(end 50.1 186.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 134.1 182.2)
		(mid 132.928427 185.028427)
		(end 130.1 186.2)
		(layer "Edge.Cuts")
	)
	(gr_text "SIM CARD"
		(at 124.4 148.105708 90)
		(layer "F.SilkS")
	)
	(gr_text "Ribbit Network\nribbitnetwork.org"
		(at 64.1 142.036302 0)
		(layer "F.SilkS")
	)
	(gr_text "ANT"
		(at 93 145.2 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 109.35 162.7 90)
		(layer "F.SilkS")
	)
	(gr_text "PANEL:\n24V DC MAX\n"
		(at 92.5 182.4 0)
		(layer "F.SilkS")
	)
	(gr_text "USB"
		(at 86.35 179.3 90)
		(layer "B.SilkS")
	)
	(gr_text "BAT"
		(at 133 169.2 90)
		(layer "B.SilkS")
	)
	(gr_text "USB"
		(at 105.4 176.5 90)
		(layer "B.SilkS")
	)
	(gr_text "ALTERNATE\nBATTERY\nIN"
		(at 90.8 143.4 0)
		(layer "B.SilkS")
	)
	(gr_text "NRF91\nDEBUG"
		(at 68.85 169.965108 0)
		(layer "B.SilkS")
	)
	(gr_text "BAT"
		(at 133.6 173.95 90)
		(layer "B.SilkS")
	)
	(gr_text "NRF52\nRESET"
		(at 59.6 161.765108 0)
		(layer "B.SilkS")
	)
	(gr_text "TPS63"
		(at 133.2 162.3 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 67.1 182.2 270)
		(layer "B.SilkS")
	)
	(gr_text "NRF91"
		(at 105.7 162.4 90)
		(layer "B.SilkS")
	)
	(gr_text "SOLAR"
		(at 98.4 175.3 90)
		(layer "B.SilkS")
	)
	(gr_text "NRF52\nDEBUG"
		(at 54.724303 176.45 0)
		(layer "B.SilkS")
	)
	(gr_text "24V MAX"
		(at 93.1 173.7 0)
		(layer "B.SilkS")
	)
	(gr_text "SBUS"
		(at 105.5 169.3 90)
		(layer "B.SilkS")
	)
	(gr_text "NRF52"
		(at 83.9 162.4 90)
		(layer "B.SilkS")
	)
	(gr_text "-"
		(at 89.3 175.3 0)
		(layer "B.SilkS")
	)
	(gr_text "NRF91\nRESET"
		(at 69.85 161.7 0)
		(layer "B.SilkS")
	)
	(gr_text "SOL"
		(at 105.3 183.7 90)
		(layer "B.SilkS")
	)
	(gr_text "18650 LiFePO4 \nCell Holder"
		(at 90.6 151.3 0)
		(layer "B.SilkS")
	)
	(gr_text "STAT"
		(at 125.85 185.45 0)
		(layer "B.SilkS")
	)
	(gr_text "SENSOR BUS"
		(at 92.15 158.7 0)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 95.3 175.3 0)
		(layer "B.SilkS")
	)
	(gr_text "SE"
		(at 231.8 143.888 0)
		(layer "Dwgs.User")
	)
	(gr_text "Ref 1"
		(at 210.1 137.8 0)
		(layer "Dwgs.User")
	)
	(gr_text "Target Impedance\n+/- 10% [ohms]"
		(at 259.3 137.9 0)
		(layer "Dwgs.User")
	)
	(gr_text "4.43"
		(at 261 93.412 0)
		(layer "Dwgs.User")
	)
	(gr_text "Dielectric 2"
		(at 174.418573 82.43 0)
		(layer "Dwgs.User")
	)
	(gr_text "L4"
		(at 199.600003 151.162 0)
		(layer "Dwgs.User")
	)
	(gr_text "IMPEDANCE TABLE"
		(at 173.688573 133.2 0)
		(layer "Dwgs.User")
	)
	(gr_text "Plated Board Edge: "
		(at 242.68571 38.028 0)
		(layer "Dwgs.User")
	)
	(gr_text "4.00 mils / 4.00 mils"
		(at 207.1 30.114 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.03 mm"
		(at 239.418571 78.824 0)
		(layer "Dwgs.User")
	)
	(gr_text "4.1 / 6.0"
		(at 242 147.524 0)
		(layer "Dwgs.User")
	)
	(gr_text "Type"
		(at 231.8 137.8 0)
		(layer "Dwgs.User")
	)
	(gr_text "Min hole diameter: "
		(at 242.68571 30.114 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.075 mm"
		(at 239.418571 104.066 0)
		(layer "Dwgs.User")
	)
	(gr_text "1080"
		(at 222.91857 75.218 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.3 mm"
		(at 267.628567 30.114 0)
		(layer "Dwgs.User")
	)
	(gr_text "Board overall dimensions: "
		(at 174.442857 26.157 0)
		(layer "Dwgs.User")
	)
	(gr_text "copper"
		(at 197.847142 100.46 0)
		(layer "Dwgs.User")
	)
	(gr_text "L2"
		(at 170.1 78.824 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.035 mm"
		(at 239.418571 114.884 0)
		(layer "Dwgs.User")
	)
	(gr_text "Layer Name"
		(at 174.418573 56.486 0)
		(layer "Dwgs.User")
	)
	(gr_text "Bare Board"
		(at 222.91857 93.248 0)
		(layer "Dwgs.User")
	)
	(gr_text "Coupled Microstrip"
		(at 174.8 147.556 0)
		(layer "Dwgs.User")
	)
	(gr_text "DK"
		(at 261 56.65 0)
		(layer "Dwgs.User")
	)
	(gr_text "3.8"
		(at 261 68.17 0)
		(layer "Dwgs.User")
	)
	(gr_text "F.Paste"
		(at 174.418573 64.4 0)
		(layer "Dwgs.User")
	)
	(gr_text "In1.Cu"
		(at 174.418573 78.824 0)
		(layer "Dwgs.User")
	)
	(gr_text "6"
		(at 207.1 22.2 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.069 mm"
		(at 239.418571 75.218 0)
		(layer "Dwgs.User")
	)
	(gr_text "Yes"
		(at 267.628567 34.071 0)
		(layer "Dwgs.User")
	)
	(gr_text "2116"
		(at 222.91857 96.854 0)
		(layer "Dwgs.User")
	)
	(gr_text "Material"
		(at 222.91857 56.486 0)
		(layer "Dwgs.User")
	)
	(gr_text "Edge card connectors: "
		(at 174.442857 41.985 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.035 mm"
		(at 239.418571 71.612 0)
		(layer "Dwgs.User")
	)
	(gr_text "L2/L5"
		(at 210.1 147.494 0)
		(layer "Dwgs.User")
	)
	(gr_text "B.Cu"
		(at 174.418573 114.884 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.025 mm"
		(at 239.418571 118.49 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.069 mm"
		(at 239.418571 111.278 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 71.612 0)
		(layer "Dwgs.User")
	)
	(gr_text "3.99"
		(at 261 82.594 0)
		(layer "Dwgs.User")
	)
	(gr_text "Not specified"
		(at 222.91857 60.794 0)
		(layer "Dwgs.User")
	)
	(gr_text "B.Mask"
		(at 174.418573 118.49 0)
		(layer "Dwgs.User")
	)
	(gr_text "L5"
		(at 170.1 107.672 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 100.46 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 107.672 0)
		(layer "Dwgs.User")
	)
	(gr_text "B.Silkscreen"
		(at 174.418573 125.702 0)
		(layer "Dwgs.User")
	)
	(gr_text "core"
		(at 197.847142 82.43 0)
		(layer "Dwgs.User")
	)
	(gr_text "Dielectric 4"
		(at 174.418573 104.066 0)
		(layer "Dwgs.User")
	)
	(gr_text "L3"
		(at 170.1 86.036 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 86.036 0)
		(layer "Dwgs.User")
	)
	(gr_text "L3"
		(at 220.9 151.162 0)
		(layer "Dwgs.User")
	)
	(gr_text "copper"
		(at 197.847142 78.824 0)
		(layer "Dwgs.User")
	)
	(gr_text "L4"
		(at 170.1 100.46 0)
		(layer "Dwgs.User")
	)
	(gr_text "Layer"
		(at 199.600003 137.862 0)
		(layer "Dwgs.User")
	)
	(gr_text "F.Silkscreen"
		(at 174.418573 60.794 0)
		(layer "Dwgs.User")
	)
	(gr_text "Dielectric 3  (1/3)"
		(at 174.418573 96.854 0)
		(layer "Dwgs.User")
	)
	(gr_text "FR4"
		(at 222.91857 82.43 0)
		(layer "Dwgs.User")
	)
	(gr_text "In4.Cu"
		(at 174.418573 107.672 0)
		(layer "Dwgs.User")
	)
	(gr_text "In3.Cu"
		(at 174.418573 100.46 0)
		(layer "Dwgs.User")
	)
	(gr_text "0 mm"
		(at 239.418571 125.702 0)
		(layer "Dwgs.User")
	)
	(gr_text "prepreg"
		(at 197.847142 111.278 0)
		(layer "Dwgs.User")
	)
	(gr_text "No"
		(at 207.1 38.028 0)
		(layer "Dwgs.User")
	)
	(gr_text "Trace / Space\n[mil]"
		(at 242 137.83 0)
		(layer "Dwgs.User")
	)
	(gr_text "Dielectric 3  (1/3)"
		(at 174.418573 89.642 0)
		(layer "Dwgs.User")
	)
	(gr_text "Ref 2"
		(at 221 137.7 0)
		(layer "Dwgs.User")
	)
	(gr_text "Min track/spacing: "
		(at 174.442857 30.114 0)
		(layer "Dwgs.User")
	)
	(gr_text "3.91"
		(at 261 75.382 0)
		(layer "Dwgs.User")
	)
	(gr_text "Top Solder Mask"
		(at 197.847142 68.006 0)
		(layer "Dwgs.User")
	)
	(gr_text "Impedance Control: "
		(at 242.68571 34.071 0)
		(layer "Dwgs.User")
	)
	(gr_text "F.Mask"
		(at 174.418573 68.006 0)
		(layer "Dwgs.User")
	)
	(gr_text "L1"
		(at 170.1 71.612 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.865 mm"
		(at 239.418571 93.248 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 122.096 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 64.4 0)
		(layer "Dwgs.User")
	)
	(gr_text "0 mm"
		(at 239.418571 122.096 0)
		(layer "Dwgs.User")
	)
	(gr_text "L1/L6"
		(at 199.600003 147.556 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.03 mm"
		(at 239.418571 107.672 0)
		(layer "Dwgs.User")
	)
	(gr_text "Castellated pads: "
		(at 174.442857 38.028 0)
		(layer "Dwgs.User")
	)
	(gr_text "90"
		(at 259.3 151.232 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.025 mm"
		(at 239.418571 68.006 0)
		(layer "Dwgs.User")
	)
	(gr_text "63.43 mils"
		(at 267.628567 22.2 0)
		(layer "Dwgs.User")
	)
	(gr_text "Type"
		(at 174.1 137.8 0)
		(layer "Dwgs.User")
	)
	(gr_text "Type"
		(at 197.847142 56.486 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.075 mm"
		(at 239.418571 82.43 0)
		(layer "Dwgs.User")
	)
	(gr_text "Copper Layer Count: "
		(at 174.442857 22.2 0)
		(layer "Dwgs.User")
	)
	(gr_text "DIFF"
		(at 231.8 151.162 0)
		(layer "Dwgs.User")
	)
	(gr_text "Copper Finish: "
		(at 174.442857 34.071 0)
		(layer "Dwgs.User")
	)
	(gr_text "Bottom Solder Paste"
		(at 197.847142 122.096 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.03 mm"
		(at 239.418571 100.46 0)
		(layer "Dwgs.User")
	)
	(gr_text "L5"
		(at 210.1 151.162 0)
		(layer "Dwgs.User")
	)
	(gr_text "Thickness (mm)"
		(at 239.418571 56.486 0)
		(layer "Dwgs.User")
	)
	(gr_text "0 mm"
		(at 239.418571 60.794 0)
		(layer "Dwgs.User")
	)
	(gr_text "Not specified"
		(at 222.91857 118.49 0)
		(layer "Dwgs.User")
	)
	(gr_text "4.16"
		(at 261 97.018 0)
		(layer "Dwgs.User")
	)
	(gr_text "prepreg"
		(at 197.847142 75.218 0)
		(layer "Dwgs.User")
	)
	(gr_text "4.16"
		(at 261 89.806 0)
		(layer "Dwgs.User")
	)
	(gr_text "ENIG"
		(at 207.1 34.071 0)
		(layer "Dwgs.User")
	)
	(gr_text "50"
		(at 259.3 143.988 0)
		(layer "Dwgs.User")
	)
	(gr_text "0 mm"
		(at 239.418571 64.4 0)
		(layer "Dwgs.User")
	)
	(gr_text "BOARD CHARACTERISTICS"
		(at 173.692857 16.706 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 259.3 147.594 0)
		(layer "Dwgs.User")
	)
	(gr_text "In2.Cu"
		(at 174.418573 86.036 0)
		(layer "Dwgs.User")
	)
	(gr_text "copper"
		(at 197.847142 71.612 0)
		(layer "Dwgs.User")
	)
	(gr_text "Top Silk Screen"
		(at 197.847142 60.794 0)
		(layer "Dwgs.User")
	)
	(gr_text "Dielectric 5"
		(at 174.418573 111.278 0)
		(layer "Dwgs.User")
	)
	(gr_text "prepreg"
		(at 197.847142 96.854 0)
		(layer "Dwgs.User")
	)
	(gr_text "Not specified"
		(at 222.91857 68.006 0)
		(layer "Dwgs.User")
	)
	(gr_text "Bottom Silk Screen"
		(at 197.847142 125.702 0)
		(layer "Dwgs.User")
	)
	(gr_text "L6"
		(at 170.1 114.884 0)
		(layer "Dwgs.User")
	)
	(gr_text "L1/L6"
		(at 199.600003 143.95 0)
		(layer "Dwgs.User")
	)
	(gr_text "3.99"
		(at 261 104.23 0)
		(layer "Dwgs.User")
	)
	(gr_text "L2/L5"
		(at 210.1 143.888 0)
		(layer "Dwgs.User")
	)
	(gr_text "3.8"
		(at 261 118.654 0)
		(layer "Dwgs.User")
	)
	(gr_text "3.91"
		(at 261 111.442 0)
		(layer "Dwgs.User")
	)
	(gr_text "2116"
		(at 222.91857 89.642 0)
		(layer "Dwgs.User")
	)
	(gr_text "Not specified"
		(at 222.91857 125.702 0)
		(layer "Dwgs.User")
	)
	(gr_text "90"
		(at 259.428572 147.588 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.03 mm"
		(at 239.418571 86.036 0)
		(layer "Dwgs.User")
	)
	(gr_text "Dielectric 3  (1/3)"
		(at 174.418573 93.248 0)
		(layer "Dwgs.User")
	)
	(gr_text "core"
		(at 197.847142 104.066 0)
		(layer "Dwgs.User")
	)
	(gr_text "copper"
		(at 197.847142 86.036 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.109 mm"
		(at 239.418571 89.642 0)
		(layer "Dwgs.User")
	)
	(gr_text "B.Paste"
		(at 174.418573 122.096 0)
		(layer "Dwgs.User")
	)
	(gr_text "0.109 mm"
		(at 239.418571 96.854 0)
		(layer "Dwgs.User")
	)
	(gr_text "Coupled Microstrip"
		(at 174.9 151.162 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 114.884 0)
		(layer "Dwgs.User")
	)
	(gr_text "prepreg"
		(at 197.847142 89.642 0)
		(layer "Dwgs.User")
	)
	(gr_text "No"
		(at 207.1 41.985 0)
		(layer "Dwgs.User")
	)
	(gr_text "copper"
		(at 197.847142 114.884 0)
		(layer "Dwgs.User")
	)
	(gr_text "No"
		(at 267.628567 38.028 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 222.91857 78.824 0)
		(layer "Dwgs.User")
	)
	(gr_text "STACKUP"
		(at 173.692857 49.794 0)
		(layer "Dwgs.User")
	)
	(gr_text "84.0 mm x 50.0 mm"
		(at 207.1 26.157 0)
		(layer "Dwgs.User")
	)
	(gr_text "Dielectric 1"
		(at 174.418573 75.218 0)
		(layer "Dwgs.User")
	)
	(gr_text "Board Thickness: "
		(at 242.68571 22.2 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 242.68571 26.157 0)
		(layer "Dwgs.User")
	)
	(gr_text ""
		(at 267.628567 26.157 0)
		(layer "Dwgs.User")
	)
	(gr_text "4.1"
		(at 242 143.918 0)
		(layer "Dwgs.User")
	)
	(gr_text "Top Solder Paste"
		(at 197.847142 64.4 0)
		(layer "Dwgs.User")
	)
	(gr_text "4.0 / 6.0"
		(at 242 151.162 0)
		(layer "Dwgs.User")
	)
	(gr_text "FR4"
		(at 222.91857 104.066 0)
		(layer "Dwgs.User")
	)
	(gr_text "Bottom Solder Mask"
		(at 197.847142 118.49 0)
		(layer "Dwgs.User")
	)
	(gr_text "Coplanar Waveguide"
		(at 174.7 143.95 0)
		(layer "Dwgs.User")
	)
	(gr_text "core"
		(at 197.847142 93.248 0)
		(layer "Dwgs.User")
	)
	(gr_text "1080"
		(at 222.91857 111.278 0)
		(layer "Dwgs.User")
	)
	(gr_text "DIFF"
		(at 231.8 147.494 0)
		(layer "Dwgs.User")
	)
	(gr_text "copper"
		(at 197.847142 107.672 0)
		(layer "Dwgs.User")
	)
	(gr_text "F.Cu"
		(at 174.418573 71.612 0)
		(layer "Dwgs.User")
	)
	(zone
		(net 32)
		(net_name "/PWR_nRF52")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 62.176306 162.170657) (xy 62.172935 161.368252) (xy 60.4 159.639145) (xy 60.4 159.1) (xy 61.5 159.1)
				(xy 62.8 159.2) (xy 62.830369 160.621475) (xy 62.830369 162.170657)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "BLE_FEED")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 63.126288 168.346829) (xy 63.212711 168.396725) (xy 63.283275 168.467289) (xy 63.333171 168.553712)
				(xy 63.359 168.650104) (xy 63.36227 168.7) (xy 63.36227 180.1) (xy 63.359 180.149896) (xy 63.333171 180.246288)
				(xy 63.283275 180.332711) (xy 63.212711 180.403275) (xy 63.126288 180.453171) (xy 63.029896 180.479)
				(xy 62.930104 180.479) (xy 62.833712 180.453171) (xy 62.747289 180.403275) (xy 62.676725 180.332711)
				(xy 62.626829 180.246288) (xy 62.601 180.149896) (xy 62.59773 180.1) (xy 62.59773 168.7) (xy 62.601 168.650104)
				(xy 62.626829 168.553712) (xy 62.676725 168.467289) (xy 62.747289 168.396725) (xy 62.833712 168.346829)
				(xy 62.930104 168.321) (xy 63.029896 168.321)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 62.616399 172.62) (xy 62.616399 171.98) (xy 63.343601 171.98) (xy 63.343601 172.62)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/Power Management/SW2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 119.125 173.65) (xy 119.125 172.6) (xy 120.225 172.6) (xy 120.225 173.65)
			)
		)
	)
	(zone
		(net 9)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.2 152.2) (xy 101.6 152.2) (xy 101.6 152) (xy 102.5 151.1) (xy 104.2 151.1)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.010345 149.751743) (xy 91.003756 149.77777) (xy 90.992973 149.802358) (xy 90.97829 149.824836)
				(xy 90.960108 149.84459) (xy 90.938922 149.861082) (xy 90.915311 149.873862) (xy 90.889918 149.882582)
				(xy 90.863437 149.887003) (xy 90.836589 149.887005) (xy 90.810107 149.882588) (xy 90.784713 149.873873)
				(xy 90.761099 149.861096) (xy 90.739911 149.844608) (xy 90.721726 149.824856) (xy 90.707039 149.802381)
				(xy 90.696253 149.777795) (xy 90.68966 149.751769) (xy 90.68744 149.725013) (xy 90.688079 149.709522)
				(xy 90.689996 149.694138) (xy 90.693176 149.678965) (xy 90.697599 149.664106) (xy 90.703234 149.649663)
				(xy 90.710043 149.635735) (xy 90.717978 149.622416) (xy 90.726986 149.609799) (xy 90.737006 149.597969)
				(xy 90.747969 149.587006) (xy 90.759799 149.576986) (xy 90.772416 149.567978) (xy 90.785735 149.560043)
				(xy 90.799663 149.553234) (xy 90.814106 149.547599) (xy 90.828965 149.543176) (xy 90.844138 149.539996)
				(xy 90.859522 149.538079) (xy 90.875013 149.53744) (xy 90.901769 149.53966) (xy 90.927795 149.546253)
				(xy 90.952381 149.557039) (xy 90.974856 149.571726) (xy 90.994608 149.589911) (xy 91.011096 149.611099)
				(xy 91.023873 149.634713) (xy 91.032588 149.660107) (xy 91.037005 149.686589) (xy 91.037003 149.713437)
				(xy 91.032582 149.739918) (xy 91.023862 149.765311) (xy 91.011082 149.788922) (xy 90.99459 149.810108)
				(xy 90.974836 149.82829) (xy 90.952358 149.842973) (xy 90.92777 149.853756) (xy 90.901743 149.860345)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 62.616399 170.22) (xy 62.616399 169.901456) (xy 63.341782 169.900428) (xy 63.343601 169.902247)
				(xy 63.343601 170.22)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "GNSS_FEED")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 82.806396 148.246) (xy 82.902788 148.271829) (xy 82.989211 148.321725) (xy 83.059775 148.392289)
				(xy 83.109671 148.478712) (xy 83.1355 148.575104) (xy 83.1355 148.674896) (xy 83.109671 148.771288)
				(xy 83.059775 148.857711) (xy 82.989211 148.928275) (xy 82.902788 148.978171) (xy 82.806396 149.004)
				(xy 82.7565 149.00727) (xy 82.223274 149.00727) (xy 82.109865 149.007272) (xy 81.88584 149.042757)
				(xy 81.670124 149.11285) (xy 81.468029 149.215825) (xy 81.28453 149.349146) (xy 81.124146 149.50953)
				(xy 80.990825 149.693029) (xy 80.88785 149.895124) (xy 80.817757 150.11084) (xy 80.782272 150.334865)
				(xy 80.78227 150.44826) (xy 80.78227 154.899118) (xy 80.782272 155.018459) (xy 80.816242 155.254712)
				(xy 80.883488 155.483725) (xy 80.982641 155.700838) (xy 81.111683 155.901629) (xy 81.267987 156.082013)
				(xy 81.448371 156.238317) (xy 81.649162 156.367359) (xy 81.866275 156.466512) (xy 82.095288 156.533758)
				(xy 82.331541 156.567728) (xy 82.450882 156.56773) (xy 86.475 156.56773) (xy 86.524896 156.571)
				(xy 86.621288 156.596829) (xy 86.707711 156.646725) (xy 86.778275 156.717289) (xy 86.828171 156.803712)
				(xy 86.854 156.900104) (xy 86.854 156.999896) (xy 86.828171 157.096288) (xy 86.778275 157.182711)
				(xy 86.707711 157.253275) (xy 86.621288 157.303171) (xy 86.524896 157.329) (xy 86.475 157.33227)
				(xy 82.450878 157.33227) (xy 82.450875 157.332269) (xy 82.450874 157.33227) (xy 82.157592 157.314527)
				(xy 81.868587 157.261562) (xy 81.588073 157.174148) (xy 81.320141 157.05356) (xy 81.068697 156.901556)
				(xy 80.837408 156.720353) (xy 80.629647 156.512592) (xy 80.448444 156.281303) (xy 80.29644 156.029859)
				(xy 80.175852 155.761927) (xy 80.088438 155.481413) (xy 80.035473 155.192408) (xy 80.01773 154.899126)
				(xy 80.01773 150.44826) (xy 80.033815 150.182414) (xy 80.081826 149.920446) (xy 80.161064 149.666174)
				(xy 80.270372 149.423307) (xy 80.408157 149.195386) (xy 80.572409 148.985734) (xy 80.760734 148.797409)
				(xy 80.970386 148.633157) (xy 81.198307 148.495372) (xy 81.441174 148.386064) (xy 81.695446 148.306826)
				(xy 81.957414 148.258815) (xy 82.22326 148.24273) (xy 82.7565 148.24273)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "LNA_FEED")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 86.799896 150.621) (xy 86.803366 150.621929) (xy 86.977967 150.635671) (xy 87.200321 150.689054)
				(xy 87.411587 150.776563) (xy 87.606562 150.896044) (xy 87.780445 151.044555) (xy 87.928956 151.218438)
				(xy 88.048437 151.413413) (xy 88.135946 151.624679) (xy 88.189329 151.847033) (xy 88.20307 152.021633)
				(xy 88.204 152.025104) (xy 88.20727 152.075) (xy 88.20727 153.599554) (xy 88.207269 153.599559)
				(xy 88.20727 153.599562) (xy 88.207313 153.599562) (xy 88.207311 153.717172) (xy 88.238008 153.950379)
				(xy 88.298882 154.177584) (xy 88.388891 154.394901) (xy 88.506495 154.598609) (xy 88.649683 154.785225)
				(xy 88.72627 154.861816) (xy 88.731839 154.866868) (xy 88.738301 154.873551) (xy 88.745306 154.879694)
				(xy 88.777781 154.91217) (xy 88.810751 154.949764) (xy 88.910925 155.063984) (xy 89.023121 155.231889)
				(xy 89.11244 155.413001) (xy 89.177355 155.604224) (xy 89.216754 155.802283) (xy 89.227953 155.973133)
				(xy 89.229743 155.991323) (xy 89.232067 156.06253) (xy 89.230426 156.112507) (xy 89.207755 156.20969)
				(xy 89.160705 156.297694) (xy 89.09248 156.370523) (xy 89.007731 156.423211) (xy 88.912232 156.452171)
				(xy 88.812493 156.455426) (xy 88.71531 156.432755) (xy 88.627306 156.385705) (xy 88.554477 156.31748)
				(xy 88.501789 156.232731) (xy 88.472829 156.137232) (xy 88.467933 156.08747) (xy 88.465609 156.016263)
				(xy 88.465904 156.007262) (xy 88.465406 156.003795) (xy 88.465423 156.003795) (xy 88.465422 155.927046)
				(xy 88.435474 155.776498) (xy 88.37673 155.634685) (xy 88.291448 155.507058) (xy 88.237177 155.452789)
				(xy 88.237178 155.452789) (xy 88.23717 155.452781) (xy 88.21127 155.426882) (xy 88.20569 155.42182)
				(xy 88.196069 155.411871) (xy 88.192217 155.408987) (xy 88.192217 155.408986) (xy 88.179272 155.3945)
				(xy 88.170931 155.385874) (xy 88.169296 155.383336) (xy 88.001009 155.195013) (xy 87.83496 154.960977)
				(xy 87.696159 154.709821) (xy 87.586352 154.444703) (xy 87.506918 154.168958) (xy 87.458857 153.886053)
				(xy 87.443032 153.604177) (xy 87.44273 153.599554) (xy 87.44273 152.006772) (xy 87.416109 151.872938)
				(xy 87.36389 151.746869) (xy 87.288079 151.63341) (xy 87.19159 151.536921) (xy 87.078131 151.46111)
				(xy 86.952062 151.408891) (xy 86.818228 151.38227) (xy 85.0435 151.38227) (xy 84.993604 151.379)
				(xy 84.897212 151.353171) (xy 84.810789 151.303275) (xy 84.740225 151.232711) (xy 84.690329 151.146288)
				(xy 84.6645 151.049896) (xy 84.6645 150.950104) (xy 84.690329 150.853712) (xy 84.740225 150.767289)
				(xy 84.810789 150.696725) (xy 84.897212 150.646829) (xy 84.993604 150.621) (xy 85.0435 150.61773)
				(xy 86.75 150.61773)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "ANT_COPLANAR")
		(hatch edge 0.5)
		(connect_pads thru_hole_only
			(clearance 0)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 62.6 168.5) (xy 62.05 168) (xy 61.630377 168.466248) (xy 62.603273 169.311731) (xy 62.603096 169.901456)
				(xy 64.75 169.9) (xy 64.75 168.975) (xy 63.7 168.110169) (xy 63.7 166.3) (xy 63.35 166.3) (xy 63.35 168.5)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/PWR_nRF91")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 83.072973 166.403729) (xy 83.072973 167.800594) (xy 83.584673 167.789353) (xy 83.651551 167.277097)
				(xy 84.155686 166.742482) (xy 84.159974 166.253757)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/Power Management/SW1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 119.125 175.3) (xy 119.125 174.25) (xy 120.225 174.25) (xy 120.225 175.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "XTAL_KO")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 70.35 171.975) (xy 70.35 167.675) (xy 65.35 167.675) (xy 65.35 171.975)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "ANT_FEED")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.021288 145.746829) (xy 91.107711 145.796725) (xy 91.178275 145.867289) (xy 91.228171 145.953712)
				(xy 91.254 146.050104) (xy 91.25727 146.1) (xy 91.25727 153.599546) (xy 91.241186 153.886058) (xy 91.193124 154.168968)
				(xy 91.113689 154.444717) (xy 91.003879 154.709839) (xy 90.865076 154.961) (xy 90.699025 155.19504)
				(xy 90.507813 155.409017) (xy 90.507783 155.408987) (xy 90.500355 155.414547) (xy 90.495306 155.420305)
				(xy 90.462831 155.452781) (xy 90.462822 155.452788) (xy 90.462822 155.452789) (xy 90.462835 155.452801)
				(xy 90.408565 155.507069) (xy 90.323285 155.634693) (xy 90.264542 155.776503) (xy 90.234595 155.927048)
				(xy 90.234594 156.003795) (xy 90.234095 156.007262) (xy 90.234391 156.016263) (xy 90.232067 156.08747)
				(xy 90.227171 156.137232) (xy 90.198211 156.232731) (xy 90.145523 156.31748) (xy 90.072694 156.385705)
				(xy 89.98469 156.432755) (xy 89.887507 156.455426) (xy 89.787768 156.452171) (xy 89.692269 156.423211)
				(xy 89.60752 156.370523) (xy 89.539295 156.297694) (xy 89.492245 156.20969) (xy 89.469574 156.112507)
				(xy 89.467933 156.06253) (xy 89.470257 155.991323) (xy 89.472097 155.972615) (xy 89.483263 155.802285)
				(xy 89.522662 155.604228) (xy 89.587575 155.413008) (xy 89.676894 155.231897) (xy 89.789089 155.063995)
				(xy 89.889204 154.949841) (xy 89.88925 154.949763) (xy 89.922219 154.912169) (xy 89.954695 154.879694)
				(xy 89.966338 154.869482) (xy 89.967157 154.868389) (xy 89.967187 154.86842) (xy 90.05035 154.785253)
				(xy 90.19354 154.598633) (xy 90.311148 154.39492) (xy 90.401159 154.177598) (xy 90.462034 153.950387)
				(xy 90.492732 153.717174) (xy 90.49273 153.599562) (xy 90.49273 146.1) (xy 90.496 146.050104) (xy 90.521829 145.953712)
				(xy 90.571725 145.867289) (xy 90.642289 145.796725) (xy 90.728712 145.746829) (xy 90.825104 145.721)
				(xy 90.924896 145.721)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Mask" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu")
		(name "ANT_")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 66.05 180.51) (xy 50.1 180.51) (xy 50.1 186.2) (xy 66.05 186.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.675 174.65) (xy 125.675 173.25) (xy 123.625 173.25) (xy 123.625 174.65)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In4.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.0254)
		)
		(polygon
			(pts
				(xy 134.1 140.2) (xy 134.098137 140.015155) (xy 134.064026 139.647042) (xy 133.996096 139.283647)
				(xy 133.894925 138.928069) (xy 133.761378 138.583344) (xy 133.596593 138.252411) (xy 133.401976 137.938094)
				(xy 133.179188 137.643075) (xy 132.930129 137.369871) (xy 132.656925 137.120812) (xy 132.361906 136.898024)
				(xy 132.047589 136.703407) (xy 131.716656 136.538622) (xy 131.371931 136.405075) (xy 131.016353 136.303904)
				(xy 130.652958 136.235974) (xy 130.284845 136.201863) (xy 130.1 136.2) (xy 54.1 136.2) (xy 53.915155 136.201863)
				(xy 53.547042 136.235974) (xy 53.183647 136.303904) (xy 52.828069 136.405075) (xy 52.483344 136.538622)
				(xy 52.152411 136.703407) (xy 51.838094 136.898024) (xy 51.543075 137.120812) (xy 51.269871 137.369871)
				(xy 51.020812 137.643075) (xy 50.798024 137.938094) (xy 50.603407 138.252411) (xy 50.438622 138.583344)
				(xy 50.305075 138.928069) (xy 50.203904 139.283647) (xy 50.135974 139.647042) (xy 50.101863 140.015155)
				(xy 50.1 140.2) (xy 50.1 186.2) (xy 130.1 186.2) (xy 130.284845 186.198137) (xy 130.652958 186.164026)
				(xy 131.016353 186.096096) (xy 131.371931 185.994925) (xy 131.716656 185.861378) (xy 132.047589 185.696593)
				(xy 132.361906 185.501976) (xy 132.656925 185.279188) (xy 132.930129 185.030129) (xy 133.179188 184.756925)
				(xy 133.401976 184.461906) (xy 133.596593 184.147589) (xy 133.761378 183.816656) (xy 133.894925 183.471931)
				(xy 133.996096 183.116353) (xy 134.064026 182.752958) (xy 134.098137 182.384845) (xy 134.1 182.2)
			)
		)
	)
	(zone
		(net 78)
		(net_name "Net-(U6-LX1)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.465 163.55) (xy 115.465 163.711044) (xy 116.84 164.7) (xy 116.84 167.6) (xy 115.64 167.6)
				(xy 115.64 164.7) (xy 115.215 163.7) (xy 115.215 163.55)
			)
		)
	)
	(zone
		(net 166)
		(net_name "/PWR_BATT")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130 161.4) (xy 132.9 161.4) (xy 132.9 167.4) (xy 130 167.4)
			)
		)
	)
	(zone
		(net 162)
		(net_name "/Power Management/PWR_SYS")
		(layer "B.Cu")
		(name "nRF91_LocalPower")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.6 172.2) (xy 121.2 171.8) (xy 121.2 163.95333) (xy 123 162.237342) (xy 123 161.9) (xy 123 161.4)
				(xy 130 161.4) (xy 130 164.1) (xy 123.3 164.1) (xy 123.3 171.6) (xy 121.7 173.2) (xy 121.6 173.2)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/PWR_BAT_IN")
		(layer "B.Cu")
		(name "ANT_COPLANAR")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads thru_hole_only
			(clearance 0.1524)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 108.6 142) (xy 107.3 142) (xy 107.3 139.8) (xy 109.8 139.8) (xy 110.8 145.5) (xy 111.1 146.2)
				(xy 111.1 146.8) (xy 108.6 146.8) (xy 108.6 145.8)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/PWR_3V3_LS_OUT")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 94.3 162.3) (xy 94.3 163.9) (xy 93.1 163.9) (xy 93.095756 162.3) (xy 92.2 162.3) (xy 92.2 165.2)
				(xy 94.4 167.4) (xy 98.1 167.4) (xy 99.6 168.9) (xy 99.6 169.9) (xy 102.3 169.9) (xy 102.3 165.3)
				(xy 99 162.3)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/Power Management/ACDRV2_S")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111.9 180.62) (xy 110.3 180.62) (xy 110.3 179.145) (xy 109.6 179.145) (xy 109.6 178.745) (xy 111.2 178.745)
				(xy 111.2 180.22) (xy 111.9 180.22)
			)
		)
	)
	(zone
		(net 173)
		(net_name "/BAT_P")
		(layer "B.Cu")
		(name "ANT_COPLANAR")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads thru_hole_only
			(clearance 0.1524)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 107.4 149) (xy 108.1 149) (xy 109 148.46) (xy 109 146.9) (xy 111.2 146.9) (xy 111.2 146.4) (xy 113.9 146.4)
				(xy 113.9 151.7) (xy 110.9 151.7) (xy 110.9 150.4) (xy 107.4 150.4)
			)
		)
	)
	(zone
		(net 77)
		(net_name "Net-(U6-LX2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.815 163.55) (xy 114.815 163.711044) (xy 113.44 164.7) (xy 113.44 167.6) (xy 114.64 167.6)
				(xy 114.64 164.7) (xy 115.065 163.7) (xy 115.065 163.55)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/USB/PWR_USB_5V0_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 77.1 180.5) (xy 76.4 179.3) (xy 77 179.3) (xy 77.85 179.825)
			)
		)
	)
	(zone
		(net 166)
		(net_name "/PWR_BATT")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 119.4 168.3) (xy 119.4 161.4) (xy 122.874535 161.4) (xy 122.868846 162.085469) (xy 121.075 163.786025)
				(xy 121.075 168.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.475 183.55) (xy 123.475 175.95) (xy 122.675 174.97) (xy 122.675 172.93) (xy 123.475 171.95)
				(xy 123.475 165.25) (xy 123.475 164.25) (xy 126.122931 164.25) (xy 126.1 171.8) (xy 124.025 172.45)
				(xy 123.6 172.8) (xy 123.6 175.05) (xy 123.975 175.45) (xy 126.175 176.1) (xy 126.175 183.55)
			)
		)
	)
	(zone
		(net 163)
		(net_name "/Power Management/PWR_TPS63_VIN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.625 163.15) (xy 115.625 163.55) (xy 115.74 163.665) (xy 116.94 164.3) (xy 119.190909 164.3)
				(xy 119.200303 161.2) (xy 132.9 161.2) (xy 132.9 158.7) (xy 117.39 158.7) (xy 117.39 162.1) (xy 116.94 162.6)
				(xy 115.74 163.035)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/Power Management/ACDRV1_S")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111.9025 174.38) (xy 110.3025 174.38) (xy 110.3025 172.905) (xy 109.6025 172.905) (xy 109.6025 172.505)
				(xy 111.2025 172.505) (xy 111.2025 173.98) (xy 111.9025 173.98)
			)
		)
	)
	(zone
		(net 174)
		(net_name "/Battery Protection/BAT_P_POL")
		(layer "B.Cu")
		(name "ANT_COPLANAR")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads thru_hole_only
			(clearance 0.1524)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 105.7 142.1) (xy 108.6 142.1) (xy 108.6 146.8) (xy 108.6 146.9) (xy 105.7 149.8)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/PWR_USB")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 25)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.8 172.9) (xy 100.8 175) (xy 102.9 175) (xy 103.4 174.5) (xy 103.400165 173.467013) (xy 102.833152 172.9)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/PWR_BAT_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 14)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.85 164.25) (xy 129.85 169.9) (xy 127.1 169.9) (xy 127 169.8) (xy 127 164.25)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PWR_3V3")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 81.401015 158.930292) (xy 77.9 158.9) (xy 77.9 160.2) (xy 79.9 160.2) (xy 81.400416 159.91252)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/PWR_PANEL_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 24)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.825 183.488551) (xy 101 183.5) (xy 99.685303 182.1) (xy 98.031277 182.1)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/Power Management/PWR_VBUS")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 119.875 175.55) (xy 119.885 175.54) (xy 120.6 175.54) (xy 120.6 177) (xy 121.5 177.9) (xy 121.5 184.7)
				(xy 121.3 184.9) (xy 113.5 184.9) (xy 112.1 183.5) (xy 112.1 174.654266) (xy 112.8 174.654266) (xy 113.8 175.7)
				(xy 113.8 182.6) (xy 115 183.8) (xy 119 183.8) (xy 119.475 183.325) (xy 119.475 179.425) (xy 120.3 178.6)
				(xy 120.3 177.7) (xy 119.875 177.275)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.44 167.6) (xy 116.84 167.6) (xy 116.84 164.7) (xy 113.44 164.7)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PWR_3V3")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.655 163.15) (xy 114.655 163.55) (xy 114.54 163.665) (xy 113.34 164.3) (xy 111.79 164.3)
				(xy 111.79 160.55) (xy 112.79 160.55) (xy 112.79 162.1) (xy 113.34 162.6) (xy 114.54 163.035)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/Power Management/SW1")
		(layers "B.Cu" "In3.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.575 174.55) (xy 120.475 174.55) (xy 120.225 174.85) (xy 120.225 175.3) (xy 119.125 175.3)
				(xy 119.125 174.25) (xy 120.225 174.25) (xy 120.375 174.25) (xy 120.575 174.25)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/Power Management/SW2")
		(layers "B.Cu" "In3.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.575 173.35) (xy 120.475 173.35) (xy 120.225 173.05) (xy 120.225 172.6) (xy 119.125 172.6)
				(xy 119.125 173.65) (xy 120.225 173.65) (xy 120.375 173.65) (xy 120.575 173.65)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 89.971874 146.35477) (xy 91.845646 146.35477) (xy 91.845646 143.321045) (xy 89.971874 143.321045)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PWR_3V3")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 28)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 108.55 159.527669) (xy 96.16205 170.841996) (xy 88.471944 170.855487) (xy 85.6 163.7) (xy 81.1 160.45)
				(xy 81.1 157.825) (xy 77.35 157.825) (xy 77.35 167.2) (xy 84.85 174.7) (xy 98.76279 174.7) (xy 108.6 165.086363)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/PWR_nRF52")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 69.35 157.7) (xy 60.1 157.7) (xy 60.1 161.2) (xy 58.4 165.4) (xy 58.4 167.2) (xy 66.1 167.2)
				(xy 68.1 169.2) (xy 74.35 169.2) (xy 74.35 160.2) (xy 71.85 160.2)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/PWR_BAT_IN")
		(layer "In3.Cu")
		(name "nRF91_LocalPower")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130.1 164.8) (xy 130.1 171.5) (xy 118.3 171.5) (xy 109.044949 162.244949) (xy 109.1 151.4) (xy 107.3 141.9)
				(xy 107.3 139.8) (xy 109.6 139.8) (xy 119.236793 151.57912) (xy 119.244025 163.048236) (xy 119.4 163.2)
				(xy 121 164.8)
			)
		)
	)
	(zone
		(net 166)
		(net_name "/PWR_BATT")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 119.4 161.4) (xy 133.6 161.4) (xy 133.6 165.4) (xy 130.2 165.4) (xy 130.2 164.8) (xy 121 164.8)
				(xy 119.4 163.2)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/PWR_nRF91")
		(layer "In3.Cu")
		(name "nRF91_LocalPower")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 81.1 151.7) (xy 108.55 151.7) (xy 108.55 159.527669) (xy 96.160608 170.843313) (xy 88.471944 170.855487)
				(xy 85.6 163.7) (xy 81.080145 160.43566) (xy 81.1 160.45)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/PWR_USB")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 23)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.6 172.95) (xy 98.76279 174.7) (xy 80.715614 174.7) (xy 77.271013 171.227469) (xy 77.35 159.95)
				(xy 77.360434 158.460434) (xy 72.6 153.7) (xy 58.85 153.7) (xy 57.35 155.2) (xy 57.35 158.7) (xy 60.1 161.2)
				(xy 60.1 157.7) (xy 69.35 157.7) (xy 71.85 160.2) (xy 74.35 160.2) (xy 74.35 173.7) (xy 77.35 176.7)
				(xy 103.6 176.7) (xy 103.6 172.95)
			)
		)
	)
	(embedded_fonts no)
)
