(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/mic")
	(net 2 "Net-(C1-Pad1)")
	(net 3 "Net-(C2-Pad1)")
	(net 4 "Net-(U3-BYPASS)")
	(net 5 "GND")
	(net 6 "Net-(C4-Pad2)")
	(net 7 "Net-(C4-Pad1)")
	(net 8 "Net-(U3-+)")
	(net 9 "Net-(C5-Pad1)")
	(net 10 "/temp")
	(net 11 "VCC")
	(net 12 "/sda")
	(net 13 "/scl")
	(net 14 "unconnected-(U2A-int-Pad8)")
	(net 15 "unconnected-(U2A-xda-Pad5)")
	(net 16 "unconnected-(U2A-xcl-Pad6)")
	(net 17 "unconnected-(U2A-ado-Pad7)")
	(footprint "keychain:ce_small"
		(layer "F.Cu")
		(at 195.54 91.22)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 191.7 92.56 180)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "U1"
			(at 4.49 1.73 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM35-LP"
			(at 1.27 2.79 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm35.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Precision centigrade temperature sensor, TO-92"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "VCC")
			(pinfunction "+V_{S}")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 180)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/temp")
			(pinfunction "V_{OUT}")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 180)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keychain:hackster logo"
		(layer "F.Cu")
		(at 193.05 78.36)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 169.34 77.16 90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "I2c"
			(at 0 9.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/scl")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/sda")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm"
		(layer "F.Cu")
		(at 165.9475 79.6325)
		(descr "Sanyo SIP-15, 78.0mm x 8.0mm bosy size, STK-437E STK-439E STK-441E STK-443E (http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf)")
		(tags "Sanyo SIP-15")
		(property "Reference" "U2"
			(at 0.7025 4.2375 90)
			(layer "F.SilkS")
		)
		(property "Value" "mpu6050"
			(at 17.78 5.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-Channel 24 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Sanyo*78.0x8.0mm*P2.54mm*")
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.2 -0.86 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 1.09 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "VCC")
			(pinfunction "vcc")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 3.63 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "gnd")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 6.17 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/scl")
			(pinfunction "scl")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 8.71 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/sda")
			(pinfunction "sda")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 11.25 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U2A-xda-Pad5)")
			(pinfunction "xda")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 13.79 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(U2A-xcl-Pad6)")
			(pinfunction "xcl")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 16.33 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U2A-ado-Pad7)")
			(pinfunction "ado")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 18.87 1.59)
			(size 1.6 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(U2A-int-Pad8)")
			(pinfunction "int")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Gyroscope/MPU6050.step"
			(offset
				(xyz 3 8 -8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "keyboared:MIC_AOM-4546P-R"
		(layer "F.Cu")
		(at 192.045 85.01)
		(property "Reference" "MK1"
			(at 3.785 -5.13 0)
			(layer "F.SilkS")
		)
		(property "Value" "AOM-4546P-R"
			(at 6.985 6.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "PUI Audio"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "4.7 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/AOM-4546P-R/PUI+Audio/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/AOM-4546P-R/PUI+Audio/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "AOM-4546P-R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "10MM ECM MIC 50~16000HZ 46DB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "PUI Audio"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr through_hole)
		(pad "N" thru_hole circle
			(at -1.25 -2)
			(size 1.228 1.228)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "P" thru_hole circle
			(at 1.25 -2)
			(size 1.228 1.228)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(C5-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Microphone/CMA-4544PF-W.step"
			(offset
				(xyz 0 0 -0.5)
			)
			(scale
				(xyz 1 1 1.1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.3 77.08 90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "sens"
			(at 0.89 8.19 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0 7.41 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/mic")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/temp")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 187.03 88.62 180)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C5"
			(at -0.235443 1.237313 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf"
			(at 1.567146 -1.20664 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 180)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(C5-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 180)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "Net-(U3-+)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 171.44 88.13)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 1.43 180)
			(layer "B.SilkS")
		)
		(property "Value" "10ohm"
			(at 0 -1.43 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Panasonic"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.45 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608-2 Panasonic"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "3/1/2020"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "ERJU03J330V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0201 anti-sulfurated resistor 0603 Anti-Sulfurated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Panasonic"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 174.99 86.97 90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C1"
			(at 1.99 0.08 180)
			(layer "B.SilkS")
		)
		(property "Value" "1uf"
			(at 1.567146 -1.20664 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/mic")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "B.Cu")
		(at 180.67 87.92 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U3"
			(at 3.03 3.38 0)
			(layer "B.SilkS")
		)
		(property "Value" "LM386"
			(at 0 -3.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm386.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Low Voltage Audio Power Amplifier, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* MSSOP*P0.65mm* TSSOP*3x3mm*P0.5mm*")
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(C4-Pad2)")
			(pinfunction "GAIN")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U3-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C1-Pad1)")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "VCC")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U3-BYPASS)")
			(pinfunction "BYPASS")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(C4-Pad1)")
			(pinfunction "GAIN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 171.445 86.25 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "100ohm"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Panasonic"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.45 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608-2 Panasonic"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "3/1/2020"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "ERJU03J330V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0201 anti-sulfurated resistor 0603 Anti-Sulfurated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Panasonic"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 181.57 93.05)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C3"
			(at 0 -1.15 180)
			(layer "B.SilkS")
		)
		(property "Value" "1uf"
			(at 1.567146 -1.20664 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "Net-(U3-BYPASS)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 174.72 91.16)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C2"
			(at 0.05 -1.14 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.047uf"
			(at 1.567146 -1.20664 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 188.69 80.46 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0.12 1.36 0)
			(layer "B.SilkS")
		)
		(property "Value" "ERJU03J330V"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Panasonic"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.45 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608-2 Panasonic"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "3/1/2020"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "ERJU03J330V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0201 anti-sulfurated resistor 0603 Anti-Sulfurated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Panasonic"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/temp")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 180.77 83.9)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C4"
			(at 0.01 -1.08 180)
			(layer "B.SilkS")
		)
		(property "Value" "1uf"
			(at 1.567146 -1.20664 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "dog_pandent.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "Net-(C4-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "Net-(C4-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 167.11 96.025)
		(mid 165.307821 95.278513)
		(end 164.561334 93.476334)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 168.32 92.437116)
		(end 167.41 91.248312)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.96 93.874929)
		(end 195.285782 93.024929)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 164.56 77.56)
		(mid 165.307268 75.755934)
		(end 167.111334 75.008666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.62 96.05)
		(end 195.351334 96.028666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.11 96.025)
		(end 171.95 96)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.561334 93.476334)
		(end 164.56 77.56)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.111334 75.008701)
		(end 195.3413 75.015)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.96 76.97)
		(end 195.285782 76.12)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 197.9 93.48)
		(mid 197.153513 95.282179)
		(end 195.351334 96.028666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.96 94.78)
		(end 187.62 94.78)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.62 94.78)
		(end 187.62 96.05)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 195.341334 75.015)
		(mid 197.147992 75.763342)
		(end 197.896334 77.57)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.896334 77.57)
		(end 197.9 93.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.95 96)
		(end 171.96 94.78)
		(layer "Edge.Cuts")
	)
	(gr_text "g"
		(at 190.43 84.54 0)
		(layer "F.SilkS")
	)
	(gr_text "vcc"
		(at 168.4 79.5 0)
		(layer "F.SilkS")
	)
	(gr_text "g\n"
		(at 171.49 79.35 0)
		(layer "F.SilkS")
	)
	(gr_text "temp"
		(at 185.53 79.46 0)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 175.92 79.52 0)
		(layer "F.SilkS")
	)
	(gr_text "scl\n"
		(at 173.44 79.53 0)
		(layer "F.SilkS")
	)
	(gr_text "mic"
		(at 183.29 79.42 0)
		(layer "F.SilkS")
	)
	(gr_text "g"
		(at 189.16 79.43 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 192.37 93.09 0)
		(layer "F.SilkS")
	)
	(gr_text "chhapliyalharshit"
		(at 196.2 78.8 90)
		(layer "B.SilkS")
	)
	(zone
		(net 11)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(hatch_thickness 0.254)
			(hatch_gap 0.254)
			(hatch_orientation 0)
			(hatch_smoothing_level 1)
			(hatch_smoothing_value 1)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 163.05 72.92) (xy 162.41 98.56) (xy 201.57 96.59) (xy 200.24 74.57) (xy 162.81 74.02)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(hatch_thickness 0.254)
			(hatch_gap 0.254)
			(hatch_orientation 0)
			(hatch_smoothing_level 3)
			(hatch_smoothing_value 1)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 163.87 73.7) (xy 163.64 97.23) (xy 201.57 96.59) (xy 200.24 74.57) (xy 162.81 74.02)
			)
		)
	)
	(embedded_fonts no)
)
