(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_0000000a_a200aaaf)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../keybored_gerber/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(U2-AREF)")
	(net 3 "VCC")
	(net 4 "DTR")
	(net 5 "RESET")
	(net 6 "Net-(D1-DOUT)")
	(net 7 "L_PROG")
	(net 8 "Net-(D2-DOUT)")
	(net 9 "Net-(D3-DOUT)")
	(net 10 "unconnected-(D4-DOUT-Pad1)")
	(net 11 "unconnected-(U2-ADC7-Pad22)")
	(net 12 "LED")
	(net 13 "Net-(D5-A)")
	(net 14 "Net-(U2-XTAL2{slash}PB7)")
	(net 15 "Net-(U2-XTAL1{slash}PB6)")
	(net 16 "SEND")
	(net 17 "C10")
	(net 18 "C4")
	(net 19 "SDA")
	(net 20 "R3")
	(net 21 "C5")
	(net 22 "C8")
	(net 23 "C9")
	(net 24 "R2")
	(net 25 "C1")
	(net 26 "RX")
	(net 27 "C3")
	(net 28 "TX")
	(net 29 "C6")
	(net 30 "C7")
	(net 31 "C2")
	(net 32 "R1")
	(net 33 "SCL")
	(net 34 "R4")
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 154.46 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "C2")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 160.44 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U16"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "C4")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 171.84 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U28"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "C6")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 150.84 58.74 90)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "D1"
			(at -2.375 0.06 180)
			(layer "F.Fab")
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D1-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "L_PROG")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/User Library-WS2812-2020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 158.79 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U25"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "C3")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 177.84 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U20"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "C8")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 163.14 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U26"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "C4")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 163.16 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "C4")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx10_Slide_Copal_CHS-10B_W7.62mm_P1.27mm.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 180.2704 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U10"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "C8")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 152.93 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U33"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "C1")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 184.6204 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U11"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "C9")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 157.28 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U34"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "C2")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 164.79 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U17"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "C5")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 186.54 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U22"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "C10")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 175.9204 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "C7")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 150.11 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "C1")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 171.86 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "C6")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 177.53 58.245 90)
		(descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x04 2.54mm single row")
		(property "Reference" "I2c"
			(at 0.915 10.48 0)
			(layer "B.SilkS")
		)
		(property "Value" "Grove_i2c"
			(at 0 10.39 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Samtec"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "CONN HEADER VERT 4POS 2.54MM"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/HMTSW-104-08-T-S-255/Samtec/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/HMTSW-104-08-T-S-255/Samtec/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "HMTSW-104-08-T-S-255"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samtec"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr through_hole)
		(fp_text user "VCC"
			(at -3.74 3.22 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at -3.782235 0.57 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "SDA"
			(at -3.782235 5.72 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "SCL"
			(at -3.76 8.25 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 1.7 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "01")
			(pintype "passive")
		)
		(pad "2" smd oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "VCC")
			(pinfunction "02")
			(pintype "passive")
		)
		(pad "3" smd oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "SDA")
			(pinfunction "03")
			(pintype "passive")
		)
		(pad "4" smd oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "SCL")
			(pinfunction "04")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 173.49 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U19"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "C7")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 158.05724 58.74 90)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "D3"
			(at -2.315 0.07 180)
			(layer "F.Fab")
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(D3-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(D2-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/User Library-WS2812-2020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 154.44862 58.74 90)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "D2"
			(at -2.345 0.11 0)
			(layer "F.Fab")
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(D2-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D1-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/User Library-WS2812-2020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keychain:meshtastic 12mm"
		(layer "F.Cu")
		(at 170.41 58.52)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 176.19 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U29"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "C7")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 184.8896 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U31"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "C9")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 173.9429 89.55)
		(tags "B3U-1000P ")
		(property "Reference" "U42"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "C10")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keychain:lora logo"
		(layer "F.Cu")
		(at 174.96 58.57)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 174.3396 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U38"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "C6")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 182.19 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U21"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "C9")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 147.57 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "C1")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 188.9704 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U12"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "C10")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 182.730002 89.56)
		(tags "B3U-1000P ")
		(property "Reference" "U1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "SEND")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 156.27 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U15"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "C3")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 167.17 89.55)
		(tags "B3U-1000P ")
		(property "Reference" "U41"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "C9")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 158.81 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "C3")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 165.98 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U36"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "C4")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keychain:seeed 4mm"
		(layer "F.Cu")
		(at 165.7 58.62)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 169.9896 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U37"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "C5")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 167.49 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U27"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "C5")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 148.58 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U32"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "C10")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 169.14 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U18"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "C6")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 154.44 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U24"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "C2")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 187.08 87.05 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "sent"
			(at 0.11 2.29 0)
			(layer "F.SilkS")
		)
		(property "Value" "597-3326-607F"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Dialight"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "SMD LED 0603 INGAN GREEN | Dialight 597-3326-607F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "0603 Dialight"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/597-3326-607F/Dialight/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "597-3326-607F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/597-3326-607F/Dialight/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 180.5396 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U30"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "C8")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 161.63 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U35"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "C3")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 160.81 89.68 -90)
		(descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x05 2.54mm single row")
		(property "Reference" "prog"
			(at 0 -2.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "programmer"
			(at 0 12.93 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Samtec"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "5 Position Receptacle Connector 0.100 (2.54mm) Through Hole Gold"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/SS-105-T-2/Samtec/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "R"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/SS-105-T-2/Samtec/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "SS-105-T-2"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samtec"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "01")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "02")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "TX")
			(pinfunction "03")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "RX")
			(pinfunction "04")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "DTR")
			(pinfunction "05")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x05_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 178.6896 83.7 90)
		(tags "B3U-1000P ")
		(property "Reference" "U39"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "C7")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 150.09 77.300002 90)
		(tags "B3U-1000P ")
		(property "Reference" "U23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "R3")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "C1")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 186.07 83.52)
		(tags "B3U-1000P ")
		(property "Reference" "U40"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "R4")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "C8")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 161.66586 58.74 90)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "D4"
			(at -2.345 0 180)
			(layer "F.Fab")
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(D4-DOUT-Pad1)")
			(pinfunction "DOUT")
			(pintype "output+no_connect")
		)
		(pad "2" smd rect
			(at -0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(D3-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/User Library-WS2812-2020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 167.51 65.11 90)
		(tags "B3U-1000P ")
		(property "Reference" "U7"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "R1")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "C5")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keychain:backspace 3mm"
		(layer "F.Cu")
		(at 166.81 87.14)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "keyboared:B3U-1000P"
		(layer "F.Cu")
		(at 151.92 71.28 90)
		(tags "B3U-1000P ")
		(property "Reference" "U14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "B3U-1000P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "B3U-1000P")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "R2")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.700002 0 90)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "C2")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keychain:ce_small"
		(layer "B.Cu")
		(at 152.2 59.17 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 160.97 85.78 90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C1"
			(at -0.235443 1.237313 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf"
			(at 1.567146 -1.20664 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(U2-AREF)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keychain:repica"
		(layer "B.Cu")
		(at 182.07 63.72 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm"
		(layer "B.Cu")
		(at 181.89 78.35)
		(descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "QFP 0.8")
		(property "Reference" "U2"
			(at 0 6.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "ATmega328P-A"
			(at 0 -6.05 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-32"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*7x7mm*P0.8mm*")
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.25 2.8)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "C2")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -4.25 2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "C3")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.25 1.2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -4.25 0.4)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -4.25 -0.4)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -4.25 -1.2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -4.25 -2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "Net-(U2-XTAL1{slash}PB6)")
			(pinfunction "XTAL1/PB6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.25 -2.8)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "Net-(U2-XTAL2{slash}PB7)")
			(pinfunction "XTAL2/PB7")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -2.8 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "C4")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -2 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "C5")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -1.2 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "C6")
			(pinfunction "PD7")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -0.4 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "C7")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0.4 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "C8")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at 1.2 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "C9")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at 2 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "C10")
			(pinfunction "PB3")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 2.8 -4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "R1")
			(pinfunction "PB4")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 4.25 -2.8)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "R2")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 4.25 -2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "VCC")
			(pinfunction "AVCC")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at 4.25 -1.2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "L_PROG")
			(pinfunction "ADC6")
			(pintype "input")
		)
		(pad "20" smd rect
			(at 4.25 -0.4)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(U2-AREF)")
			(pinfunction "AREF")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 4.25 0.4)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 4.25 1.2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "unconnected-(U2-ADC7-Pad22)")
			(pinfunction "ADC7")
			(pintype "input+no_connect")
		)
		(pad "23" smd rect
			(at 4.25 2)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "R3")
			(pinfunction "PC0")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.25 2.8)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "R4")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 2.8 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "SEND")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 2 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "LED")
			(pinfunction "PC3")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 1.2 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "SDA")
			(pinfunction "PC4")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 0.4 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "SCL")
			(pinfunction "PC5")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at -0.4 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "RESET")
			(pinfunction "~{RESET}/PC6")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at -1.2 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "RX")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at -2 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "TX")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -2.8 4.25 270)
			(size 1.6 0.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "C1")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 174.1 76.07 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "1MR"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Panasonic"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.45 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608-2 Panasonic"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "3/1/2020"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "ERJU03J330V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0201 anti-sulfurated resistor 0603 Anti-Sulfurated"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Panasonic"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U2-XTAL2{slash}PB7)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U2-XTAL1{slash}PB6)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 168.49 85.39 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C3"
			(at -0.235443 1.237313 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf"
			(at 1.567146 -1.20664 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "DTR")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "RESET")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "keyboared:XTAL_ECS-160-9-33B-CKY-TR"
		(layer "B.Cu")
		(at 170.59 76.14)
		(property "Reference" "Y1"
			(at -0.527085 2.109127 0)
			(layer "B.SilkS")
		)
		(property "Value" "ECS-160-9-33B-CKY-TR"
			(at 5.577063 -2.097864 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "ECS Inc."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "16 MHz ±10ppm Crystal 9pF 60 Ohms 4-SMD, No Lead"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "ECS-33B ECS Inc."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ECS-160-9-33B-CKY-TR/ECS/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "ECS-160-9-33B-CKY-TR"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ECS-160-9-33B-CKY-TR/ECS/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.15 -0.9)
			(size 1.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "Net-(U2-XTAL2{slash}PB7)")
			(pinfunction "IN/OUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 1.15 -0.9)
			(size 1.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 1.15 0.9)
			(size 1.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "Net-(U2-XTAL1{slash}PB6)")
			(pinfunction "OUT/IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -1.15 0.9)
			(size 1.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 183.85 86.59 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "200R"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Panasonic"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.45 mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608-2 Panasonic"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "3/1/2020"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "ERJU03J330V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0201 anti-sulfurated resistor 0603 Anti-Sulfurated"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Panasonic"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "LED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0603capc:CAPC1608X90"
		(layer "B.Cu")
		(at 170.97 85.39 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C2"
			(at -0.235443 1.237313 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf"
			(at 1.567146 -1.20664 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Capacitor, Ceramic, 0603 1nF 50V X7R10% | KEMET C0603X102K5RAC3316"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "0603 KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "C0603X102K5RAC3316"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603X102K5RAC3316/KEMET/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "VCC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 174.07 83.21 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "10KR"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Panasonic"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.45 mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608-2 Panasonic"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "3/1/2020"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ERJU03J330V/Panasonic/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "ERJU03J330V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0201 anti-sulfurated resistor 0603 Anti-Sulfurated"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Panasonic"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "keyboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "RESET")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 145.87 56.385)
		(end 146.04 56.335)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.4575 90.699203)
		(end 192.45 90.86)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.21 57.365)
		(end 192.3 57.525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.53 56.235)
		(end 146.69 56.205)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.09 92.23)
		(end 191.96 92.44)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.427483 58.50542)
		(end 144.43 58.105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.75 92.13)
		(end 144.66 91.97)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.04 92.52)
		(end 144.88 92.36)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.78 93.16)
		(end 190.6 93.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.92 56.975)
		(end 192.08 57.135)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.6 93.23)
		(end 146.29 93.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.32 91.71)
		(end 192.21 92.03)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.43 91.07)
		(end 192.39 91.39)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.427483 58.50542)
		(end 144.393575 90.799203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.423575 90.959203)
		(end 144.393575 90.799203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.9875 56.199403)
		(end 190.3 56.26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.29 93.26)
		(end 190.13 93.29)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 146.924527 58.699203)
		(end 147.924527 58.699203)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.51 56.655)
		(end 191.72 56.785)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.88 92.36)
		(end 144.75 92.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.13 93.29)
		(end 189.9575 93.299203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.3 56.26)
		(end 190.67 56.355)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.96 92.44)
		(end 191.77 92.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.69 56.205)
		(end 146.923575 56.199203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.5 57.785)
		(end 144.61 57.465)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.52 91.53)
		(end 144.48 91.35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.43 58.105)
		(end 144.5 57.785)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 146.894527 90.799003)
		(end 147.894527 90.799003)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.08 57.135)
		(end 192.21 57.365)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.893575 93.299203)
		(end 146.6 93.23)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.95 93.11)
		(end 190.78 93.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.1 93.06)
		(end 190.95 93.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.6 93.2)
		(end 190.44 93.24)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.38 56.255)
		(end 146.53 56.235)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.39 57.795)
		(end 192.44 57.965)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.97 93.07)
		(end 145.65 92.96)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.44 93.24)
		(end 190.29 93.26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.6 56.475)
		(end 145.72 56.435)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.4825 58.480796)
		(end 192.4575 90.699203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.48 58.2)
		(end 192.4825 58.480796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.61 57.465)
		(end 144.73 57.265)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.05 56.855)
		(end 145.21 56.695)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.34 57.645)
		(end 192.39 57.795)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.72 56.435)
		(end 145.87 56.385)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.48 91.35)
		(end 144.44 91.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.73 57.265)
		(end 144.86 57.055)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 189.9875 58.699203)
		(end 190.9875 58.699203)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.86 57.055)
		(end 145.05 56.855)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.44 56.565)
		(end 145.6 56.475)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.62 91.85)
		(end 144.57 91.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.39 91.39)
		(end 192.32 91.71)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.21 56.695)
		(end 145.44 56.565)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.65 92.96)
		(end 145.45 92.84)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.923575 56.199203)
		(end 189.9875 56.199403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.22 93.02)
		(end 191.1 93.06)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 189.9575 90.799403)
		(end 190.9575 90.799403)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.61 92.8)
		(end 191.38 92.93)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.44 57.965)
		(end 192.48 58.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.99 56.425)
		(end 191.31 56.535)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.57 91.7)
		(end 144.52 91.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.66 91.97)
		(end 144.62 91.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.72 56.785)
		(end 191.92 56.975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.9575 93.299203)
		(end 146.893575 93.299203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.67 56.355)
		(end 190.99 56.425)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.45 90.86)
		(end 192.43 91.07)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.24 92.71)
		(end 145.04 92.52)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.04 56.335)
		(end 146.22 56.295)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.77 92.64)
		(end 191.61 92.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.31 56.535)
		(end 191.51 56.655)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.45 92.84)
		(end 145.24 92.71)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.21 92.03)
		(end 192.09 92.23)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.38 92.93)
		(end 191.22 93.02)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.44 91.19)
		(end 144.423575 90.959203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.22 56.295)
		(end 146.38 56.255)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.3 57.525)
		(end 192.34 57.645)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.29 93.15)
		(end 145.97 93.07)
		(layer "Edge.Cuts")
	)
	(gr_text "I"
		(at 177.33 69.06 0)
		(layer "F.SilkS")
	)
	(gr_text "#"
		(at 159.18 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "V"
		(at 165.49 81.47 0)
		(layer "F.SilkS")
	)
	(gr_text "VCC"
		(at 157.05 88.33 0)
		(layer "F.SilkS")
	)
	(gr_text "F"
		(at 162.84 75.07 0)
		(layer "F.SilkS")
	)
	(gr_text "Z"
		(at 152.43 81.46 0)
		(layer "F.SilkS")
	)
	(gr_text "1 "
		(at 149.63 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 175.327584 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "$"
		(at 163.54 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "W"
		(at 151.54 69.06 0)
		(layer "F.SilkS")
	)
	(gr_text ")"
		(at 189.35 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 152.26 88.33 0)
		(layer "F.SilkS")
	)
	(gr_text "%"
		(at 167.84 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "Y"
		(at 168.67 69.05 0)
		(layer "F.SilkS")
	)
	(gr_text "G"
		(at 166.93 75.08 0)
		(layer "F.SilkS")
	)
	(gr_text "Q"
		(at 147.01 68.66 0)
		(layer "F.SilkS")
	)
	(gr_text "&"
		(at 176.16 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "D"
		(at 158.37 75.04 0)
		(layer "F.SilkS")
	)
	(gr_text "M"
		(at 178.22 81.48 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 166.893794 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "C"
		(at 161.05 81.47 0)
		(layer "F.SilkS")
	)
	(gr_text "SEND\n"
		(at 180.72 88.09 0)
		(layer "F.SilkS")
	)
	(gr_text "("
		(at 184.76 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "0"
		(at 188.360926 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "A"
		(at 149.63 75.09 0)
		(layer "F.SilkS")
	)
	(gr_text "S"
		(at 153.95 75.07 0)
		(layer "F.SilkS")
	)
	(gr_text "T"
		(at 164.23 69.05 0)
		(layer "F.SilkS")
	)
	(gr_text "shift"
		(at 147.49 81.36 0)
		(layer "F.SilkS")
	)
	(gr_text "G"
		(at 160.48 88.36 0)
		(layer "F.SilkS")
	)
	(gr_text "N"
		(at 173.84 81.48 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 179.597443 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 162.505196 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 171.33725 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "^"
		(at 172.25 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "K"
		(at 180.03 75.09 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 158.198883 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "B"
		(at 169.48 81.44 0)
		(layer "F.SilkS")
	)
	(gr_text "L"
		(at 184.45 75.07 0)
		(layer "F.SilkS")
	)
	(gr_text "U"
		(at 172.98 69.05 0)
		(layer "F.SilkS")
	)
	(gr_text "H"
		(at 171.33 75.1 0)
		(layer "F.SilkS")
	)
	(gr_text "@"
		(at 154.78 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 183.794041 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 154.93 88.35 0)
		(layer "F.SilkS")
	)
	(gr_text "!"
		(at 150.44 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "R"
		(at 159.95 69.05 0)
		(layer "F.SilkS")
	)
	(gr_text "*"
		(at 180.49 62.61 0)
		(layer "F.SilkS")
	)
	(gr_text "O"
		(at 181.76 69.03 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 153.92 62.838646 0)
		(layer "F.SilkS")
	)
	(gr_text "X"
		(at 156.78 81.45 0)
		(layer "F.SilkS")
	)
	(gr_text "J"
		(at 175.7 75.05 0)
		(layer "F.SilkS")
	)
	(gr_text "E"
		(at 155.87 69.05 0)
		(layer "F.SilkS")
	)
	(gr_text "OK"
		(at 185.1 82.13 0)
		(layer "F.SilkS")
	)
	(gr_text "P"
		(at 186.31 69.04 0)
		(layer "F.SilkS")
	)
	(gr_text "DTR"
		(at 149.32 88.35 0)
		(layer "F.SilkS")
	)
	(gr_text "G"
		(at 161.41 88.37 0)
		(layer "B.SilkS")
	)
	(gr_text "TX"
		(at 156.35 88.37 0)
		(layer "B.SilkS")
	)
	(gr_text "DTR"
		(at 151.31 88.33 0)
		(layer "B.SilkS")
	)
	(gr_text "www.hackster.io/iwantmyspace2002"
		(at 146.79 88.17 270)
		(layer "B.SilkS")
	)
	(gr_text "RX"
		(at 153.95 88.33 0)
		(layer "B.SilkS")
	)
	(gr_text "grove compatibe"
		(at 163.32 57.96 0)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 159.41 88.33 0)
		(layer "B.SilkS")
	)
	(zone
		(net 3)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 10)
			(hatch_thickness 0.25)
			(hatch_gap 0.25)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 139.48 51.91) (xy 142.71 97.67) (xy 206.14 95.83) (xy 197.84 46.68) (xy 133.19 55.28) (xy 140.21 54.34)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 10)
			(hatch_thickness 0.25)
			(hatch_gap 0.25)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 144.73 86.18) (xy 144.8 59.83) (xy 144.81 58.39) (xy 144.95 57.71) (xy 145.22 57.21) (xy 145.6 56.87)
				(xy 145.94 56.68) (xy 146.29 56.59) (xy 146.76 56.52) (xy 146.93 56.5) (xy 190.23 56.54) (xy 190.86 56.67)
				(xy 191.35 56.85) (xy 191.6 57.08) (xy 191.85 57.36) (xy 192.02 57.75) (xy 192.12 58.13) (xy 192.16 58.51)
				(xy 192.14 58.86) (xy 192.15 77.84) (xy 192.19 80.03) (xy 175.84 80.03) (xy 166.08 80.06) (xy 166.11 68.67)
				(xy 166.09 62.74) (xy 144.4 62.75) (xy 144.79 62.75)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 10)
			(hatch_thickness 0.25)
			(hatch_gap 0.25)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 144.73 86.17) (xy 144.74 91.29) (xy 144.98 91.97) (xy 145.43 92.48) (xy 146.05 92.79) (xy 146.67 92.95)
				(xy 147.8 92.97) (xy 189.87 92.85) (xy 191.02 92.66) (xy 191.71 92.13) (xy 192.04 91.29) (xy 192.08 90.34)
				(xy 192.05 83.37) (xy 188.23 83.41) (xy 188.23 86.35) (xy 144.93 86.29) (xy 144.73 86.29)
			)
		)
	)
	(embedded_fonts no)
)
