(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADPD4200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 4.826 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ADPD4200_0_1")
		(symbol "ADPD4200_1_1"
			(pin output line
				(at -11.43 -2.54 0)
				(length 2.54)
				(name "LED1A")
				(number "A4")
			)
			(pin output line
				(at -11.43 -3.81 0)
				(length 2.54)
				(name "LED2A")
				(number "A3")
			)
			(pin output line
				(at -11.43 -5.08 0)
				(length 2.54)
				(name "LED3A")
				(number "B3")
			)
			(pin power_out line
				(at -11.43 -6.35 0)
				(length 2.54)
				(name "LED4A")
				(number "A2")
			)
			(pin input line
				(at -11.43 -10.16 0)
				(length 2.54)
				(name "IN1")
				(number "F4")
			)
			(pin input line
				(at -11.43 -11.43 0)
				(length 2.54)
				(name "IN2")
				(number "F3")
			)
			(pin input line
				(at -11.43 -12.7 0)
				(length 2.54)
				(name "IN7")
				(number "F2")
			)
			(pin input line
				(at -11.43 -13.97 0)
				(length 2.54)
				(name "IN8")
				(number "F1")
			)
			(pin power_out line
				(at -2.54 -19.05 90)
				(length 2.54)
				(name "LGND")
				(number "B4")
			)
			(pin power_in line
				(at -1.27 1.27 270)
				(length 2.54)
				(name "AVDD")
				(number "C4")
			)
			(pin power_in line
				(at -1.27 -19.05 90)
				(length 2.54)
				(name "AGND")
				(number "D3")
			)
			(pin power_in line
				(at 0 1.27 270)
				(length 2.54)
				(name "DVDD1")
				(number "D2")
			)
			(pin power_in line
				(at 1.27 1.27 270)
				(length 2.54)
				(name "IOVDD")
				(number "D1")
			)
			(pin power_in line
				(at 1.27 -19.05 90)
				(length 2.54)
				(name "DGND")
				(number "E2")
			)
			(pin power_out line
				(at 2.54 -19.05 90)
				(length 2.54)
				(name "IOGND")
				(number "E1")
			)
			(pin power_out line
				(at 3.81 1.27 270)
				(length 2.54)
				(name "VC1")
				(number "E4")
			)
			(pin power_out line
				(at 5.08 1.27 270)
				(length 2.54)
				(name "VC2")
				(number "E3")
			)
			(pin passive line
				(at 6.35 1.27 270)
				(length 2.54)
				(name "Vref")
				(number "D4")
			)
			(pin bidirectional line
				(at 11.43 -6.35 180)
				(length 2.54)
				(name "CS")
				(number "C2")
			)
			(pin bidirectional line
				(at 11.43 -7.62 180)
				(length 2.54)
				(name "SCLK")
				(number "C3")
			)
			(pin bidirectional line
				(at 11.43 -8.89 180)
				(length 2.54)
				(name "MOSI")
				(number "C1")
			)
			(pin output line
				(at 11.43 -10.16 180)
				(length 2.54)
				(name "MISO")
				(number "B1")
			)
			(pin bidirectional line
				(at 11.43 -12.7 180)
				(length 2.54)
				(name "GPIO0")
				(number "A1")
			)
			(pin bidirectional line
				(at 11.43 -13.97 180)
				(length 2.54)
				(name "GPIO1")
				(number "B2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADPD4200BCBZR7"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 22.86 10.16 0)
		)
		(property "Value" "ADPD4200BCBZR7"
			(at 22.86 7.62 0)
		)
		(property "Footprint" "ADPD4200BCBZR7_ADI"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adpd4200.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "ADPD4200BCBZR7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ADPD4200BCBZR7_ADI ADPD4200BCBZR7_ADI-M ADPD4200BCBZR7_ADI-L"
			(at 0 0 0)
		)
		(symbol "ADPD4200BCBZR7_0_1"
			(pin bidirectional line
				(at 0 0 0)
				(length 7.62)
				(name "GPIO0")
				(number "A1")
			)
			(pin unspecified line
				(at 0 -2.54 0)
				(length 7.62)
				(name "LED4A")
				(number "A2")
			)
			(pin unspecified line
				(at 0 -5.08 0)
				(length 7.62)
				(name "LED2A")
				(number "A3")
			)
			(pin unspecified line
				(at 0 -7.62 0)
				(length 7.62)
				(name "LED1A")
				(number "A4")
			)
			(pin bidirectional line
				(at 0 -10.16 0)
				(length 7.62)
				(name "MISO")
				(number "B1")
			)
			(pin bidirectional line
				(at 0 -12.7 0)
				(length 7.62)
				(name "GPIO1")
				(number "B2")
			)
			(pin unspecified line
				(at 0 -15.24 0)
				(length 7.62)
				(name "LED3A")
				(number "B3")
			)
			(pin power_out line
				(at 0 -17.78 0)
				(length 7.62)
				(name "LGND")
				(number "B4")
			)
			(pin bidirectional line
				(at 0 -20.32 0)
				(length 7.62)
				(name "MOSI")
				(number "C1")
			)
			(pin input line
				(at 0 -22.86 0)
				(length 7.62)
				(name "*CS")
				(number "C2")
			)
			(pin input line
				(at 0 -25.4 0)
				(length 7.62)
				(name "SCLK")
				(number "C3")
			)
			(pin power_in line
				(at 0 -27.94 0)
				(length 7.62)
				(name "AVDD")
				(number "C4")
			)
			(pin input line
				(at 45.72 0 180)
				(length 7.62)
				(name "IN1")
				(number "F4")
			)
			(pin input line
				(at 45.72 -2.54 180)
				(length 7.62)
				(name "IN2")
				(number "F3")
			)
			(pin input line
				(at 45.72 -5.08 180)
				(length 7.62)
				(name "IN7")
				(number "F2")
			)
			(pin input line
				(at 45.72 -7.62 180)
				(length 7.62)
				(name "IN8")
				(number "F1")
			)
			(pin output line
				(at 45.72 -10.16 180)
				(length 7.62)
				(name "VC1")
				(number "E4")
			)
			(pin output line
				(at 45.72 -12.7 180)
				(length 7.62)
				(name "VC2")
				(number "E3")
			)
			(pin power_out line
				(at 45.72 -15.24 180)
				(length 7.62)
				(name "DGND")
				(number "E2")
			)
			(pin power_out line
				(at 45.72 -17.78 180)
				(length 7.62)
				(name "IOGND")
				(number "E1")
			)
			(pin unspecified line
				(at 45.72 -20.32 180)
				(length 7.62)
				(name "VREF")
				(number "D4")
			)
			(pin power_out line
				(at 45.72 -22.86 180)
				(length 7.62)
				(name "AGND")
				(number "D3")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 7.62)
				(name "DVDD1")
				(number "D2")
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 7.62)
				(name "IOVDD")
				(number "D1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FM9908A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 -1.524 0)
		)
		(property "Value" "FM9908A"
			(at 7.366 -1.27 0)
		)
		(property "Footprint" "Package_SO:JEITA_SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "FM9908A_0_1")
		(symbol "FM9908A_1_1"
			(pin power_in line
				(at -12.7 -3.81 0)
				(length 2.54)
				(name "Vcc")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -6.35 0)
				(length 2.54)
				(name "Icharge_Prog")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "WLED")
				(number "6")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin output line
				(at -7.62 -29.21 90)
				(length 2.54)
				(name "LED0")
				(number "9")
			)
			(pin output line
				(at -5.08 -29.21 90)
				(length 2.54)
				(name "LED1")
				(number "8")
			)
			(pin output line
				(at -2.54 -29.21 90)
				(length 2.54)
				(name "LED2")
				(number "11")
			)
			(pin output line
				(at 0 -29.21 90)
				(length 2.54)
				(name "LED3")
				(number "12")
			)
			(pin output line
				(at 7.62 -29.21 90)
				(length 2.54)
				(name "PGND")
				(number "14")
			)
			(pin output line
				(at 10.16 -29.21 90)
				(length 2.54)
				(name "PGND")
				(number "13")
			)
			(pin output line
				(at 12.7 -29.21 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_out line
				(at 16.51 -3.81 180)
				(length 2.54)
				(name "Vout")
				(number "1")
			)
			(pin power_out line
				(at 16.51 -6.35 180)
				(length 2.54)
				(name "Vout")
				(number "2")
			)
			(pin power_out line
				(at 16.51 -8.89 180)
				(length 2.54)
				(name "SW")
				(number "15")
			)
			(pin power_out line
				(at 16.51 -11.43 180)
				(length 2.54)
				(name "SW")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LXZ1-PM01"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 12.7 8.89 0)
		)
		(property "Value" "LXZ1-PM01"
			(at 12.7 6.35 0)
		)
		(property "Footprint" "LXZ1PH02"
			(at 12.7 -93.65 0)
		)
		(property "Datasheet" "https://www.futureelectronics.com/p/semiconductors--lighting-solutions--led-emitters--high-power-led-emitters-rev/lxz1-pm01-lumileds-9022561"
			(at 12.7 -193.65 0)
		)
		(property "Description" "LUXEON Z High Power SMT LED Emitter Green Lambertian 500 mA 2.85 V"
			(at 0 0 0)
		)
		(property "Height" "0.96"
			(at 12.7 -393.65 0)
		)
		(property "Manufacturer_Name" "Lumileds"
			(at 12.7 -493.65 0)
		)
		(property "Manufacturer_Part_Number" "LXZ1-PM01"
			(at 12.7 -593.65 0)
		)
		(property "Mouser Part Number" "997-LXZ1PM01"
			(at 12.7 -693.65 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Lumileds/LXZ1-PM01?qs=7Vwje68bFtOUicMtSTN0uA%3D%3D"
			(at 12.7 -793.65 0)
		)
		(property "Arrow Part Number" "LXZ1-PM01"
			(at 12.7 -893.65 0)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/lxz1-pm01/lumileds?region=europe"
			(at 12.7 -993.65 0)
		)
		(symbol "LXZ1-PM01_1_1"
			(pin passive line
				(at 0 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MM8130-2600"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 36.83 15.24 0)
		)
		(property "Value" "MM8130-2600"
			(at 36.83 12.7 0)
		)
		(property "Footprint" "MM81302600"
			(at 36.83 -87.3 0)
		)
		(property "Datasheet" "https://www.murata.com/-/media/webrenewal/support/library/catalog/products/connector/o30e.ashx?la=en&cvid=20230202042145000000"
			(at 36.83 -187.3 0)
		)
		(property "Description" "SWF Connector Receptacle, Female Socket 50 Ohms Surface Mount Solder"
			(at 0 0 0)
		)
		(property "Height" "1.5"
			(at 36.83 -387.3 0)
		)
		(property "Manufacturer_Name" "Murata Electronics"
			(at 36.83 -487.3 0)
		)
		(property "Manufacturer_Part_Number" "MM8130-2600"
			(at 36.83 -587.3 0)
		)
		(property "Mouser Part Number" "N/A"
			(at 36.83 -687.3 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/MM8130-2600?qs=qEIx2DuoqD9f2sRdYSdpFA%3D%3D"
			(at 36.83 -787.3 0)
		)
		(property "Arrow Part Number" ""
			(at 36.83 -887.3 0)
		)
		(property "Arrow Price/Stock" ""
			(at 36.83 -987.3 0)
		)
		(symbol "MM8130-2600_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "GROUND_1")
				(number "3")
			)
			(pin passive line
				(at 0 -2.54 0)
				(length 5.08)
				(name "GROUND_2")
				(number "4")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(name "OUT")
				(number "2")
			)
			(pin passive line
				(at 20.32 -15.24 90)
				(length 5.08)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 40.64 0 180)
				(length 5.08)
				(name "GROUND_4")
				(number "6")
			)
			(pin passive line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "GROUND_3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC9119D10AMR-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 24.13 7.62 0)
		)
		(property "Value" "XC9119D10AMR-G"
			(at 24.13 5.08 0)
		)
		(property "Footprint" "SOT95P280X130-5N"
			(at 24.13 -94.92 0)
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc9119/XC9119.pdf"
			(at 24.13 -194.92 0)
		)
		(property "Description" "Switching Voltage Regulators 1MHz PWM StepUp DCDC Converter"
			(at 0 0 0)
		)
		(property "Height" "1.3"
			(at 24.13 -394.92 0)
		)
		(property "Manufacturer_Name" "Torex"
			(at 24.13 -494.92 0)
		)
		(property "Manufacturer_Part_Number" "XC9119D10AMR-G"
			(at 24.13 -594.92 0)
		)
		(property "Mouser Part Number" "865-XC9119D10AMR-G"
			(at 24.13 -694.92 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Torex-Semiconductor/XC9119D10AMR-G?qs=AsjdqWjXhJ9lLOEDfbv9Sw%3D%3D"
			(at 24.13 -794.92 0)
		)
		(property "Arrow Part Number" ""
			(at 24.13 -894.92 0)
		)
		(property "Arrow Price/Stock" ""
			(at 24.13 -994.92 0)
		)
		(symbol "XC9119D10AMR-G_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "LX")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 0)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 0)
				(length 5.08)
				(name "FB")
				(number "3")
			)
			(pin passive line
				(at 27.94 0 180)
				(length 5.08)
				(name "CE/SS")
				(number "4")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "mt3608L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 21.59 7.62 0)
		)
		(property "Value" "mt3608L"
			(at 21.59 5.08 0)
		)
		(property "Footprint" "SOT95P280X145-6N"
			(at 21.59 -94.92 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2201121530_XI-AN-Aerosemi-Tech-MT3608L_C2932326.pdf"
			(at 21.59 -194.92 0)
		)
		(property "Description" "gfgb"
			(at 0 0 0)
		)
		(property "Height" "1.45"
			(at 21.59 -394.92 0)
		)
		(property "Manufacturer_Name" "Aerosemi"
			(at 21.59 -494.92 0)
		)
		(property "Manufacturer_Part_Number" "mt3608L"
			(at 21.59 -594.92 0)
		)
		(property "Mouser Part Number" ""
			(at 21.59 -694.92 0)
		)
		(property "Mouser Price/Stock" ""
			(at 21.59 -794.92 0)
		)
		(property "Arrow Part Number" ""
			(at 21.59 -894.92 0)
		)
		(property "Arrow Price/Stock" ""
			(at 21.59 -994.92 0)
		)
		(symbol "mt3608L_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "SW")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 0)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 0)
				(length 5.08)
				(name "FB")
				(number "3")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 5.08)
				(name "OC")
				(number "6")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VIN")
				(number "5")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "EN")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
)
