(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(U1-VBUS-Pad14)")
	(net 2 "unconnected-(U1-GPIO8{slash}D9{slash}A9{slash}MISO-Pad10)")
	(net 3 "/VBAT_IN")
	(net 4 "/D3")
	(net 5 "unconnected-(U1-GPIO7{slash}D8{slash}A8{slash}SCK-Pad9)")
	(net 6 "GND")
	(net 7 "Net-(D1-A)")
	(net 8 "/3V3_REGOUT")
	(net 9 "/3V3")
	(net 10 "/D1")
	(net 11 "unconnected-(U1-GPIO1{slash}D0{slash}A0-Pad1)")
	(net 12 "unconnected-(U1-GPIO9{slash}D10{slash}A10{slash}MOSI-Pad11)")
	(net 13 "/I2C_SCL")
	(net 14 "/I2C_SDA")
	(net 15 "unconnected-(U1-U0RXD{slash}D7{slash}RX-Pad8)")
	(net 16 "unconnected-(U2-NC-Pad4)")
	(net 17 "/D2")
	(net 18 "unconnected-(U1-U0TXD{slash}D6{slash}TX-Pad7)")
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 132.08 96.52)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H3"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 172.72 96.52)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H4"
			(at -5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 163.83 58.42 180)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 1.27 -2.96 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/D2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 153.67 74.93 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.54 180)
			(layer "F.SilkS")
		)
		(property "Value" "JP_EXT3V3_EN"
			(at 0 4.92 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/3V3_REGOUT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 170.18 70.4088)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H5"
			(at -5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering"
		(layer "F.Cu")
		(at 152.4 69.85 -90)
		(descr "5-pin SOT23 package")
		(tags "SOT-23-5 hand-soldering")
		(property "Reference" "U2"
			(at 0 -2.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "AP2112K-3.3"
			(at 0 2.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?5*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.35 -0.95 270)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/VBAT_IN")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.35 0 270)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.35 0.95 270)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/VBAT_IN")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.35 0.95 270)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "unconnected-(U2-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 1.35 -0.95 270)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/3V3_REGOUT")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 132.08 63.5 -90)
		(descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "J4"
			(at 3.75 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 3.75 4.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 2.7 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 6 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/I2C_SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.5 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/I2C_SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 167.64 64.77 90)
		(descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x03 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.77 180)
			(layer "F.SilkS")
		)
		(property "Value" "J_SW420"
			(at 0 7.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/D1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 11.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -180 -0)
			)
		)
		(model "/Users/samuel/Documents/KiCad/SW-420 v2.step"
			(offset
				(xyz -14.4 -2.5 12)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Buzzer_Beeper:Buzzer_12x9.5RM7.6"
		(layer "F.Cu")
		(at 156.2 58.42 180)
		(descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
		(tags "buzzer")
		(property "Reference" "BZ1"
			(at 11.42 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Buzzer"
			(at 3.8 7.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buzzer, polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Buzzer*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at -0.01 -2.54 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 3.8 -4 0)
			(layer "F.Fab")
		)
		(fp_text user "+"
			(at -0.01 -2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/D3")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.6 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 132.08 55.88)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H1"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Seeed Studio XIAO Series Library:XIAO-ESP32S3-DIP"
		(layer "F.Cu")
		(at 152.4 88.9 180)
		(property "Reference" "U1"
			(at -6.35 11.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "XIAO-ESP32-S3-DIP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -8.455 -7.62)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 11 "unconnected-(U1-GPIO1{slash}D0{slash}A0-Pad1)")
			(pinfunction "GPIO1/D0/A0")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" thru_hole circle
			(at -7.62 -7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(U1-GPIO1{slash}D0{slash}A0-Pad1)")
			(pinfunction "GPIO1/D0/A0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -8.455 -5.08)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 10 "/D1")
			(pinfunction "GPIO2/DA/A1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole circle
			(at -7.62 -5.08)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/D1")
			(pinfunction "GPIO2/DA/A1")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -8.455 -2.54)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 17 "/D2")
			(pinfunction "GPIO3/D2/A2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole circle
			(at -7.62 -2.54)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/D2")
			(pinfunction "GPIO3/D2/A2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -8.455 0)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 4 "/D3")
			(pinfunction "GPIO4/D3/A3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole circle
			(at -7.62 0)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/D3")
			(pinfunction "GPIO4/D3/A3")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -8.455 2.54)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 14 "/I2C_SDA")
			(pinfunction "GPIO5/D4/I2C_SDA")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole circle
			(at -7.62 2.54)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/I2C_SDA")
			(pinfunction "GPIO5/D4/I2C_SDA")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -8.455 5.08)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 13 "/I2C_SCL")
			(pinfunction "GPIO9/D5/I2C_SCL")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" thru_hole circle
			(at -7.62 5.08)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/I2C_SCL")
			(pinfunction "GPIO9/D5/I2C_SCL")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -8.455 7.62)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 18 "unconnected-(U1-U0TXD{slash}D6{slash}TX-Pad7)")
			(pinfunction "U0TXD/D6/TX")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" thru_hole circle
			(at -7.62 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(U1-U0TXD{slash}D6{slash}TX-Pad7)")
			(pinfunction "U0TXD/D6/TX")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 7.62 7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U1-U0RXD{slash}D7{slash}RX-Pad8)")
			(pinfunction "U0RXD/D7/RX")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 8.455 7.62 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 15 "unconnected-(U1-U0RXD{slash}D7{slash}RX-Pad8)")
			(pinfunction "U0RXD/D7/RX")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "9" thru_hole circle
			(at 7.62 5.08 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(U1-GPIO7{slash}D8{slash}A8{slash}SCK-Pad9)")
			(pinfunction "GPIO7/D8/A8/SCK")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 8.455 5.08 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 5 "unconnected-(U1-GPIO7{slash}D8{slash}A8{slash}SCK-Pad9)")
			(pinfunction "GPIO7/D8/A8/SCK")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "10" thru_hole circle
			(at 7.62 2.54 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(U1-GPIO8{slash}D9{slash}A9{slash}MISO-Pad10)")
			(pinfunction "GPIO8/D9/A9/MISO")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 8.455 2.54 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 2 "unconnected-(U1-GPIO8{slash}D9{slash}A9{slash}MISO-Pad10)")
			(pinfunction "GPIO8/D9/A9/MISO")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "11" thru_hole circle
			(at 7.62 0 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(U1-GPIO9{slash}D10{slash}A10{slash}MOSI-Pad11)")
			(pinfunction "GPIO9/D10/A10/MOSI")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 8.455 0 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 12 "unconnected-(U1-GPIO9{slash}D10{slash}A10{slash}MOSI-Pad11)")
			(pinfunction "GPIO9/D10/A10/MOSI")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "12" thru_hole circle
			(at 7.62 -2.54 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/3V3")
			(pinfunction "VCC_3V3")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 8.455 -2.54 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 9 "/3V3")
			(pinfunction "VCC_3V3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "13" thru_hole circle
			(at 7.62 -5.08 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 8.455 -5.08 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "14" thru_hole circle
			(at 7.62 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(U1-VBUS-Pad14)")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 8.455 -7.62 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 1 "unconnected-(U1-VBUS-Pad14)")
			(pinfunction "VBUS")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "/Users/samuel/Documents/KiCad/Seeed Studio XIAO-ESP32-S3-Sense.step"
			(offset
				(xyz 6.1 -1.7 12)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.step"
			(offset
				(xyz -7.65 7.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.step"
			(offset
				(xyz 7.65 7.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.step"
			(offset
				(xyz 7.65 7.6 11.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -180 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.step"
			(offset
				(xyz -7.65 7.6 11.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -180 -0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 133.35 82.55 -90)
		(descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J1"
			(at 2.54 -6.32 180)
			(layer "F.SilkS")
		)
		(property "Value" "CN3791"
			(at -3.81 1.27 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 3 "/VBAT_IN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Radial_D5.0mm_H5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 142.78 66.04)
		(descr "C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=5mm, Non-Polar Electrolytic Capacitor")
		(tags "C Radial series Radial pin pitch 2.00mm diameter 5mm height 5mm Non-Polar Electrolytic Capacitor")
		(property "Reference" "C1"
			(at -3.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "CIN"
			(at 1 3.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VBAT_IN")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D5.0mm_H5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Radial_D5.0mm_H5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 142.78 73.66)
		(descr "C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=5mm, Non-Polar Electrolytic Capacitor")
		(tags "C Radial series Radial pin pitch 2.00mm diameter 5mm height 5mm Non-Polar Electrolytic Capacitor")
		(property "Reference" "C2"
			(at -3.08 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "COUT"
			(at 1 3.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/3V3_REGOUT")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D5.0mm_H5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 161.29 74.93 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at 3.81 -1.92 180)
			(layer "F.SilkS")
		)
		(property "Value" "R_US"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 172.72 55.88)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H2"
			(at -5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "ForestWatcher.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 172.72 101.6)
		(end 132.08 101.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.08 50.8)
		(end 172.72 50.8)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127 55.88)
		(mid 128.487898 52.287898)
		(end 132.08 50.8)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.8 96.52)
		(mid 176.312102 100.112102)
		(end 172.72 101.6)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 132.08 101.6)
		(mid 128.487898 100.112102)
		(end 127 96.52)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.72 50.8)
		(mid 176.312102 52.287898)
		(end 177.8 55.88)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 96.52)
		(end 127 55.88)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 55.88)
		(end 177.8 96.52)
		(layer "Edge.Cuts")
	)
	(gr_text "SAMUEL ALEXANDER - 2025"
		(at 176.784 92.075 90)
		(layer "F.SilkS")
	)
	(gr_text "with Edge AI Foundation \nand NextPCB"
		(at 174.752 74.295 90)
		(layer "B.SilkS")
	)
	(gr_text "Edge AI Earth Guardians"
		(at 171.45 74.295 90)
		(layer "B.SilkS" knockout)
	)
	(zone
		(net 9)
		(net_name "/3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127 50.8) (xy 177.8 50.8) (xy 177.8 101.6) (xy 127 101.6)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VBAT_IN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127 84.455) (xy 139.065 84.455) (xy 139.065 69.85) (xy 154.94 69.85) (xy 154.94 63.5) (xy 135.255 63.5)
				(xy 135.255 79.375) (xy 127 79.375)
			)
		)
	)
	(zone
		(net 6)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127 50.8) (xy 177.8 50.8) (xy 177.8 101.6) (xy 127 101.6)
			)
		)
	)
	(embedded_fonts no)
)
