(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "C:/Users/mfada/Documents/KiKad/")
		)
	)
	(net 0 "")
	(net 1 "Net-(J3-GP26)")
	(net 2 "Net-(J3-GP16)")
	(net 3 "Net-(J3-GP24)")
	(net 4 "Net-(J3-GP0)")
	(net 5 "Net-(J3-GP7)")
	(net 6 "Net-(J3-GP29)")
	(net 7 "Net-(J3-GP33)")
	(net 8 "Net-(J3-GP30)")
	(net 9 "Net-(J3-GP13)")
	(net 10 "Net-(J3-GP22)")
	(net 11 "Net-(J3-GP25)")
	(net 12 "Net-(J3-GP18)")
	(net 13 "Net-(J3-GP3)")
	(net 14 "Net-(J3-GP17)")
	(net 15 "Net-(J3-GP28)")
	(net 16 "Net-(J3-GP6)")
	(net 17 "Net-(J3-GP31)")
	(net 18 "Net-(J3-GP2)")
	(net 19 "Net-(J3-GP21)")
	(net 20 "Net-(J3-GP19)")
	(net 21 "Net-(J3-GP1)")
	(net 22 "Net-(J3-GP5)")
	(net 23 "Net-(J3-GP20)")
	(net 24 "Net-(J3-GP11)")
	(net 25 "Net-(J3-GP32)")
	(net 26 "Net-(J3-GP14)")
	(net 27 "Net-(J3-GP12)")
	(net 28 "Net-(J3-GP8)")
	(net 29 "Net-(J3-GP27)")
	(net 30 "Net-(J3-GP23)")
	(net 31 "Net-(J3-GP4)")
	(net 32 "Net-(J3-GP10)")
	(net 33 "Net-(J3-GP9)")
	(net 34 "Net-(J3-GP15)")
	(net 35 "unconnected-(J2-CC2-Pad6)")
	(net 36 "unconnected-(J2-CC1-Pad3)")
	(net 37 "Net-(J2-VBUS)")
	(net 38 "Net-(J2-D+)")
	(net 39 "Net-(J2-D-)")
	(net 40 "Net-(J2-GND)")
	(net 41 "unconnected-(J3-LDO_EN-Pad50)")
	(net 42 "unconnected-(J3-GP34-Pad35)")
	(net 43 "unconnected-(J3-GP42-Pad43)")
	(net 44 "unconnected-(J3-GP46-Pad47)")
	(net 45 "unconnected-(J3-VBAT-Pad52)")
	(net 46 "unconnected-(J3-GP43-Pad44)")
	(net 47 "unconnected-(J3-GP38-Pad39)")
	(net 48 "unconnected-(J3-3P3V-Pad54)")
	(net 49 "unconnected-(J3-GP47-Pad48)")
	(net 50 "unconnected-(J3-GP36-Pad37)")
	(net 51 "unconnected-(J3-GP35-Pad36)")
	(net 52 "unconnected-(J3-GP41-Pad42)")
	(net 53 "unconnected-(J3-GP40-Pad41)")
	(net 54 "unconnected-(J3-GP45-Pad46)")
	(net 55 "unconnected-(J3-SWCLK-Pad58)")
	(net 56 "unconnected-(J3-GP37-Pad38)")
	(net 57 "unconnected-(J3-SWDIO-Pad57)")
	(net 58 "unconnected-(J3-BATSTAT-Pad49)")
	(net 59 "unconnected-(J3-GP39-Pad40)")
	(net 60 "unconnected-(J3-GP44-Pad45)")
	(net 61 "unconnected-(J3-RESET-Pad59)")
	(net 62 "unconnected-(J3-BOOTSEL-Pad60)")
	(footprint "34pinLibrary:34 pin header"
		(layer "F.Cu")
		(at 168.73 82.68)
		(property "Reference" "J1"
			(at -5.0068 -3.18 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FPC Breakout"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "2350B_Keybd_Cntrl.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -5.03 -3.18 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J3-GP33)")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J3-GP32)")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at 2.54 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J3-GP31)")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at 0 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J3-GP30)")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 2.54 5.08)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J3-GP29)")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 0 5.08)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J3-GP28)")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 2.54 7.62)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J3-GP27)")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 0 7.62)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J3-GP26)")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 2.54 10.16)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-GP25)")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 0 10.16)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J3-GP24)")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 2.54 12.7)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J3-GP23)")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 0 12.7)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-GP22)")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole circle
			(at 2.54 15.24)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J3-GP21)")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at 0 15.24)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J3-GP20)")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 2.54 17.78)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J3-GP19)")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at 0 17.78)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-GP18)")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at 2.54 20.32)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J3-GP17)")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole circle
			(at 0 20.32)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-GP16)")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at 2.54 22.86)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J3-GP15)")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at 0 22.86)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J3-GP14)")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 2.54 25.4)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J3-GP13)")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 0 25.4)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J3-GP12)")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole circle
			(at 2.54 27.94)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J3-GP11)")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole circle
			(at 0 27.94)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J3-GP10)")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 2.54 30.48)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J3-GP9)")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 0 30.48)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J3-GP8)")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 2.54 33.02)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J3-GP7)")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole circle
			(at 0 33.02)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J3-GP6)")
			(pintype "bidirectional")
		)
		(pad "29" thru_hole circle
			(at 2.54 35.56)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J3-GP5)")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at 0 35.56)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J3-GP4)")
			(pintype "bidirectional")
		)
		(pad "31" thru_hole circle
			(at 2.54 38.1)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J3-GP3)")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 0 38.1)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J3-GP2)")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole circle
			(at 2.54 40.64)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J3-GP1)")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole circle
			(at 0 40.64)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J3-GP0)")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
	)
	(footprint "34pinLibrary:USB_C"
		(layer "F.Cu")
		(at 112.08 93.4)
		(property "Reference" "J2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "USB C Breakout"
			(at 5.6236 13.153 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "2350B_Keybd_Cntrl.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 7.62)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J2-VBUS)")
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(pad "2" thru_hole circle
			(at 0 10.16)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J2-GND)")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" thru_hole circle
			(at 0 12.7)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J2-CC1-Pad3)")
			(pinfunction "CC1")
			(pintype "power_in+no_connect")
		)
		(pad "4" thru_hole circle
			(at 0 15.24)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J2-D-)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 0 17.78)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J2-D+)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 0 20.32)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(J2-CC2-Pad6)")
			(pinfunction "CC2")
			(pintype "power_in+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "34pinLibrary:RP2350 Stamp XL"
		(layer "F.Cu")
		(at 137.26 67.66)
		(property "Reference" "J3"
			(at -16.61 0.92 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RP2350 STAMP XL"
			(at -16.8132 12.5532 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "2350B_Keybd_Cntrl.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -16.61 0.92 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -10.16 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J3-GP0)")
			(pinfunction "GP0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -7.62 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J3-GP1)")
			(pinfunction "GP1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at -5.08 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J3-GP2)")
			(pinfunction "GP2")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at -2.54 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J3-GP3)")
			(pinfunction "GP3")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 0 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J3-GP4)")
			(pinfunction "GP4")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 2.54 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J3-GP5)")
			(pinfunction "GP5")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 5.08 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J3-GP6)")
			(pinfunction "GP6")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 7.62 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J3-GP7)")
			(pinfunction "GP7")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 10.16 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J3-GP8)")
			(pinfunction "GP8")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 12.7 55.88)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J3-GP9)")
			(pinfunction "GP9")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 15.24 53.34)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J3-GP10)")
			(pinfunction "GP10")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 15.24 50.8)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J3-GP11)")
			(pinfunction "GP11")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole circle
			(at 15.24 48.26)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J3-GP12)")
			(pinfunction "GP12")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at 15.24 45.72)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J3-GP13)")
			(pinfunction "GP13")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 15.24 43.18)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J3-GP14)")
			(pinfunction "GP14")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at 15.24 40.64)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J3-GP15)")
			(pinfunction "GP15")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at 15.24 38.1)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-GP16)")
			(pinfunction "GP16")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole circle
			(at 15.24 35.56)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J3-GP17)")
			(pinfunction "GP17")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at 15.24 33.02)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-GP18)")
			(pinfunction "GP18")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at 15.24 30.48)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J3-GP19)")
			(pinfunction "GP19")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 15.24 27.94)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J3-GP20)")
			(pinfunction "GP20")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 15.24 25.4)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J3-GP21)")
			(pinfunction "GP21")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole circle
			(at 15.24 22.86)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-GP22)")
			(pinfunction "GP22")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole circle
			(at 15.24 20.32)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J3-GP23)")
			(pinfunction "GP23")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 15.24 17.78)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J3-GP24)")
			(pinfunction "GP24")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 15.24 15.24)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-GP25)")
			(pinfunction "GP25")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 15.24 12.7)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J3-GP26)")
			(pinfunction "GP26")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole circle
			(at 15.24 10.16)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J3-GP27)")
			(pinfunction "GP27")
			(pintype "bidirectional")
		)
		(pad "29" thru_hole circle
			(at 15.24 7.62)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J3-GP28)")
			(pinfunction "GP28")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at 15.24 5.08)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J3-GP29)")
			(pinfunction "GP29")
			(pintype "bidirectional")
		)
		(pad "31" thru_hole circle
			(at 12.7 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J3-GP30)")
			(pinfunction "GP30")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 10.16 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J3-GP31)")
			(pinfunction "GP31")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole circle
			(at 7.62 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J3-GP32)")
			(pinfunction "GP32")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole circle
			(at 5.08 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J3-GP33)")
			(pinfunction "GP33")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole circle
			(at 2.54 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(J3-GP34-Pad35)")
			(pinfunction "GP34")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" thru_hole circle
			(at 0 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(J3-GP35-Pad36)")
			(pinfunction "GP35")
			(pintype "bidirectional+no_connect")
		)
		(pad "37" thru_hole circle
			(at -2.54 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(J3-GP36-Pad37)")
			(pinfunction "GP36")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" thru_hole circle
			(at -5.08 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(J3-GP37-Pad38)")
			(pinfunction "GP37")
			(pintype "bidirectional+no_connect")
		)
		(pad "39" thru_hole circle
			(at -7.62 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(J3-GP38-Pad39)")
			(pinfunction "GP38")
			(pintype "bidirectional+no_connect")
		)
		(pad "40" thru_hole circle
			(at -10.16 2.54)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(J3-GP39-Pad40)")
			(pinfunction "GP39")
			(pintype "bidirectional+no_connect")
		)
		(pad "41" thru_hole circle
			(at -12.7 5.08)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(J3-GP40-Pad41)")
			(pinfunction "GP40")
			(pintype "bidirectional+no_connect")
		)
		(pad "42" thru_hole circle
			(at -12.7 7.62)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(J3-GP41-Pad42)")
			(pinfunction "GP41")
			(pintype "bidirectional+no_connect")
		)
		(pad "43" thru_hole circle
			(at -12.7 10.16)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(J3-GP42-Pad43)")
			(pinfunction "GP42")
			(pintype "bidirectional+no_connect")
		)
		(pad "44" thru_hole circle
			(at -12.7 12.7)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(J3-GP43-Pad44)")
			(pinfunction "GP43")
			(pintype "bidirectional+no_connect")
		)
		(pad "45" thru_hole circle
			(at -12.7 15.24)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(J3-GP44-Pad45)")
			(pinfunction "GP44")
			(pintype "bidirectional+no_connect")
		)
		(pad "46" thru_hole circle
			(at -12.7 17.78)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(J3-GP45-Pad46)")
			(pinfunction "GP45")
			(pintype "bidirectional+no_connect")
		)
		(pad "47" thru_hole circle
			(at -12.7 20.32)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(J3-GP46-Pad47)")
			(pinfunction "GP46")
			(pintype "bidirectional+no_connect")
		)
		(pad "48" thru_hole circle
			(at -12.7 22.86)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(J3-GP47-Pad48)")
			(pinfunction "GP47")
			(pintype "bidirectional+no_connect")
		)
		(pad "49" thru_hole circle
			(at -12.7 25.4)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(J3-BATSTAT-Pad49)")
			(pinfunction "BATSTAT")
			(pintype "bidirectional+no_connect")
		)
		(pad "50" thru_hole circle
			(at -12.7 27.94)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(J3-LDO_EN-Pad50)")
			(pinfunction "LDO_EN")
			(pintype "bidirectional+no_connect")
		)
		(pad "51" thru_hole circle
			(at -12.7 30.48)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J2-GND)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "52" thru_hole circle
			(at -12.7 33.02)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(J3-VBAT-Pad52)")
			(pinfunction "VBAT")
			(pintype "bidirectional+no_connect")
		)
		(pad "53" thru_hole circle
			(at -12.7 35.56)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J2-VBUS)")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "54" thru_hole circle
			(at -12.7 38.1)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(J3-3P3V-Pad54)")
			(pinfunction "3P3V")
			(pintype "power_out+no_connect")
		)
		(pad "55" thru_hole circle
			(at -12.7 40.64)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J2-D-)")
			(pinfunction "USB_D-")
			(pintype "bidirectional")
		)
		(pad "56" thru_hole circle
			(at -12.7 43.18)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J2-D+)")
			(pinfunction "USB_D+")
			(pintype "bidirectional")
		)
		(pad "57" thru_hole circle
			(at -12.7 45.72)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J3-SWDIO-Pad57)")
			(pinfunction "SWDIO")
			(pintype "bidirectional+no_connect")
		)
		(pad "58" thru_hole circle
			(at -12.7 48.26)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J3-SWCLK-Pad58)")
			(pinfunction "SWCLK")
			(pintype "bidirectional+no_connect")
		)
		(pad "59" thru_hole circle
			(at -12.7 50.8)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(J3-RESET-Pad59)")
			(pinfunction "RESET")
			(pintype "bidirectional+no_connect")
		)
		(pad "60" thru_hole circle
			(at -12.7 53.34)
			(size 1.8 1.8)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "unconnected-(J3-BOOTSEL-Pad60)")
			(pinfunction "BOOTSEL")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 104.775 134.62)
		(end 104.775 66.675)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 173.1 131.2)
		(end 173.4 129.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 108.5 130.8)
		(end 108.8 129.1)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 173 70.3)
		(end 173.3 68.6)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.53 134.62)
		(end 104.775 134.62)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 108.5 70.4)
		(end 108.8 68.7)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.53 66.675)
		(end 176.53 134.62)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.775 66.675)
		(end 176.53 66.675)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 104.7496 104.4448 0)
		(layer "F.SilkS")
	)
	(gr_text "USB Connector"
		(at 116.713 114.7826 90)
		(layer "F.SilkS")
	)
	(gr_text "RP2350 Stamp XL"
		(at 130.4798 128.9812 0)
		(layer "F.SilkS")
	)
	(gr_text "D+"
		(at 105.9942 111.8362 0)
		(layer "F.SilkS")
	)
	(gr_text "FPC Breakout\nConnector"
		(at 159.9 78.6 0)
		(layer "F.SilkS")
	)
	(gr_text "CC1"
		(at 104.9782 107.0356 0)
		(layer "F.SilkS")
	)
	(gr_text "D-"
		(at 106.045 109.3724 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 106.4514 101.8794 0)
		(layer "F.SilkS")
	)
	(gr_text "CC2"
		(at 104.8766 114.5794 0)
		(layer "F.SilkS")
	)
	(gr_text "https://github.com/thedalles77"
		(at 151.8 131.2 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
