(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A2)")
	(net 2 "POE_V+")
	(net 3 "POE_V-")
	(net 4 "Net-(U1-VIN+)")
	(net 5 "Net-(U1-VIN-)")
	(net 6 "Net-(D3-A)")
	(net 7 "Net-(D1-A1)")
	(net 8 "Net-(J2-Pin_2)")
	(net 9 "Net-(J2-Pin_3)")
	(net 10 "Net-(J2-Pin_1)")
	(net 11 "Net-(J2-Pin_4)")
	(net 12 "Net-(F1-Pad1)")
	(net 13 "GND")
	(net 14 "+5V")
	(net 15 "Net-(U2-+Input)")
	(net 16 "Net-(L2-Pad2)")
	(net 17 "Net-(L3-Pad2)")
	(net 18 "Net-(L5-Pad2)")
	(net 19 "Net-(L6-Pad2)")
	(net 20 "unconnected-(U1-IC-Pad4)")
	(net 21 "Net-(D7-A)")
	(net 22 "unconnected-(U1-IC-Pad6)")
	(net 23 "unconnected-(U1-AT-DET-Pad3)")
	(net 24 "unconnected-(U1-IC-Pad5)")
	(net 25 "Net-(U2-Trim)")
	(net 26 "unconnected-(U2-Remote-Pad6)")
	(net 27 "Net-(U1-ADJ)")
	(footprint "footprints:PJ-037A-PLURAF"
		(locked yes)
		(layer "F.Cu")
		(at 47.5996 47.0154 90)
		(property "Reference" "J1"
			(at 0 4.3434 90)
			(layer "F.SilkS")
		)
		(property "Value" "PJ-037A"
			(at 0.0127 -0.97282 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Barrel Jack"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 13.8 90)
			(size 4.6 2.6)
			(drill oval 3 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(F1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 7.5 90)
			(size 4.6 2.6)
			(drill oval 3 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A2)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 53.61 36.322 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "MPZ2012S102A"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 17 "Net-(L3-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(U1-VIN+)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 68.072 33.782 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF 100V"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "POE_V+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "POE_V-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:HHXC800ARA470MJA0G"
		(layer "F.Cu")
		(at 86.868 43.914 -90)
		(property "Reference" "C1"
			(at 0.6424 -2.286 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF 80V"
			(at -1.8595 -6.6675 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0.617 0.254 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0.617 0.254 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -3.569 0.254 270)
			(size 4.038 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1-A1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4.854 0.254 270)
			(size 4.008 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A2)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 64.008 36.322 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "MPZ2012S102A"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "POE_V+")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(L2-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:AG5400"
		(layer "F.Cu")
		(at 99.772 25.166)
		(property "Reference" "U1"
			(at -15.91056 -2.91846 0)
			(layer "F.SilkS")
		)
		(property "Value" "AG5400"
			(at -15.91056 -0.78994 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -43.18 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1-VIN+)")
			(pinfunction "VIN+")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at -40.64 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-VIN-)")
			(pinfunction "VIN-")
			(pintype "power_in")
		)
		(pad "3" thru_hole circle
			(at -38.1 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(U1-AT-DET-Pad3)")
			(pinfunction "AT-DET")
			(pintype "input+no_connect")
		)
		(pad "4" thru_hole circle
			(at -35.56 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(U1-IC-Pad4)")
			(pinfunction "IC")
			(pintype "no_connect")
		)
		(pad "5" thru_hole circle
			(at -33.02 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U1-IC-Pad5)")
			(pinfunction "IC")
			(pintype "no_connect")
		)
		(pad "6" thru_hole circle
			(at -30.48 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(U1-IC-Pad6)")
			(pinfunction "IC")
			(pintype "no_connect")
		)
		(pad "7" thru_hole circle
			(at 0 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "-VDC")
			(pintype "power_out")
		)
		(pad "8" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D3-A)")
			(pinfunction "+VDC")
			(pintype "power_out")
		)
		(pad "9" thru_hole circle
			(at 5.08 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(U1-ADJ)")
			(pinfunction "ADJ")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at 7.62 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "-VDC")
			(pintype "power_out")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:D_SMA"
		(layer "F.Cu")
		(at 79.121 47.371 -90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D1"
			(at 0 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "SMAJ30A"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 30Vrwm, DO-214AA"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMB*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.25 0 270)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1-A1)")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.25 0 270)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A2)")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SF-2410FP315T-2"
		(layer "F.Cu")
		(at 69.4436 46.228)
		(property "Reference" "F1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SF-2410FP315T-2"
			(at 0 13.462 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 12.462 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 12.462 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -3.048 0)
			(size 2.2 3.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(F1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.048 0)
			(size 2.2 3.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1-A1)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Symbol:WEEE-Logo_4.2x6mm_SilkScreen"
		(locked yes)
		(layer "F.Cu")
		(at 99.822 47.625)
		(descr "Waste Electrical and Electronic Equipment Directive")
		(tags "Logo WEEE")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WEEE-Logo_4.2x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(footprint "footprints:D_SMA"
		(layer "F.Cu")
		(at 118.364 45.212 180)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D3"
			(at 0 2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "SK54A-LTP"
			(at 0 2.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.25 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.25 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PCR1C471MCL6GS"
		(layer "F.Cu")
		(at 103.6828 36.0172 180)
		(property "Reference" "C5"
			(at 0.0508 5.7912 180)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at -0.0508 -2.7432 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -3.445 0 180)
			(size 3.27 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.445 0 180)
			(size 3.27 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 127.762 47.752 180)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "J3"
			(at 3.175 4.699 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_02x02_Counter_Clockwise"
			(at 1.27 4.87 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "PWR"
			(at 1.143 4.572 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "+5V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:hole-2.5m"
		(locked yes)
		(layer "F.Cu")
		(at 79 39)
		(property "Reference" "REF**"
			(at -0.1 3.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "hole-2.5m"
			(at -0.1 2.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(clearance 1.2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 67.072 30.226 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L5"
			(at 0 1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "MPZ2012S102A"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "POE_V-")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(L5-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LQH43PN1R0N26L"
		(layer "F.Cu")
		(at 94.996 44.323 90)
		(property "Reference" "L1"
			(at -5.334 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1uH"
			(at 3.048 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at -0.635 8.255 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with iron core"
			(at -0.635 8.255 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.286 0 90)
			(size 2.54 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1-A1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.286 0 90)
			(size 2.54 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(U2-+Input)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:hole-2.5m"
		(locked yes)
		(layer "F.Cu")
		(at 133.3 48.26)
		(property "Reference" "REF**"
			(at -0.1 3.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "hole-2.5m"
			(at -0.1 2.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(clearance 1.2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 56.674 30.226 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L7"
			(at 0 1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "MPZ2012S102A"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 19 "Net-(L6-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "Net-(U1-VIN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:EC4SBW-S"
		(layer "F.Cu")
		(at 123.825 29.8 180)
		(property "Reference" "U2"
			(at 0 -3.556 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EC4SBW-24S05"
			(at -0.254 3.302 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 2.54 10.15 180)
			(size 2.6 2.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(U2-+Input)")
			(pinfunction "+Input")
			(pintype "power_in")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at -2.56 10.15 180)
			(size 2.6 2.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A2)")
			(pinfunction "-Input")
			(pintype "power_in")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 10.16 -10.15 180)
			(size 2.6 2.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D7-A)")
			(pinfunction "+V_Output")
			(pintype "power_out")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0 -10.15 180)
			(size 2.6 2.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(U2-Trim)")
			(pinfunction "Trim")
			(pintype "input")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at -10.16 -10.15 180)
			(size 2.6 2.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "-V_Output")
			(pintype "power_out")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at -10.16 10.15 180)
			(size 2.6 2.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(U2-Remote-Pad6)")
			(pinfunction "Remote")
			(pintype "input+no_connect")
			(thermal_bridge_angle 90)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 73.7362 39.0398 180)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "J2"
			(at -2.7178 2.5908 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_02x02_Counter_Clockwise"
			(at 1.27 4.87 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "PoE"
			(at 1.3462 4.8768 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 58.928 36.322 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "MPZ2012S102A"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(L2-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 17 "Net-(L3-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 61.992 30.226 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L6"
			(at 0 1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "MPZ2012S102A"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(L5-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 19 "Net-(L6-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Diode_Bridge_Diotec_SO-DIL-Slim"
		(layer "B.Cu")
		(at 55.362 35.7066 -90)
		(descr "SMD diode bridge Diotec SO-DIL Slim, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40fs.pdf")
		(tags "DFS SO-DIL Slim")
		(property "Reference" "D6"
			(at -1.778 1.611 90)
			(layer "B.SilkS")
		)
		(property "Value" "DF01S"
			(at 0 -5.2 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MDB8S-D.PDF"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 1A If, TSSOP-4"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x5mm*P4mm*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 1.589 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.2 2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "POE_V+")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2 -2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "POE_V-")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 4.2 -2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "Net-(J2-Pin_4)")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 4.2 2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(J2-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/Diode_Bridge_Diotec_SO-DIL-Slim.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 129.1355 39.878)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 1.65 180)
			(layer "B.SilkS")
		)
		(property "Value" "3.4K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(U2-Trim)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 106.1 21.336)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 1.65 180)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(U1-ADJ)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SMA"
		(layer "B.Cu")
		(at 74.2188 30.6832 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D4"
			(at -0.1778 2.7432 90)
			(layer "B.SilkS")
		)
		(property "Value" "SMAJ58CA"
			(at 0 -2.6 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 30Vrwm, DO-214AA"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMB*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.25 0 90)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "POE_V+")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.25 0 90)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "POE_V-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder"
		(layer "B.Cu")
		(at 85.09 36.068)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7nF 2000V"
			(at 0 -2.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0)
			(size 1.575 3.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15873)
			(net 5 "Net-(U1-VIN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0)
			(size 1.575 3.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15873)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SMA"
		(layer "B.Cu")
		(at 118.364 45.212 180)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D7"
			(at 0 2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "SK54A-LTP"
			(at 0 -2.6 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.25 0 180)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.25 0 180)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder"
		(layer "B.Cu")
		(at 84.9845 19.304)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7nF 2000V"
			(at 0 -2.65 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0)
			(size 1.575 3.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15873)
			(net 4 "Net-(U1-VIN+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0)
			(size 1.575 3.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15873)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Diode_Bridge_Diotec_SO-DIL-Slim"
		(layer "B.Cu")
		(at 64.653 35.7066 -90)
		(descr "SMD diode bridge Diotec SO-DIL Slim, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40fs.pdf")
		(tags "DFS SO-DIL Slim")
		(property "Reference" "D5"
			(at 0.254 1.524 90)
			(layer "B.SilkS")
		)
		(property "Value" "DF01S"
			(at 0 -5.2 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MDB8S-D.PDF"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 1A If, TSSOP-4"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x5mm*P4mm*")
		(sheetname "Root")
		(sheetfile "poe-ce.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 1.589 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.2 2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "POE_V+")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2 -2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "POE_V-")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 4.2 -2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 4.2 2.55 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "Net-(J2-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/Diode_Bridge_Diotec_SO-DIL-Slim.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 52.07 51.562)
		(end 135.022 51.562)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 52.07 51.562)
		(mid 50.992369 51.115631)
		(end 50.546 50.038)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 50.546 18.542)
		(mid 50.992369 17.464369)
		(end 52.07 17.018)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 136.591014 50.038)
		(mid 136.128653 51.131661)
		(end 135.022 51.561999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 135.022 17.018)
		(mid 136.128653 17.448339)
		(end 136.591014 18.542)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 50.546 18.542)
		(end 50.546 50.038)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.591014 18.542)
		(end 136.591014 50.038)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 52.07 17.018)
		(end 135.022 17.018)
		(layer "Edge.Cuts")
	)
	(gr_text "Rev 2.0"
		(at 65.786 51.054 0)
		(layer "F.SilkS")
	)
	(gr_text "+5V"
		(at 129.413 45.72 0)
		(layer "F.SilkS")
	)
	(gr_text "Designed by\nPluraf Embedded AB"
		(at 109 51.308 0)
		(layer "F.SilkS")
	)
	(gr_text "9-24 VDC"
		(at 58.928 42.037 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 130.81 49.53 90)
		(layer "F.SilkS")
	)
	(zone
		(net 6)
		(net_name "Net-(D3-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 100.33 24.892) (xy 103.632 24.892) (xy 104.394 26.416) (xy 110.744 26.416) (xy 110.744 27.178)
				(xy 110.744 40.64) (xy 105.791 40.64)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1-A1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 83.947 38.354) (xy 89.535 38.354) (xy 89.535 43.942) (xy 83.947 43.942)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(U1-VIN-)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 58.42 24.892) (xy 53.848 29.464) (xy 53.848 34.29) (xy 70.104 34.29) (xy 70.104 27.432) (xy 60.96 27.432)
				(xy 60.452 24.892)
			)
		)
	)
	(zone
		(net 13)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 110.744 24.892) (xy 110.744 17.272) (xy 98.552 17.272) (xy 98.552 24.892)
			)
		)
	)
	(zone
		(net 13)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 136.652 51.562) (xy 136.652 37.338) (xy 132.08 37.338) (xy 121.666 51.562)
			)
		)
	)
	(zone
		(net 13)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 102.997 33.401) (xy 102.997 38.354) (xy 94.996 38.354) (xy 94.996 33.401)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(U1-VIN+)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 51.054 17.272) (xy 51.054 38.1) (xy 52.9844 38.0492) (xy 53.0352 29.0322) (xy 60.325 21.6916)
				(xy 60.3758 17.272)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Net-(D1-A2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 50.419 43.942) (xy 50.165 51.3842) (xy 86.7918 51.435) (xy 86.741 43.942)
			)
		)
	)
	(embedded_fonts no)
)
