(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 61)
    (no_connects 61)
    (area 110.084999 44.619037 253.458513 105.397)
    (thickness 1.6)
    (drawings 4)
    (tracks 1)
    (zones 0)
    (modules 19)
    (nets 95)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 4)
    (user_trace_width 5)
    (user_trace_width 6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 27.686 127.508)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /5V)
  (net 2 GND)
  (net 3 "Net-(P1-Pad1)")
  (net 4 "Net-(P1-Pad2)")
  (net 5 "Net-(P1-Pad3)")
  (net 6 "Net-(P1-Pad4)")
  (net 7 "Net-(P1-Pad5)")
  (net 8 "Net-(P1-Pad6)")
  (net 9 "Net-(P1-Pad7)")
  (net 10 "Net-(P1-Pad8)")
  (net 11 /KEY_INPUT1)
  (net 12 /KEY_INPUT2)
  (net 13 /KEY_INPUT6)
  (net 14 "Net-(P3-Pad1)")
  (net 15 "Net-(P3-Pad2)")
  (net 16 /LCD_D0)
  (net 17 /LCD_D1)
  (net 18 /LCD_D2)
  (net 19 /LCD_D3)
  (net 20 /LCD_D4)
  (net 21 /LCD_D5)
  (net 22 /LCD_D6)
  (net 23 /LCD_D7)
  (net 24 "Net-(P3-Pad11)")
  (net 25 "Net-(P3-Pad19)")
  (net 26 "Net-(P3-Pad20)")
  (net 27 "Net-(P3-Pad21)")
  (net 28 "Net-(P3-Pad22)")
  (net 29 "Net-(P3-Pad23)")
  (net 30 "Net-(P3-Pad24)")
  (net 31 "Net-(P3-Pad25)")
  (net 32 "Net-(P3-Pad26)")
  (net 33 "Net-(P3-Pad27)")
  (net 34 "Net-(P3-Pad28)")
  (net 35 "Net-(P3-Pad29)")
  (net 36 "Net-(P3-Pad30)")
  (net 37 /SD_DO)
  (net 38 /LCD_DI)
  (net 39 /SD_SCK)
  (net 40 "Net-(P3-Pad34)")
  (net 41 "Net-(P3-Pad35)")
  (net 42 "Net-(P3-Pad36)")
  (net 43 "Net-(P4-Pad1)")
  (net 44 "Net-(P4-Pad2)")
  (net 45 /RGB_B)
  (net 46 "Net-(P4-Pad4)")
  (net 47 "Net-(P4-Pad6)")
  (net 48 "Net-(P4-Pad7)")
  (net 49 "Net-(P4-Pad8)")
  (net 50 "Net-(P15-Pad1)")
  (net 51 "Net-(P6-Pad1)")
  (net 52 "Net-(P6-Pad2)")
  (net 53 "Net-(P6-Pad3)")
  (net 54 /12V)
  (net 55 "Net-(P7-Pad2)")
  (net 56 "Net-(P7-Pad3)")
  (net 57 "Net-(P7-Pad4)")
  (net 58 "Net-(P7-Pad5)")
  (net 59 "Net-(P7-Pad6)")
  (net 60 "Net-(P7-Pad7)")
  (net 61 "Net-(P7-Pad8)")
  (net 62 "Net-(P7-Pad9)")
  (net 63 "Net-(P7-Pad10)")
  (net 64 /LCD_RD)
  (net 65 /LCD_WR)
  (net 66 /LCD_RS)
  (net 67 /LCD_CS)
  (net 68 /LCD_RST)
  (net 69 "Net-(P9-Pad6)")
  (net 70 "Net-(P9-Pad7)")
  (net 71 "Net-(P9-Pad8)")
  (net 72 "Net-(P10-Pad1)")
  (net 73 "Net-(P10-Pad2)")
  (net 74 /SD_SS)
  (net 75 /HEATER_ON_OFF)
  (net 76 "Net-(P10-Pad5)")
  (net 77 "Net-(P10-Pad6)")
  (net 78 "Net-(P10-Pad7)")
  (net 79 "Net-(P10-Pad8)")
  (net 80 "Net-(P10-Pad9)")
  (net 81 "Net-(P10-Pad10)")
  (net 82 "Net-(P11-Pad1)")
  (net 83 "Net-(P11-Pad2)")
  (net 84 "Net-(P11-Pad3)")
  (net 85 "Net-(P11-Pad4)")
  (net 86 "Net-(P11-Pad8)")
  (net 87 "Net-(U1-Pad4)")
  (net 88 "Net-(U1-Pad5)")
  (net 89 "Net-(U1-Pad6)")
  (net 90 "Net-(U1-Pad7)")
  (net 91 "Net-(U1-Pad10)")
  (net 92 "Net-(U1-Pad11)")
  (net 93 "Net-(U1-Pad12)")
  (net 94 "Net-(U1-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /12V)
    (add_net /5V)
    (add_net /HEATER_ON_OFF)
    (add_net /KEY_INPUT1)
    (add_net /KEY_INPUT2)
    (add_net /KEY_INPUT6)
    (add_net /LCD_CS)
    (add_net /LCD_D0)
    (add_net /LCD_D1)
    (add_net /LCD_D2)
    (add_net /LCD_D3)
    (add_net /LCD_D4)
    (add_net /LCD_D5)
    (add_net /LCD_D6)
    (add_net /LCD_D7)
    (add_net /LCD_DI)
    (add_net /LCD_RD)
    (add_net /LCD_RS)
    (add_net /LCD_RST)
    (add_net /LCD_WR)
    (add_net /RGB_B)
    (add_net /SD_DO)
    (add_net /SD_SCK)
    (add_net /SD_SS)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P10-Pad10)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P10-Pad5)")
    (add_net "Net-(P10-Pad6)")
    (add_net "Net-(P10-Pad7)")
    (add_net "Net-(P10-Pad8)")
    (add_net "Net-(P10-Pad9)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P11-Pad2)")
    (add_net "Net-(P11-Pad3)")
    (add_net "Net-(P11-Pad4)")
    (add_net "Net-(P11-Pad8)")
    (add_net "Net-(P15-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad11)")
    (add_net "Net-(P3-Pad19)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad20)")
    (add_net "Net-(P3-Pad21)")
    (add_net "Net-(P3-Pad22)")
    (add_net "Net-(P3-Pad23)")
    (add_net "Net-(P3-Pad24)")
    (add_net "Net-(P3-Pad25)")
    (add_net "Net-(P3-Pad26)")
    (add_net "Net-(P3-Pad27)")
    (add_net "Net-(P3-Pad28)")
    (add_net "Net-(P3-Pad29)")
    (add_net "Net-(P3-Pad30)")
    (add_net "Net-(P3-Pad34)")
    (add_net "Net-(P3-Pad35)")
    (add_net "Net-(P3-Pad36)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P7-Pad10)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P7-Pad5)")
    (add_net "Net-(P7-Pad6)")
    (add_net "Net-(P7-Pad7)")
    (add_net "Net-(P7-Pad8)")
    (add_net "Net-(P7-Pad9)")
    (add_net "Net-(P9-Pad6)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(P9-Pad8)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 0)
    (at 179.578 77.724)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1 -3.8) (layer F.SilkS))
    (fp_text value 100uF (at 1 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 2 thru_hole circle (at 2 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 0)
    (at 187.198 69.596)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 -2.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 57C2AFD5)
    (at 168.656 100.076 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value COMMUNICATION (at 3.048 -1.524 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0910 (layer F.Cu) (tedit 0)
    (at 180.086 60.452 270)
    (descr "Molex PicoBlade 1.25mm shrouded header. Vertical. 9 ways")
    (tags "connector PicoBlade header")
    (fp_text reference P2 (at 5 2.35 270) (layer F.SilkS))
    (fp_text value KEY_INPUT (at 5 -3.25 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 /KEY_INPUT2))
    (pad 3 thru_hole oval (at 2.5 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 4 thru_hole oval (at 3.75 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 5 thru_hole oval (at 5 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 6 thru_hole oval (at 6.25 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 /KEY_INPUT6))
    (pad 7 thru_hole oval (at 7.5 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 8 thru_hole oval (at 8.75 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 9 thru_hole oval (at 10 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0910.wrl
      (at (xyz 0.19685 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x18 (layer F.Cu) (tedit 0)
    (at 152.908 55.372)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS))
    (fp_text value DIGITAL_PIN (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LCD_D0))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /LCD_D1))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LCD_D2))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /LCD_D3))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LCD_D4))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LCD_D5))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LCD_D6))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /LCD_D7))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P3-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /KEY_INPUT6))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /KEY_INPUT2))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /KEY_INPUT1))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P3-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P3-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P3-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P3-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P3-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P3-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P3-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P3-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P3-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P3-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P3-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P3-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /SD_DO))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /LCD_DI))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /SD_SCK))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P3-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P3-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P3-Pad36)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x18.wrl
      (at (xyz 0.05 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-08_08x2.54mm_Straight (layer F.Cu) (tedit 56C6219D)
    (at 194.818 99.822)
    (descr "Connector Headers with Friction Lock, 22-27-2081, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2081")
    (fp_text reference P4 (at 1 -4.5) (layer F.SilkS))
    (fp_text value "PWM 1" (at 8.89 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 45 /RGB_B))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 45 /RGB_B))
    (pad 6 thru_hole oval (at 12.7 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P4-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P4-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P4-Pad8)"))
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0410 (layer F.Cu) (tedit 0)
    (at 186.182 76.962)
    (descr "Molex PicoBlade 1.25mm shrouded header. Vertical. 4 ways")
    (tags "connector PicoBlade header")
    (fp_text reference P5 (at 1.875 2.35) (layer F.SilkS))
    (fp_text value TEMP_SENSOR (at 1.875 -3.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(P15-Pad1)"))
    (pad 3 thru_hole oval (at 2.5 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 4 thru_hole oval (at 3.75 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0410.wrl
      (at (xyz 0.07381890000000001 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0410 (layer F.Cu) (tedit 0)
    (at 226.314 63.754 270)
    (descr "Molex PicoBlade 1.25mm shrouded header. Vertical. 4 ways")
    (tags "connector PicoBlade header")
    (fp_text reference P6 (at 1.875 2.35 270) (layer F.SilkS))
    (fp_text value "RGB LED" (at 1.875 -3.25 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 2.5 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 3.75 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 54 /12V))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0410.wrl
      (at (xyz 0.07381890000000001 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_JST:JST_EH_B10B-EH-A_10x2.50mm_Straight (layer F.Cu) (tedit 56EE9564)
    (at 194.31 50.038)
    (descr "JST EH series connector, B10B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P7 (at 0 -3) (layer F.SilkS))
    (fp_text value "ANALOG IN 2" (at 0 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(P15-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(P7-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P7-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(P7-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(P7-Pad5)"))
    (pad 6 thru_hole circle (at 12.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(P7-Pad6)"))
    (pad 7 thru_hole circle (at 15 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P7-Pad7)"))
    (pad 8 thru_hole circle (at 17.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(P7-Pad8)"))
    (pad 9 thru_hole circle (at 20 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(P7-Pad9)"))
    (pad 10 thru_hole circle (at 22.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(P7-Pad10)"))
    (model Connectors_JST.3dshapes/JST_EH_B10B-EH-A_10x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x02 (layer F.Cu) (tedit 0)
    (at 243.078 84.582)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P8 (at 0 -4.75) (layer F.SilkS))
    (fp_text value 12V (at 0 -2.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /12V))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_JST:JST_EH_B08B-EH-A_08x2.50mm_Straight (layer F.Cu) (tedit 56EE9564)
    (at 187.198 51.054 180)
    (descr "JST EH series connector, B08B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P9 (at 0 -3 180) (layer F.SilkS))
    (fp_text value "ANALOG_INPUT 1" (at 0 5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 64 /LCD_RD))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 65 /LCD_WR))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 66 /LCD_RS))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 67 /LCD_CS))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 68 /LCD_RST))
    (pad 6 thru_hole circle (at 12.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P9-Pad6)"))
    (pad 7 thru_hole circle (at 15 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P9-Pad7)"))
    (pad 8 thru_hole circle (at 17.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(P9-Pad8)"))
    (model Connectors_JST.3dshapes/JST_EH_B08B-EH-A_08x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B10B-EH-A_10x2.50mm_Straight (layer F.Cu) (tedit 56EE9564)
    (at 223.266 99.314)
    (descr "JST EH series connector, B10B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P10 (at 0 -3) (layer F.SilkS))
    (fp_text value "PWM 2" (at 0 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(P10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(P10-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 74 /SD_SS))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 75 /HEATER_ON_OFF))
    (pad 5 thru_hole circle (at 10 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(P10-Pad5)"))
    (pad 6 thru_hole circle (at 12.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(P10-Pad6)"))
    (pad 7 thru_hole circle (at 15 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(P10-Pad7)"))
    (pad 8 thru_hole circle (at 17.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(P10-Pad8)"))
    (pad 9 thru_hole circle (at 20 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(P10-Pad9)"))
    (pad 10 thru_hole circle (at 22.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(P10-Pad10)"))
    (model Connectors_JST.3dshapes/JST_EH_B10B-EH-A_10x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B08B-EH-A_08x2.50mm_Straight (layer F.Cu) (tedit 56EE9564)
    (at 224.282 50.038)
    (descr "JST EH series connector, B08B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P11 (at 0 -3) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(P11-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(P11-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(P11-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(P11-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 6 thru_hole circle (at 12.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole circle (at 15 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole circle (at 17.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(P11-Pad8)"))
    (model Connectors_JST.3dshapes/JST_EH_B08B-EH-A_08x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_S02B-EH_02x2.50mm_Angled (layer F.Cu) (tedit 56EE956A)
    (at 229.87 89.916)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference P12 (at 0 4) (layer F.SilkS))
    (fp_text value "SSR CONTROL" (at 0 6) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 75 /HEATER_ON_OFF))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Harwin:Harwin_LTek-Male_02x2.00mm_Straight (layer F.Cu) (tedit 5753B054)
    (at 178.054 92.964)
    (descr "Harwin LTek Connector, 2 pins, single row male, vertical entry")
    (tags "connector harwin ltek M80")
    (fp_text reference P13 (at 1 -3.5) (layer F.SilkS))
    (fp_text value 5V (at 1 4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /5V))
    (model Connectors_Harwin.3dshapes/Harwin_LTek-Male_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:IDC_Header_Straight_20pins (layer F.Cu) (tedit 0)
    (at 168.91 86.36 90)
    (descr "20 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P14 (at 11.43 -7.62 90) (layer F.SilkS))
    (fp_text value TFT_LCD_CON (at 11.43 5.223 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(P11-Pad4)"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 /LCD_RD))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 /LCD_WR))
    (pad 6 thru_hole oval (at 5.08 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 /SD_SS))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 /LCD_RS))
    (pad 8 thru_hole oval (at 7.62 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /LCD_DI))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /LCD_CS))
    (pad 10 thru_hole oval (at 10.16 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /SD_DO))
    (pad 11 thru_hole oval (at 12.7 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /LCD_RST))
    (pad 12 thru_hole oval (at 12.7 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /SD_SCK))
    (pad 13 thru_hole oval (at 15.24 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LCD_D0))
    (pad 14 thru_hole oval (at 15.24 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /LCD_D7))
    (pad 15 thru_hole oval (at 17.78 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /LCD_D1))
    (pad 16 thru_hole oval (at 17.78 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LCD_D6))
    (pad 17 thru_hole oval (at 20.32 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LCD_D2))
    (pad 18 thru_hole oval (at 20.32 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LCD_D5))
    (pad 19 thru_hole oval (at 22.86 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /LCD_D3))
    (pad 20 thru_hole oval (at 22.86 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LCD_D4))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 197.612 84.074 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference P15 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value TEMP_R_SET (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 50 "Net-(P15-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 186.436 60.452)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.05892 -3.50012) (layer F.SilkS))
    (fp_text value 15K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 50 "Net-(P15-Pad1)"))
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 54130A77)
    (at 213.868 63.246)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 -5.22) (layer F.SilkS))
    (fp_text value UNL2003 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 /RGB_B))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P4-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 /RGB_B))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(U1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 54 /12V))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(U1-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P6-Pad3)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P6-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P6-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 148.408512 44.669038) (end 148.408512 104.669038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 253.408512 44.669038) (end 148.408512 44.669038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 253.408512 104.669038) (end 253.408512 44.669038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.408512 104.669038) (end 253.408512 104.669038) (layer Edge.Cuts) (width 0.1))
)
