(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 42)
    (no_connects 0)
    (area 143.805 40.164999 200.735001 117.435)
    (thickness 1.6)
    (drawings 4)
    (tracks 53)
    (zones 0)
    (modules 22)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01000_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(A1-Pad30)")
  (net 3 "Net-(A1-Pad1)")
  (net 4 "Net-(A1-Pad17)")
  (net 5 "Net-(A1-Pad2)")
  (net 6 "Net-(A1-Pad18)")
  (net 7 "Net-(A1-Pad3)")
  (net 8 "Net-(A1-Pad19)")
  (net 9 /3V3)
  (net 10 "Net-(A1-Pad20)")
  (net 11 /5V)
  (net 12 "Net-(A1-Pad21)")
  (net 13 "Net-(A1-Pad22)")
  (net 14 "Net-(A1-Pad23)")
  (net 15 /Vin)
  (net 16 "Net-(A1-Pad24)")
  (net 17 "Net-(A1-Pad9)")
  (net 18 "Net-(A1-Pad25)")
  (net 19 "Net-(A1-Pad10)")
  (net 20 "Net-(A1-Pad26)")
  (net 21 "Net-(A1-Pad11)")
  (net 22 "Net-(A1-Pad27)")
  (net 23 "Net-(A1-Pad12)")
  (net 24 "Net-(A1-Pad28)")
  (net 25 "Net-(A1-Pad13)")
  (net 26 "Net-(A1-Pad14)")
  (net 27 "Net-(A1-Pad15)")
  (net 28 "Net-(A1-Pad16)")
  (net 29 "Net-(C1-Pad1)")
  (net 30 "Net-(C2-Pad1)")
  (net 31 "Net-(C3-Pad1)")
  (net 32 "Net-(C3-Pad2)")
  (net 33 "Net-(C4-Pad1)")
  (net 34 "Net-(C4-Pad2)")
  (net 35 "Net-(C5-Pad1)")
  (net 36 "Net-(C5-Pad2)")
  (net 37 "Net-(C6-Pad1)")
  (net 38 "Net-(C6-Pad2)")
  (net 39 "Net-(C7-Pad2)")
  (net 40 "Net-(C8-Pad2)")
  (net 41 "Net-(RV1-Pad2)")
  (net 42 "Net-(RV2-Pad2)")
  (net 43 "Net-(C9-Pad2)")
  (net 44 "Net-(C10-Pad2)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /5V)
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(RV2-Pad2)")
  )
  (module Modules:Arduino_UNO_R2 (layer B.Cu) (tedit 58AB6071)
    (at 148.59 74.93 270)
    (descr "Arduino UNO R2, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R2")
    (fp_text reference A1 (at 1.27 3.81 450) (layer B.SilkS))
    (fp_text value Arduino_UNO_R2 (at 0 -21.59 270) (layer B.Fab))
    (fp_text user %R (at 0 -19.05 450) (layer B.Fab))
    (pad 29 thru_hole oval (at -1.52 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 30 thru_hole oval (at -4.06 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad30)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad1)"))
    (pad 17 thru_hole oval (at 30.48 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad17)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad2)"))
    (pad 18 thru_hole oval (at 27.94 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad18)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad3)"))
    (pad 19 thru_hole oval (at 25.4 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad19)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /3V3))
    (pad 20 thru_hole oval (at 22.86 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad20)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /5V))
    (pad 21 thru_hole oval (at 20.32 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad21)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole oval (at 17.78 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad22)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole oval (at 13.72 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad23)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /Vin))
    (pad 24 thru_hole oval (at 11.18 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad24)"))
    (pad 9 thru_hole oval (at 22.86 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad9)"))
    (pad 25 thru_hole oval (at 8.64 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad25)"))
    (pad 10 thru_hole oval (at 25.4 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad10)"))
    (pad 26 thru_hole oval (at 6.1 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad26)"))
    (pad 11 thru_hole oval (at 27.94 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad11)"))
    (pad 27 thru_hole oval (at 3.56 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad27)"))
    (pad 12 thru_hole oval (at 30.48 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad12)"))
    (pad 28 thru_hole oval (at 1.02 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad28)"))
    (pad 13 thru_hole oval (at 33.02 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad13)"))
    (pad 14 thru_hole oval (at 35.56 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad14)"))
    (pad 15 thru_hole oval (at 35.56 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad15)"))
    (pad 16 thru_hole oval (at 33.02 -48.26 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad16)"))
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 176.53 83.82)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.31) (layer F.SilkS))
    (fp_text value CP1 (at 2.5 6.31) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 176.53 101.6)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 2.5 -6.31) (layer F.SilkS))
    (fp_text value CP1 (at 2.5 6.31) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 185.42 71.12 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C7 (at 2.5 -6.31 180) (layer F.SilkS))
    (fp_text value CP1 (at 2.5 6.31 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 168.91 109.22 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C8 (at 2.5 -6.31 270) (layer F.SilkS))
    (fp_text value CP1 (at 2.5 6.31 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_BL-FL7680RGB (layer F.Cu) (tedit 59F6ACD6)
    (at 187.96 91.44 90)
    (descr "'Piranha' RGB LED, through hole, common anode, 7.62x7.62mm, BGRA pin order, https://cdn-shop.adafruit.com/datasheets/BL-FL7680RGB.pdf")
    (tags "RGB LED Piranha Super-Flux BetLux")
    (fp_text reference D3 (at 2.54 -2.27 90) (layer F.SilkS))
    (fp_text value LED_CRGB (at 2.54 7.35 90) (layer F.Fab))
    (fp_text user %R (at 2.54 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad23)"))
    (pad 4 thru_hole circle (at 5.08 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad25)"))
    (pad 3 thru_hole circle (at 5.08 5.08 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad24)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_BL-FL7680RGB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 191.77 81.28 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R10 (at 6.35 -2.66 90) (layer F.SilkS))
    (fp_text value R (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 181.61 111.76)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R11 (at 6.35 -2.66) (layer F.SilkS))
    (fp_text value R (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C6-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 163.83 78.74)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value LM386 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C3-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(RV2-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C9-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 163.83 96.52)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value LM386 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C4-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(RV1-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C10-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_ACP_CA6h_Vertical (layer F.Cu) (tedit 58826B0A)
    (at 160.02 104.14 270)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, Vishay T73XX Single, Vishay T73XX Single, Vishay T73YP Single, Piher PT-6h Single, Piher PT-6v Single, Piher PT-6v Single, Piher PT-10h2.5 Single, Piher PT-10h5 Single, Piher PT-101h3.8 Single, Piher PT-10v10 Single, Piher PT-10v10 Single, Piher PT-10v5 Single, Piher PT-15h5 Single, Piher PT-15h2.5 Single, Piher PT-15B Single, Piher PT-15hc5 Single, Piher PT-15v12.5 Single, Piher PT-15v12.5 Single, Piher PT-15v15 Single, Piher PT-15v15 Single, ACP CA6h Single, http://www.acptechnologies.com/wp-content/uploads/2016/12/ACP-CAT%C3%81LOGO-ENTERO-2016.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single  Vishay T73XX Single  Vishay T73XX Single  Vishay T73YP Single  Piher PT-6h Single  Piher PT-6v Single  Piher PT-6v Single  Piher PT-10h2.5 Single  Piher PT-10h5 Single  Piher PT-101h3.8 Single  Piher PT-10v10 Single  Piher PT-10v10 Single  Piher PT-10v5 Single  Piher PT-15h5 Single  Piher PT-15h2.5 Single  Piher PT-15B Single  Piher PT-15hc5 Single  Piher PT-15v12.5 Single  Piher PT-15v12.5 Single  Piher PT-15v15 Single  Piher PT-15v15 Single  ACP CA6h Single")
    (fp_text reference RV1 (at 0 -2.06 270) (layer F.SilkS))
    (fp_text value POT (at 0 7.06 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5 270) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5 270) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(RV1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad10)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA6h_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_ACP_CA6h_Vertical (layer F.Cu) (tedit 58826B0A)
    (at 154.94 93.98 90)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, Vishay T73XX Single, Vishay T73XX Single, Vishay T73YP Single, Piher PT-6h Single, Piher PT-6v Single, Piher PT-6v Single, Piher PT-10h2.5 Single, Piher PT-10h5 Single, Piher PT-101h3.8 Single, Piher PT-10v10 Single, Piher PT-10v10 Single, Piher PT-10v5 Single, Piher PT-15h5 Single, Piher PT-15h2.5 Single, Piher PT-15B Single, Piher PT-15hc5 Single, Piher PT-15v12.5 Single, Piher PT-15v12.5 Single, Piher PT-15v15 Single, Piher PT-15v15 Single, ACP CA6h Single, http://www.acptechnologies.com/wp-content/uploads/2016/12/ACP-CAT%C3%81LOGO-ENTERO-2016.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single  Vishay T73XX Single  Vishay T73XX Single  Vishay T73YP Single  Piher PT-6h Single  Piher PT-6v Single  Piher PT-6v Single  Piher PT-10h2.5 Single  Piher PT-10h5 Single  Piher PT-101h3.8 Single  Piher PT-10v10 Single  Piher PT-10v10 Single  Piher PT-10v5 Single  Piher PT-15h5 Single  Piher PT-15h2.5 Single  Piher PT-15B Single  Piher PT-15hc5 Single  Piher PT-15v12.5 Single  Piher PT-15v12.5 Single  Piher PT-15v15 Single  Piher PT-15v15 Single  ACP CA6h Single")
    (fp_text reference RV2 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value POT (at 0 7.06 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5 90) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5 90) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(RV2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad9)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA6h_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 176.53 90.17)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2mm Capacitor")
    (fp_text reference C5 (at 2.5 -2.31) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.31) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 176.53 107.95)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2mm Capacitor")
    (fp_text reference C6 (at 2.5 -2.31) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.31) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 152.4 96.52)
    (fp_text reference J1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad9)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 152.4 101.6)
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad10)"))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 166.37 73.66)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.25 -3.81) (layer F.SilkS))
    (fp_text value CP1 (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 166.37 91.44)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 1.25 -3.81) (layer F.SilkS))
    (fp_text value CP1 (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 181.61 77.47 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2mm Capacitor")
    (fp_text reference C9 (at 2.5 -2.31 180) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.31 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 181.61 95.25 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2mm Capacitor")
    (fp_text reference C10 (at 2.5 -2.31 180) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.31 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 161.29 68.58 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference LS1 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value Speaker (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 161.29 114.3 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference LS2 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value Speaker (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 200.66 64.77) (end 144.78 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 116.84) (end 200.66 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 116.84) (end 200.66 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 64.77) (end 144.78 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.66 116.84) (xy 144.78 116.84) (xy 144.78 64.77) (xy 200.66 64.77)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.66 116.84) (xy 144.78 116.84) (xy 144.78 64.77) (xy 200.66 64.77)
      )
    )
  )
)
