(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 43)
    (no_connects 0)
    (area 91.1255 55.616499 160.537501 109.737501)
    (thickness 1.6)
    (drawings 22)
    (tracks 233)
    (zones 0)
    (modules 19)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x03000_80000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory freescale/04/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad1)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(J1-Pad5)")
  (net 10 "Net-(J1-Pad6)")
  (net 11 "Net-(J1-Pad7)")
  (net 12 "Net-(J1-Pad8)")
  (net 13 "Net-(J1-Pad9)")
  (net 14 "Net-(J1-Pad10)")
  (net 15 "Net-(J1-Pad13)")
  (net 16 "Net-(J1-Pad14)")
  (net 17 "Net-(J1-Pad23)")
  (net 18 "Net-(J1-Pad24)")
  (net 19 "Net-(P1-Pad4)")
  (net 20 "Net-(P1-Pad5)")
  (net 21 "Net-(P1-Pad3)")
  (net 22 "Net-(P1-Pad2)")
  (net 23 "Net-(R5-Pad2)")
  (net_class Default "Esta é a classe de net default."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(R5-Pad2)")
  )
  (module w_conn_misc:arduino_header (layer F.Cu) (tedit 576DA392)
    (at 124.587 82.677)
    (descr "Arduino Header")
    (tags Arduino)
    (fp_text reference J1 (at -23.241 -24.003) (layer F.SilkS))
    (fp_text value Arduino_Header (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -2.54 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 2.54 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 5.08 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 7.62 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 10.16 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 12.7 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 17.78 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 20.32 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 22.86 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 25.4 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 27.94 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 30.48 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad14)"))
    (pad "" np_thru_hole circle (at -19.05 24.13) (size 3.19786 3.19786) (drill 3.19786) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 33.02 19.05) (size 3.19786 3.19786) (drill 3.19786) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 30.48 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 27.94 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole oval (at 25.4 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole oval (at 22.86 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad1)"))
    (pad 19 thru_hole oval (at 20.32 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole oval (at 17.78 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole oval (at 15.24 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole oval (at 12.7 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole oval (at 8.636 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad23)"))
    (pad 24 thru_hole oval (at 6.096 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-Pad24)"))
    (pad 25 thru_hole oval (at 3.556 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole oval (at 1.016 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D4-Pad1)"))
    (pad 27 thru_hole oval (at -1.524 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D3-Pad1)"))
    (pad 28 thru_hole oval (at -4.064 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad1)"))
    (pad 29 thru_hole oval (at -6.604 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole oval (at -9.14146 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -17.78 -24.13) (size 3.19786 3.19786) (drill 3.19786) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole oval (at -11.684 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole oval (at -14.224 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 33.02 -8.89) (size 3.19786 3.19786) (drill 3.19786) (layers *.Cu *.Mask F.SilkS))
    (model walter/conn_misc/arduino_header.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_indicators:led_5mm_clear (layer F.Cu) (tedit 576DA3CF)
    (at 116.713 67.945)
    (descr "5mm clear led")
    (tags led)
    (fp_text reference D1 (at 0.254 3.937) (layer F.SilkS))
    (fp_text value LED1 (at 0 -4) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 0 1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (model walter/indicators/led_5mm_clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_indicators:led_5mm_clear (layer F.Cu) (tedit 532D9A66)
    (at 110.236 67.945)
    (descr "5mm clear led")
    (tags led)
    (fp_text reference D2 (at 0 4) (layer F.SilkS))
    (fp_text value LED0 (at 0 -4) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 0 1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (model walter/indicators/led_5mm_clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_indicators:led_5mm_clear (layer F.Cu) (tedit 532D9A66)
    (at 123.063 68.072)
    (descr "5mm clear led")
    (tags led)
    (fp_text reference D3 (at 0 4) (layer F.SilkS))
    (fp_text value LED2 (at 0 -4) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 0 1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (model walter/indicators/led_5mm_clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_indicators:led_5mm_clear (layer F.Cu) (tedit 532D9A66)
    (at 129.286 68.072)
    (descr "5mm clear led")
    (tags led)
    (fp_text reference D4 (at 0 4) (layer F.SilkS))
    (fp_text value LED3 (at 0 -4) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 0 1.27) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad2)"))
    (model walter/indicators/led_5mm_clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mstbva_2,5-5-g-5,08 (layer F.Cu) (tedit 576DA4F9)
    (at 153.924 87.884 270)
    (descr "Terminal block 5 pins, Phoenix MSTBVA 2,5/5-G-5,08")
    (tags DEV)
    (fp_text reference P1 (at -15.748 0.889 270) (layer F.SilkS))
    (fp_text value sensor (at 0 6.604 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -10.16 0 270) (size 2.99974 2.99974) (drill 1.39954) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad7)"))
    (pad 4 thru_hole circle (at 5.08 0 270) (size 2.99974 2.99974) (drill 1.39954) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 2.99974 2.99974) (drill 1.39954) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P1-Pad5)"))
    (pad 3 thru_hole circle (at 0 0 270) (size 2.99974 2.99974) (drill 1.39954) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at -5.08 0 270) (size 2.99974 2.99974) (drill 1.39954) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad2)"))
    (model walter/conn_screw/mstbva_2,5-5-g-5,08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mstbva_2,5-2-g-5,08 (layer F.Cu) (tedit 576DA389)
    (at 132.969 94.869 270)
    (descr "Terminal block 2 pins, Phoenix MSTBVA 2,5/2-G-5,08")
    (tags DEV)
    (fp_text reference P2 (at -7.239 -2.54 360) (layer F.SilkS))
    (fp_text value "" (at 0 6.604 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.99974 2.99974) (drill 1.39954) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad8)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.99974 2.99974) (drill 1.39954) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad6)"))
    (model walter/conn_screw/mstbva_2,5-2-g-5,08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINHEAD1-3 (layer F.Cu) (tedit 0)
    (at 143.383 68.834)
    (attr virtual)
    (fp_text reference P3 (at 0.05 -3.8) (layer F.SilkS))
    (fp_text value relés (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.54 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad24)"))
    (pad 2 thru_hole oval (at 0 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad23)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad7)"))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 135.636 80.899)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(P1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 135.636 65.913)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(P1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 135.636 70.993)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(P1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 137.16 91.948 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(P1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 135.636 75.946)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 150.495 89.535 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 116.713 74.676 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 123.063 74.676 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 129.159 74.676 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 110.236 74.676 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_14-300 (layer F.Cu) (tedit 576DA4FE)
    (at 143.891 88.265 270)
    (descr "IC, DIL14 x 0,3\"")
    (tags DIL)
    (fp_text reference U1 (at 11.43 0.635 270) (layer F.SilkS))
    (fp_text value LM324AN (at -11.43 0 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at -7.62 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad13)"))
    (pad 2 thru_hole oval (at -5.08 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at -2.54 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R5-Pad2)"))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad5)"))
    (pad 5 thru_hole oval (at 2.54 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R5-Pad2)"))
    (pad 6 thru_hole oval (at 5.08 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P1-Pad5)"))
    (pad 7 thru_hole oval (at 7.62 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 7.62 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 5.08 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad4)"))
    (pad 10 thru_hole oval (at 2.54 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R5-Pad2)"))
    (pad 11 thru_hole oval (at 0 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad7)"))
    (pad 12 thru_hole oval (at -2.54 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R5-Pad2)"))
    (pad 13 thru_hole oval (at -5.08 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P1-Pad3)"))
    (pad 14 thru_hole oval (at -7.62 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad14)"))
    (model walter/pth_circuits/dil_14-300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 157.607 106.807) (end 160.147 104.267) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.607 109.347) (end 157.607 106.807) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.123 109.347) (end 157.607 109.347) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.091 109.347) (end 95.123 109.347) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.821 109.347) (end 93.091 109.347) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.694 109.22) (end 91.821 109.347) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.567 109.093) (end 91.694 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.567 107.188) (end 91.567 109.093) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.567 57.658) (end 91.567 107.188) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.567 56.134) (end 91.567 57.658) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.694 56.007) (end 91.567 56.134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.71 56.007) (end 91.694 56.007) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.321 56.007) (end 92.71 56.007) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.337 56.007) (end 155.321 56.007) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.607 57.277) (end 156.337 56.007) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.607 67.31) (end 157.607 57.277) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.607 68.707) (end 157.607 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.147 71.247) (end 157.607 68.707) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.147 104.267) (end 160.147 71.247) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text cleaps-tech@gmail.com (at 94.488 80.264 90) (layer F.SilkS))
  (gr_text "Level sensor" (at 111.252 95.885) (layer F.SilkS))
  (gr_text "CLEAPS-TECH\n" (at 112.141 88.773) (layer F.SilkS))
)
