| Nordic Thingy:52 v2.0.0

Data Structures | Macros | Typedefs | Functions
ble_tes.h File Reference

Go to the source code of this file.

## Data Structures

struct | ble_tes_init_t
| Thingy Environment Service initialization structure. More...
struct | ble_tes_s
| Thingy Environment Service structure. More...

## Macros

#define | BLE_TES_MAX_DATA_LEN (BLE_GATT_ATT_MTU_DEFAULT - 3)
#define | BLE_UUID_TES_SERVICE 0x0200

## Typedefs

typedef void(* | ble_tes_evt_handler_t) (ble_tes_t *p_tes, ble_tes_evt_type_t evt_type, uint8_t *p_data, uint16_t length)
| Thingy Environment Service event handler type.

## Functions

uint32_t | ble_tes_color_set (ble_tes_t *p_tes, ble_tes_color_t *p_data)
| Function for setting the color data. More...
uint32_t | ble_tes_gas_set (ble_tes_t *p_tes, ble_tes_gas_t *p_data)
| Function for setting the gas data. More...
uint32_t | ble_tes_humidity_set (ble_tes_t *p_tes, ble_tes_humidity_t *p_data)
| Function for setting the humidity. More...
uint32_t | ble_tes_init (ble_tes_t *p_tes, const ble_tes_init_t *p_tes_init)
| Function for initializing the Thingy Environment Service. More...
void | ble_tes_on_ble_evt (ble_tes_t *p_tes, ble_evt_t *p_ble_evt)
| Function for handling the Thingy Environment Service's BLE events. More...
uint32_t | ble_tes_pressure_set (ble_tes_t *p_tes, ble_tes_pressure_t *p_data)
| Function for setting the pressure. More...
uint32_t | ble_tes_temperature_set (ble_tes_t *p_tes, ble_tes_temperature_t *p_data)
| Function for setting the temperature. More...